{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["Search Tool","Products","Field Install Kits","Wiring","PS Products"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":13,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Search Tool","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Products","index":1,"n_rows":26428,"n_cols":9,"rows_kept":4500,"cut":true,"hidden":false,"merged":[],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["CI Code","Description","Product","PS Solution ","Mounting Options","Remote mount enclosure","Field Install Instruction","Remote Kit","In-Fixture Kit"]
[{"$f":"(LEFT((RIGHT(C2,7)),6))","v":"234X5X"},{"$f":"LEFT(C2,SEARCH(\"(CI-\",C2)-2)","v":"2ACL2 20L EZ1 LP830"},"2ACL2 20L EZ1 LP830 (CI-234X5X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233FUA","2ACL2 20L EZ1 LP835","2ACL2 20L EZ1 LP835 (CI-233FUA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233AJR","2ACL2 20L EZ1 LP840","2ACL2 20L EZ1 LP840 (CI-233AJR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234Y58","2ACL2 20L EZ1 LP840 N100","2ACL2 20L EZ1 LP840 N100 (CI-234Y58)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234L4W","2ACL2 20L EZ1 LP850","2ACL2 20L EZ1 LP850 (CI-234L4W)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["207J0W","2ACL2 33L D41 LP835 N100","2ACL2 33L D41 LP835 N100 (CI-207J0W)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["207L3L","2ACL2 33L D41 LP835 N100 SSQ","2ACL2 33L D41 LP835 N100 SSQ (CI-207L3L)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["207J0Y","2ACL2 33L D41 LP835 N80","2ACL2 33L D41 LP835 N80 (CI-207J0Y)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231XG6","2ACL2 33L EZ1 LP830","2ACL2 33L EZ1 LP830 (CI-231XG6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231RW8","2ACL2 33L EZ1 LP835","2ACL2 33L EZ1 LP835 (CI-231RW8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231L03","2ACL2 33L EZ1 LP835 N100","2ACL2 33L EZ1 LP835 N100 (CI-231L03)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231TAY","2ACL2 33L EZ1 LP840","2ACL2 33L EZ1 LP840 (CI-231TAY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233FU9","2ACL2 33L EZ1 LP840 N100","2ACL2 33L EZ1 LP840 N100 (CI-233FU9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234AVL","2ACL2 33L EZ1 LP840 N80","2ACL2 33L EZ1 LP840 N80 (CI-234AVL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234EK9","2ACL2 33L EZ1 LP840 NOM","2ACL2 33L EZ1 LP840 NOM (CI-234EK9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231RUG","2ACL2 33L EZ1 PWS1836 LP830","2ACL2 33L EZ1 PWS1836 LP830 (CI-231RUG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234H13","2ACL2 33L EZ1 PWS1836 LP835","2ACL2 33L EZ1 PWS1836 LP835 (CI-234H13)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233RH4","2ACL2 33L EZB LP835","2ACL2 33L EZB LP835 (CI-233RH4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231TWW","2ACL2 33L SLD LP830","2ACL2 33L SLD LP830 (CI-231TWW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231TWP","2ACL2 33L SLD LP840","2ACL2 33L SLD LP840 (CI-231TWP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["220PPF","2ACL2 35L D38 LP830 N100","2ACL2 35L D38 LP830 N100 (CI-220PPF)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["221M8E","2ACL2 35L D38 LP830 N80","2ACL2 35L D38 LP830 N80 (CI-221M8E)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["220VKJ","2ACL2 35L D38 LP830 NX","2ACL2 35L D38 LP830 NX (CI-220VKJ)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["219X2H","2ACL2 35L D38 LP835 BLD","2ACL2 35L D38 LP835 BLD (CI-219X2H)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["211HP5","2ACL2 35L D38 LP835 N100","2ACL2 35L D38 LP835 N100 (CI-211HP5)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["225YVF","2ACL2 35L D38 LP835 N100 NOM","2ACL2 35L D38 LP835 N100 NOM (CI-225YVF)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["211GXT","2ACL2 35L D38 LP835 N80","2ACL2 35L D38 LP835 N80 (CI-211GXT)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["212YN3","2ACL2 35L D38 LP835 NX","2ACL2 35L D38 LP835 NX (CI-212YN3)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["230VHT","2ACL2 35L D38 LP835 NX USPOM","2ACL2 35L D38 LP835 NX USPOM (CI-230VHT)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["216U53","2ACL2 35L D38 LP840 BLD","2ACL2 35L D38 LP840 BLD (CI-216U53)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["211GXG","2ACL2 35L D38 LP840 N100","2ACL2 35L D38 LP840 N100 (CI-211GXG)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["216HK1","2ACL2 35L D38 LP840 N100 NOM","2ACL2 35L D38 LP840 N100 NOM (CI-216HK1)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["215VTA","2ACL2 35L D38 LP840 N100 USPOM","2ACL2 35L D38 LP840 N100 USPOM (CI-215VTA)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["211A92","2ACL2 35L D38 LP840 N80","2ACL2 35L D38 LP840 N80 (CI-211A92)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["214TFF","2ACL2 35L D38 LP840 N80 USPOM","2ACL2 35L D38 LP840 N80 USPOM (CI-214TFF)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["213UYK","2ACL2 35L D38 LP840 NX","2ACL2 35L D38 LP840 NX (CI-213UYK)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["226W7E","2ACL2 35L D38 LP840 NX USPOM","2ACL2 35L D38 LP840 NX USPOM (CI-226W7E)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["224XTJ","2ACL2 35L D38 LP840 XPD","2ACL2 35L D38 LP840 XPD (CI-224XTJ)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["221M7Y","2ACL2 35L D38 LP850 BLD","2ACL2 35L D38 LP850 BLD (CI-221M7Y)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["215KX1","2ACL2 35L D38 LP850 N100","2ACL2 35L D38 LP850 N100 (CI-215KX1)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["218XLC","2ACL2 35L D38 LP850 N80","2ACL2 35L D38 LP850 N80 (CI-218XLC)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["215KL4","2ACL2 35L D38 LP850 NX","2ACL2 35L D38 LP850 NX (CI-215KL4)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["217LLC","2ACL2 35L D38 PWS1436 LP835 N100","2ACL2 35L D38 PWS1436 LP835 N100 (CI-217LLC)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["226N0U","2ACL2 35L D38 PWS1436 LP835 NX","2ACL2 35L D38 PWS1436 LP835 NX (CI-226N0U)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["220AEM","2ACL2 35L D38 PWS1836 LP835 N80","2ACL2 35L D38 PWS1836 LP835 N80 (CI-220AEM)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["228RVH","2ACL2 35L D38 PWS1836 LP835 NX","2ACL2 35L D38 PWS1836 LP835 NX (CI-228RVH)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["217N0K","2ACL2 35L D38 PWS1836 LP840 N100","2ACL2 35L D38 PWS1836 LP840 N100 (CI-217N0K)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["217UU1","2ACL2 35L D38 PWS1836 LP840 N80","2ACL2 35L D38 PWS1836 LP840 N80 (CI-217UU1)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["217E03","2ACL2 35L D38 PWS1836 LP840 NX","2ACL2 35L D38 PWS1836 LP840 NX (CI-217E03)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["218PW3","2ACL2 35L D38 PWS1836 LP850 NX","2ACL2 35L D38 PWS1836 LP850 NX (CI-218PW3)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["230TUV","2ACL2 35L D38 PWS1856LV LP835 NX RFD182823","2ACL2 35L D38 PWS1856LV LP835 NX RFD182823 (CI-230TUV)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["232N7V","2ACL2 40L EZ1 LP830","2ACL2 40L EZ1 LP830 (CI-232N7V)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232TH4","2ACL2 40L EZ1 LP830 N100","2ACL2 40L EZ1 LP830 N100 (CI-232TH4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232HWR","2ACL2 40L EZ1 LP835","2ACL2 40L EZ1 LP835 (CI-232HWR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233HVR","2ACL2 40L EZ1 LP835 N100","2ACL2 40L EZ1 LP835 N100 (CI-233HVR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234F2T","2ACL2 40L EZ1 LP840","2ACL2 40L EZ1 LP840 (CI-234F2T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232FFV","2ACL2 40L EZ1 LP840 N80","2ACL2 40L EZ1 LP840 N80 (CI-232FFV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231TAX","2ACL2 40L EZ1 LP850","2ACL2 40L EZ1 LP850 (CI-231TAX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232U9N","2ACL2 40L EZ1 PWS1836 LP835 N100","2ACL2 40L EZ1 PWS1836 LP835 N100 (CI-232U9N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231XJA","2ACL2 40L EZ1 PWS1836 LP850 N100","2ACL2 40L EZ1 PWS1836 LP850 N100 (CI-231XJA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234Y50","2ACL4 30L EZ1 LP840 N100","2ACL4 30L EZ1 LP840 N100 (CI-234Y50)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233AJ4","2ACL4 40L EZ1 LP835","2ACL4 40L EZ1 LP835 (CI-233AJ4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233TNA","2ACL4 40L EZ1 LP840","2ACL4 40L EZ1 LP840 (CI-233TNA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229P86","2ACL4 48L D50 LP830 N100","2ACL4 48L D50 LP830 N100 (CI-229P86)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C66,7)),6))","v":"227JY6"},{"$f":"LEFT(C66,SEARCH(\"(CI-\",C66)-2)","v":"2ACL4 48L D50 LP830 NX"},"2ACL4 48L D50 LP830 NX (CI-227JY6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["215G65","2ACL4 48L D50 LP835 BLD","2ACL4 48L D50 LP835 BLD (CI-215G65)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["212R0N","2ACL4 48L D50 LP835 N100","2ACL4 48L D50 LP835 N100 (CI-212R0N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["212UA8","2ACL4 48L D50 LP835 N80","2ACL4 48L D50 LP835 N80 (CI-212UA8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["214TF8","2ACL4 48L D50 LP835 NX","2ACL4 48L D50 LP835 NX (CI-214TF8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230VHL","2ACL4 48L D50 LP835 NX USPOM","2ACL4 48L D50 LP835 NX USPOM (CI-230VHL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["207KWN","2ACL4 48L D50 LP840 N100","2ACL4 48L D50 LP840 N100 (CI-207KWN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["219V1X","2ACL4 48L D50 LP840 N100 RFD145437","2ACL4 48L D50 LP840 N100 RFD145437 (CI-219V1X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["212U98","2ACL4 48L D50 LP840 N80","2ACL4 48L D50 LP840 N80 (CI-212U98)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["214UT1","2ACL4 48L D50 LP840 NX","2ACL4 48L D50 LP840 NX (CI-214UT1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226W59","2ACL4 48L D50 LP840 NX USPOM","2ACL4 48L D50 LP840 NX USPOM (CI-226W59)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["213YP8","2ACL4 48L D50 LP850 N100","2ACL4 48L D50 LP850 N100 (CI-213YP8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["216K2W","2ACL4 48L D50 LP850 NX","2ACL4 48L D50 LP850 NX (CI-216K2W)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225E4C","2ACL4 48L D50 PWS1836 LP840 NX","2ACL4 48L D50 PWS1836 LP840 NX (CI-225E4C)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225HHW","2ACL4 48L D50 PWS1836 LP840 NX USPOM","2ACL4 48L D50 PWS1836 LP840 NX USPOM (CI-225HHW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231RW3","2ACL4 48L EZ1 LP830","2ACL4 48L EZ1 LP830 (CI-231RW3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232T9E","2ACL4 48L EZ1 LP830 N100","2ACL4 48L EZ1 LP830 N100 (CI-232T9E)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231YF9","2ACL4 48L EZ1 LP835","2ACL4 48L EZ1 LP835 (CI-231YF9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231NG2","2ACL4 48L EZ1 LP835 N100","2ACL4 48L EZ1 LP835 N100 (CI-231NG2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231LY5","2ACL4 48L EZ1 LP840","2ACL4 48L EZ1 LP840 (CI-231LY5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231PCK","2ACL4 48L EZ1 LP840 N80","2ACL4 48L EZ1 LP840 N80 (CI-231PCK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234J51","2ACL4 48L EZ1 LP850","2ACL4 48L EZ1 LP850 (CI-234J51)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234L9L","2ACL4 48L EZ1 PWS1836 LP835","2ACL4 48L EZ1 PWS1836 LP835 (CI-234L9L)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233JUH","2ACL4 48L SLD LP835","2ACL4 48L SLD LP835 (CI-233JUH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233HHJ","2ACL4 60L EZ1 LP840","2ACL4 60L EZ1 LP840 (CI-233HHJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234AMA","2ACL4 60L EZ1 PWS1836 LP840","2ACL4 60L EZ1 PWS1836 LP840 (CI-234AMA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232HW1","2ACL4 72L EZ1 LP840","2ACL4 72L EZ1 LP840 (CI-232HW1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232TLL","2ACL4 72L EZ1 LP850","2ACL4 72L EZ1 LP850 (CI-232TLL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234AU4","2ACL4 72L EZ1 PWS1836 LP840","2ACL4 72L EZ1 PWS1836 LP840 (CI-234AU4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238E6R","2ACL2 20L EZ1 LP830 CP","2ACL2 20L EZ1 LP830 CP (CI-238E6R)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238AY3","2ACL2 20L EZ1 LP835 N100","2ACL2 20L EZ1 LP835 N100 (CI-238AY3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240RY0","2ACL2 20L EZ1 LP835 N80","2ACL2 20L EZ1 LP835 N80 (CI-240RY0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239WV9","2ACL2 20L EZ1 LP840 N80","2ACL2 20L EZ1 LP840 N80 (CI-239WV9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239N2P","2ACL2 33L 120 EZ1 GLR LP840","2ACL2 33L 120 EZ1 GLR LP840 (CI-239N2P)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236JH0","2ACL2 33L 120 EZ1 LP835 CS1WL10 SSQ","2ACL2 33L 120 EZ1 LP835 CS1WL10 SSQ (CI-236JH0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["210TG6","2ACL2 33L D41 LP835 N100 CS1WL10 SSQ","2ACL2 33L D41 LP835 N100 CS1WL10 SSQ (CI-210TG6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239KMG","2ACL2 33L EZ1 LP830 N100","2ACL2 33L EZ1 LP830 N100 (CI-239KMG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235MFN","2ACL2 33L EZ1 LP835","2ACL2 33L EZ1 LP835 (CI-235MFN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240VXU","2ACL2 33L EZ1 LP835 CP N100","2ACL2 33L EZ1 LP835 CP N100 (CI-240VXU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235KX5","2ACL2 33L EZ1 LP835 N80","2ACL2 33L EZ1 LP835 N80 (CI-235KX5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239Y0L","2ACL2 33L EZ1 LP835 USPOM","2ACL2 33L EZ1 LP835 USPOM (CI-239Y0L)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241LEF","2ACL2 33L EZ1 LP840 N80EMG","2ACL2 33L EZ1 LP840 N80EMG (CI-241LEF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241LG1","2ACL2 33L EZ1 LP840 N80EMG USPOM","2ACL2 33L EZ1 LP840 N80EMG USPOM (CI-241LG1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238NNN","2ACL2 33L EZ1 LP840 USPOM","2ACL2 33L EZ1 LP840 USPOM (CI-238NNN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236P96","2ACL2 33L EZ1 LP850","2ACL2 33L EZ1 LP850 (CI-236P96)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241FYJ","2ACL2 33L EZ1 PWS1836 LP840 N80","2ACL2 33L EZ1 PWS1836 LP840 N80 (CI-241FYJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239CFY","2ACL2 33L EZ1 PWS1856LV LP835","2ACL2 33L EZ1 PWS1856LV LP835 (CI-239CFY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237H28","2ACL2 33L SLD LP835","2ACL2 33L SLD LP835 (CI-237H28)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["224APR","2ACL2 35L D38 LP830 N100EMG","2ACL2 35L D38 LP830 N100EMG (CI-224APR)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["211VVA","2ACL2 35L D38 LP835 N100EMG","2ACL2 35L D38 LP835 N100EMG (CI-211VVA)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["213GR9","2ACL2 35L D38 LP835 N80EMG","2ACL2 35L D38 LP835 N80EMG (CI-213GR9)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["214J65","2ACL2 35L D38 LP840 N100EMG","2ACL2 35L D38 LP840 N100EMG (CI-214J65)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["218LYJ","2ACL2 35L D38 LP840 N80EMG","2ACL2 35L D38 LP840 N80EMG (CI-218LYJ)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["214TFH","2ACL2 35L D38 LP840 N80EMG USPOM","2ACL2 35L D38 LP840 N80EMG USPOM (CI-214TFH)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["229ELE","2ACL2 35L D38 PWS1836 LP830 NX","2ACL2 35L D38 PWS1836 LP830 NX (CI-229ELE)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["217N0M","2ACL2 35L D38 PWS1836 LP840 N100EMG","2ACL2 35L D38 PWS1836 LP840 N100EMG (CI-217N0M)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["240XN4","2ACL2 40L EZ1 LP835 N100EMG","2ACL2 40L EZ1 LP835 N100EMG (CI-240XN4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245H4W","2ACL2 40L EZ1 LP835 USPOM","2ACL2 40L EZ1 LP835 USPOM (CI-245H4W)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236TP0","2ACL2 40L EZ1 LP840 N100","2ACL2 40L EZ1 LP840 N100 (CI-236TP0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232AMM","2ACL2 40L EZ1 LP840 NOM","2ACL2 40L EZ1 LP840 NOM (CI-232AMM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240FH0","2ACL2 40L EZ1 PWS1836 LP835","2ACL2 40L EZ1 PWS1836 LP835 (CI-240FH0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236VGL","2ACL2 40L EZ1 PWS1836 LP835 USPOM","2ACL2 40L EZ1 PWS1836 LP835 USPOM (CI-236VGL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245WFX","2ACL2 40L EZB LP835","2ACL2 40L EZB LP835 (CI-245WFX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231WVU","2ACL2 40L EZB LP835 N100","2ACL2 40L EZB LP835 N100 (CI-231WVU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C130,7)),6))","v":"245V94"},{"$f":"LEFT(C130,SEARCH(\"(CI-\",C130)-2)","v":"2ACL2 40L EZB LP840"},"2ACL2 40L EZB LP840 (CI-245V94)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238P4U","2ACL4 30L EZ1 LP830","2ACL4 30L EZ1 LP830 (CI-238P4U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234R98","2ACL4 30L EZ1 LP835","2ACL4 30L EZ1 LP835 (CI-234R98)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238V4J","2ACL4 30L EZ1 LP835 N100","2ACL4 30L EZ1 LP835 N100 (CI-238V4J)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238RCR","2ACL4 30L EZ1 LP840","2ACL4 30L EZ1 LP840 (CI-238RCR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239KWA","2ACL4 30L EZ1 LP840 NOM","2ACL4 30L EZ1 LP840 NOM (CI-239KWA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241LEN","2ACL4 40L EZ1 LP830 N100","2ACL4 40L EZ1 LP830 N100 (CI-241LEN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245UYN","2ACL4 40L EZ1 LP835 CP","2ACL4 40L EZ1 LP835 CP (CI-245UYN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239LV5","2ACL4 40L EZ1 LP835 N100","2ACL4 40L EZ1 LP835 N100 (CI-239LV5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238A4X","2ACL4 40L EZ1 LP840 N100","2ACL4 40L EZ1 LP840 N100 (CI-238A4X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235V4P","2ACL4 40L EZ1 LP840 N80","2ACL4 40L EZ1 LP840 N80 (CI-235V4P)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["247V2M","2ACL4 40L EZ1 PWS1836 LP835","2ACL4 40L EZ1 PWS1836 LP835 (CI-247V2M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238CY7","2ACL4 40L EZ1 PWS1836 LP840","2ACL4 40L EZ1 PWS1836 LP840 (CI-238CY7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239AT6","2ACL4 40L EZB LP835 CP N100","2ACL4 40L EZB LP835 CP N100 (CI-239AT6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237WM8","2ACL4 40L EZB LP840","2ACL4 40L EZB LP840 (CI-237WM8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238MFX","2ACL4 40L EZB LP840 N100","2ACL4 40L EZB LP840 N100 (CI-238MFX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239N30","2ACL4 48L 120 EZ1 GLR LP840","2ACL4 48L 120 EZ1 GLR LP840 (CI-239N30)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["214Y5Y","2ACL4 48L D50 LP835 N100EMG","2ACL4 48L D50 LP835 N100EMG (CI-214Y5Y)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225RPX","2ACL4 48L D50 LP835 N80EMG","2ACL4 48L D50 LP835 N80EMG (CI-225RPX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["219U9H","2ACL4 48L D50 LP840 N100EMG","2ACL4 48L D50 LP840 N100EMG (CI-219U9H)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237MAA","2ACL4 48L EZ1 LP835 N80","2ACL4 48L EZ1 LP835 N80 (CI-237MAA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236C62","2ACL4 48L EZ1 LP840 N100","2ACL4 48L EZ1 LP840 N100 (CI-236C62)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239HFP","2ACL4 48L EZ1 LP840 NOM","2ACL4 48L EZ1 LP840 NOM (CI-239HFP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237WM0","2ACL4 48L EZB LP840","2ACL4 48L EZB LP840 (CI-237WM0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240N2Y","2ACL4 48L EZB PWS1856LV LP835","2ACL4 48L EZB PWS1856LV LP835 (CI-240N2Y)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238CR0","2ACL4 48L SLD LP840","2ACL4 48L SLD LP840 (CI-238CR0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237H24","2ACL4 60L EDB LP850","2ACL4 60L EDB LP850 (CI-237H24)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235GLR","2ACL4 60L EZ1 LP830","2ACL4 60L EZ1 LP830 (CI-235GLR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237XUP","2ACL4 60L EZ1 LP835","2ACL4 60L EZ1 LP835 (CI-237XUP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238KTU","2ACL4 60L EZ1 LP840 N100","2ACL4 60L EZ1 LP840 N100 (CI-238KTU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["247U7X","2ACL4 60L EZB LP840","2ACL4 60L EZB LP840 (CI-247U7X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240N9W","2ACL4 72L EZ1 LP835","2ACL4 72L EZ1 LP835 (CI-240N9W)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237VEM","2ACL4 72L EZ1 LP835 N100","2ACL4 72L EZ1 LP835 N100 (CI-237VEM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233P02","2ALL2 20L EZ1 LP830","2ALL2 20L EZ1 LP830 (CI-233P02)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232UA8","2ALL2 20L EZ1 LP835","2ALL2 20L EZ1 LP835 (CI-232UA8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232HL1","2ALL2 20L EZ1 LP840","2ALL2 20L EZ1 LP840 (CI-232HL1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233H87","2ALL2 20L EZ1 PWS1836 LP835","2ALL2 20L EZ1 PWS1836 LP835 (CI-233H87)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234NVM","2ALL2 20L EZB LP830","2ALL2 20L EZB LP830 (CI-234NVM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230GVT","2ALL2 30L EZ1 LP830 RFD180942","2ALL2 30L EZ1 LP830 RFD180942 (CI-230GVT)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["233C8F","2ALL2 33L EZ1 LP830","2ALL2 33L EZ1 LP830 (CI-233C8F)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234XNX","2ALL2 33L EZ1 LP830 N80","2ALL2 33L EZ1 LP830 N80 (CI-234XNX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231U02","2ALL2 33L EZ1 LP835","2ALL2 33L EZ1 LP835 (CI-231U02)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232HE2","2ALL2 33L EZ1 LP835 N100","2ALL2 33L EZ1 LP835 N100 (CI-232HE2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232PJY","2ALL2 33L EZ1 LP835 N80","2ALL2 33L EZ1 LP835 N80 (CI-232PJY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234PYX","2ALL2 33L EZ1 LP835 USPOM","2ALL2 33L EZ1 LP835 USPOM (CI-234PYX)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MR9"]
["231TAV","2ALL2 33L EZ1 LP840","2ALL2 33L EZ1 LP840 (CI-231TAV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232XG7","2ALL2 33L EZ1 LP840 N100","2ALL2 33L EZ1 LP840 N100 (CI-232XG7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232UA2","2ALL2 33L EZ1 LP840 N80","2ALL2 33L EZ1 LP840 N80 (CI-232UA2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233EJR","2ALL2 33L EZ1 PWS1836 LP835","2ALL2 33L EZ1 PWS1836 LP835 (CI-233EJR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233Y72","2ALL2 33L EZ1 PWS1836 LP835 N100","2ALL2 33L EZ1 PWS1836 LP835 N100 (CI-233Y72)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232EGH","2ALL2 33L EZ1 PWS1836 LP840","2ALL2 33L EZ1 PWS1836 LP840 (CI-232EGH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232T6X","2ALL2 33L EZ1 PWS1856LV LP835","2ALL2 33L EZ1 PWS1856LV LP835 (CI-232T6X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233J0U","2ALL2 33L EZB LP840","2ALL2 33L EZB LP840 (CI-233J0U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228WTG","2ALL2 37L D37 LP830 BLD","2ALL2 37L D37 LP830 BLD (CI-228WTG)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["228YKR","2ALL2 37L D37 LP830 N100","2ALL2 37L D37 LP830 N100 (CI-228YKR)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["223KK5","2ALL2 37L D37 LP830 N100 RFD159840","2ALL2 37L D37 LP830 N100 RFD159840 (CI-223KK5)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["226WNT","2ALL2 37L D37 LP830 N80","2ALL2 37L D37 LP830 N80 (CI-226WNT)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["222K6N","2ALL2 37L D37 LP830 N80 RFD152107","2ALL2 37L D37 LP830 N80 RFD152107 (CI-222K6N)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["225E7K","2ALL2 37L D37 LP830 NX","2ALL2 37L D37 LP830 NX (CI-225E7K)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["218E9P","2ALL2 37L D37 LP835 BLD","2ALL2 37L D37 LP835 BLD (CI-218E9P)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["225H7U","2ALL2 37L D37 LP835 CP NX","2ALL2 37L D37 LP835 CP NX (CI-225H7U)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["224M5L","2ALL2 37L D37 LP835 CP NX RFD164195","2ALL2 37L D37 LP835 CP NX RFD164195 (CI-224M5L)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["215NKP","2ALL2 37L D37 LP835 N100","2ALL2 37L D37 LP835 N100 (CI-215NKP)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["214M41","2ALL2 37L D37 LP835 N80","2ALL2 37L D37 LP835 N80 (CI-214M41)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
[{"$f":"(LEFT((RIGHT(C194,7)),6))","v":"216MFT"},{"$f":"LEFT(C194,SEARCH(\"(CI-\",C194)-2)","v":"2ALL2 37L D37 LP835 NX"},"2ALL2 37L D37 LP835 NX (CI-216MFT)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["218JF1","2ALL2 37L D37 LP835 NX PWS1836","2ALL2 37L D37 LP835 NX PWS1836 (CI-218JF1)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["225CH4","2ALL2 37L D37 LP835 NX PWS1856LV","2ALL2 37L D37 LP835 NX PWS1856LV (CI-225CH4)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["227EMW","2ALL2 37L D37 LP835 NX RFD172463","2ALL2 37L D37 LP835 NX RFD172463 (CI-227EMW)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["223RWV","2ALL2 37L D37 LP835 NX USPOM","2ALL2 37L D37 LP835 NX USPOM (CI-223RWV)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["222MRK","2ALL2 37L D37 LP840 BLD","2ALL2 37L D37 LP840 BLD (CI-222MRK)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["224LCA","2ALL2 37L D37 LP840 BLD USPOM","2ALL2 37L D37 LP840 BLD USPOM (CI-224LCA)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["224V37","2ALL2 37L D37 LP840 CP NX","2ALL2 37L D37 LP840 CP NX (CI-224V37)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["216LAH","2ALL2 37L D37 LP840 N100","2ALL2 37L D37 LP840 N100 (CI-216LAH)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["217RC4","2ALL2 37L D37 LP840 N80","2ALL2 37L D37 LP840 N80 (CI-217RC4)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["221UV4","2ALL2 37L D37 LP840 N80 USPOM","2ALL2 37L D37 LP840 N80 USPOM (CI-221UV4)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["215P6J","2ALL2 37L D37 LP840 NX","2ALL2 37L D37 LP840 NX (CI-215P6J)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["227EMN","2ALL2 37L D37 LP840 NX RFD172463","2ALL2 37L D37 LP840 NX RFD172463 (CI-227EMN)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["231N1L","2ALL2 37L D37 LP840 NX USPOM","2ALL2 37L D37 LP840 NX USPOM (CI-231N1L)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["218RMV","2ALL2 37L D37 LP850 N100","2ALL2 37L D37 LP850 N100 (CI-218RMV)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["216N19","2ALL2 37L D37 LP850 N80","2ALL2 37L D37 LP850 N80 (CI-216N19)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["222HU5","2ALL2 37L D37 LP850 NX","2ALL2 37L D37 LP850 NX (CI-222HU5)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["231PW2","2ALL2 37L D37 LP935 BLD RFD181989","2ALL2 37L D37 LP935 BLD RFD181989 (CI-231PW2)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["228N9A","2ALL2 37L D37 PWS1436 LP835 NX","2ALL2 37L D37 PWS1436 LP835 NX (CI-228N9A)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["225ARJ","2ALL2 37L D37 PWS1836 LP835 N100","2ALL2 37L D37 PWS1836 LP835 N100 (CI-225ARJ)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["229G3M","2ALL2 37L D37 PWS1836 LP835 N80","2ALL2 37L D37 PWS1836 LP835 N80 (CI-229G3M)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["222V9L","2ALL2 37L D37 PWS1836 LP835 NX","2ALL2 37L D37 PWS1836 LP835 NX (CI-222V9L)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["224R0R","2ALL2 37L D37 PWS1836 LP840 N100","2ALL2 37L D37 PWS1836 LP840 N100 (CI-224R0R)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["231H6K","2ALL2 37L D37 PWS1836 LP840 N80","2ALL2 37L D37 PWS1836 LP840 N80 (CI-231H6K)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["225JVG","2ALL2 37L D37 PWS1836 LP840 NX","2ALL2 37L D37 PWS1836 LP840 NX (CI-225JVG)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["223H42","2ALL2 37L D37 PWS1856 LP835 NX","2ALL2 37L D37 PWS1856 LP835 NX (CI-223H42)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["224F9N","2ALL2 37L D37 PWS1856LV LP835 NX RFD162427","2ALL2 37L D37 PWS1856LV LP835 NX RFD162427 (CI-224F9N)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["234N44","2ALL2 40L 120 EZ1 GLR LP835","2ALL2 40L 120 EZ1 GLR LP835 (CI-234N44)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231XMA","2ALL2 40L EZ1 LP830","2ALL2 40L EZ1 LP830 (CI-231XMA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232HWY","2ALL2 40L EZ1 LP830 N100","2ALL2 40L EZ1 LP830 N100 (CI-232HWY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231RA0","2ALL2 40L EZ1 LP835","2ALL2 40L EZ1 LP835 (CI-231RA0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231NHE","2ALL2 40L EZ1 LP835 N100","2ALL2 40L EZ1 LP835 N100 (CI-231NHE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231WKW","2ALL2 40L EZ1 LP835 N100 RFD185489","2ALL2 40L EZ1 LP835 N100 RFD185489 (CI-231WKW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231WF9","2ALL2 40L EZ1 LP835 N100 RFD185493","2ALL2 40L EZ1 LP835 N100 RFD185493 (CI-231WF9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231TYW","2ALL2 40L EZ1 LP835 N80","2ALL2 40L EZ1 LP835 N80 (CI-231TYW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231T2V","2ALL2 40L EZ1 LP840","2ALL2 40L EZ1 LP840 (CI-231T2V)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231MNC","2ALL2 40L EZ1 LP840 N100","2ALL2 40L EZ1 LP840 N100 (CI-231MNC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231T2K","2ALL2 40L EZ1 LP840 N80","2ALL2 40L EZ1 LP840 N80 (CI-231T2K)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232RYT","2ALL2 40L EZ1 LP840 USPOM","2ALL2 40L EZ1 LP840 USPOM (CI-232RYT)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MR9"]
["231T2M","2ALL2 40L EZ1 LP850","2ALL2 40L EZ1 LP850 (CI-231T2M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232RJL","2ALL2 40L EZ1 LP850 N100","2ALL2 40L EZ1 LP850 N100 (CI-232RJL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234AAX","2ALL2 40L EZ1 LP850 N80","2ALL2 40L EZ1 LP850 N80 (CI-234AAX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231N58","2ALL2 40L EZ1 PWS1836 LP835","2ALL2 40L EZ1 PWS1836 LP835 (CI-231N58)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232EGL","2ALL2 40L EZ1 PWS1836 LP840","2ALL2 40L EZ1 PWS1836 LP840 (CI-232EGL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232AUN","2ALL2 40L EZ1 PWS1836 LP840 N80","2ALL2 40L EZ1 PWS1836 LP840 N80 (CI-232AUN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233FRF","2ALL2 40L EZ1 PWS1846 LP835","2ALL2 40L EZ1 PWS1846 LP835 (CI-233FRF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232VYC","2ALL2 40L EZ1 PWS1856LV LP835","2ALL2 40L EZ1 PWS1856LV LP835 (CI-232VYC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232F3V","2ALL2 40L EZB LP835","2ALL2 40L EZB LP835 (CI-232F3V)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231WUL","2ALL2 40L EZB LP835 N100","2ALL2 40L EZB LP835 N100 (CI-231WUL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234M2T","2ALL2 40L EZB LP840","2ALL2 40L EZB LP840 (CI-234M2T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232CR8","2ALL2 CTRF 20L EZ1 LP835","2ALL2 CTRF 20L EZ1 LP835 (CI-232CR8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232VLN","2ALL2 CTRF 20L EZ1 LP835 N100","2ALL2 CTRF 20L EZ1 LP835 N100 (CI-232VLN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232YPG","2ALL2 CTRF 20L EZ1 LP840","2ALL2 CTRF 20L EZ1 LP840 (CI-232YPG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232CPE","2ALL2 CTRF 33L EZ1 LP835","2ALL2 CTRF 33L EZ1 LP835 (CI-232CPE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232VK5","2ALL2 CTRF 33L EZ1 LP835 N100","2ALL2 CTRF 33L EZ1 LP835 N100 (CI-232VK5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232W20","2ALL2 CTRF 33L EZ1 LP840","2ALL2 CTRF 33L EZ1 LP840 (CI-232W20)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234F3R","2ALL2 CTRF 33L EZ1 PWS1836 LP835","2ALL2 CTRF 33L EZ1 PWS1836 LP835 (CI-234F3R)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229XC1","2ALL2 CTRF 40L EXA1 LP840","2ALL2 CTRF 40L EXA1 LP840 (CI-229XC1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231KHW","2ALL2 CTRF 40L EZ1 LP835","2ALL2 CTRF 40L EZ1 LP835 (CI-231KHW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234AXM","2ALL2 CTRF 40L EZ1 LP835 N100","2ALL2 CTRF 40L EZ1 LP835 N100 (CI-234AXM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232JX5","2ALL2 CTRF 40L EZ1 LP840","2ALL2 CTRF 40L EZ1 LP840 (CI-232JX5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229XAY","2ALL2 CTRF 40L EZ1 LP840 N100","2ALL2 CTRF 40L EZ1 LP840 N100 (CI-229XAY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232ARF","2ALL2 CTRF 40L EZ1 LP840 N80","2ALL2 CTRF 40L EZ1 LP840 N80 (CI-232ARF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231Y3T","2ALL2 CTRF 40L EZB LP840","2ALL2 CTRF 40L EZB LP840 (CI-231Y3T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C258,7)),6))","v":"233RW6"},{"$f":"LEFT(C258,SEARCH(\"(CI-\",C258)-2)","v":"2ALL2 CTRF 40L SLD PWS1846 LP835"},"2ALL2 CTRF 40L SLD PWS1846 LP835 (CI-233RW6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228HP2","2ALL4 22L EZ1 LP835 N80 RFD174571","2ALL4 22L EZ1 LP835 N80 RFD174571 (CI-228HP2)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["232VT3","2ALL4 30L EZ1 LP830","2ALL4 30L EZ1 LP830 (CI-232VT3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232AH1","2ALL4 30L EZ1 LP835","2ALL4 30L EZ1 LP835 (CI-232AH1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233R2X","2ALL4 30L EZ1 LP840","2ALL4 30L EZ1 LP840 (CI-233R2X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234K98","2ALL4 40L EZ1 LP830 N100","2ALL4 40L EZ1 LP830 N100 (CI-234K98)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232AKR","2ALL4 40L EZ1 LP835","2ALL4 40L EZ1 LP835 (CI-232AKR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234G50","2ALL4 40L EZ1 LP835 N100","2ALL4 40L EZ1 LP835 N100 (CI-234G50)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231W0U","2ALL4 40L EZ1 LP840","2ALL4 40L EZ1 LP840 (CI-231W0U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233NKC","2ALL4 40L EZ1 LP840 N80","2ALL4 40L EZ1 LP840 N80 (CI-233NKC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234C54","2ALL4 40L SLD LP835","2ALL4 40L SLD LP835 (CI-234C54)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234X6A","2ALL4 40L SLD LP840","2ALL4 40L SLD LP840 (CI-234X6A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234N3Y","2ALL4 48L 120 EZ1 GLR LP835","2ALL4 48L 120 EZ1 GLR LP835 (CI-234N3Y)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231XME","2ALL4 48L EZ1 LP830","2ALL4 48L EZ1 LP830 (CI-231XME)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231R9R","2ALL4 48L EZ1 LP835","2ALL4 48L EZ1 LP835 (CI-231R9R)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232K34","2ALL4 48L EZ1 LP835 CP","2ALL4 48L EZ1 LP835 CP (CI-232K34)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231NH8","2ALL4 48L EZ1 LP835 N100","2ALL4 48L EZ1 LP835 N100 (CI-231NH8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231WK8","2ALL4 48L EZ1 LP835 N100 RFD185490","2ALL4 48L EZ1 LP835 N100 RFD185490 (CI-231WK8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231WG6","2ALL4 48L EZ1 LP835 N100 RFD185494","2ALL4 48L EZ1 LP835 N100 RFD185494 (CI-231WG6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231TXP","2ALL4 48L EZ1 LP835 N80","2ALL4 48L EZ1 LP835 N80 (CI-231TXP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232CV8","2ALL4 48L EZ1 LP835 USPOM UAL","2ALL4 48L EZ1 LP835 USPOM UAL (CI-232CV8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231NMF","2ALL4 48L EZ1 LP840","2ALL4 48L EZ1 LP840 (CI-231NMF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231NHG","2ALL4 48L EZ1 LP840 N100","2ALL4 48L EZ1 LP840 N100 (CI-231NHG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231R9M","2ALL4 48L EZ1 LP840 N80","2ALL4 48L EZ1 LP840 N80 (CI-231R9M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232YPF","2ALL4 48L EZ1 LP840 USPOM","2ALL4 48L EZ1 LP840 USPOM (CI-232YPF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231Y1J","2ALL4 48L EZ1 LP850","2ALL4 48L EZ1 LP850 (CI-231Y1J)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232XX4","2ALL4 48L EZB LP835","2ALL4 48L EZB LP835 (CI-232XX4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234M2K","2ALL4 48L EZB LP840","2ALL4 48L EZB LP840 (CI-234M2K)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234V96","2ALL4 48L EZB PWS1836 LP835","2ALL4 48L EZB PWS1836 LP835 (CI-234V96)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234FWE","2ALL4 48L EZB PWS1856LV LP840","2ALL4 48L EZB PWS1856LV LP840 (CI-234FWE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232F4L","2ALL4 48L SLD LP835","2ALL4 48L SLD LP835 (CI-232F4L)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232PN9","2ALL4 48L SLD LP840","2ALL4 48L SLD LP840 (CI-232PN9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233M1L","2ALL4 48L SLD PWS1836 LP835","2ALL4 48L SLD PWS1836 LP835 (CI-233M1L)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233R40","2ALL4 48L SLD PWS1846 LP835","2ALL4 48L SLD PWS1846 LP835 (CI-233R40)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233X33","2ALL4 48L SLD PWS1846 LP850","2ALL4 48L SLD PWS1846 LP850 (CI-233X33)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230W6W","2ALL4 49L 120 D50 GLR LP835 NX USPOM","2ALL4 49L 120 D50 GLR LP835 NX USPOM (CI-230W6W)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["227VPV","2ALL4 49L 120 D50 GLR LP840 BLD","2ALL4 49L 120 D50 GLR LP840 BLD (CI-227VPV)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["228HLR","2ALL4 49L D50 277 LP835 NX QFC211GA RFD174622","2ALL4 49L D50 277 LP835 NX QFC211GA RFD174622 (CI-228HLR)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["216HH8","2ALL4 49L D50 LP830 N100  RFD120461","2ALL4 49L D50 LP830 N100  RFD120461 (CI-216HH8)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["218RMP","2ALL4 49L D50 LP830 N100 RFD139804","2ALL4 49L D50 LP830 N100 RFD139804 (CI-218RMP)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["223KK2","2ALL4 49L D50 LP830 N100 RFD159839","2ALL4 49L D50 LP830 N100 RFD159839 (CI-223KK2)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["227MUV","2ALL4 49L D50 LP830 NX","2ALL4 49L D50 LP830 NX (CI-227MUV)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["220RAG","2ALL4 49L D50 LP835 BLD","2ALL4 49L D50 LP835 BLD (CI-220RAG)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["215TYL","2ALL4 49L D50 LP835 N100","2ALL4 49L D50 LP835 N100 (CI-215TYL)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["214M4E","2ALL4 49L D50 LP835 N80","2ALL4 49L D50 LP835 N80 (CI-214M4E)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["215N5E","2ALL4 49L D50 LP835 NX","2ALL4 49L D50 LP835 NX (CI-215N5E)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["229YMC","2ALL4 49L D50 LP835 NX UAL USPOM","2ALL4 49L D50 LP835 NX UAL USPOM (CI-229YMC)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["223RXG","2ALL4 49L D50 LP835 NX USPOM","2ALL4 49L D50 LP835 NX USPOM (CI-223RXG)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["220W5J","2ALL4 49L D50 LP840 BLD","2ALL4 49L D50 LP840 BLD (CI-220W5J)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["224LCE","2ALL4 49L D50 LP840 BLD USPOM","2ALL4 49L D50 LP840 BLD USPOM (CI-224LCE)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["224V3E","2ALL4 49L D50 LP840 CP NX","2ALL4 49L D50 LP840 CP NX (CI-224V3E)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["215T7U","2ALL4 49L D50 LP840 N100","2ALL4 49L D50 LP840 N100 (CI-215T7U)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["216A2Y","2ALL4 49L D50 LP840 N80","2ALL4 49L D50 LP840 N80 (CI-216A2Y)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["216G6L","2ALL4 49L D50 LP840 NX","2ALL4 49L D50 LP840 NX (CI-216G6L)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["224LCC","2ALL4 49L D50 LP840 NX USPOM","2ALL4 49L D50 LP840 NX USPOM (CI-224LCC)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["216RWY","2ALL4 49L D50 LP850 N100","2ALL4 49L D50 LP850 N100 (CI-216RWY)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["228NNN","2ALL4 49L D50 LP850 N80","2ALL4 49L D50 LP850 N80 (CI-228NNN)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["217XHK","2ALL4 49L D50 LP850 NX","2ALL4 49L D50 LP850 NX (CI-217XHK)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["222YHF","2ALL4 49L D50 PWS1836 LP835 N100","2ALL4 49L D50 PWS1836 LP835 N100 (CI-222YHF)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["227K18","2ALL4 49L D50 PWS1836 LP835 N80","2ALL4 49L D50 PWS1836 LP835 N80 (CI-227K18)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["222V9P","2ALL4 49L D50 PWS1836 LP835 NX","2ALL4 49L D50 PWS1836 LP835 NX (CI-222V9P)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["228R4P","2ALL4 49L D50 PWS1836 LP840 N100","2ALL4 49L D50 PWS1836 LP840 N100 (CI-228R4P)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["231GWX","2ALL4 49L D50 PWS1836 LP840 N80","2ALL4 49L D50 PWS1836 LP840 N80 (CI-231GWX)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["226KYT","2ALL4 49L D50 PWS1836 LP840 NX","2ALL4 49L D50 PWS1836 LP840 NX (CI-226KYT)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
[{"$f":"(LEFT((RIGHT(C322,7)),6))","v":"226VEF"},{"$f":"LEFT(C322,SEARCH(\"(CI-\",C322)-2)","v":"2ALL4 49L D50 PWS1846 LP840 BLD"},"2ALL4 49L D50 PWS1846 LP840 BLD (CI-226VEF)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["234N4M","2ALL4 60L 120 EZ1 GLR LP835","2ALL4 60L 120 EZ1 GLR LP835 (CI-234N4M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226WAL","2ALL4 60L D60 LP840 NX RFD169891","2ALL4 60L D60 LP840 NX RFD169891 (CI-226WAL)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["234C4C","2ALL4 60L EZ1 LP830","2ALL4 60L EZ1 LP830 (CI-234C4C)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231TXT","2ALL4 60L EZ1 LP835","2ALL4 60L EZ1 LP835 (CI-231TXT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234MM2","2ALL4 60L EZ1 LP835 N100","2ALL4 60L EZ1 LP835 N100 (CI-234MM2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232A9U","2ALL4 60L EZ1 LP835 N80","2ALL4 60L EZ1 LP835 N80 (CI-232A9U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232T2R","2ALL4 60L EZ1 LP840","2ALL4 60L EZ1 LP840 (CI-232T2R)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233LYJ","2ALL4 60L EZ1 LP850","2ALL4 60L EZ1 LP850 (CI-233LYJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232X9J","2ALL4 60L EZ1 PWS1836 LP835","2ALL4 60L EZ1 PWS1836 LP835 (CI-232X9J)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233LNX","2ALL4 60L EZ1 PWS1836 LP840","2ALL4 60L EZ1 PWS1836 LP840 (CI-233LNX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234W7W","2ALL4 60L EZB PWS1856LV LP840","2ALL4 60L EZB PWS1856LV LP840 (CI-234W7W)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234C4N","2ALL4 60L SLD LP835","2ALL4 60L SLD LP835 (CI-234C4N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233T3N","2ALL4 72L EZ1 LP835","2ALL4 72L EZ1 LP835 (CI-233T3N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233FU6","2ALL4 72L EZ1 LP840","2ALL4 72L EZ1 LP840 (CI-233FU6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234Y47","2ALL4 72L EZ1 LP850 N80","2ALL4 72L EZ1 LP850 N80 (CI-234Y47)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234ATR","2ALL4 72L EZ1 PWS1836 LP840","2ALL4 72L EZ1 PWS1836 LP840 (CI-234ATR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232P9F","2ALL4 CTRF 30L 120 EZ1 GLR LP835","2ALL4 CTRF 30L 120 EZ1 GLR LP835 (CI-232P9F)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232GKW","2ALL4 CTRF 30L EZ1 LP835","2ALL4 CTRF 30L EZ1 LP835 (CI-232GKW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232FUT","2ALL4 CTRF 40L EZ1 LP835","2ALL4 CTRF 40L EZ1 LP835 (CI-232FUT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233WVU","2ALL4 CTRF 40L EZ1 LP835 N100","2ALL4 CTRF 40L EZ1 LP835 N100 (CI-233WVU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232G0P","2ALL4 CTRF 40L EZ1 LP840","2ALL4 CTRF 40L EZ1 LP840 (CI-232G0P)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233AN9","2ALL4 CTRF 40L EZ1 LP840 N100","2ALL4 CTRF 40L EZ1 LP840 N100 (CI-233AN9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232Y0E","2ALL4 CTRF 40L EZ1 LP950 N80 RFD189375","2ALL4 CTRF 40L EZ1 LP950 N80 RFD189375 (CI-232Y0E)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233FGN","2ALL4 CTRF 40L EZ1 PWS1836 LP835 N80","2ALL4 CTRF 40L EZ1 PWS1836 LP835 N80 (CI-233FGN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234UF9","2ALL4 CTRF 40L EZ1 PWS1856LV LP835","2ALL4 CTRF 40L EZ1 PWS1856LV LP835 (CI-234UF9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234LK5","2ALL4 CTRF 40L SLD LP835","2ALL4 CTRF 40L SLD LP835 (CI-234LK5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232PA5","2ALL4 CTRF 48L 120 EZ1 GLR LP835","2ALL4 CTRF 48L 120 EZ1 GLR LP835 (CI-232PA5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231KHU","2ALL4 CTRF 48L EZ1 LP835","2ALL4 CTRF 48L EZ1 LP835 (CI-231KHU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234AYA","2ALL4 CTRF 48L EZ1 LP835 N100","2ALL4 CTRF 48L EZ1 LP835 N100 (CI-234AYA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232TGG","2ALL4 CTRF 48L EZ1 LP840","2ALL4 CTRF 48L EZ1 LP840 (CI-232TGG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234J2X","2ALL4 CTRF 48L EZ1 LP840 N100","2ALL4 CTRF 48L EZ1 LP840 N100 (CI-234J2X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231Y67","2ALL4 CTRF 48L EZ1 LP840 N80","2ALL4 CTRF 48L EZ1 LP840 N80 (CI-231Y67)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234L5P","2ALL4 CTRF 48L EZ1 LP840 N80 USPOM","2ALL4 CTRF 48L EZ1 LP840 N80 USPOM (CI-234L5P)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234V17","2ALL4 CTRF 48L EZ1 LP850","2ALL4 CTRF 48L EZ1 LP850 (CI-234V17)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233WVV","2ALL4 CTRF 48L EZ1 PWS1836 LP840","2ALL4 CTRF 48L EZ1 PWS1836 LP840 (CI-233WVV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231Y49","2ALL4 CTRF 48L EZB LP840","2ALL4 CTRF 48L EZB LP840 (CI-231Y49)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234TF1","2ALL4 CTRF 48L SLD LP835","2ALL4 CTRF 48L SLD LP835 (CI-234TF1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229Y4N","2ALL4 CTRF 60L EXA1 LP840","2ALL4 CTRF 60L EXA1 LP840 (CI-229Y4N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232VTE","2ALL4 CTRF 60L EZ1 LP835","2ALL4 CTRF 60L EZ1 LP835 (CI-232VTE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233VEN","2ALL4 CTRF 60L EZ1 LP835 N100","2ALL4 CTRF 60L EZ1 LP835 N100 (CI-233VEN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232TGM","2ALL4 CTRF 60L EZ1 LP840","2ALL4 CTRF 60L EZ1 LP840 (CI-232TGM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229Y4L","2ALL4 CTRF 60L EZ1 LP840 N100","2ALL4 CTRF 60L EZ1 LP840 N100 (CI-229Y4L)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233EM5","2ALL4 CTRF 60L EZ1 PWS1836 LP840","2ALL4 CTRF 60L EZ1 PWS1836 LP840 (CI-233EM5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234LLU","2ALL4 CTRF 60L SLD LP835","2ALL4 CTRF 60L SLD LP835 (CI-234LLU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234L6X","2ALL4 CTRF 72L 277 EZ1 GLR LP840","2ALL4 CTRF 72L 277 EZ1 GLR LP840 (CI-234L6X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232UUY","2ALL4 CTRF 72L EZ1 LP835","2ALL4 CTRF 72L EZ1 LP835 (CI-232UUY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233YRY","2ALL4 CTRF 72L EZ1 LP850","2ALL4 CTRF 72L EZ1 LP850 (CI-233YRY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234AEH","2ALL4 CTRF 72L EZ1 LP850 N80","2ALL4 CTRF 72L EZ1 LP850 N80 (CI-234AEH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233KKX","2ALL4 CTRF 72L EZ1 PWS1836 LP840","2ALL4 CTRF 72L EZ1 PWS1836 LP840 (CI-233KKX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234M66","2ALL4 CTRF 72L SLD LP835","2ALL4 CTRF 72L SLD LP835 (CI-234M66)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225CGW","2ALLS4 49L D50 LP850 NX","2ALLS4 49L D50 LP850 NX (CI-225CGW)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["220Y2G","2ALLX2 37L D37 LP835 N100","2ALLX2 37L D37 LP835 N100 (CI-220Y2G)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["220Y2L","2ALLX4 49L D50 LP835 N100","2ALLX4 49L D50 LP835 N100 (CI-220Y2L)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["228WUC","ALL4 21L 120 D24 QFC311GA LP835 NX","ALL4 21L 120 D24 QFC311GA LP835 NX (CI-228WUC)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["229AK1","ALL4 21L D24 120 QFC211GA LP835 N80","ALL4 21L D24 120 QFC211GA LP835 N80 (CI-229AK1)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["228YVV","ALL4 21L D24 120 QFC311GAB LP835 BLD","ALL4 21L D24 120 QFC311GAB LP835 BLD (CI-228YVV)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["226ACX","ALL4 43L D50 PWS1836 LP835 NX","ALL4 43L D50 PWS1836 LP835 NX (CI-226ACX)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["226KYF","ALL4 43L D50 PWS1836 LP840 NX","ALL4 43L D50 PWS1836 LP840 NX (CI-226KYF)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["222C1R","ALL4 64L D75 LP840 N80 USPOM","ALL4 64L D75 LP840 N80 USPOM (CI-222C1R)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["240LG3","2ALL2 20L 277 EZ1 GLR LP835","2ALL2 20L 277 EZ1 GLR LP835 (CI-240LG3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235KT4","2ALL2 20L EZ1 LP830 CP","2ALL2 20L EZ1 LP830 CP (CI-235KT4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241L8V","2ALL2 20L EZ1 LP830 N80","2ALL2 20L EZ1 LP830 N80 (CI-241L8V)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238WN3","2ALL2 20L EZ1 LP830 N80EMG","2ALL2 20L EZ1 LP830 N80EMG (CI-238WN3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C386,7)),6))","v":"235E7W"},{"$f":"LEFT(C386,SEARCH(\"(CI-\",C386)-2)","v":"2ALL2 20L EZ1 LP835 N100"},"2ALL2 20L EZ1 LP835 N100 (CI-235E7W)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236PV5","2ALL2 20L EZ1 LP835 N80","2ALL2 20L EZ1 LP835 N80 (CI-236PV5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["247PWT","2ALL2 20L EZ1 LP835 ST3","2ALL2 20L EZ1 LP835 ST3 (CI-247PWT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238W3H","2ALL2 20L EZ1 LP840 N100","2ALL2 20L EZ1 LP840 N100 (CI-238W3H)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241H58","2ALL2 20L EZ1 LP840 N100EMG","2ALL2 20L EZ1 LP840 N100EMG (CI-241H58)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235LL0","2ALL2 20L EZ1 LP850","2ALL2 20L EZ1 LP850 (CI-235LL0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240U4P","2ALL2 20L EZ1 PWS1836 LP840 LATC","2ALL2 20L EZ1 PWS1836 LP840 LATC (CI-240U4P)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239WPL","2ALL2 20L EZ1 PWS1856LV LP835","2ALL2 20L EZ1 PWS1856LV LP835 (CI-239WPL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237UYR","2ALL2 20L EZB LP835","2ALL2 20L EZB LP835 (CI-237UYR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237HLJ","2ALL2 20L EZB LP835 N80","2ALL2 20L EZB LP835 N80 (CI-237HLJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237HLN","2ALL2 20L EZB LP835 N80EMG","2ALL2 20L EZB LP835 N80EMG (CI-237HLN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241TCP","2ALL2 20L EZB LP840","2ALL2 20L EZB LP840 (CI-241TCP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237YHY","2ALL2 20L EZB PWS1856LV LP835","2ALL2 20L EZB PWS1856LV LP835 (CI-237YHY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240APA","2ALL2 33L 120 EZ1 GLR LP835","2ALL2 33L 120 EZ1 GLR LP835 (CI-240APA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232HAA","2ALL2 33L 120 EZ1 LP835 N100 CS1WL10 SSQ","2ALL2 33L 120 EZ1 LP835 N100 CS1WL10 SSQ (CI-232HAA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234A11","2ALL2 33L 120 EZ1 LP850 CS1WL10 SSQ","2ALL2 33L 120 EZ1 LP850 CS1WL10 SSQ (CI-234A11)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245JHA","2ALL2 33L EDB LP835","2ALL2 33L EDB LP835 (CI-245JHA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238AH0","2ALL2 33L EZ1 LP830 CP","2ALL2 33L EZ1 LP830 CP (CI-238AH0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234L4N","2ALL2 33L EZ1 LP830 N100","2ALL2 33L EZ1 LP830 N100 (CI-234L4N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238JMU","2ALL2 33L EZ1 LP835 CP","2ALL2 33L EZ1 LP835 CP (CI-238JMU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236MAN","2ALL2 33L EZ1 LP835 N100EMG","2ALL2 33L EZ1 LP835 N100EMG (CI-236MAN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233TLM","2ALL2 33L EZ1 LP835 N80EMG","2ALL2 33L EZ1 LP835 N80EMG (CI-233TLM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["247PWU","2ALL2 33L EZ1 LP835 ST3","2ALL2 33L EZ1 LP835 ST3 (CI-247PWU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236YJ4","2ALL2 33L EZ1 LP840 N100EMG","2ALL2 33L EZ1 LP840 N100EMG (CI-236YJ4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240VRW","2ALL2 33L EZ1 LP850","2ALL2 33L EZ1 LP850 (CI-240VRW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236C7E","2ALL2 33L EZ1 PWS1436 LP840","2ALL2 33L EZ1 PWS1436 LP840 (CI-236C7E)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239AV2","2ALL2 33L EZ1 PWS1836 LP830","2ALL2 33L EZ1 PWS1836 LP830 (CI-239AV2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238FP9","2ALL2 33L EZ1 PWS1836 LP835 N80","2ALL2 33L EZ1 PWS1836 LP835 N80 (CI-238FP9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239X3H","2ALL2 33L EZ1 PWS1836 LP840 LATC","2ALL2 33L EZ1 PWS1836 LP840 LATC (CI-239X3H)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241HF3","2ALL2 33L EZ1 PWS1836 LP840 LATC N100","2ALL2 33L EZ1 PWS1836 LP840 LATC N100 (CI-241HF3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241HEV","2ALL2 33L EZ1 PWS1846 LP840 LATC","2ALL2 33L EZ1 PWS1846 LP840 LATC (CI-241HEV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237GCX","2ALL2 33L EZ1 PWS1856LV LP830","2ALL2 33L EZ1 PWS1856LV LP830 (CI-237GCX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236XJ9","2ALL2 33L EZ1 PWS1856LV LP840","2ALL2 33L EZ1 PWS1856LV LP840 (CI-236XJ9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239G99","2ALL2 33L EZ1 PWS1856LV LP940","2ALL2 33L EZ1 PWS1856LV LP940 (CI-239G99)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235TNM","2ALL2 33L EZB LP835","2ALL2 33L EZB LP835 (CI-235TNM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237KUN","2ALL2 33L EZB LP835 N80","2ALL2 33L EZB LP835 N80 (CI-237KUN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240CJA","2ALL2 33L EZB LP840 N100","2ALL2 33L EZB LP840 N100 (CI-240CJA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240CJE","2ALL2 33L EZB LP840 N100EMG","2ALL2 33L EZB LP840 N100EMG (CI-240CJE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239N8W","2ALL2 33L EZB LP840 N80","2ALL2 33L EZB LP840 N80 (CI-239N8W)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235HHA","2ALL2 33L SLD LP830","2ALL2 33L SLD LP830 (CI-235HHA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235F4M","2ALL2 33L SLD LP835","2ALL2 33L SLD LP835 (CI-235F4M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241J17","2ALL2 33L SLD PWS1846 LP835","2ALL2 33L SLD PWS1846 LP835 (CI-241J17)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229V62","2ALL2 37L D37 LP830 N100EMG","2ALL2 37L D37 LP830 N100EMG (CI-229V62)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["225M8G","2ALL2 37L D37 LP835 N100EMG","2ALL2 37L D37 LP835 N100EMG (CI-225M8G)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["218Y76","2ALL2 37L D37 LP835 N80EMG","2ALL2 37L D37 LP835 N80EMG (CI-218Y76)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["222TP7","2ALL2 37L D37 LP835 N80EMG USPOM","2ALL2 37L D37 LP835 N80EMG USPOM (CI-222TP7)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["227U4M","2ALL2 37L D37 LP840 N100EMG","2ALL2 37L D37 LP840 N100EMG (CI-227U4M)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["218GRW","2ALL2 37L D37 LP840 N80EMG","2ALL2 37L D37 LP840 N80EMG (CI-218GRW)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["228U8Y","2ALL2 37L D37 LP850 N100EMG","2ALL2 37L D37 LP850 N100EMG (CI-228U8Y)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["229XN5","2ALL2 37L D37 PWS1836 LP835 N80EMG","2ALL2 37L D37 PWS1836 LP835 N80EMG (CI-229XN5)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["224R44","2ALL2 37L D37 PWS1836 LP840 N100EMG","2ALL2 37L D37 PWS1836 LP840 N100EMG (CI-224R44)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["229G3E","2ALL2 37L D37 PWS1846 LP835 N80EMG","2ALL2 37L D37 PWS1846 LP835 N80EMG (CI-229G3E)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["239J1X","2ALL2 40L 120 EZ1 GLR LP840","2ALL2 40L 120 EZ1 GLR LP840 (CI-239J1X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232HA8","2ALL2 40L 120 EZ1 LP835 N100 CS1WL10 SSQ","2ALL2 40L 120 EZ1 LP835 N100 CS1WL10 SSQ (CI-232HA8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241ERJ","2ALL2 40L 277 EZ1 GMF LP840","2ALL2 40L 277 EZ1 GMF LP840 (CI-241ERJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232HEW","2ALL2 40L EZ1 LP835 N100EMG","2ALL2 40L EZ1 LP835 N100EMG (CI-232HEW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231V49","2ALL2 40L EZ1 LP835 N80EMG","2ALL2 40L EZ1 LP835 N80EMG (CI-231V49)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233PJT","2ALL2 40L EZ1 LP835 NAWT","2ALL2 40L EZ1 LP835 NAWT (CI-233PJT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237WHG","2ALL2 40L EZ1 LP835 USPOM","2ALL2 40L EZ1 LP835 USPOM (CI-237WHG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["247VL7","2ALL2 40L EZ1 LP840 N100 USPOM","2ALL2 40L EZ1 LP840 N100 USPOM (CI-247VL7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235VTY","2ALL2 40L EZ1 LP840 N100EMG","2ALL2 40L EZ1 LP840 N100EMG (CI-235VTY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232TW9","2ALL2 40L EZ1 LP840 N80EMG","2ALL2 40L EZ1 LP840 N80EMG (CI-232TW9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234RKJ","2ALL2 40L EZ1 LP850 N100EMG","2ALL2 40L EZ1 LP850 N100EMG (CI-234RKJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235XA6","2ALL2 40L EZ1 PWS1836 LP830","2ALL2 40L EZ1 PWS1836 LP830 (CI-235XA6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C450,7)),6))","v":"241MPT"},{"$f":"LEFT(C450,SEARCH(\"(CI-\",C450)-2)","v":"2ALL2 40L EZ1 PWS1836 LP835 N100"},"2ALL2 40L EZ1 PWS1836 LP835 N100 (CI-241MPT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239U7R","2ALL2 40L EZ1 PWS1836 LP835 N80","2ALL2 40L EZ1 PWS1836 LP835 N80 (CI-239U7R)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239X46","2ALL2 40L EZ1 PWS1836 LP840 LATC","2ALL2 40L EZ1 PWS1836 LP840 LATC (CI-239X46)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239X5M","2ALL2 40L EZ1 PWS1836 LP840 LATC N100","2ALL2 40L EZ1 PWS1836 LP840 LATC N100 (CI-239X5M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238RAJ","2ALL2 40L EZ1 PWS1846 LP835 N100","2ALL2 40L EZ1 PWS1846 LP835 N100 (CI-238RAJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237HKR","2ALL2 40L EZB LP835 N80","2ALL2 40L EZB LP835 N80 (CI-237HKR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237HLA","2ALL2 40L EZB LP835 N80EMG","2ALL2 40L EZB LP835 N80EMG (CI-237HLA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239K4G","2ALL2 40L EZB LP840 N100","2ALL2 40L EZB LP840 N100 (CI-239K4G)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235CNM","2ALL2 CTRF 20L EZ1 LP830","2ALL2 CTRF 20L EZ1 LP830 (CI-235CNM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240J3Y","2ALL2 CTRF 20L EZ1 LP835 N80","2ALL2 CTRF 20L EZ1 LP835 N80 (CI-240J3Y)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237ANY","2ALL2 CTRF 20L EZ1 LP835 USPOM","2ALL2 CTRF 20L EZ1 LP835 USPOM (CI-237ANY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["239A72","2ALL2 CTRF 20L EZ1 LP840 N100","2ALL2 CTRF 20L EZ1 LP840 N100 (CI-239A72)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["241LEY","2ALL2 CTRF 20L EZ1 LP840 N100EMG","2ALL2 CTRF 20L EZ1 LP840 N100EMG (CI-241LEY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236E1N","2ALL2 CTRF 20L EZ1 PWS1836 LP830","2ALL2 CTRF 20L EZ1 PWS1836 LP830 (CI-236E1N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235E46","2ALL2 CTRF 20L EZ1 PWS1836 LP835","2ALL2 CTRF 20L EZ1 PWS1836 LP835 (CI-235E46)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235ATE","2ALL2 CTRF 20L EZ1 PWS1856LV LP830","2ALL2 CTRF 20L EZ1 PWS1856LV LP830 (CI-235ATE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236NXE","2ALL2 CTRF 20L EZ1 PWS1856LV LP835","2ALL2 CTRF 20L EZ1 PWS1856LV LP835 (CI-236NXE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230W0Y","2ALL2 CTRF 33L 120 EZ1 CS1WL10 LP835 N100 SSQ","2ALL2 CTRF 33L 120 EZ1 CS1WL10 LP835 N100 SSQ (CI-230W0Y)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236J0F","2ALL2 CTRF 33L 120 EZ1 LP830 CS1WL10 SSQ","2ALL2 CTRF 33L 120 EZ1 LP830 CS1WL10 SSQ (CI-236J0F)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234A4F","2ALL2 CTRF 33L 120 EZ1 LP850 CS1WL10 SSQ","2ALL2 CTRF 33L 120 EZ1 LP850 CS1WL10 SSQ (CI-234A4F)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235MX0","2ALL2 CTRF 33L 120 EZ1 QFC211GA LP840","2ALL2 CTRF 33L 120 EZ1 QFC211GA LP840 (CI-235MX0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234ELU","2ALL2 CTRF 33L EZ1 LP830","2ALL2 CTRF 33L EZ1 LP830 (CI-234ELU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["249P8M","2ALL2 CTRF 33L EZ1 LP830 CP","2ALL2 CTRF 33L EZ1 LP830 CP (CI-249P8M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["245WXV","2ALL2 CTRF 33L EZ1 LP830 N100","2ALL2 CTRF 33L EZ1 LP830 N100 (CI-245WXV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["245WY2","2ALL2 CTRF 33L EZ1 LP830 N100EMG","2ALL2 CTRF 33L EZ1 LP830 N100EMG (CI-245WY2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236MMK","2ALL2 CTRF 33L EZ1 LP835 N100EMG","2ALL2 CTRF 33L EZ1 LP835 N100EMG (CI-236MMK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236K8A","2ALL2 CTRF 33L EZ1 LP835 N80","2ALL2 CTRF 33L EZ1 LP835 N80 (CI-236K8A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["241N76","2ALL2 CTRF 33L EZ1 LP835 USPOM","2ALL2 CTRF 33L EZ1 LP835 USPOM (CI-241N76)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235E5L","2ALL2 CTRF 33L EZ1 LP840 N100","2ALL2 CTRF 33L EZ1 LP840 N100 (CI-235E5L)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240L68","2ALL2 CTRF 33L EZ1 LP840 N100EMG","2ALL2 CTRF 33L EZ1 LP840 N100EMG (CI-240L68)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235PNG","2ALL2 CTRF 33L EZ1 LP840 N80","2ALL2 CTRF 33L EZ1 LP840 N80 (CI-235PNG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236AKR","2ALL2 CTRF 33L EZ1 LP840 N80EMG","2ALL2 CTRF 33L EZ1 LP840 N80EMG (CI-236AKR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["239L28","2ALL2 CTRF 33L EZ1 LP840 ST3","2ALL2 CTRF 33L EZ1 LP840 ST3 (CI-239L28)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236E1L","2ALL2 CTRF 33L EZ1 PWS1836 LP830","2ALL2 CTRF 33L EZ1 PWS1836 LP830 (CI-236E1L)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235WMY","2ALL2 CTRF 33L EZ1 PWS1836 LP835 N100","2ALL2 CTRF 33L EZ1 PWS1836 LP835 N100 (CI-235WMY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237L6F","2ALL2 CTRF 33L EZ1 PWS1836 LP835 USPOM","2ALL2 CTRF 33L EZ1 PWS1836 LP835 USPOM (CI-237L6F)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233ELG","2ALL2 CTRF 33L EZ1 PWS1836 LP840","2ALL2 CTRF 33L EZ1 PWS1836 LP840 (CI-233ELG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240J21","2ALL2 CTRF 33L EZ1 PWS1836 LP840 N100","2ALL2 CTRF 33L EZ1 PWS1836 LP840 N100 (CI-240J21)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236RTY","2ALL2 CTRF 33L EZ1 PWS1856LV LP835","2ALL2 CTRF 33L EZ1 PWS1856LV LP835 (CI-236RTY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["239K34","2ALL2 CTRF 33L EZ1 PWS1856LV LP835 LATC","2ALL2 CTRF 33L EZ1 PWS1856LV LP835 LATC (CI-239K34)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235XH5","2ALL2 CTRF 33L EZ1 PWS1856LV LP840","2ALL2 CTRF 33L EZ1 PWS1856LV LP840 (CI-235XH5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234YKW","2ALL2 CTRF 33L EZ1 PWS1856LV LP850","2ALL2 CTRF 33L EZ1 PWS1856LV LP850 (CI-234YKW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235CNK","2ALL2 CTRF 40L EZ1 LP830","2ALL2 CTRF 40L EZ1 LP830 (CI-235CNK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240KX3","2ALL2 CTRF 40L EZ1 LP835 N100EMG","2ALL2 CTRF 40L EZ1 LP835 N100EMG (CI-240KX3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234MXV","2ALL2 CTRF 40L EZ1 LP835 N80","2ALL2 CTRF 40L EZ1 LP835 N80 (CI-234MXV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["241N79","2ALL2 CTRF 40L EZ1 LP835 USPOM","2ALL2 CTRF 40L EZ1 LP835 USPOM (CI-241N79)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237NU0","2ALL2 CTRF 40L EZ1 LP840 N100EMG","2ALL2 CTRF 40L EZ1 LP840 N100EMG (CI-237NU0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236AKM","2ALL2 CTRF 40L EZ1 LP840 N80EMG","2ALL2 CTRF 40L EZ1 LP840 N80EMG (CI-236AKM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["249R22","2ALL2 CTRF 40L EZ1 LP840 USPOM","2ALL2 CTRF 40L EZ1 LP840 USPOM (CI-249R22)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237PUT","2ALL2 CTRF 40L EZ1 PWS1856LV LP835","2ALL2 CTRF 40L EZ1 PWS1856LV LP835 (CI-237PUT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235XH3","2ALL2 CTRF 40L EZ1 PWS1856LV LP840","2ALL2 CTRF 40L EZ1 PWS1856LV LP840 (CI-235XH3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235CPH","2ALL2 CTRF 40L SLD LP830","2ALL2 CTRF 40L SLD LP830 (CI-235CPH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235RWG","2ALL2 CTRF 40L SLD LP835","2ALL2 CTRF 40L SLD LP835 (CI-235RWG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235J2N","2ALL2 CTRF 40L SLD LP840","2ALL2 CTRF 40L SLD LP840 (CI-235J2N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240A55","2ALL4 30L 277 EZ1 GLR LP835 LATC","2ALL4 30L 277 EZ1 GLR LP835 LATC (CI-240A55)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240AFJ","2ALL4 30L 277 EZ1 GLR LP835 LATC USPOM","2ALL4 30L 277 EZ1 GLR LP835 LATC USPOM (CI-240AFJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240U80","2ALL4 30L EZ1 LP830 N80","2ALL4 30L EZ1 LP830 N80 (CI-240U80)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237KMH","2ALL4 30L EZ1 LP835 N100","2ALL4 30L EZ1 LP835 N100 (CI-237KMH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235N7U","2ALL4 30L EZ1 LP840 N100","2ALL4 30L EZ1 LP840 N100 (CI-235N7U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241MK3","2ALL4 30L EZ1 LP840 N80","2ALL4 30L EZ1 LP840 N80 (CI-241MK3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240G71","2ALL4 30L EZ1 LP840 USPOM","2ALL4 30L EZ1 LP840 USPOM (CI-240G71)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235CN6","2ALL4 30L EZ1 LP850","2ALL4 30L EZ1 LP850 (CI-235CN6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239AUW","2ALL4 30L EZ1 PWS1836 LP830","2ALL4 30L EZ1 PWS1836 LP830 (CI-239AUW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237WK4","2ALL4 30L EZ1 PWS1836 LP835","2ALL4 30L EZ1 PWS1836 LP835 (CI-237WK4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C514,7)),6))","v":"241HFK"},{"$f":"LEFT(C514,SEARCH(\"(CI-\",C514)-2)","v":"2ALL4 30L EZ1 PWS1836 LP840 LATC N100"},"2ALL4 30L EZ1 PWS1836 LP840 LATC N100 (CI-241HFK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236X4T","2ALL4 30L EZ1 PWS1856LV LP835","2ALL4 30L EZ1 PWS1856LV LP835 (CI-236X4T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238P4H","2ALL4 30L EZ1 PWS1856LV LP840","2ALL4 30L EZ1 PWS1856LV LP840 (CI-238P4H)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237UYK","2ALL4 30L EZB LP835","2ALL4 30L EZB LP835 (CI-237UYK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241TWL","2ALL4 30L EZB LP835 N80","2ALL4 30L EZB LP835 N80 (CI-241TWL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236GEW","2ALL4 30L EZB LP840","2ALL4 30L EZB LP840 (CI-236GEW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236TLV","2ALL4 40L 277 EZ1 GLR LP835","2ALL4 40L 277 EZ1 GLR LP835 (CI-236TLV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234YMU","2ALL4 40L EZ1 LP830","2ALL4 40L EZ1 LP830 (CI-234YMU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241C63","2ALL4 40L EZ1 LP835 CP","2ALL4 40L EZ1 LP835 CP (CI-241C63)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235E0G","2ALL4 40L EZ1 LP835 N80","2ALL4 40L EZ1 LP835 N80 (CI-235E0G)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236KXH","2ALL4 40L EZ1 LP835 N80EMG","2ALL4 40L EZ1 LP835 N80EMG (CI-236KXH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235MLF","2ALL4 40L EZ1 LP840 N100","2ALL4 40L EZ1 LP840 N100 (CI-235MLF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239NW5","2ALL4 40L EZ1 LP840 N80EMG","2ALL4 40L EZ1 LP840 N80EMG (CI-239NW5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240G6Y","2ALL4 40L EZ1 LP840 USPOM","2ALL4 40L EZ1 LP840 USPOM (CI-240G6Y)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235NGH","2ALL4 40L EZ1 LP850","2ALL4 40L EZ1 LP850 (CI-235NGH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239UT3","2ALL4 40L EZ1 LP850 N100","2ALL4 40L EZ1 LP850 N100 (CI-239UT3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236C86","2ALL4 40L EZ1 PWS1436 LP840","2ALL4 40L EZ1 PWS1436 LP840 (CI-236C86)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233GY6","2ALL4 40L EZ1 PWS1836 LP835","2ALL4 40L EZ1 PWS1836 LP835 (CI-233GY6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238UNW","2ALL4 40L EZ1 PWS1836 LP835 N100EMG","2ALL4 40L EZ1 PWS1836 LP835 N100EMG (CI-238UNW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235TRN","2ALL4 40L EZ1 PWS1836 LP840","2ALL4 40L EZ1 PWS1836 LP840 (CI-235TRN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241HFT","2ALL4 40L EZ1 PWS1836 LP840 LATC N100","2ALL4 40L EZ1 PWS1836 LP840 LATC N100 (CI-241HFT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235RVJ","2ALL4 40L EZ1 PWS1836 LP840 N100","2ALL4 40L EZ1 PWS1836 LP840 N100 (CI-235RVJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238RA1","2ALL4 40L EZ1 PWS1846 LP835 N100","2ALL4 40L EZ1 PWS1846 LP835 N100 (CI-238RA1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241HG2","2ALL4 40L EZ1 PWS1846 LP840 LATC N100EMG","2ALL4 40L EZ1 PWS1846 LP840 LATC N100EMG (CI-241HG2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235PJA","2ALL4 40L EZ1 PWS1856LV LP835","2ALL4 40L EZ1 PWS1856LV LP835 (CI-235PJA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240LG7","2ALL4 40L EZ1 PWS1856LV LP840","2ALL4 40L EZ1 PWS1856LV LP840 (CI-240LG7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245H63","2ALL4 40L EZB LP830 CP","2ALL4 40L EZB LP830 CP (CI-245H63)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235MHX","2ALL4 40L EZB LP835","2ALL4 40L EZB LP835 (CI-235MHX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235WUY","2ALL4 40L EZB LP840","2ALL4 40L EZB LP840 (CI-235WUY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238K0F","2ALL4 48L 120 EZ1 GLR LP840","2ALL4 48L 120 EZ1 GLR LP840 (CI-238K0F)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235HJY","2ALL4 48L 120 EZ1 GLR PWS1836 LP840","2ALL4 48L 120 EZ1 GLR PWS1836 LP840 (CI-235HJY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240LG2","2ALL4 48L 277 EZ1 GLR LP835","2ALL4 48L 277 EZ1 GLR LP835 (CI-240LG2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236FME","2ALL4 48L EDB LP850","2ALL4 48L EDB LP850 (CI-236FME)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232HH5","2ALL4 48L EZ1 LP835 N100EMG","2ALL4 48L EZ1 LP835 N100EMG (CI-232HH5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233V8J","2ALL4 48L EZ1 LP835 N80EMG","2ALL4 48L EZ1 LP835 N80EMG (CI-233V8J)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241TF2","2ALL4 48L EZ1 LP835 USPOM","2ALL4 48L EZ1 LP835 USPOM (CI-241TF2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["247VL5","2ALL4 48L EZ1 LP840 N100 USPOM","2ALL4 48L EZ1 LP840 N100 USPOM (CI-247VL5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236WGP","2ALL4 48L EZ1 LP840 N100EMG","2ALL4 48L EZ1 LP840 N100EMG (CI-236WGP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240L9C","2ALL4 48L EZ1 LP850 N100","2ALL4 48L EZ1 LP850 N100 (CI-240L9C)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238RV6","2ALL4 48L EZ1 PWS1236 LP835","2ALL4 48L EZ1 PWS1236 LP835 (CI-238RV6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["249REK","2ALL4 48L EZ1 PWS1236 LP840","2ALL4 48L EZ1 PWS1236 LP840 (CI-249REK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233MLV","2ALL4 48L EZ1 PWS1436 LP835","2ALL4 48L EZ1 PWS1436 LP835 (CI-233MLV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241A48","2ALL4 48L EZ1 PWS1436 PWSLV LP835","2ALL4 48L EZ1 PWS1436 PWSLV LP835 (CI-241A48)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235XA9","2ALL4 48L EZ1 PWS1836 LP830","2ALL4 48L EZ1 PWS1836 LP830 (CI-235XA9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231N5R","2ALL4 48L EZ1 PWS1836 LP835","2ALL4 48L EZ1 PWS1836 LP835 (CI-231N5R)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232EM5","2ALL4 48L EZ1 PWS1836 LP840","2ALL4 48L EZ1 PWS1836 LP840 (CI-232EM5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239X2U","2ALL4 48L EZ1 PWS1836 LP840 LATC","2ALL4 48L EZ1 PWS1836 LP840 LATC (CI-239X2U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241HGM","2ALL4 48L EZ1 PWS1836 LP840 LATC N100","2ALL4 48L EZ1 PWS1836 LP840 LATC N100 (CI-241HGM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["249R1V","2ALL4 48L EZ1 PWS1836 LP840 N100","2ALL4 48L EZ1 PWS1836 LP840 N100 (CI-249R1V)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233X27","2ALL4 48L EZ1 PWS1836 LP850","2ALL4 48L EZ1 PWS1836 LP850 (CI-233X27)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232NCE","2ALL4 48L EZ1 PWS1846 LP835","2ALL4 48L EZ1 PWS1846 LP835 (CI-232NCE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232PNX","2ALL4 48L EZ1 PWS1846 LP840","2ALL4 48L EZ1 PWS1846 LP840 (CI-232PNX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241HKK","2ALL4 48L EZ1 PWS1846 LP840 LATC N100EMG","2ALL4 48L EZ1 PWS1846 LP840 LATC N100EMG (CI-241HKK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235HJ1","2ALL4 48L EZ1 PWS1856LV LP835","2ALL4 48L EZ1 PWS1856LV LP835 (CI-235HJ1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232YPT","2ALL4 48L EZ1 PWS1856LV LP840","2ALL4 48L EZ1 PWS1856LV LP840 (CI-232YPT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240MG4","2ALL4 48L EZB LP835 CP","2ALL4 48L EZB LP835 CP (CI-240MG4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235JA0","2ALL4 48L EZB LP840 N100","2ALL4 48L EZB LP840 N100 (CI-235JA0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240E55","2ALL4 48L EZB LP840 N100EMG","2ALL4 48L EZB LP840 N100EMG (CI-240E55)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236JJ7","2ALL4 48L SLD PWS1846 LP840","2ALL4 48L SLD PWS1846 LP840 (CI-236JJ7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227YFF","2ALL4 49L 120 D50 LP840 BLD GLR","2ALL4 49L 120 D50 LP840 BLD GLR (CI-227YFF)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["230XF0","2ALL4 49L D50 LP835 N100EMG","2ALL4 49L D50 LP835 N100EMG (CI-230XF0)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["218Y9L","2ALL4 49L D50 LP835 N80EMG","2ALL4 49L D50 LP835 N80EMG (CI-218Y9L)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["222TPY","2ALL4 49L D50 LP835 N80EMG USPOM","2ALL4 49L D50 LP835 N80EMG USPOM (CI-222TPY)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["224WX8","2ALL4 49L D50 LP840 N100EMG","2ALL4 49L D50 LP840 N100EMG (CI-224WX8)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
[{"$f":"(LEFT((RIGHT(C578,7)),6))","v":"221UU7"},{"$f":"LEFT(C578,SEARCH(\"(CI-\",C578)-2)","v":"2ALL4 49L D50 LP840 N80 USPOM"},"2ALL4 49L D50 LP840 N80 USPOM (CI-221UU7)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["224G6N","2ALL4 49L D50 LP840 N80EMG","2ALL4 49L D50 LP840 N80EMG (CI-224G6N)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["228U93","2ALL4 49L D50 LP850 N100EMG","2ALL4 49L D50 LP850 N100EMG (CI-228U93)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["228N9J","2ALL4 49L D50 PWS1836 LP835 N80EMG","2ALL4 49L D50 PWS1836 LP835 N80EMG (CI-228N9J)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["228P87","2ALL4 49L D50 PWS1836 LP840 N100EMG","2ALL4 49L D50 PWS1836 LP840 N100EMG (CI-228P87)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["225ELW","2ALL4 49L D50 PWS1846 LP835 BLD","2ALL4 49L D50 PWS1846 LP835 BLD (CI-225ELW)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["229G3A","2ALL4 49L D50 PWS1846 LP835 N80EMG","2ALL4 49L D50 PWS1846 LP835 N80EMG (CI-229G3A)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["240FP0","2ALL4 60L 277 EZ1 GLR LP835","2ALL4 60L 277 EZ1 GLR LP835 (CI-240FP0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241ERF","2ALL4 60L 277 EZ1 GMF LP840","2ALL4 60L 277 EZ1 GMF LP840 (CI-241ERF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245LW5","2ALL4 60L EZ1 LP835 N80EMG","2ALL4 60L EZ1 LP835 N80EMG (CI-245LW5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245NV6","2ALL4 60L EZ1 LP840 N100","2ALL4 60L EZ1 LP840 N100 (CI-245NV6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237RKM","2ALL4 60L EZ1 LP840 N80","2ALL4 60L EZ1 LP840 N80 (CI-237RKM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237KC6","2ALL4 60L EZ1 LP850 USPOM","2ALL4 60L EZ1 LP850 USPOM (CI-237KC6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241MPR","2ALL4 60L EZ1 PWS1836 LP835 N100","2ALL4 60L EZ1 PWS1836 LP835 N100 (CI-241MPR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241HLL","2ALL4 60L EZ1 PWS1836 LP840 LATC N100","2ALL4 60L EZ1 PWS1836 LP840 LATC N100 (CI-241HLL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["249R0M","2ALL4 60L EZ1 PWS1836 LP840 N100","2ALL4 60L EZ1 PWS1836 LP840 N100 (CI-249R0M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236K8G","2ALL4 60L EZ1 PWS1856LV LP835","2ALL4 60L EZ1 PWS1856LV LP835 (CI-236K8G)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241GPE","2ALL4 60L EZ1 PWS1856LV LP840","2ALL4 60L EZ1 PWS1856LV LP840 (CI-241GPE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240LLJ","2ALL4 60L EZB LP835","2ALL4 60L EZB LP835 (CI-240LLJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235AJG","2ALL4 60L EZB LP840 N80","2ALL4 60L EZB LP840 N80 (CI-235AJG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235LR5","2ALL4 60L SLD LP840","2ALL4 60L SLD LP840 (CI-235LR5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["247R8K","2ALL4 72L EZ1 LP830","2ALL4 72L EZ1 LP830 (CI-247R8K)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["238PP9","2ALL4 72L EZ1 LP835 N100","2ALL4 72L EZ1 LP835 N100 (CI-238PP9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236X49","2ALL4 72L EZ1 LP840 N100","2ALL4 72L EZ1 LP840 N100 (CI-236X49)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["238WA3","2ALL4 72L EZ1 LP840 N100EMG","2ALL4 72L EZ1 LP840 N100EMG (CI-238WA3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237RKK","2ALL4 72L EZ1 LP840 N80","2ALL4 72L EZ1 LP840 N80 (CI-237RKK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236ETA","2ALL4 72L EZ1 LP850","2ALL4 72L EZ1 LP850 (CI-236ETA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240L84","2ALL4 72L EZ1 LP850 N100","2ALL4 72L EZ1 LP850 N100 (CI-240L84)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["241MPL","2ALL4 72L EZ1 PWS1836 LP835 N100","2ALL4 72L EZ1 PWS1836 LP835 N100 (CI-241MPL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["239X2L","2ALL4 72L EZ1 PWS1836 LP840 LATC","2ALL4 72L EZ1 PWS1836 LP840 LATC (CI-239X2L)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["239X6T","2ALL4 72L EZ1 PWS1836 LP840 LATC N100","2ALL4 72L EZ1 PWS1836 LP840 LATC N100 (CI-239X6T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["249R1C","2ALL4 72L EZ1 PWS1836 LP840 N100","2ALL4 72L EZ1 PWS1836 LP840 N100 (CI-249R1C)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["239GCX","2ALL4 72L EZ1 PWS1856LV LP835","2ALL4 72L EZ1 PWS1856LV LP835 (CI-239GCX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237MAL","2ALL4 72L EZ1 PWS1856LV LP840","2ALL4 72L EZ1 PWS1856LV LP840 (CI-237MAL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237UYT","2ALL4 72L EZB LP835","2ALL4 72L EZB LP835 (CI-237UYT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240E5A","2ALL4 72L EZB LP840 N100","2ALL4 72L EZB LP840 N100 (CI-240E5A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240EJP","2ALL4 72L EZB LP840 N100EMG","2ALL4 72L EZB LP840 N100EMG (CI-240EJP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239J4N","2ALL4 CTRF 30L EZ1 LP830","2ALL4 CTRF 30L EZ1 LP830 (CI-239J4N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240T40","2ALL4 CTRF 30L EZ1 LP835 N100","2ALL4 CTRF 30L EZ1 LP835 N100 (CI-240T40)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236X09","2ALL4 CTRF 30L EZ1 LP840","2ALL4 CTRF 30L EZ1 LP840 (CI-236X09)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239A82","2ALL4 CTRF 30L EZ1 LP840 N100","2ALL4 CTRF 30L EZ1 LP840 N100 (CI-239A82)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241F7G","2ALL4 CTRF 30L EZ1 LP840 N100EMG","2ALL4 CTRF 30L EZ1 LP840 N100EMG (CI-241F7G)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232U3G","2ALL4 CTRF 30L EZ1 LP850","2ALL4 CTRF 30L EZ1 LP850 (CI-232U3G)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234K6X","2ALL4 CTRF 30L EZ1 PWS1836 LP835","2ALL4 CTRF 30L EZ1 PWS1836 LP835 (CI-234K6X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237L6E","2ALL4 CTRF 30L EZ1 PWS1836 LP835 USPOM","2ALL4 CTRF 30L EZ1 PWS1836 LP835 USPOM (CI-237L6E)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240J23","2ALL4 CTRF 30L EZ1 PWS1836 LP840 N100","2ALL4 CTRF 30L EZ1 PWS1836 LP840 N100 (CI-240J23)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240M2N","2ALL4 CTRF 30L EZ1 PWS1836 LP840 USPOM","2ALL4 CTRF 30L EZ1 PWS1836 LP840 USPOM (CI-240M2N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238RVF","2ALL4 CTRF 30L EZ1 PWS1856LV LP835","2ALL4 CTRF 30L EZ1 PWS1856LV LP835 (CI-238RVF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239J5T","2ALL4 CTRF 30L EZB LP835","2ALL4 CTRF 30L EZB LP835 (CI-239J5T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245L6U","2ALL4 CTRF 40L 277 EZ1 GLR LP840","2ALL4 CTRF 40L 277 EZ1 GLR LP840 (CI-245L6U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236KXV","2ALL4 CTRF 40L EZ1 LP830","2ALL4 CTRF 40L EZ1 LP830 (CI-236KXV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["249P92","2ALL4 CTRF 40L EZ1 LP830 CP","2ALL4 CTRF 40L EZ1 LP830 CP (CI-249P92)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238AY8","2ALL4 CTRF 40L EZ1 LP830 N100","2ALL4 CTRF 40L EZ1 LP830 N100 (CI-238AY8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245JGL","2ALL4 CTRF 40L EZ1 LP835 N80","2ALL4 CTRF 40L EZ1 LP835 N80 (CI-245JGL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245KME","2ALL4 CTRF 40L EZ1 LP835 N80EMG","2ALL4 CTRF 40L EZ1 LP835 N80EMG (CI-245KME)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237ALU","2ALL4 CTRF 40L EZ1 LP835 USPOM","2ALL4 CTRF 40L EZ1 LP835 USPOM (CI-237ALU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241LG5","2ALL4 CTRF 40L EZ1 LP840 N100EMG","2ALL4 CTRF 40L EZ1 LP840 N100EMG (CI-241LG5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239L3H","2ALL4 CTRF 40L EZ1 LP840 ST3","2ALL4 CTRF 40L EZ1 LP840 ST3 (CI-239L3H)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238AA2","2ALL4 CTRF 40L EZ1 LP840 USPOM","2ALL4 CTRF 40L EZ1 LP840 USPOM (CI-238AA2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238M77","2ALL4 CTRF 40L EZ1 LP850","2ALL4 CTRF 40L EZ1 LP850 (CI-238M77)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235TT3","2ALL4 CTRF 40L EZ1 LP850 N80","2ALL4 CTRF 40L EZ1 LP850 N80 (CI-235TT3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235E5R","2ALL4 CTRF 40L EZ1 PWS1836 LP835","2ALL4 CTRF 40L EZ1 PWS1836 LP835 (CI-235E5R)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["249NXU","2ALL4 CTRF 40L EZ1 PWS1836 LP840","2ALL4 CTRF 40L EZ1 PWS1836 LP840 (CI-249NXU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240J24","2ALL4 CTRF 40L EZ1 PWS1836 LP840 N100","2ALL4 CTRF 40L EZ1 PWS1836 LP840 N100 (CI-240J24)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C642,7)),6))","v":"240M2R"},{"$f":"LEFT(C642,SEARCH(\"(CI-\",C642)-2)","v":"2ALL4 CTRF 40L EZ1 PWS1836 LP840 USPOM"},"2ALL4 CTRF 40L EZ1 PWS1836 LP840 USPOM (CI-240M2R)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237YLR","2ALL4 CTRF 40L EZ1 PWS1856LV LP840","2ALL4 CTRF 40L EZ1 PWS1856LV LP840 (CI-237YLR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238C78","2ALL4 CTRF 40L EZB LP835","2ALL4 CTRF 40L EZB LP835 (CI-238C78)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245MG9","2ALL4 CTRF 40L EZB LP835 N100","2ALL4 CTRF 40L EZB LP835 N100 (CI-245MG9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235P5X","2ALL4 CTRF 40L EZB LP840 N100","2ALL4 CTRF 40L EZB LP840 N100 (CI-235P5X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241RKU","2ALL4 CTRF 40L SLD LP840","2ALL4 CTRF 40L SLD LP840 (CI-241RKU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["249PF7","2ALL4 CTRF 40L SLD PWS1846 LP835","2ALL4 CTRF 40L SLD PWS1846 LP835 (CI-249PF7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245MME","2ALL4 CTRF 48L 120 EZ1 GLR LP840 USPOM","2ALL4 CTRF 48L 120 EZ1 GLR LP840 USPOM (CI-245MME)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239LKY","2ALL4 CTRF 48L 277 EZ1 GLR LP840","2ALL4 CTRF 48L 277 EZ1 GLR LP840 (CI-239LKY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235E1M","2ALL4 CTRF 48L 277 EZ1 QFC211GA LP835","2ALL4 CTRF 48L 277 EZ1 QFC211GA LP835 (CI-235E1M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235ARC","2ALL4 CTRF 48L EZ1 LP830","2ALL4 CTRF 48L EZ1 LP830 (CI-235ARC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240KWY","2ALL4 CTRF 48L EZ1 LP835 N100EMG","2ALL4 CTRF 48L EZ1 LP835 N100EMG (CI-240KWY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235RVN","2ALL4 CTRF 48L EZ1 LP835 N80","2ALL4 CTRF 48L EZ1 LP835 N80 (CI-235RVN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241MM3","2ALL4 CTRF 48L EZ1 LP840 N100EMG","2ALL4 CTRF 48L EZ1 LP840 N100EMG (CI-241MM3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239L3U","2ALL4 CTRF 48L EZ1 LP840 ST3","2ALL4 CTRF 48L EZ1 LP840 ST3 (CI-239L3U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237UH6","2ALL4 CTRF 48L EZ1 PWS1236 LP835","2ALL4 CTRF 48L EZ1 PWS1236 LP835 (CI-237UH6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238KRK","2ALL4 CTRF 48L EZ1 PWS1836 LP830","2ALL4 CTRF 48L EZ1 PWS1836 LP830 (CI-238KRK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236L9E","2ALL4 CTRF 48L EZ1 PWS1836 LP835","2ALL4 CTRF 48L EZ1 PWS1836 LP835 (CI-236L9E)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239P75","2ALL4 CTRF 48L EZ1 PWS1856LV LP830","2ALL4 CTRF 48L EZ1 PWS1856LV LP830 (CI-239P75)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235VJT","2ALL4 CTRF 48L EZ1 PWS1856LV LP835","2ALL4 CTRF 48L EZ1 PWS1856LV LP835 (CI-235VJT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236V95","2ALL4 CTRF 48L EZ1 PWS1856LV LP840","2ALL4 CTRF 48L EZ1 PWS1856LV LP840 (CI-236V95)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235P33","2ALL4 CTRF 48L EZB LP840 N100","2ALL4 CTRF 48L EZB LP840 N100 (CI-235P33)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241MFU","2ALL4 CTRF 48L SLD LP830","2ALL4 CTRF 48L SLD LP830 (CI-241MFU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235J2P","2ALL4 CTRF 48L SLD LP840","2ALL4 CTRF 48L SLD LP840 (CI-235J2P)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["251P1J","2ALL4 CTRF 48L SLD PWS1846 LP835","2ALL4 CTRF 48L SLD PWS1846 LP835 (CI-251P1J)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240N10","2ALL4 CTRF 48L SLD PWS1846 LP835(DUP)","2ALL4 CTRF 48L SLD PWS1846 LP835(DUP) (CI-240N10)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245L6W","2ALL4 CTRF 60L 277 EZ1 GLR LP840","2ALL4 CTRF 60L 277 EZ1 GLR LP840 (CI-245L6W)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235CN9","2ALL4 CTRF 60L EZ1 LP830","2ALL4 CTRF 60L EZ1 LP830 (CI-235CN9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236MMJ","2ALL4 CTRF 60L EZ1 LP835 N100EMG","2ALL4 CTRF 60L EZ1 LP835 N100EMG (CI-236MMJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240J41","2ALL4 CTRF 60L EZ1 LP835 N80","2ALL4 CTRF 60L EZ1 LP835 N80 (CI-240J41)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241N71","2ALL4 CTRF 60L EZ1 LP835 USPOM","2ALL4 CTRF 60L EZ1 LP835 USPOM (CI-241N71)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235PAJ","2ALL4 CTRF 60L EZ1 LP840 N100EMG","2ALL4 CTRF 60L EZ1 LP840 N100EMG (CI-235PAJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237UJH","2ALL4 CTRF 60L EZ1 PWS1236 LP835","2ALL4 CTRF 60L EZ1 PWS1236 LP835 (CI-237UJH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235LNP","2ALL4 CTRF 60L EZ1 PWS1836 LP835","2ALL4 CTRF 60L EZ1 PWS1836 LP835 (CI-235LNP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237L69","2ALL4 CTRF 60L EZ1 PWS1836 LP835 USPOM","2ALL4 CTRF 60L EZ1 PWS1836 LP835 USPOM (CI-237L69)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238RVJ","2ALL4 CTRF 60L EZ1 PWS1856LV LP835","2ALL4 CTRF 60L EZ1 PWS1856LV LP835 (CI-238RVJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240H8W","2ALL4 CTRF 60L EZB LP835 N100","2ALL4 CTRF 60L EZB LP835 N100 (CI-240H8W)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236G8V","2ALL4 CTRF 60L SLD LP840","2ALL4 CTRF 60L SLD LP840 (CI-236G8V)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240AP8","2ALL4 CTRF 72L 120 EZ1 GLR LP835","2ALL4 CTRF 72L 120 EZ1 GLR LP835 (CI-240AP8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236UVR","2ALL4 CTRF 72L EZ1 LP830","2ALL4 CTRF 72L EZ1 LP830 (CI-236UVR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["245NLX","2ALL4 CTRF 72L EZ1 LP835 N100","2ALL4 CTRF 72L EZ1 LP835 N100 (CI-245NLX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["245P00","2ALL4 CTRF 72L EZ1 LP835 N100EMG","2ALL4 CTRF 72L EZ1 LP835 N100EMG (CI-245P00)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235AT9","2ALL4 CTRF 72L EZ1 LP840","2ALL4 CTRF 72L EZ1 LP840 (CI-235AT9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237LWH","2ALL4 CTRF 72L EZ1 LP840 N100","2ALL4 CTRF 72L EZ1 LP840 N100 (CI-237LWH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["245MAE","2ALL4 CTRF 72L EZ1 LP840 N80","2ALL4 CTRF 72L EZ1 LP840 N80 (CI-245MAE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["245NYH","2ALL4 CTRF 72L EZ1 LP840 N80EMG","2ALL4 CTRF 72L EZ1 LP840 N80EMG (CI-245NYH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["238HFX","2ALL4 CTRF 72L EZ1 PWS1436 LP835","2ALL4 CTRF 72L EZ1 PWS1436 LP835 (CI-238HFX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240AWN","2ALL4 CTRF 72L EZ1 PWS1836 LP840 N100","2ALL4 CTRF 72L EZ1 PWS1836 LP840 N100 (CI-240AWN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["239CFT","2ALL4 CTRF 72L EZ1 PWS1856LV LP835","2ALL4 CTRF 72L EZ1 PWS1856LV LP835 (CI-239CFT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["239J61","2ALL4 CTRF 72L EZB LP835","2ALL4 CTRF 72L EZB LP835 (CI-239J61)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236KKM","2ALL4 CTRF 72L SLD PWS1846 LP835","2ALL4 CTRF 72L SLD PWS1846 LP835 (CI-236KKM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["239WK2","ALL4 20L 120 EZ1 GLR LP835","ALL4 20L 120 EZ1 GLR LP835 (CI-239WK2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236RPF","ALL4 20L EZ1 LP830","ALL4 20L EZ1 LP830 (CI-236RPF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236EYK","ALL4 20L EZ1 LP830 N80","ALL4 20L EZ1 LP830 N80 (CI-236EYK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232JWN","ALL4 20L EZ1 LP835","ALL4 20L EZ1 LP835 (CI-232JWN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236E9A","ALL4 20L EZ1 LP835 N100","ALL4 20L EZ1 LP835 N100 (CI-236E9A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236E96","ALL4 20L EZ1 LP835 N100EMG","ALL4 20L EZ1 LP835 N100EMG (CI-236E96)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235JHP","ALL4 20L EZ1 LP835 N80","ALL4 20L EZ1 LP835 N80 (CI-235JHP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231YAP","ALL4 20L EZ1 LP840","ALL4 20L EZ1 LP840 (CI-231YAP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235KWR","ALL4 20L EZ1 LP840 N80","ALL4 20L EZ1 LP840 N80 (CI-235KWR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231W3G","ALL4 20L EZ1 LP850","ALL4 20L EZ1 LP850 (CI-231W3G)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238UP5","ALL4 20L EZ1 PWS1836 LP835","ALL4 20L EZ1 PWS1836 LP835 (CI-238UP5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235PJ3","ALL4 20L EZ1 PWS1856LV LP835","ALL4 20L EZ1 PWS1856LV LP835 (CI-235PJ3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232JT8","ALL4 20L SLD LP840","ALL4 20L SLD LP840 (CI-232JT8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C706,7)),6))","v":"224JXC"},{"$f":"LEFT(C706,SEARCH(\"(CI-\",C706)-2)","v":"ALL4 21L D24 LP830 NX"},"ALL4 21L D24 LP830 NX (CI-224JXC)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["226PNN","ALL4 21L D24 LP835 N100","ALL4 21L D24 LP835 N100 (CI-226PNN)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["227JYF","ALL4 21L D24 LP835 N100EMG","ALL4 21L D24 LP835 N100EMG (CI-227JYF)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["226JX2","ALL4 21L D24 LP835 N80","ALL4 21L D24 LP835 N80 (CI-226JX2)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["226JWN","ALL4 21L D24 LP835 N80EMG","ALL4 21L D24 LP835 N80EMG (CI-226JWN)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["223LUY","ALL4 21L D24 LP835 NX","ALL4 21L D24 LP835 NX (CI-223LUY)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["228WTV","ALL4 21L D24 LP840 BLD","ALL4 21L D24 LP840 BLD (CI-228WTV)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["224AX6","ALL4 21L D24 LP840 N80","ALL4 21L D24 LP840 N80 (CI-224AX6)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["223LE6","ALL4 21L D24 LP840 NX","ALL4 21L D24 LP840 NX (CI-223LE6)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["227RWF","ALL4 21L D24 PWS1836 LP830 N100","ALL4 21L D24 PWS1836 LP830 N100 (CI-227RWF)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["227T2P","ALL4 21L D24 PWS1836 LP835 N100","ALL4 21L D24 PWS1836 LP835 N100 (CI-227T2P)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["231ANY","ALL4 21L D24 PWS1836 LP835 N80","ALL4 21L D24 PWS1836 LP835 N80 (CI-231ANY)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["227RWH","ALL4 21L D24 PWS1836 LP835 NX","ALL4 21L D24 PWS1836 LP835 NX (CI-227RWH)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["235G5F","ALL4 30L EZ1 LP830","ALL4 30L EZ1 LP830 (CI-235G5F)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232E7M","ALL4 30L EZ1 LP835","ALL4 30L EZ1 LP835 (CI-232E7M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245WFK","ALL4 30L EZ1 LP835 CP","ALL4 30L EZ1 LP835 CP (CI-245WFK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239UU1","ALL4 30L EZ1 LP835 N100","ALL4 30L EZ1 LP835 N100 (CI-239UU1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238R8G","ALL4 30L EZ1 LP835 N80","ALL4 30L EZ1 LP835 N80 (CI-238R8G)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238R94","ALL4 30L EZ1 LP835 N80EMG","ALL4 30L EZ1 LP835 N80EMG (CI-238R94)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235F4C","ALL4 30L EZ1 LP840","ALL4 30L EZ1 LP840 (CI-235F4C)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233E08","ALL4 30L EZ1 LP840 N80","ALL4 30L EZ1 LP840 N80 (CI-233E08)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232LP9","ALL4 30L EZ1 LP850","ALL4 30L EZ1 LP850 (CI-232LP9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238UA8","ALL4 30L EZ1 PWS1836 LP835","ALL4 30L EZ1 PWS1836 LP835 (CI-238UA8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238UP2","ALL4 30L EZ1 PWS1846 LP835","ALL4 30L EZ1 PWS1846 LP835 (CI-238UP2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236KA5","ALL4 30L EZ1 PWS1856 LP840","ALL4 30L EZ1 PWS1856 LP840 (CI-236KA5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237NTT","ALL4 30L EZ1 PWS1856LV LP835","ALL4 30L EZ1 PWS1856LV LP835 (CI-237NTT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236LPU","ALL4 30L EZ1 PWS1856LV LP840","ALL4 30L EZ1 PWS1856LV LP840 (CI-236LPU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231YAW","ALL4 40L EZ1 LP830","ALL4 40L EZ1 LP830 (CI-231YAW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237X8J","ALL4 40L EZ1 LP830 N100","ALL4 40L EZ1 LP830 N100 (CI-237X8J)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231XPP","ALL4 40L EZ1 LP835","ALL4 40L EZ1 LP835 (CI-231XPP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245PFY","ALL4 40L EZ1 LP835 CP","ALL4 40L EZ1 LP835 CP (CI-245PFY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245PF1","ALL4 40L EZ1 LP835 CP/ not used","ALL4 40L EZ1 LP835 CP/ not used (CI-245PF1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233RNL","ALL4 40L EZ1 LP835 N100","ALL4 40L EZ1 LP835 N100 (CI-233RNL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232K7W","ALL4 40L EZ1 LP835 N80","ALL4 40L EZ1 LP835 N80 (CI-232K7W)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231XMC","ALL4 40L EZ1 LP840","ALL4 40L EZ1 LP840 (CI-231XMC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231YFY","ALL4 40L EZ1 LP840 N80","ALL4 40L EZ1 LP840 N80 (CI-231YFY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235VH5","ALL4 40L EZ1 LP840 N80EMG","ALL4 40L EZ1 LP840 N80EMG (CI-235VH5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231TYE","ALL4 40L EZ1 LP850","ALL4 40L EZ1 LP850 (CI-231TYE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235P5G","ALL4 40L EZ1 LP850 N80","ALL4 40L EZ1 LP850 N80 (CI-235P5G)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235LPE","ALL4 40L EZ1 PWS1836 LP835","ALL4 40L EZ1 PWS1836 LP835 (CI-235LPE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232PNN","ALL4 40L EZ1 PWS1846 LP840","ALL4 40L EZ1 PWS1846 LP840 (CI-232PNN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231NWH","ALL4 40L EZ1 PWS1856LV LP835","ALL4 40L EZ1 PWS1856LV LP835 (CI-231NWH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239WUG","ALL4 40L EZ1 PWS1856LV LP840","ALL4 40L EZ1 PWS1856LV LP840 (CI-239WUG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245PG3","ALL4 40L EZB LP835 CP","ALL4 40L EZB LP835 CP (CI-245PG3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225KA1","ALL4 43L D50 LP830 N100","ALL4 43L D50 LP830 N100 (CI-225KA1)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["224AXF","ALL4 43L D50 LP830 NX","ALL4 43L D50 LP830 NX (CI-224AXF)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["222PNX","ALL4 43L D50 LP835 N100","ALL4 43L D50 LP835 N100 (CI-222PNX)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["230H2T","ALL4 43L D50 LP835 N100EMG","ALL4 43L D50 LP835 N100EMG (CI-230H2T)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["224YW2","ALL4 43L D50 LP835 N80","ALL4 43L D50 LP835 N80 (CI-224YW2)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["222PNR","ALL4 43L D50 LP835 NX","ALL4 43L D50 LP835 NX (CI-222PNR)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["231CN5","ALL4 43L D50 LP840 CP NX","ALL4 43L D50 LP840 CP NX (CI-231CN5)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["225T31","ALL4 43L D50 LP840 N100","ALL4 43L D50 LP840 N100 (CI-225T31)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["229UHR","ALL4 43L D50 LP840 N80","ALL4 43L D50 LP840 N80 (CI-229UHR)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["222U2X","ALL4 43L D50 LP840 NX","ALL4 43L D50 LP840 NX (CI-222U2X)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["224VUT","ALL4 43L D50 LP850 NX","ALL4 43L D50 LP850 NX (CI-224VUT)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["225JV9","ALL4 43L D50 PWS1836 LP835 N100","ALL4 43L D50 PWS1836 LP835 N100 (CI-225JV9)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["236VCC","ALL4 48L EZ1 LP830","ALL4 48L EZ1 LP830 (CI-236VCC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232EM0","ALL4 48L EZ1 LP835","ALL4 48L EZ1 LP835 (CI-232EM0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236G8M","ALL4 48L EZ1 LP835 N100","ALL4 48L EZ1 LP835 N100 (CI-236G8M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237L37","ALL4 48L EZ1 LP835 N100EMG","ALL4 48L EZ1 LP835 N100EMG (CI-237L37)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["247UG7","ALL4 48L EZ1 LP835 N80","ALL4 48L EZ1 LP835 N80 (CI-247UG7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233R37","ALL4 48L EZ1 LP840","ALL4 48L EZ1 LP840 (CI-233R37)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233C21","ALL4 48L EZ1 LP840 LATC","ALL4 48L EZ1 LP840 LATC (CI-233C21)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234F2R","ALL4 48L EZ1 LP840 N100","ALL4 48L EZ1 LP840 N100 (CI-234F2R)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C770,7)),6))","v":"232C8C"},{"$f":"LEFT(C770,SEARCH(\"(CI-\",C770)-2)","v":"ALL4 48L EZ1 PWS1836 LP835"},"ALL4 48L EZ1 PWS1836 LP835 (CI-232C8C)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232C6W","ALL4 48L EZ1 PWS1846 LP835","ALL4 48L EZ1 PWS1846 LP835 (CI-232C6W)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231RWF","ALL4 48L EZ1 PWS1856LV LP835","ALL4 48L EZ1 PWS1856LV LP835 (CI-231RWF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240LFJ","ALL4 48L EZB LP835","ALL4 48L EZB LP835 (CI-240LFJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239AA7","ALL4 48L EZB PWS1856LV LP840","ALL4 48L EZB PWS1856LV LP840 (CI-239AA7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236VC9","ALL4 60L EZ1 LP830","ALL4 60L EZ1 LP830 (CI-236VC9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232CFX","ALL4 60L EZ1 LP835","ALL4 60L EZ1 LP835 (CI-232CFX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["243P31","ALL4 60L EZ1 LP835 N80","ALL4 60L EZ1 LP835 N80 (CI-243P31)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231YFJ","ALL4 60L EZ1 LP840","ALL4 60L EZ1 LP840 (CI-231YFJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233L7C","ALL4 60L EZ1 LP840 N100","ALL4 60L EZ1 LP840 N100 (CI-233L7C)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234RKY","ALL4 60L EZ1 LP850","ALL4 60L EZ1 LP850 (CI-234RKY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232C6P","ALL4 60L EZ1 PWS1836 LP835","ALL4 60L EZ1 PWS1836 LP835 (CI-232C6P)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232C6C","ALL4 60L EZ1 PWS1846 LP835","ALL4 60L EZ1 PWS1846 LP835 (CI-232C6C)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225NPH","ALL4 64L D75 LP835 N100","ALL4 64L D75 LP835 N100 (CI-225NPH)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["229HAL","ALL4 64L D75 LP835 N80","ALL4 64L D75 LP835 N80 (CI-229HAL)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["226LX8","ALL4 64L D75 LP835 NX","ALL4 64L D75 LP835 NX (CI-226LX8)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["229CEY","ALL4 64L D75 LP835 NX USPOM","ALL4 64L D75 LP835 NX USPOM (CI-229CEY)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["225TKA","ALL4 64L D75 LP840 N100","ALL4 64L D75 LP840 N100 (CI-225TKA)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["225NPJ","ALL4 64L D75 LP840 NX","ALL4 64L D75 LP840 NX (CI-225NPJ)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["228YK7","ALL4 64L D75 PWS1836 LP835 N80","ALL4 64L D75 PWS1836 LP835 N80 (CI-228YK7)","PS1030","3 inches minimum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["238YAK","ALL4 CTRF 20L EZ1 LP830","ALL4 CTRF 20L EZ1 LP830 (CI-238YAK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232F4E","ALL4 CTRF 20L EZ1 LP835","ALL4 CTRF 20L EZ1 LP835 (CI-232F4E)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233GLW","ALL4 CTRF 20L EZ1 LP840","ALL4 CTRF 20L EZ1 LP840 (CI-233GLW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["238CUG","ALL4 CTRF 20L EZ1 PWS1836 LP835","ALL4 CTRF 20L EZ1 PWS1836 LP835 (CI-238CUG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231Y5H","ALL4 CTRF 20L EZB LP840","ALL4 CTRF 20L EZB LP840 (CI-231Y5H)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["251P29","ALL4 CTRF 30L 277 EZ1 GMF LP835","ALL4 CTRF 30L 277 EZ1 GMF LP835 (CI-251P29)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232F7N","ALL4 CTRF 30L EZ1 LP835","ALL4 CTRF 30L EZ1 LP835 (CI-232F7N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["241L5R","ALL4 CTRF 30L EZ1 LP835 N100 CS1WL10 SSQ","ALL4 CTRF 30L EZ1 LP835 N100 CS1WL10 SSQ (CI-241L5R)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["241KK0","ALL4 CTRF 30L EZ1 LP835 N100 SSQ","ALL4 CTRF 30L EZ1 LP835 N100 SSQ (CI-241KK0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235V80","ALL4 CTRF 30L EZ1 LP840","ALL4 CTRF 30L EZ1 LP840 (CI-235V80)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237L31","ALL4 CTRF 30L EZ1 LP840 N80","ALL4 CTRF 30L EZ1 LP840 N80 (CI-237L31)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["245P0G","ALL4 CTRF 30L EZ1 LP840 N80EMG","ALL4 CTRF 30L EZ1 LP840 N80EMG (CI-245P0G)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240XWJ","ALL4 CTRF 30L EZ1 PWS1836 LP835","ALL4 CTRF 30L EZ1 PWS1836 LP835 (CI-240XWJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240J1M","ALL4 CTRF 30L EZ1 PWS1836 LP840","ALL4 CTRF 30L EZ1 PWS1836 LP840 (CI-240J1M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235ATG","ALL4 CTRF 30L EZ1 PWS1856LV LP830","ALL4 CTRF 30L EZ1 PWS1856LV LP830 (CI-235ATG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["238CUT","ALL4 CTRF 30L EZ1 PWS1856LV LP835","ALL4 CTRF 30L EZ1 PWS1856LV LP835 (CI-238CUT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["241FR0","ALL4 CTRF 30L EZ1 PWS1856LV LP840","ALL4 CTRF 30L EZ1 PWS1856LV LP840 (CI-241FR0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231KHM","ALL4 CTRF 40L EZ1 LP835","ALL4 CTRF 40L EZ1 LP835 (CI-231KHM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234AY3","ALL4 CTRF 40L EZ1 LP835 N100","ALL4 CTRF 40L EZ1 LP835 N100 (CI-234AY3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240L2X","ALL4 CTRF 40L EZ1 LP835 N100EMG","ALL4 CTRF 40L EZ1 LP835 N100EMG (CI-240L2X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233XJE","ALL4 CTRF 40L EZ1 LP840","ALL4 CTRF 40L EZ1 LP840 (CI-233XJE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237G48","ALL4 CTRF 40L EZ1 LP840 N100","ALL4 CTRF 40L EZ1 LP840 N100 (CI-237G48)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["239ML8","ALL4 CTRF 40L EZ1 LP840 ST3","ALL4 CTRF 40L EZ1 LP840 ST3 (CI-239ML8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232K8Y","ALL4 CTRF 40L EZ1 LP850","ALL4 CTRF 40L EZ1 LP850 (CI-232K8Y)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237V8T","ALL4 CTRF 40L EZ1 PWS1236 LP835","ALL4 CTRF 40L EZ1 PWS1236 LP835 (CI-237V8T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237A58","ALL4 CTRF 40L EZ1 PWS1856LV LP835","ALL4 CTRF 40L EZ1 PWS1856LV LP835 (CI-237A58)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240HYA","ALL4 CTRF 40L EZB LP835 N100","ALL4 CTRF 40L EZB LP835 N100 (CI-240HYA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233KJN","ALL4 CTRF 40L SLD LP835","ALL4 CTRF 40L SLD LP835 (CI-233KJN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232F4E","ALL4 CTRF 20L EZ1 LP835","ALL4 CTRF 20L EZ1 LP835 (CI-232F4E)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233GLW","ALL4 CTRF 20L EZ1 LP840","ALL4 CTRF 20L EZ1 LP840 (CI-233GLW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231Y5H","ALL4 CTRF 20L EZB LP840","ALL4 CTRF 20L EZB LP840 (CI-231Y5H)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232F7N","ALL4 CTRF 30L EZ1 LP835","ALL4 CTRF 30L EZ1 LP835 (CI-232F7N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231KHM","ALL4 CTRF 40L EZ1 LP835","ALL4 CTRF 40L EZ1 LP835 (CI-231KHM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234AY3","ALL4 CTRF 40L EZ1 LP835 N100","ALL4 CTRF 40L EZ1 LP835 N100 (CI-234AY3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233XJE","ALL4 CTRF 40L EZ1 LP840","ALL4 CTRF 40L EZ1 LP840 (CI-233XJE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232K8Y","ALL4 CTRF 40L EZ1 LP850","ALL4 CTRF 40L EZ1 LP850 (CI-232K8Y)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233KJN","ALL4 CTRF 40L SLD LP835","ALL4 CTRF 40L SLD LP835 (CI-233KJN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232GKL","ALLS4 20L EZ1 LP835","ALLS4 20L EZ1 LP835 (CI-232GKL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231YG8","ALLS4 20L EZ1 LP840","ALLS4 20L EZ1 LP840 (CI-231YG8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234G3G","ALLS4 20L EZ1 LP840 N80","ALLS4 20L EZ1 LP840 N80 (CI-234G3G)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232NVC","ALLS4 20L EZB LP835","ALLS4 20L EZB LP835 (CI-232NVC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233GTN","ALLS4 30L EZ1 LP835","ALLS4 30L EZ1 LP835 (CI-233GTN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233G1U","ALLS4 30L EZ1 LP835 N80","ALLS4 30L EZ1 LP835 N80 (CI-233G1U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232X8Y","ALLS4 30L EZ1 LP840","ALLS4 30L EZ1 LP840 (CI-232X8Y)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C834,7)),6))","v":"232CP0"},{"$f":"LEFT(C834,SEARCH(\"(CI-\",C834)-2)","v":"ALLS4 30L EZ1 LP850 N80"},"ALLS4 30L EZ1 LP850 N80 (CI-232CP0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231XKW","ALLS4 40L EZ1 LP835","ALLS4 40L EZ1 LP835 (CI-231XKW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233K92","ALLS4 40L EZ1 LP835 N80","ALLS4 40L EZ1 LP835 N80 (CI-233K92)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231TXX","ALLS4 40L EZ1 LP840","ALLS4 40L EZ1 LP840 (CI-231TXX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234XNR","ALLS4 40L EZ1 LP840 N100","ALLS4 40L EZ1 LP840 N100 (CI-234XNR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233HX7","ALLS4 40L EZ1 LP840 N80","ALLS4 40L EZ1 LP840 N80 (CI-233HX7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233X39","ALLS4 40L EZ1 LP850","ALLS4 40L EZ1 LP850 (CI-233X39)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234XPV","ALLS4 40L EZB LP840","ALLS4 40L EZB LP840 (CI-234XPV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232XXU","ALLS4 40L SLD LP840","ALLS4 40L SLD LP840 (CI-232XXU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232LM3","ALLS4 48L EZ1 LP835","ALLS4 48L EZ1 LP835 (CI-232LM3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231VE8","ALLS4 48L EZ1 LP840","ALLS4 48L EZ1 LP840 (CI-231VE8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232Y70","ALLS4 48L EZ1 LP840 N100","ALLS4 48L EZ1 LP840 N100 (CI-232Y70)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232WJW","ALLS4 60L EZ1 LP835","ALLS4 60L EZ1 LP835 (CI-232WJW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231Y3R","2AVL2 20L ADP EZ1 LP835","2AVL2 20L ADP EZ1 LP835 (CI-231Y3R)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234FK4","2AVL2 20L ADP EZ1 LP835 JP20","2AVL2 20L ADP EZ1 LP835 JP20 (CI-234FK4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229UFY","2AVL2 20L MDR EZ1 LP830","2AVL2 20L MDR EZ1 LP830 (CI-229UFY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233E3U","2AVL2 20L MDR EZ1 LP830 JP20","2AVL2 20L MDR EZ1 LP830 JP20 (CI-233E3U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232MW1","2AVL2 20L MDR EZ1 LP830 N100","2AVL2 20L MDR EZ1 LP830 N100 (CI-232MW1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232MW6","2AVL2 20L MDR EZ1 LP830 N100 JP20","2AVL2 20L MDR EZ1 LP830 N100 JP20 (CI-232MW6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231G7G","2AVL2 20L MDR EZ1 LP830 N80","2AVL2 20L MDR EZ1 LP830 N80 (CI-231G7G)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233VXU","2AVL2 20L MDR EZ1 LP830 N80 RFD192914","2AVL2 20L MDR EZ1 LP830 N80 RFD192914 (CI-233VXU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230YLY","2AVL2 20L MDR EZ1 LP835","2AVL2 20L MDR EZ1 LP835 (CI-230YLY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234L5C","2AVL2 20L MDR EZ1 LP835 JP20","2AVL2 20L MDR EZ1 LP835 JP20 (CI-234L5C)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230AGX","2AVL2 20L MDR EZ1 LP835 N100","2AVL2 20L MDR EZ1 LP835 N100 (CI-230AGX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231T6C","2AVL2 20L MDR EZ1 LP835 N80","2AVL2 20L MDR EZ1 LP835 N80 (CI-231T6C)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231C61","2AVL2 20L MDR EZ1 LP840","2AVL2 20L MDR EZ1 LP840 (CI-231C61)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232G12","2AVL2 20L MDR EZ1 LP840 JP20","2AVL2 20L MDR EZ1 LP840 JP20 (CI-232G12)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232XGR","2AVL2 20L MDR EZ1 PWS1836 LP830 N100","2AVL2 20L MDR EZ1 PWS1836 LP830 N100 (CI-232XGR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234L7R","2AVL2 20L MDR EZ1 PWS1836 LP840","2AVL2 20L MDR EZ1 PWS1836 LP840 (CI-234L7R)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234HMV","2AVL2 20L MDR EZ1 PWS1856LV LP835","2AVL2 20L MDR EZ1 PWS1856LV LP835 (CI-234HMV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232YG5","2AVL2 30L ADP EZ1 LP835","2AVL2 30L ADP EZ1 LP835 (CI-232YG5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234HG6","2AVL2 30L ADP EZ1 LP835 JP20","2AVL2 30L ADP EZ1 LP835 JP20 (CI-234HG6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231E75","2AVL2 30L ADP EZ1 LP835 N100","2AVL2 30L ADP EZ1 LP835 N100 (CI-231E75)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231E64","2AVL2 30L ADP EZ1 LP835 N100 JP20","2AVL2 30L ADP EZ1 LP835 N100 JP20 (CI-231E64)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231AVY","2AVL2 30L ADP EZ1 LP840","2AVL2 30L ADP EZ1 LP840 (CI-231AVY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232VJ3","2AVL2 30L ADP EZ1 LP840 N100","2AVL2 30L ADP EZ1 LP840 N100 (CI-232VJ3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232VHP","2AVL2 30L ADP EZ1 LP840 N100 JP20","2AVL2 30L ADP EZ1 LP840 N100 JP20 (CI-232VHP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229E51","2AVL2 30L MDR EZ1 LP830","2AVL2 30L MDR EZ1 LP830 (CI-229E51)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233XNT","2AVL2 30L MDR EZ1 LP830 CP","2AVL2 30L MDR EZ1 LP830 CP (CI-233XNT)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233XP1","2AVL2 30L MDR EZ1 LP830 CP JP20","2AVL2 30L MDR EZ1 LP830 CP JP20 (CI-233XP1)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232EYH","2AVL2 30L MDR EZ1 LP830 JP20","2AVL2 30L MDR EZ1 LP830 JP20 (CI-232EYH)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233HMC","2AVL2 30L MDR EZ1 LP830 N100","2AVL2 30L MDR EZ1 LP830 N100 (CI-233HMC)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233JG6","2AVL2 30L MDR EZ1 LP830 N100 JP20","2AVL2 30L MDR EZ1 LP830 N100 JP20 (CI-233JG6)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231G7A","2AVL2 30L MDR EZ1 LP830 N80","2AVL2 30L MDR EZ1 LP830 N80 (CI-231G7A)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["229E42","2AVL2 30L MDR EZ1 LP835","2AVL2 30L MDR EZ1 LP835 (CI-229E42)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230KF8","2AVL2 30L MDR EZ1 LP835 JP20","2AVL2 30L MDR EZ1 LP835 JP20 (CI-230KF8)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234J8M","2AVL2 30L MDR EZ1 LP835 LATC","2AVL2 30L MDR EZ1 LP835 LATC (CI-234J8M)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234J9J","2AVL2 30L MDR EZ1 LP835 LATC JP20","2AVL2 30L MDR EZ1 LP835 LATC JP20 (CI-234J9J)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230AGA","2AVL2 30L MDR EZ1 LP835 N100","2AVL2 30L MDR EZ1 LP835 N100 (CI-230AGA)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232W3L","2AVL2 30L MDR EZ1 LP835 N100 JP20","2AVL2 30L MDR EZ1 LP835 N100 JP20 (CI-232W3L)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231T6G","2AVL2 30L MDR EZ1 LP835 N80","2AVL2 30L MDR EZ1 LP835 N80 (CI-231T6G)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["229E54","2AVL2 30L MDR EZ1 LP840","2AVL2 30L MDR EZ1 LP840 (CI-229E54)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231GE4","2AVL2 30L MDR EZ1 LP840 JP20","2AVL2 30L MDR EZ1 LP840 JP20 (CI-231GE4)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231T6L","2AVL2 30L MDR EZ1 LP840 N100","2AVL2 30L MDR EZ1 LP840 N100 (CI-231T6L)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231T6H","2AVL2 30L MDR EZ1 LP840 N100 JP20","2AVL2 30L MDR EZ1 LP840 N100 JP20 (CI-231T6H)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234FA0","2AVL2 30L MDR EZ1 LP850","2AVL2 30L MDR EZ1 LP850 (CI-234FA0)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230MRL","2AVL2 30L MDR EZ1 LP850 N100","2AVL2 30L MDR EZ1 LP850 N100 (CI-230MRL)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234KCP","2AVL2 30L MDR EZ1 PWS1836 LP835","2AVL2 30L MDR EZ1 PWS1836 LP835 (CI-234KCP)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234GVG","2AVL2 30L MDR EZ1 PWS1856LV LP835","2AVL2 30L MDR EZ1 PWS1856LV LP835 (CI-234GVG)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234GVT","2AVL2 30L MDR EZ1 PWS1856LV LP835 JP16","2AVL2 30L MDR EZ1 PWS1856LV LP835 JP16 (CI-234GVT)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231AVU","2AVL2 30L SBL EZ1 LP835","2AVL2 30L SBL EZ1 LP835 (CI-231AVU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233R6H","2AVL2 30L SBL EZ1 LP835 JP20","2AVL2 30L SBL EZ1 LP835 JP20 (CI-233R6H)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232AHY","2AVL2 40L ADP EZ1 LP835","2AVL2 40L ADP EZ1 LP835 (CI-232AHY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234AXV","2AVL2 40L ADP EZ1 LP835 JP20","2AVL2 40L ADP EZ1 LP835 JP20 (CI-234AXV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C898,7)),6))","v":"232AK3"},{"$f":"LEFT(C898,SEARCH(\"(CI-\",C898)-2)","v":"2AVL2 40L ADP EZ1 LP840"},"2AVL2 40L ADP EZ1 LP840 (CI-232AK3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232CNP","2AVL2 40L ADP EZ1 LP840 CP","2AVL2 40L ADP EZ1 LP840 CP (CI-232CNP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232VHY","2AVL2 40L ADP EZ1 LP840 N100","2AVL2 40L ADP EZ1 LP840 N100 (CI-232VHY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232VHW","2AVL2 40L ADP EZ1 LP840 N100 JP20","2AVL2 40L ADP EZ1 LP840 N100 JP20 (CI-232VHW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233N1L","2AVL2 40L MDR EZ1 LP830","2AVL2 40L MDR EZ1 LP830 (CI-233N1L)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["229E4H","2AVL2 40L MDR EZ1 LP835","2AVL2 40L MDR EZ1 LP835 (CI-229E4H)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["230TL3","2AVL2 40L MDR EZ1 LP835 JP20","2AVL2 40L MDR EZ1 LP835 JP20 (CI-230TL3)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["230MU0","2AVL2 40L MDR EZ1 LP835 N100","2AVL2 40L MDR EZ1 LP835 N100 (CI-230MU0)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["233AXE","2AVL2 40L MDR EZ1 LP835 N100 JP20","2AVL2 40L MDR EZ1 LP835 N100 JP20 (CI-233AXE)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["230NWY","2AVL2 40L MDR EZ1 LP835 N80","2AVL2 40L MDR EZ1 LP835 N80 (CI-230NWY)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["230NK5","2AVL2 40L MDR EZ1 LP835 N80 JP20","2AVL2 40L MDR EZ1 LP835 N80 JP20 (CI-230NK5)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["230G0M","2AVL2 40L MDR EZ1 LP840","2AVL2 40L MDR EZ1 LP840 (CI-230G0M)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["232XEU","2AVL2 40L MDR EZ1 LP840 JP20","2AVL2 40L MDR EZ1 LP840 JP20 (CI-232XEU)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["231MV3","2AVL2 40L MDR EZ1 LP840 N100","2AVL2 40L MDR EZ1 LP840 N100 (CI-231MV3)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["233GGA","2AVL2 40L MDR EZ1 LP840 N100 JP20","2AVL2 40L MDR EZ1 LP840 N100 JP20 (CI-233GGA)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["232VGE","2AVL2 40L MDR EZ1 LP840 N80","2AVL2 40L MDR EZ1 LP840 N80 (CI-232VGE)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["231A26","2AVL2 40L MDR EZ1 LP850","2AVL2 40L MDR EZ1 LP850 (CI-231A26)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["231JTP","2AVL2 40L MDR EZ1 PWS1836 LP835","2AVL2 40L MDR EZ1 PWS1836 LP835 (CI-231JTP)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["232CK0","2AVL2 40L MDR EZ1 PWS1836 LP835 JP20","2AVL2 40L MDR EZ1 PWS1836 LP835 JP20 (CI-232CK0)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["232NJT","2AVL2 40L MDR EZ1 PWS1836 LP840","2AVL2 40L MDR EZ1 PWS1836 LP840 (CI-232NJT)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["234FAJ","2AVL2 40L MDR EZ1 PWS1856LV LP835","2AVL2 40L MDR EZ1 PWS1856LV LP835 (CI-234FAJ)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["233L2W","2AVL2 40L SBL EZ1 LP835","2AVL2 40L SBL EZ1 LP835 (CI-233L2W)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230MPT","2AVL2 40L SBL EZ1 LP835 N100","2AVL2 40L SBL EZ1 LP835 N100 (CI-230MPT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231FNC","2AVL2 A 30L MDR EZ1 LP835","2AVL2 A 30L MDR EZ1 LP835 (CI-231FNC)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233EPG","2AVL2 A 40L MDR EZ1 LP835 N100","2AVL2 A 40L MDR EZ1 LP835 N100 (CI-233EPG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234F3A","2AVL2 A 40L SBL EZ1 LP835","2AVL2 A 40L SBL EZ1 LP835 (CI-234F3A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231EV7","2AVL4 30L ADP EZ1 LP835","2AVL4 30L ADP EZ1 LP835 (CI-231EV7)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231R5N","2AVL4 30L ADP EZ1 LP835 JP10","2AVL4 30L ADP EZ1 LP835 JP10 (CI-231R5N)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234XT4","2AVL4 30L ADP EZ1 LP840 N100","2AVL4 30L ADP EZ1 LP840 N100 (CI-234XT4)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234XT1","2AVL4 30L ADP EZ1 LP840 N100 JP10","2AVL4 30L ADP EZ1 LP840 N100 JP10 (CI-234XT1)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231A1N","2AVL4 30L MDR EZ1 LP830","2AVL4 30L MDR EZ1 LP830 (CI-231A1N)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233HLH","2AVL4 30L MDR EZ1 LP830 N100","2AVL4 30L MDR EZ1 LP830 N100 (CI-233HLH)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233HL4","2AVL4 30L MDR EZ1 LP830 N100 JP10","2AVL4 30L MDR EZ1 LP830 N100 JP10 (CI-233HL4)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230V5N","2AVL4 30L MDR EZ1 LP835","2AVL4 30L MDR EZ1 LP835 (CI-230V5N)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233VPJ","2AVL4 30L MDR EZ1 LP835 CP","2AVL4 30L MDR EZ1 LP835 CP (CI-233VPJ)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231YU2","2AVL4 30L MDR EZ1 LP835 JP10","2AVL4 30L MDR EZ1 LP835 JP10 (CI-231YU2)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233TY0","2AVL4 30L MDR EZ1 LP835 N100","2AVL4 30L MDR EZ1 LP835 N100 (CI-233TY0)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233U2Y","2AVL4 30L MDR EZ1 LP835 N80","2AVL4 30L MDR EZ1 LP835 N80 (CI-233U2Y)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233U2U","2AVL4 30L MDR EZ1 LP835 N80 JP10","2AVL4 30L MDR EZ1 LP835 N80 JP10 (CI-233U2U)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232PCT","2AVL4 30L MDR EZ1 LP840","2AVL4 30L MDR EZ1 LP840 (CI-232PCT)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232RRV","2AVL4 30L MDR EZ1 LP840 JP10","2AVL4 30L MDR EZ1 LP840 JP10 (CI-232RRV)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233FF3","2AVL4 30L MDR EZ1 LP840 N100","2AVL4 30L MDR EZ1 LP840 N100 (CI-233FF3)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234HR0","2AVL4 30L MDR EZ1 LP840 N100 USPOM","2AVL4 30L MDR EZ1 LP840 N100 USPOM (CI-234HR0)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234HR3","2AVL4 30L MDR EZ1 LP840 N100 USPOM JP10","2AVL4 30L MDR EZ1 LP840 N100 USPOM JP10 (CI-234HR3)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232L38","2AVL4 30L MDR EZ1 LP850","2AVL4 30L MDR EZ1 LP850 (CI-232L38)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232P32","2AVL4 30L MDR EZ1 PWS1836 LP835","2AVL4 30L MDR EZ1 PWS1836 LP835 (CI-232P32)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232P10","2AVL4 30L MDR EZ1 PWS1836 LP835 JP10","2AVL4 30L MDR EZ1 PWS1836 LP835 JP10 (CI-232P10)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234HP3","2AVL4 30L MDR EZ1 PWS1836 LP835 N80","2AVL4 30L MDR EZ1 PWS1836 LP835 N80 (CI-234HP3)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234HR6","2AVL4 30L MDR EZ1 PWS1856LV LP835","2AVL4 30L MDR EZ1 PWS1856LV LP835 (CI-234HR6)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234HRK","2AVL4 30L MDR EZ1 PWS1856LV LP835 JP10","2AVL4 30L MDR EZ1 PWS1856LV LP835 JP10 (CI-234HRK)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232GJ0","2AVL4 40L ADP EZ1 LP835","2AVL4 40L ADP EZ1 LP835 (CI-232GJ0)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230F35","2AVL4 40L ADP EZ1 LP835 N80","2AVL4 40L ADP EZ1 LP835 N80 (CI-230F35)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231AW4","2AVL4 40L ADP EZ1 LP840","2AVL4 40L ADP EZ1 LP840 (CI-231AW4)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231AWM","2AVL4 40L ADP EZ1 LP840 JP10","2AVL4 40L ADP EZ1 LP840 JP10 (CI-231AWM)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234TK7","2AVL4 40L ADP EZ1 PWS1856LV LP835","2AVL4 40L ADP EZ1 PWS1856LV LP835 (CI-234TK7)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233YWF","2AVL4 40L ADP EZ1 PWS1856LV LP840","2AVL4 40L ADP EZ1 PWS1856LV LP840 (CI-233YWF)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231GV5","2AVL4 40L MDR EZ1 LP830","2AVL4 40L MDR EZ1 LP830 (CI-231GV5)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232T22","2AVL4 40L MDR EZ1 LP830 JP10","2AVL4 40L MDR EZ1 LP830 JP10 (CI-232T22)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234JNC","2AVL4 40L MDR EZ1 LP830 N100","2AVL4 40L MDR EZ1 LP830 N100 (CI-234JNC)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234JNK","2AVL4 40L MDR EZ1 LP830 N100 JP10","2AVL4 40L MDR EZ1 LP830 N100 JP10 (CI-234JNK)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["229E8F","2AVL4 40L MDR EZ1 LP835","2AVL4 40L MDR EZ1 LP835 (CI-229E8F)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230YM5","2AVL4 40L MDR EZ1 LP835 JP10","2AVL4 40L MDR EZ1 LP835 JP10 (CI-230YM5)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230GX9","2AVL4 40L MDR EZ1 LP835 N100","2AVL4 40L MDR EZ1 LP835 N100 (CI-230GX9)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230P0W","2AVL4 40L MDR EZ1 LP835 N100 JP10","2AVL4 40L MDR EZ1 LP835 N100 JP10 (CI-230P0W)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
[{"$f":"(LEFT((RIGHT(C962,7)),6))","v":"229E8T"},{"$f":"LEFT(C962,SEARCH(\"(CI-\",C962)-2)","v":"2AVL4 40L MDR EZ1 LP835 N80"},"2AVL4 40L MDR EZ1 LP835 N80 (CI-229E8T)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233PH4","2AVL4 40L MDR EZ1 LP835 N80 JP10","2AVL4 40L MDR EZ1 LP835 N80 JP10 (CI-233PH4)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230G0P","2AVL4 40L MDR EZ1 LP840","2AVL4 40L MDR EZ1 LP840 (CI-230G0P)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231UYW","2AVL4 40L MDR EZ1 LP840 JP10","2AVL4 40L MDR EZ1 LP840 JP10 (CI-231UYW)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230GET","2AVL4 40L MDR EZ1 LP840 N100","2AVL4 40L MDR EZ1 LP840 N100 (CI-230GET)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232GJ8","2AVL4 40L MDR EZ1 LP840 N100 JP10","2AVL4 40L MDR EZ1 LP840 N100 JP10 (CI-232GJ8)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231WFV","2AVL4 40L MDR EZ1 LP840 N80","2AVL4 40L MDR EZ1 LP840 N80 (CI-231WFV)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231A22","2AVL4 40L MDR EZ1 LP850","2AVL4 40L MDR EZ1 LP850 (CI-231A22)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233P0E","2AVL4 40L MDR EZ1 LP850 JP10","2AVL4 40L MDR EZ1 LP850 JP10 (CI-233P0E)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233VH3","2AVL4 40L MDR EZ1 LP850 N100","2AVL4 40L MDR EZ1 LP850 N100 (CI-233VH3)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234JYR","2AVL4 40L MDR EZ1 PWS1836 LP835","2AVL4 40L MDR EZ1 PWS1836 LP835 (CI-234JYR)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234K01","2AVL4 40L MDR EZ1 PWS1836 LP835 JP10","2AVL4 40L MDR EZ1 PWS1836 LP835 JP10 (CI-234K01)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232YGF","2AVL4 40L MDR EZ1 PWS1836 LP840","2AVL4 40L MDR EZ1 PWS1836 LP840 (CI-232YGF)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232YFF","2AVL4 40L MDR EZ1 PWS1836 LP840 JP10","2AVL4 40L MDR EZ1 PWS1836 LP840 JP10 (CI-232YFF)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234XPC","2AVL4 40L MDR EZ1 PWS1856LV LP835 JP10","2AVL4 40L MDR EZ1 PWS1856LV LP835 JP10 (CI-234XPC)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234EEW","2AVL4 40L SBL EZ1 LP835","2AVL4 40L SBL EZ1 LP835 (CI-234EEW)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233R6N","2AVL4 40L SBL EZ1 LP835 JP10","2AVL4 40L SBL EZ1 LP835 JP10 (CI-233R6N)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233U9V","2AVL4 40L SBL EZ1 LP840","2AVL4 40L SBL EZ1 LP840 (CI-233U9V)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231EC2","2AVL4 40L SBL EZ1 LP840 JP10","2AVL4 40L SBL EZ1 LP840 JP10 (CI-231EC2)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230AFJ","2AVL4 40L SBL EZ1 LP840 N80","2AVL4 40L SBL EZ1 LP840 N80 (CI-230AFJ)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231RK9","2AVL4 50L ADP EZ1 LP835","2AVL4 50L ADP EZ1 LP835 (CI-231RK9)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233YE9","2AVL4 50L ADP EZ1 LP835 JP10","2AVL4 50L ADP EZ1 LP835 JP10 (CI-233YE9)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231U60","2AVL4 50L ADP EZ1 LP840","2AVL4 50L ADP EZ1 LP840 (CI-231U60)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234K7T","2AVL4 50L ADP EZ1 LP840 N100","2AVL4 50L ADP EZ1 LP840 N100 (CI-234K7T)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233YYX","2AVL4 50L ADP EZ1 PWS1856LV LP840","2AVL4 50L ADP EZ1 PWS1856LV LP840 (CI-233YYX)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233F5A","2AVL4 50L MDR EZ1 LP830","2AVL4 50L MDR EZ1 LP830 (CI-233F5A)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233F58","2AVL4 50L MDR EZ1 LP830 JP10","2AVL4 50L MDR EZ1 LP830 JP10 (CI-233F58)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["229E8L","2AVL4 50L MDR EZ1 LP835","2AVL4 50L MDR EZ1 LP835 (CI-229E8L)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231RR8","2AVL4 50L MDR EZ1 LP835 JP10","2AVL4 50L MDR EZ1 LP835 JP10 (CI-231RR8)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232KYN","2AVL4 50L MDR EZ1 LP835 N100","2AVL4 50L MDR EZ1 LP835 N100 (CI-232KYN)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232LC0","2AVL4 50L MDR EZ1 LP835 N100 JP10","2AVL4 50L MDR EZ1 LP835 N100 JP10 (CI-232LC0)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232F41","2AVL4 50L MDR EZ1 LP835 N80","2AVL4 50L MDR EZ1 LP835 N80 (CI-232F41)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232F5M","2AVL4 50L MDR EZ1 LP835 N80 JP10","2AVL4 50L MDR EZ1 LP835 N80 JP10 (CI-232F5M)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230T40","2AVL4 50L MDR EZ1 LP840","2AVL4 50L MDR EZ1 LP840 (CI-230T40)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231E1V","2AVL4 50L MDR EZ1 LP840 JP10","2AVL4 50L MDR EZ1 LP840 JP10 (CI-231E1V)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231V8V","2AVL4 50L MDR EZ1 LP840 N100","2AVL4 50L MDR EZ1 LP840 N100 (CI-231V8V)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234C0M","2AVL4 50L MDR EZ1 LP840 N100 JP10","2AVL4 50L MDR EZ1 LP840 N100 JP10 (CI-234C0M)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234HPT","2AVL4 50L MDR EZ1 LP840 N100 USPOM","2AVL4 50L MDR EZ1 LP840 N100 USPOM (CI-234HPT)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233TPC","2AVL4 50L MDR EZ1 LP840 N80","2AVL4 50L MDR EZ1 LP840 N80 (CI-233TPC)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233UFT","2AVL4 50L MDR EZ1 LP840 N80 JP10","2AVL4 50L MDR EZ1 LP840 N80 JP10 (CI-233UFT)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232L7P","2AVL4 50L MDR EZ1 LP850","2AVL4 50L MDR EZ1 LP850 (CI-232L7P)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232L78","2AVL4 50L MDR EZ1 LP850 JP10","2AVL4 50L MDR EZ1 LP850 JP10 (CI-232L78)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230MJH","2AVL4 50L MDR EZ1 LP850 N100","2AVL4 50L MDR EZ1 LP850 N100 (CI-230MJH)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234V55","2AVL4 50L MDR EZ1 PWS1836 LP835","2AVL4 50L MDR EZ1 PWS1836 LP835 (CI-234V55)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231TCM","2AVL4 50L MDR EZ1 PWS1836 LP835 JP10","2AVL4 50L MDR EZ1 PWS1836 LP835 JP10 (CI-231TCM)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234T2T","2AVL4 50L MDR EZ1 PWS1836 LP840","2AVL4 50L MDR EZ1 PWS1836 LP840 (CI-234T2T)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234T2Y","2AVL4 50L MDR EZ1 PWS1836 LP840 JP10","2AVL4 50L MDR EZ1 PWS1836 LP840 JP10 (CI-234T2Y)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232N1R","2AVL4 50L MDR EZ1 PWS1856LV LP835","2AVL4 50L MDR EZ1 PWS1856LV LP835 (CI-232N1R)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232N23","2AVL4 50L MDR EZ1 PWS1856LV LP835 JP10","2AVL4 50L MDR EZ1 PWS1856LV LP835 JP10 (CI-232N23)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233CL2","2AVL4 50L SBL EZ1 LP835","2AVL4 50L SBL EZ1 LP835 (CI-233CL2)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234CW7","2AVL4 50L SBL EZ1 LP835 JP10","2AVL4 50L SBL EZ1 LP835 JP10 (CI-234CW7)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233VW8","2AVL4 50L SBL EZ1 LP840","2AVL4 50L SBL EZ1 LP840 (CI-233VW8)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233AFR","2AVL4 50L SBL EZ1 PWS1836 LP840","2AVL4 50L SBL EZ1 PWS1836 LP840 (CI-233AFR)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233AE8","2AVL4 50L SBL EZ1 PWS1836 LP840 JP10","2AVL4 50L SBL EZ1 PWS1836 LP840 JP10 (CI-233AE8)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232RUX","2AVL4 A 30L MDR EZ1 LP835","2AVL4 A 30L MDR EZ1 LP835 (CI-232RUX)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232CG0","2AVL4 A 40L MDR EZ1 LP835","2AVL4 A 40L MDR EZ1 LP835 (CI-232CG0)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232RRW","2AVL4 A 40L MDR EZ1 LP835 JP10","2AVL4 A 40L MDR EZ1 LP835 JP10 (CI-232RRW)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233VY2","2AVL4 A 40L MDR EZ1 LP840","2AVL4 A 40L MDR EZ1 LP840 (CI-233VY2)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234M23","2AVL4 A 40L MDR EZ1 LP840 N100","2AVL4 A 40L MDR EZ1 LP840 N100 (CI-234M23)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234M2C","2AVL4 A 40L MDR EZ1 LP840 N100 JP10","2AVL4 A 40L MDR EZ1 LP840 N100 JP10 (CI-234M2C)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233LC9","2AVL4 A 40L SBL EZ1 LP835","2AVL4 A 40L SBL EZ1 LP835 (CI-233LC9)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233LC2","2AVL4 A 40L SBL EZ1 LP835 JP10","2AVL4 A 40L SBL EZ1 LP835 JP10 (CI-233LC2)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233EPA","2AVL4 A 50L MDR EZ1 LP835 N100","2AVL4 A 50L MDR EZ1 LP835 N100 (CI-233EPA)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["229E80","AVL 15L MDR EZ1 LP835","AVL 15L MDR EZ1 LP835 (CI-229E80)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C1026,7)),6))","v":"229E86"},{"$f":"LEFT(C1026,SEARCH(\"(CI-\",C1026)-2)","v":"AVL 25L MDR EZ1 LP835 N80"},"AVL 25L MDR EZ1 LP835 N80 (CI-229E86)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234XTV","AVL4 18L MDR EZ1 LP830","AVL4 18L MDR EZ1 LP830 (CI-234XTV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230TJ5","AVL4 18L MDR EZ1 LP835","AVL4 18L MDR EZ1 LP835 (CI-230TJ5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234P9A","AVL4 18L MDR EZ1 LP835 N80","AVL4 18L MDR EZ1 LP835 N80 (CI-234P9A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232W5M","AVL4 18L MDR EZ1 LP840","AVL4 18L MDR EZ1 LP840 (CI-232W5M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232N44","AVL4 18L SBL EZ1 LP850","AVL4 18L SBL EZ1 LP850 (CI-232N44)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234LGG","AVL4 25L MDR EZ1 LP830","AVL4 25L MDR EZ1 LP830 (CI-234LGG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232HGG","AVL4 25L MDR EZ1 LP835","AVL4 25L MDR EZ1 LP835 (CI-232HGG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233Y2C","AVL4 25L MDR EZ1 LP835 N80","AVL4 25L MDR EZ1 LP835 N80 (CI-233Y2C)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232AHL","AVL4 25L MDR EZ1 LP840","AVL4 25L MDR EZ1 LP840 (CI-232AHL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230R31","AVL4 25L MDR EZ1 LP840 N80","AVL4 25L MDR EZ1 LP840 N80 (CI-230R31)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240A47","2AVL2 20L ADP EZ1 LP830","2AVL2 20L ADP EZ1 LP830 (CI-240A47)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237GX8","2AVL2 20L ADP EZ1 LP835 N100","2AVL2 20L ADP EZ1 LP835 N100 (CI-237GX8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238R6N","2AVL2 20L ADP EZ1 LP835 N80","2AVL2 20L ADP EZ1 LP835 N80 (CI-238R6N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236P6L","2AVL2 20L ADP EZ1 LP840","2AVL2 20L ADP EZ1 LP840 (CI-236P6L)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235FWG","2AVL2 20L MDR 277 EZ1 GLR LP840","2AVL2 20L MDR 277 EZ1 GLR LP840 (CI-235FWG)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232EW7","2AVL2 20L MDR EZ1 LP830 N80 USPOM","2AVL2 20L MDR EZ1 LP830 N80 USPOM (CI-232EW7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241HJ2","2AVL2 20L MDR EZ1 LP835 MMC JP20","2AVL2 20L MDR EZ1 LP835 MMC JP20 (CI-241HJ2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235XV2","2AVL2 20L MDR EZ1 LP835 N100 JP20","2AVL2 20L MDR EZ1 LP835 N100 JP20 (CI-235XV2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239LHM","2AVL2 20L MDR EZ1 LP835 N100 MMC JP20","2AVL2 20L MDR EZ1 LP835 N100 MMC JP20 (CI-239LHM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230AH4","2AVL2 20L MDR EZ1 LP835 N100EMG","2AVL2 20L MDR EZ1 LP835 N100EMG (CI-230AH4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232EA4","2AVL2 20L MDR EZ1 LP835 N100EMG USPOM","2AVL2 20L MDR EZ1 LP835 N100EMG USPOM (CI-232EA4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232G0V","2AVL2 20L MDR EZ1 LP840 JP20/DUP","2AVL2 20L MDR EZ1 LP840 JP20/DUP (CI-232G0V)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236FAT","2AVL2 20L MDR EZ1 LP840 LATC","2AVL2 20L MDR EZ1 LP840 LATC (CI-236FAT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236TNM","2AVL2 20L MDR EZ1 LP840 N100","2AVL2 20L MDR EZ1 LP840 N100 (CI-236TNM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240NK5","2AVL2 20L MDR EZ1 LP840 N100 MMC JP20","2AVL2 20L MDR EZ1 LP840 N100 MMC JP20 (CI-240NK5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236TNW","2AVL2 20L MDR EZ1 LP840 N100EMG","2AVL2 20L MDR EZ1 LP840 N100EMG (CI-236TNW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236PEY","2AVL2 20L MDR EZ1 LP840 N80","2AVL2 20L MDR EZ1 LP840 N80 (CI-236PEY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236H1A","2AVL2 20L MDR EZ1 LP840 N80 JP20","2AVL2 20L MDR EZ1 LP840 N80 JP20 (CI-236H1A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240NFT","2AVL2 20L MDR EZ1 LP840 N80EMG","2AVL2 20L MDR EZ1 LP840 N80EMG (CI-240NFT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232EVX","2AVL2 20L MDR EZ1 LP840 USPOM","2AVL2 20L MDR EZ1 LP840 USPOM (CI-232EVX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236Y8P","2AVL2 20L MDR EZ1 LP850","2AVL2 20L MDR EZ1 LP850 (CI-236Y8P)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237HC7","2AVL2 20L MDR EZ1 PWS1836 LP830","2AVL2 20L MDR EZ1 PWS1836 LP830 (CI-237HC7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236N5N","2AVL2 20L MDR EZ1 PWS1836 LP835","2AVL2 20L MDR EZ1 PWS1836 LP835 (CI-236N5N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238G0A","2AVL2 20L MDR EZ1 PWS1836 LP835 JP20","2AVL2 20L MDR EZ1 PWS1836 LP835 JP20 (CI-238G0A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236RE3","2AVL2 20L MDR EZ1 PWS1856LV LP830","2AVL2 20L MDR EZ1 PWS1856LV LP830 (CI-236RE3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236RFP","2AVL2 20L MDR EZ1 PWS1856LV LP830 JP20","2AVL2 20L MDR EZ1 PWS1856LV LP830 JP20 (CI-236RFP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236T14","2AVL2 20L SBL EZ1 LP835","2AVL2 20L SBL EZ1 LP835 (CI-236T14)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235YTK","2AVL2 20L SBL EZ1 LP840","2AVL2 20L SBL EZ1 LP840 (CI-235YTK)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235YTV","2AVL2 20L SBL EZ1 LP840 JP20","2AVL2 20L SBL EZ1 LP840 JP20 (CI-235YTV)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237YT9","2AVL2 30L ADP EZ1 LP830","2AVL2 30L ADP EZ1 LP830 (CI-237YT9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245WEK","2AVL2 30L ADP EZ1 LP835 CP","2AVL2 30L ADP EZ1 LP835 CP (CI-245WEK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231E2J","2AVL2 30L ADP EZ1 LP835 N100EMG","2AVL2 30L ADP EZ1 LP835 N100EMG (CI-231E2J)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237GEW","2AVL2 30L ADP EZ1 LP835 N80","2AVL2 30L ADP EZ1 LP835 N80 (CI-237GEW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235T3H","2AVL2 30L ADP EZ1 LP840 JP20","2AVL2 30L ADP EZ1 LP840 JP20 (CI-235T3H)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["243P67","2AVL2 30L ADP EZ1 PWS1836 LP835","2AVL2 30L ADP EZ1 PWS1836 LP835 (CI-243P67)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237CC6","2AVL2 30L ADP EZ1 PWS1856LV LP835","2AVL2 30L ADP EZ1 PWS1856LV LP835 (CI-237CC6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240GNW","2AVL2 30L MDR 120 EZ1 LP830 CS1WL10 SSQ","2AVL2 30L MDR 120 EZ1 LP830 CS1WL10 SSQ (CI-240GNW)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["229E7E","2AVL2 30L MDR 120 EZ1 LP835 N100 CS1WL10 SSQ","2AVL2 30L MDR 120 EZ1 LP835 N100 CS1WL10 SSQ (CI-229E7E)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["229E7T","2AVL2 30L MDR 120 EZ1 LP840 N100 CS1WL10 SSQ","2AVL2 30L MDR 120 EZ1 LP840 N100 CS1WL10 SSQ (CI-229E7T)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236AHM","2AVL2 30L MDR 277 EZ1 GMF LP840","2AVL2 30L MDR 277 EZ1 GMF LP840 (CI-236AHM)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234RAX","2AVL2 30L MDR EZ1 LP830 N100EMG","2AVL2 30L MDR EZ1 LP830 N100EMG (CI-234RAX)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234RC0","2AVL2 30L MDR EZ1 LP830 N100EMG JP20","2AVL2 30L MDR EZ1 LP830 N100EMG JP20 (CI-234RC0)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["238KP1","2AVL2 30L MDR EZ1 LP835 CP","2AVL2 30L MDR EZ1 LP835 CP (CI-238KP1)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232RKF","2AVL2 30L MDR EZ1 LP835 N100EMG","2AVL2 30L MDR EZ1 LP835 N100EMG (CI-232RKF)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233CHT","2AVL2 30L MDR EZ1 LP835 N100EMG JP20","2AVL2 30L MDR EZ1 LP835 N100EMG JP20 (CI-233CHT)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235FVV","2AVL2 30L MDR EZ1 LP835 N80 JP20","2AVL2 30L MDR EZ1 LP835 N80 JP20 (CI-235FVV)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233C1J","2AVL2 30L MDR EZ1 LP835 N80EMG","2AVL2 30L MDR EZ1 LP835 N80EMG (CI-233C1J)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232YNV","2AVL2 30L MDR EZ1 LP835 N80EMG JP20","2AVL2 30L MDR EZ1 LP835 N80EMG JP20 (CI-232YNV)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232EWM","2AVL2 30L MDR EZ1 LP840 N100 USPOM JP20","2AVL2 30L MDR EZ1 LP840 N100 USPOM JP20 (CI-232EWM)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234L56","2AVL2 30L MDR EZ1 LP840 N100EMG","2AVL2 30L MDR EZ1 LP840 N100EMG (CI-234L56)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236YN9","2AVL2 30L MDR EZ1 LP840 N80","2AVL2 30L MDR EZ1 LP840 N80 (CI-236YN9)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236YNN","2AVL2 30L MDR EZ1 LP840 N80 JP20","2AVL2 30L MDR EZ1 LP840 N80 JP20 (CI-236YNN)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237ALE","2AVL2 30L MDR EZ1 LP840 USPOM","2AVL2 30L MDR EZ1 LP840 USPOM (CI-237ALE)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
[{"$f":"(LEFT((RIGHT(C1090,7)),6))","v":"237AM7"},{"$f":"LEFT(C1090,SEARCH(\"(CI-\",C1090)-2)","v":"2AVL2 30L MDR EZ1 LP840 USPOM JP20"},"2AVL2 30L MDR EZ1 LP840 USPOM JP20 (CI-237AM7)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232EU6","2AVL2 30L MDR EZ1 LP850 N100 USPOM","2AVL2 30L MDR EZ1 LP850 N100 USPOM (CI-232EU6)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236FCF","2AVL2 30L MDR EZ1 PWS1836 LP840","2AVL2 30L MDR EZ1 PWS1836 LP840 (CI-236FCF)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["241VYH","2AVL2 30L MDR EZ1 PWS1836 LP850","2AVL2 30L MDR EZ1 PWS1836 LP850 (CI-241VYH)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236REY","2AVL2 30L MDR EZ1 PWS1856LV LP830","2AVL2 30L MDR EZ1 PWS1856LV LP830 (CI-236REY)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235TP9","2AVL2 30L MDR EZ1 PWS1856LV LP835 JP20","2AVL2 30L MDR EZ1 PWS1856LV LP835 JP20 (CI-235TP9)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["241CC0","2AVL2 30L MDR EZ1 PWS1856LV LP840","2AVL2 30L MDR EZ1 PWS1856LV LP840 (CI-241CC0)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["241JKF","2AVL2 30L SBL EZ1 LP830","2AVL2 30L SBL EZ1 LP830 (CI-241JKF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236KH3","2AVL2 30L SBL EZ1 LP840","2AVL2 30L SBL EZ1 LP840 (CI-236KH3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["247RMF","2AVL2 30L SBL EZ1 PWS1436 LP835","2AVL2 30L SBL EZ1 PWS1436 LP835 (CI-247RMF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237P7E","2AVL2 40L ADP EZ1 LP830","2AVL2 40L ADP EZ1 LP830 (CI-237P7E)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236FVH","2AVL2 40L ADP EZ1 LP835 N100","2AVL2 40L ADP EZ1 LP835 N100 (CI-236FVH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236FVL","2AVL2 40L ADP EZ1 LP835 N100 JP20","2AVL2 40L ADP EZ1 LP835 N100 JP20 (CI-236FVL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236JUF","2AVL2 40L ADP EZ1 LP840 JP20","2AVL2 40L ADP EZ1 LP840 JP20 (CI-236JUF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239Y2P","2AVL2 40L ADP EZ1 LP840 N80","2AVL2 40L ADP EZ1 LP840 N80 (CI-239Y2P)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241R3C","2AVL2 40L ADP EZ1 LP850 N80","2AVL2 40L ADP EZ1 LP850 N80 (CI-241R3C)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236VCE","2AVL2 40L ADP EZ1 PWS1856LV LP840","2AVL2 40L ADP EZ1 PWS1856LV LP840 (CI-236VCE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239WHH","2AVL2 40L MDR EZ1 LP830 N100","2AVL2 40L MDR EZ1 LP830 N100 (CI-239WHH)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["239WHL","2AVL2 40L MDR EZ1 LP830 N100 JP20","2AVL2 40L MDR EZ1 LP830 N100 JP20 (CI-239WHL)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["239WJL","2AVL2 40L MDR EZ1 LP830 N100EMG","2AVL2 40L MDR EZ1 LP830 N100EMG (CI-239WJL)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["234GP1","2AVL2 40L MDR EZ1 LP835 N100EMG","2AVL2 40L MDR EZ1 LP835 N100EMG (CI-234GP1)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["232EUV","2AVL2 40L MDR EZ1 LP835 N80 USPOM","2AVL2 40L MDR EZ1 LP835 N80 USPOM (CI-232EUV)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["230VJU","2AVL2 40L MDR EZ1 LP835 N80EMG","2AVL2 40L MDR EZ1 LP835 N80EMG (CI-230VJU)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["232MGJ","2AVL2 40L MDR EZ1 LP840 N100EMG","2AVL2 40L MDR EZ1 LP840 N100EMG (CI-232MGJ)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["233GW2","2AVL2 40L MDR EZ1 LP840 N100EMG JP20","2AVL2 40L MDR EZ1 LP840 N100EMG JP20 (CI-233GW2)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["236YP0","2AVL2 40L MDR EZ1 LP840 N80 JP20","2AVL2 40L MDR EZ1 LP840 N80 JP20 (CI-236YP0)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["238L59","2AVL2 40L MDR EZ1 PWS1836 LP830","2AVL2 40L MDR EZ1 PWS1836 LP830 (CI-238L59)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["235XE3","2AVL2 40L MDR EZ1 PWS1856LV LP835 JP20","2AVL2 40L MDR EZ1 PWS1856LV LP835 JP20 (CI-235XE3)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["247UK8","2AVL2 40L MDR EZ1 PWS1856LV LP840","2AVL2 40L MDR EZ1 PWS1856LV LP840 (CI-247UK8)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["239MEK","2AVL2 40L SBL EZ1 LP830 N100","2AVL2 40L SBL EZ1 LP830 N100 (CI-239MEK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237KXT","2AVL2 40L SBL EZ1 LP835 JP20","2AVL2 40L SBL EZ1 LP835 JP20 (CI-237KXT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237CU1","2AVL2 40L SBL EZ1 LP835 N80","2AVL2 40L SBL EZ1 LP835 N80 (CI-237CU1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236R0P","2AVL2 40L SBL EZ1 LP840","2AVL2 40L SBL EZ1 LP840 (CI-236R0P)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236R11","2AVL2 40L SBL EZ1 LP840 JP20","2AVL2 40L SBL EZ1 LP840 JP20 (CI-236R11)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235XRP","2AVL2 40L SBL EZ1 LP840 N80","2AVL2 40L SBL EZ1 LP840 N80 (CI-235XRP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["249PXU","2AVL2 40L SBL EZ1 LP850","2AVL2 40L SBL EZ1 LP850 (CI-249PXU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235Y0C","2AVL2 40L SBL EZ1 LP850 N100","2AVL2 40L SBL EZ1 LP850 N100 (CI-235Y0C)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235LV2","2AVL2 A 20L ADP EZ1 LP840","2AVL2 A 20L ADP EZ1 LP840 (CI-235LV2)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["240U0M","2AVL2 A 20L MDR EZ1 LP830","2AVL2 A 20L MDR EZ1 LP830 (CI-240U0M)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236G87","2AVL2 A 20L MDR EZ1 LP835","2AVL2 A 20L MDR EZ1 LP835 (CI-236G87)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["245J0W","2AVL2 A 20L MDR EZ1 LP835 CP","2AVL2 A 20L MDR EZ1 LP835 CP (CI-245J0W)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["245J0F","2AVL2 A 20L MDR EZ1 LP835 CP JP20","2AVL2 A 20L MDR EZ1 LP835 CP JP20 (CI-245J0F)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236G8R","2AVL2 A 20L MDR EZ1 LP835 JP20","2AVL2 A 20L MDR EZ1 LP835 JP20 (CI-236G8R)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236AH4","2AVL2 A 20L MDR EZ1 LP840","2AVL2 A 20L MDR EZ1 LP840 (CI-236AH4)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["240RU4","2AVL2 A 30L ADP EZ1 LP830","2AVL2 A 30L ADP EZ1 LP830 (CI-240RU4)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236RFJ","2AVL2 A 30L ADP EZ1 LP835","2AVL2 A 30L ADP EZ1 LP835 (CI-236RFJ)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236A1P","2AVL2 A 30L MDR EZ1 LP830","2AVL2 A 30L MDR EZ1 LP830 (CI-236A1P)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["238GCV","2AVL2 A 30L MDR EZ1 LP830 JP20","2AVL2 A 30L MDR EZ1 LP830 JP20 (CI-238GCV)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["239FL2","2AVL2 A 30L MDR EZ1 LP835 JP20","2AVL2 A 30L MDR EZ1 LP835 JP20 (CI-239FL2)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["239JEM","2AVL2 A 30L MDR EZ1 LP840","2AVL2 A 30L MDR EZ1 LP840 (CI-239JEM)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["238KHH","2AVL2 A 30L MDR EZ1 PWS1836 LP835","2AVL2 A 30L MDR EZ1 PWS1836 LP835 (CI-238KHH)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235K4M","2AVL2 A 30L SBL EZ1 LP835","2AVL2 A 30L SBL EZ1 LP835 (CI-235K4M)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["240NHU","2AVL2 A 40L ADP EZ1 LP835","2AVL2 A 40L ADP EZ1 LP835 (CI-240NHU)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["239MVK","2AVL2 A 40L MDR EZ1 LP830","2AVL2 A 40L MDR EZ1 LP830 (CI-239MVK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235TV0","2AVL2 A 40L MDR EZ1 LP835","2AVL2 A 40L MDR EZ1 LP835 (CI-235TV0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237MCP","2AVL2 A 40L MDR EZ1 LP835 N80 USPOM","2AVL2 A 40L MDR EZ1 LP835 N80 USPOM (CI-237MCP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237MCX","2AVL2 A 40L MDR EZ1 LP835 N80EMG USPOM","2AVL2 A 40L MDR EZ1 LP835 N80EMG USPOM (CI-237MCX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["249PX1","2AVL2 A 40L MDR EZ1 LP840","2AVL2 A 40L MDR EZ1 LP840 (CI-249PX1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238WFY","2AVL2 A 40L MDR EZ1 LP840 N100","2AVL2 A 40L MDR EZ1 LP840 N100 (CI-238WFY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238WHL","2AVL2 A 40L MDR EZ1 LP840 N100EMG","2AVL2 A 40L MDR EZ1 LP840 N100EMG (CI-238WHL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236TNE","2AVL2 ST 20L ADP EZ1 LP835","2AVL2 ST 20L ADP EZ1 LP835 (CI-236TNE)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232WHA","2AVL2 ST 20L MDR EZ1 LP830","2AVL2 ST 20L MDR EZ1 LP830 (CI-232WHA)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232P0G","2AVL2 ST 20L MDR EZ1 LP830 N100","2AVL2 ST 20L MDR EZ1 LP830 N100 (CI-232P0G)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232CKV","2AVL2 ST 20L MDR EZ1 LP835","2AVL2 ST 20L MDR EZ1 LP835 (CI-232CKV)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
[{"$f":"(LEFT((RIGHT(C1154,7)),6))","v":"232R76"},{"$f":"LEFT(C1154,SEARCH(\"(CI-\",C1154)-2)","v":"2AVL2 ST 20L MDR EZ1 LP835 JP20"},"2AVL2 ST 20L MDR EZ1 LP835 JP20 (CI-232R76)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232P18","2AVL2 ST 20L MDR EZ1 LP835 N100","2AVL2 ST 20L MDR EZ1 LP835 N100 (CI-232P18)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230GFU","2AVL2 ST 20L MDR EZ1 LP835 N80","2AVL2 ST 20L MDR EZ1 LP835 N80 (CI-230GFU)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230HV0","2AVL2 ST 20L MDR EZ1 LP835 N80EMG","2AVL2 ST 20L MDR EZ1 LP835 N80EMG (CI-230HV0)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231P7F","2AVL2 ST 20L MDR EZ1 LP840","2AVL2 ST 20L MDR EZ1 LP840 (CI-231P7F)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233M54","2AVL2 ST 20L MDR EZ1 LP840 N100","2AVL2 ST 20L MDR EZ1 LP840 N100 (CI-233M54)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233M58","2AVL2 ST 20L MDR EZ1 LP840 N100EMG","2AVL2 ST 20L MDR EZ1 LP840 N100EMG (CI-233M58)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237WWE","2AVL2 ST 20L SBL EZ1 LP840 N100","2AVL2 ST 20L SBL EZ1 LP840 N100 (CI-237WWE)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237WWF","2AVL2 ST 20L SBL EZ1 LP840 N100EMG","2AVL2 ST 20L SBL EZ1 LP840 N100EMG (CI-237WWF)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["238HL2","2AVL2 ST 30L ADP EZ1 LP835","2AVL2 ST 30L ADP EZ1 LP835 (CI-238HL2)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235NAJ","2AVL2 ST 30L ADP EZ1 LP835 JP20","2AVL2 ST 30L ADP EZ1 LP835 JP20 (CI-235NAJ)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233PVH","2AVL2 ST 30L MDR EZ1 LP830","2AVL2 ST 30L MDR EZ1 LP830 (CI-233PVH)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233PV0","2AVL2 ST 30L MDR EZ1 LP830 JP20","2AVL2 ST 30L MDR EZ1 LP830 JP20 (CI-233PV0)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232VGK","2AVL2 ST 30L MDR EZ1 LP830 N100EMG","2AVL2 ST 30L MDR EZ1 LP830 N100EMG (CI-232VGK)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230X4J","2AVL2 ST 30L MDR EZ1 LP835","2AVL2 ST 30L MDR EZ1 LP835 (CI-230X4J)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233X31","2AVL2 ST 30L MDR EZ1 LP835 CP","2AVL2 ST 30L MDR EZ1 LP835 CP (CI-233X31)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233WVE","2AVL2 ST 30L MDR EZ1 LP835 CP JP20","2AVL2 ST 30L MDR EZ1 LP835 CP JP20 (CI-233WVE)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233FYT","2AVL2 ST 30L MDR EZ1 LP835 JP20","2AVL2 ST 30L MDR EZ1 LP835 JP20 (CI-233FYT)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230X4P","2AVL2 ST 30L MDR EZ1 LP835 N100","2AVL2 ST 30L MDR EZ1 LP835 N100 (CI-230X4P)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235TE1","2AVL2 ST 30L MDR EZ1 LP835 N100 JP20","2AVL2 ST 30L MDR EZ1 LP835 N100 JP20 (CI-235TE1)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236EV6","2AVL2 ST 30L MDR EZ1 LP835 N100EMG","2AVL2 ST 30L MDR EZ1 LP835 N100EMG (CI-236EV6)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236Y8J","2AVL2 ST 30L MDR EZ1 LP835 N100EMG JP20","2AVL2 ST 30L MDR EZ1 LP835 N100EMG JP20 (CI-236Y8J)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235LUL","2AVL2 ST 30L MDR EZ1 LP835 N80","2AVL2 ST 30L MDR EZ1 LP835 N80 (CI-235LUL)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235LUN","2AVL2 ST 30L MDR EZ1 LP835 N80EMG","2AVL2 ST 30L MDR EZ1 LP835 N80EMG (CI-235LUN)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232NK9","2AVL2 ST 30L MDR EZ1 LP840","2AVL2 ST 30L MDR EZ1 LP840 (CI-232NK9)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["229UGM","2AVL2 ST 30L MDR EZ1 LP840 N100","2AVL2 ST 30L MDR EZ1 LP840 N100 (CI-229UGM)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230GGN","2AVL2 ST 30L MDR EZ1 LP840 N100EMG","2AVL2 ST 30L MDR EZ1 LP840 N100EMG (CI-230GGN)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231GA2","2AVL2 ST 30L SBL EZ1 LP840","2AVL2 ST 30L SBL EZ1 LP840 (CI-231GA2)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237X01","2AVL2 ST 30L SBL EZ1 LP840 N100","2AVL2 ST 30L SBL EZ1 LP840 N100 (CI-237X01)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237WYW","2AVL2 ST 30L SBL EZ1 LP840 N100EMG","2AVL2 ST 30L SBL EZ1 LP840 N100EMG (CI-237WYW)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["239AR0","2AVL2 ST 40L ADP EZ1 LP835","2AVL2 ST 40L ADP EZ1 LP835 (CI-239AR0)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["231M3Y","2AVL2 ST 40L ADP EZ1 LP840","2AVL2 ST 40L ADP EZ1 LP840 (CI-231M3Y)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["238XYA","2AVL2 ST 40L MDR EZ1 LP830","2AVL2 ST 40L MDR EZ1 LP830 (CI-238XYA)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["229UJ5","2AVL2 ST 40L MDR EZ1 LP835","2AVL2 ST 40L MDR EZ1 LP835 (CI-229UJ5)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["230P18","2AVL2 ST 40L MDR EZ1 LP835 JP20","2AVL2 ST 40L MDR EZ1 LP835 JP20 (CI-230P18)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["231G8R","2AVL2 ST 40L MDR EZ1 LP835 N100","2AVL2 ST 40L MDR EZ1 LP835 N100 (CI-231G8R)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["231LGW","2AVL2 ST 40L MDR EZ1 LP835 N100EMG","2AVL2 ST 40L MDR EZ1 LP835 N100EMG (CI-231LGW)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["231PJ8","2AVL2 ST 40L MDR EZ1 LP835 N80","2AVL2 ST 40L MDR EZ1 LP835 N80 (CI-231PJ8)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["236KXP","2AVL2 ST 40L MDR EZ1 LP835 N80 JP20","2AVL2 ST 40L MDR EZ1 LP835 N80 JP20 (CI-236KXP)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["232YAG","2AVL2 ST 40L MDR EZ1 LP835 N80EMG","2AVL2 ST 40L MDR EZ1 LP835 N80EMG (CI-232YAG)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["230FYU","2AVL2 ST 40L MDR EZ1 LP840","2AVL2 ST 40L MDR EZ1 LP840 (CI-230FYU)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["239L8H","2AVL2 ST 40L MDR EZ1 LP840 N100","2AVL2 ST 40L MDR EZ1 LP840 N100 (CI-239L8H)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["239L8M","2AVL2 ST 40L MDR EZ1 LP840 N100EMG","2AVL2 ST 40L MDR EZ1 LP840 N100EMG (CI-239L8M)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["237FK2","2AVL2 ST 40L MDR EZ1 LP840 N80","2AVL2 ST 40L MDR EZ1 LP840 N80 (CI-237FK2)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["237FK9","2AVL2 ST 40L MDR EZ1 LP840 N80EMG","2AVL2 ST 40L MDR EZ1 LP840 N80EMG (CI-237FK9)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["237X22","2AVL2 ST 40L SBL EZ1 LP840 N100","2AVL2 ST 40L SBL EZ1 LP840 N100 (CI-237X22)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["249PXE","2AVL2 ST A 20L MDR EZ1 LP830","2AVL2 ST A 20L MDR EZ1 LP830 (CI-249PXE)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235WR1","2AVL2 ST A 20L MDR EZ1 LP835 N80","2AVL2 ST A 20L MDR EZ1 LP835 N80 (CI-235WR1)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235WR8","2AVL2 ST A 20L MDR EZ1 LP835 N80 JP20","2AVL2 ST A 20L MDR EZ1 LP835 N80 JP20 (CI-235WR8)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230AHT","2AVL2 ST A 20L MDR EZ1 LP840","2AVL2 ST A 20L MDR EZ1 LP840 (CI-230AHT)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233JG8","2AVL2 ST A 30L MDR EZ1 LP830","2AVL2 ST A 30L MDR EZ1 LP830 (CI-233JG8)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233JG9","2AVL2 ST A 30L MDR EZ1 LP830 JP20","2AVL2 ST A 30L MDR EZ1 LP830 JP20 (CI-233JG9)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231U9L","2AVL2 ST A 30L MDR EZ1 LP835","2AVL2 ST A 30L MDR EZ1 LP835 (CI-231U9L)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234G5G","2AVL2 ST A 30L MDR EZ1 LP835 JP20","2AVL2 ST A 30L MDR EZ1 LP835 JP20 (CI-234G5G)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232MAA","2AVL2 ST A 30L MDR EZ1 LP835 N80","2AVL2 ST A 30L MDR EZ1 LP835 N80 (CI-232MAA)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232MAK","2AVL2 ST A 30L MDR EZ1 LP835 N80 JP20","2AVL2 ST A 30L MDR EZ1 LP835 N80 JP20 (CI-232MAK)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237TN7","2AVL2 ST A 30L MDR EZ1 LP840 N100","2AVL2 ST A 30L MDR EZ1 LP840 N100 (CI-237TN7)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236NRE","2AVL2 ST A 30L SBL EZ1 LP840 N100","2AVL2 ST A 30L SBL EZ1 LP840 N100 (CI-236NRE)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["241VM8","2AVL2 ST A 30L SBL EZ1 LP840 N100 JP20","2AVL2 ST A 30L SBL EZ1 LP840 N100 JP20 (CI-241VM8)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234HWC","2AVL2 ST A 40L MDR EZ1 LP830","2AVL2 ST A 40L MDR EZ1 LP830 (CI-234HWC)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["234V8F","2AVL2 ST A 40L MDR EZ1 LP835","2AVL2 ST A 40L MDR EZ1 LP835 (CI-234V8F)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["238PUV","2AVL2 ST A 40L MDR EZ1 LP835 N100","2AVL2 ST A 40L MDR EZ1 LP835 N100 (CI-238PUV)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["238PUW","2AVL2 ST A 40L MDR EZ1 LP835 N100EMG","2AVL2 ST A 40L MDR EZ1 LP835 N100EMG (CI-238PUW)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["231LWY","2AVL2 ST A 40L MDR EZ1 LP835 N80","2AVL2 ST A 40L MDR EZ1 LP835 N80 (CI-231LWY)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
[{"$f":"(LEFT((RIGHT(C1218,7)),6))","v":"232MAY"},{"$f":"LEFT(C1218,SEARCH(\"(CI-\",C1218)-2)","v":"2AVL2 ST A 40L MDR EZ1 LP835 N80 JP20"},"2AVL2 ST A 40L MDR EZ1 LP835 N80 JP20 (CI-232MAY)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["235Y09","2AVL2 ST A 40L MDR EZ1 LP835 N80EMG","2AVL2 ST A 40L MDR EZ1 LP835 N80EMG (CI-235Y09)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["234PL3","2AVL2 ST A 40L SBL EZ1 LP840 N100","2AVL2 ST A 40L SBL EZ1 LP840 N100 (CI-234PL3)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["234PLN","2AVL2 ST A 40L SBL EZ1 LP840 N100 JP20","2AVL2 ST A 40L SBL EZ1 LP840 N100 JP20 (CI-234PLN)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["234PL7","2AVL2 ST A 40L SBL EZ1 LP840 N100EMG","2AVL2 ST A 40L SBL EZ1 LP840 N100EMG (CI-234PL7)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["238A4A","2AVL4 30L ADP EZ1 LP830","2AVL4 30L ADP EZ1 LP830 (CI-238A4A)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["245WCR","2AVL4 30L ADP EZ1 LP835 CP","2AVL4 30L ADP EZ1 LP835 CP (CI-245WCR)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["238CNY","2AVL4 30L ADP EZ1 LP835 N100","2AVL4 30L ADP EZ1 LP835 N100 (CI-238CNY)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["238A7N","2AVL4 30L ADP EZ1 LP835 N80 USPOM","2AVL4 30L ADP EZ1 LP835 N80 USPOM (CI-238A7N)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237ERH","2AVL4 30L ADP EZ1 LP835 N80EMG","2AVL4 30L ADP EZ1 LP835 N80EMG (CI-237ERH)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["245V0N","2AVL4 30L ADP EZ1 LP835 USPOM","2AVL4 30L ADP EZ1 LP835 USPOM (CI-245V0N)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235R5R","2AVL4 30L ADP EZ1 LP840","2AVL4 30L ADP EZ1 LP840 (CI-235R5R)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237CEL","2AVL4 30L ADP EZ1 PWS1856LV LP835","2AVL4 30L ADP EZ1 PWS1856LV LP835 (CI-237CEL)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236PK8","2AVL4 30L MDR EZ1 LP830 JP10","2AVL4 30L MDR EZ1 LP830 JP10 (CI-236PK8)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235XFC","2AVL4 30L MDR EZ1 LP830 N100EMG","2AVL4 30L MDR EZ1 LP830 N100EMG (CI-235XFC)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235XFK","2AVL4 30L MDR EZ1 LP830 N100EMG JP10","2AVL4 30L MDR EZ1 LP830 N100EMG JP10 (CI-235XFK)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236HAT","2AVL4 30L MDR EZ1 LP835 CP JP10","2AVL4 30L MDR EZ1 LP835 CP JP10 (CI-236HAT)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233U51","2AVL4 30L MDR EZ1 LP835 N100 JP10","2AVL4 30L MDR EZ1 LP835 N100 JP10 (CI-233U51)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233Y22","2AVL4 30L MDR EZ1 LP835 N80EMG","2AVL4 30L MDR EZ1 LP835 N80EMG (CI-233Y22)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234EYP","2AVL4 30L MDR EZ1 LP835 N80EMG JP10","2AVL4 30L MDR EZ1 LP835 N80EMG JP10 (CI-234EYP)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237KTN","2AVL4 30L MDR EZ1 LP835 USPOM","2AVL4 30L MDR EZ1 LP835 USPOM (CI-237KTN)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236FAK","2AVL4 30L MDR EZ1 LP840 LATC","2AVL4 30L MDR EZ1 LP840 LATC (CI-236FAK)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236T0N","2AVL4 30L MDR EZ1 LP840 N100EMG","2AVL4 30L MDR EZ1 LP840 N100EMG (CI-236T0N)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["238GEM","2AVL4 30L MDR EZ1 LP840 N80","2AVL4 30L MDR EZ1 LP840 N80 (CI-238GEM)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237JF5","2AVL4 30L MDR EZ1 LP850 N100","2AVL4 30L MDR EZ1 LP850 N100 (CI-237JF5)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["238L51","2AVL4 30L MDR EZ1 PWS1836 LP830","2AVL4 30L MDR EZ1 PWS1836 LP830 (CI-238L51)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["240GX0","2AVL4 30L MDR EZ1 PWS1836 LP840","2AVL4 30L MDR EZ1 PWS1836 LP840 (CI-240GX0)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["239CUV","2AVL4 30L MDR EZ1 PWS1836 LP840 JP10","2AVL4 30L MDR EZ1 PWS1836 LP840 JP10 (CI-239CUV)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["245HNU","2AVL4 30L MDR EZ1 PWS1856LV LP840","2AVL4 30L MDR EZ1 PWS1856LV LP840 (CI-245HNU)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235WC3","2AVL4 30L SBL EZ1 LP830","2AVL4 30L SBL EZ1 LP830 (CI-235WC3)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236KG9","2AVL4 30L SBL EZ1 LP835","2AVL4 30L SBL EZ1 LP835 (CI-236KG9)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236KGW","2AVL4 30L SBL EZ1 LP835 JP10","2AVL4 30L SBL EZ1 LP835 JP10 (CI-236KGW)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235YTA","2AVL4 30L SBL EZ1 LP840","2AVL4 30L SBL EZ1 LP840 (CI-235YTA)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237P7C","2AVL4 40L ADP EZ1 LP830","2AVL4 40L ADP EZ1 LP830 (CI-237P7C)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236K7K","2AVL4 40L ADP EZ1 LP835 CP","2AVL4 40L ADP EZ1 LP835 CP (CI-236K7K)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236K8C","2AVL4 40L ADP EZ1 LP835 CP JP10","2AVL4 40L ADP EZ1 LP835 CP JP10 (CI-236K8C)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235K57","2AVL4 40L ADP EZ1 LP835 JP10","2AVL4 40L ADP EZ1 LP835 JP10 (CI-235K57)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["238CP1","2AVL4 40L ADP EZ1 LP835 N100","2AVL4 40L ADP EZ1 LP835 N100 (CI-238CP1)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237GVN","2AVL4 40L ADP EZ1 LP840 N100","2AVL4 40L ADP EZ1 LP840 N100 (CI-237GVN)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230GE1","2AVL4 40L ADP EZ1 LP840 N80","2AVL4 40L ADP EZ1 LP840 N80 (CI-230GE1)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["243P28","2AVL4 40L ADP EZ1 PWS1836 LP835","2AVL4 40L ADP EZ1 PWS1836 LP835 (CI-243P28)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["243NW7","2AVL4 40L ADP EZ1 PWS1836 LP835 JP10","2AVL4 40L ADP EZ1 PWS1836 LP835 JP10 (CI-243NW7)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["239H0F","2AVL4 40L ADP EZ1 PWS1836 LP840","2AVL4 40L ADP EZ1 PWS1836 LP840 (CI-239H0F)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["240CMM","2AVL4 40L ADP EZ1 PWS1856LV LP835 JP10","2AVL4 40L ADP EZ1 PWS1856LV LP835 JP10 (CI-240CMM)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236Y8Y","2AVL4 40L MDR 120 EZ1 GLR LP840","2AVL4 40L MDR 120 EZ1 GLR LP840 (CI-236Y8Y)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235FWM","2AVL4 40L MDR 277 EZ1 GLR LP840","2AVL4 40L MDR 277 EZ1 GLR LP840 (CI-235FWM)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235U8P","2AVL4 40L MDR 277 EZ1 GLR LP840 JP10","2AVL4 40L MDR 277 EZ1 GLR LP840 JP10 (CI-235U8P)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236AT5","2AVL4 40L MDR 277 EZ1 GMF LP840","2AVL4 40L MDR 277 EZ1 GMF LP840 (CI-236AT5)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237UY5","2AVL4 40L MDR EZ1 LP830 N80","2AVL4 40L MDR EZ1 LP830 N80 (CI-237UY5)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["240ELA","2AVL4 40L MDR EZ1 LP835 LATC","2AVL4 40L MDR EZ1 LP835 LATC (CI-240ELA)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["241H2U","2AVL4 40L MDR EZ1 LP835 LATC N80","2AVL4 40L MDR EZ1 LP835 LATC N80 (CI-241H2U)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["241HJ0","2AVL4 40L MDR EZ1 LP835 MMC JP10","2AVL4 40L MDR EZ1 LP835 MMC JP10 (CI-241HJ0)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["239LHL","2AVL4 40L MDR EZ1 LP835 N100 MMC JP10","2AVL4 40L MDR EZ1 LP835 N100 MMC JP10 (CI-239LHL)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232G0G","2AVL4 40L MDR EZ1 LP835 N100EMG","2AVL4 40L MDR EZ1 LP835 N100EMG (CI-232G0G)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232RKL","2AVL4 40L MDR EZ1 LP835 N100EMG JP10","2AVL4 40L MDR EZ1 LP835 N100EMG JP10 (CI-232RKL)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232E8T","2AVL4 40L MDR EZ1 LP835 N80 USPOM","2AVL4 40L MDR EZ1 LP835 N80 USPOM (CI-232E8T)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233PH8","2AVL4 40L MDR EZ1 LP835 N80EMG","2AVL4 40L MDR EZ1 LP835 N80EMG (CI-233PH8)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232E6J","2AVL4 40L MDR EZ1 LP835 USPOM","2AVL4 40L MDR EZ1 LP835 USPOM (CI-232E6J)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236FA6","2AVL4 40L MDR EZ1 LP840 LATC","2AVL4 40L MDR EZ1 LP840 LATC (CI-236FA6)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["240NK3","2AVL4 40L MDR EZ1 LP840 N100 MMC JP10","2AVL4 40L MDR EZ1 LP840 N100 MMC JP10 (CI-240NK3)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230GEV","2AVL4 40L MDR EZ1 LP840 N100EMG","2AVL4 40L MDR EZ1 LP840 N100EMG (CI-230GEV)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232ETX","2AVL4 40L MDR EZ1 LP840 N100EMG USPOM","2AVL4 40L MDR EZ1 LP840 N100EMG USPOM (CI-232ETX)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233N7N","2AVL4 40L MDR EZ1 LP840 N80EMG","2AVL4 40L MDR EZ1 LP840 N80EMG (CI-233N7N)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237KXR","2AVL4 40L MDR EZ1 LP850 N80","2AVL4 40L MDR EZ1 LP850 N80 (CI-237KXR)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
[{"$f":"(LEFT((RIGHT(C1282,7)),6))","v":"238TKF"},{"$f":"LEFT(C1282,SEARCH(\"(CI-\",C1282)-2)","v":"2AVL4 40L MDR EZ1 PWS1836 LP835 N100"},"2AVL4 40L MDR EZ1 PWS1836 LP835 N100 (CI-238TKF)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237KY6","2AVL4 40L MDR EZ1 PWS1836 LP850","2AVL4 40L MDR EZ1 PWS1836 LP850 (CI-237KY6)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["239CK1","2AVL4 40L MDR EZ1 PWS1856LV LP830","2AVL4 40L MDR EZ1 PWS1856LV LP830 (CI-239CK1)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235A55","2AVL4 40L MDR EZ1 PWS1856LV LP835","2AVL4 40L MDR EZ1 PWS1856LV LP835 (CI-235A55)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237CA8","2AVL4 40L MDR EZ1 PWS1856LV LP840","2AVL4 40L MDR EZ1 PWS1856LV LP840 (CI-237CA8)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["240YXM","2AVL4 40L SBL EZ1 LP830","2AVL4 40L SBL EZ1 LP830 (CI-240YXM)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["238T16","2AVL4 40L SBL EZ1 LP840 N100","2AVL4 40L SBL EZ1 LP840 N100 (CI-238T16)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["241VKT","2AVL4 40L SBL EZ1 PWS1856LV LP835","2AVL4 40L SBL EZ1 PWS1856LV LP835 (CI-241VKT)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236K8K","2AVL4 50L ADP EZ1 LP835 CP","2AVL4 50L ADP EZ1 LP835 CP (CI-236K8K)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236K91","2AVL4 50L ADP EZ1 LP835 CP JP10","2AVL4 50L ADP EZ1 LP835 CP JP10 (CI-236K91)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["240UFA","2AVL4 50L ADP EZ1 LP835 N100","2AVL4 50L ADP EZ1 LP835 N100 (CI-240UFA)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["245JL2","2AVL4 50L ADP EZ1 LP850","2AVL4 50L ADP EZ1 LP850 (CI-245JL2)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237TGC","2AVL4 50L ADP EZ1 PWS1836 LP840","2AVL4 50L ADP EZ1 PWS1836 LP840 (CI-237TGC)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["240G33","2AVL4 50L MDR 120 EZ1 GLR LP840","2AVL4 50L MDR 120 EZ1 GLR LP840 (CI-240G33)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235FXL","2AVL4 50L MDR 277 EZ1 GLR LP840","2AVL4 50L MDR 277 EZ1 GLR LP840 (CI-235FXL)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["240YH3","2AVL4 50L MDR EZ1 LP830 N100","2AVL4 50L MDR EZ1 LP830 N100 (CI-240YH3)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237UYA","2AVL4 50L MDR EZ1 LP830 N80","2AVL4 50L MDR EZ1 LP830 N80 (CI-237UYA)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["239XNR","2AVL4 50L MDR EZ1 LP835 LATC","2AVL4 50L MDR EZ1 LP835 LATC (CI-239XNR)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["239XNU","2AVL4 50L MDR EZ1 LP835 LATC JP10","2AVL4 50L MDR EZ1 LP835 LATC JP10 (CI-239XNU)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["241PW2","2AVL4 50L MDR EZ1 LP835 N100EMG","2AVL4 50L MDR EZ1 LP835 N100EMG (CI-241PW2)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["238P4G","2AVL4 50L MDR EZ1 LP835 N80EMG","2AVL4 50L MDR EZ1 LP835 N80EMG (CI-238P4G)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232E7P","2AVL4 50L MDR EZ1 LP835 USPOM","2AVL4 50L MDR EZ1 LP835 USPOM (CI-232E7P)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232EWJ","2AVL4 50L MDR EZ1 LP835 USPOM JP10","2AVL4 50L MDR EZ1 LP835 USPOM JP10 (CI-232EWJ)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234FYF","2AVL4 50L MDR EZ1 LP840 N100EMG","2AVL4 50L MDR EZ1 LP840 N100EMG (CI-234FYF)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233N7X","2AVL4 50L MDR EZ1 LP840 N80EMG","2AVL4 50L MDR EZ1 LP840 N80EMG (CI-233N7X)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237KTV","2AVL4 50L MDR EZ1 LP840 USPOM","2AVL4 50L MDR EZ1 LP840 USPOM (CI-237KTV)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236VMW","2AVL4 50L MDR EZ1 PWS1836 LP835 N100","2AVL4 50L MDR EZ1 PWS1836 LP835 N100 (CI-236VMW)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233WNN","2AVL4 50L MDR EZ1 PWS1836 LP840 N100","2AVL4 50L MDR EZ1 PWS1836 LP840 N100 (CI-233WNN)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233WU9","2AVL4 50L MDR EZ1 PWS1846 LP840 N100EMG","2AVL4 50L MDR EZ1 PWS1846 LP840 N100EMG (CI-233WU9)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236RCH","2AVL4 50L MDR EZ1 PWS1856LV LP830","2AVL4 50L MDR EZ1 PWS1856LV LP830 (CI-236RCH)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236R2F","2AVL4 50L MDR EZ1 PWS1856LV LP830 JP10","2AVL4 50L MDR EZ1 PWS1856LV LP830 JP10 (CI-236R2F)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235UXN","2AVL4 50L SBL EZ1 LP830","2AVL4 50L SBL EZ1 LP830 (CI-235UXN)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235UXU","2AVL4 50L SBL EZ1 LP830 JP10","2AVL4 50L SBL EZ1 LP830 JP10 (CI-235UXU)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["239MAJ","2AVL4 50L SBL EZ1 LP830 N100","2AVL4 50L SBL EZ1 LP830 N100 (CI-239MAJ)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236VFW","2AVL4 50L SBL EZ1 LP840 JP10","2AVL4 50L SBL EZ1 LP840 JP10 (CI-236VFW)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["241TJ9","2AVL4 50L SBL EZ1 LP840 N100","2AVL4 50L SBL EZ1 LP840 N100 (CI-241TJ9)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237CTU","2AVL4 50L SBL EZ1 LP840 N80","2AVL4 50L SBL EZ1 LP840 N80 (CI-237CTU)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235Y07","2AVL4 50L SBL EZ1 LP850 N100","2AVL4 50L SBL EZ1 LP850 N100 (CI-235Y07)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235Y08","2AVL4 50L SBL EZ1 LP850 N100 JP10","2AVL4 50L SBL EZ1 LP850 N100 JP10 (CI-235Y08)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["240P72","2AVL4 50L SBL EZ1 PWS1856LV LP840","2AVL4 50L SBL EZ1 PWS1856LV LP840 (CI-240P72)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["240PLW","2AVL4 A 30L MDR EZ1 LP835 CP","2AVL4 A 30L MDR EZ1 LP835 CP (CI-240PLW)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["240CXM","2AVL4 A 30L MDR EZ1 LP835 JP10","2AVL4 A 30L MDR EZ1 LP835 JP10 (CI-240CXM)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235KMM","2AVL4 A 30L MDR EZ1 LP840","2AVL4 A 30L MDR EZ1 LP840 (CI-235KMM)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["238FH4","2AVL4 A 30L MDR EZ1 LP840 JP10","2AVL4 A 30L MDR EZ1 LP840 JP10 (CI-238FH4)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["249RR4","2AVL4 A 30L MDR EZ1 PWS1856LV LP835","2AVL4 A 30L MDR EZ1 PWS1856LV LP835 (CI-249RR4)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["240RU8","2AVL4 A 40L ADP EZ1 LP830","2AVL4 A 40L ADP EZ1 LP830 (CI-240RU8)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["240RUH","2AVL4 A 40L ADP EZ1 LP830 JP10","2AVL4 A 40L ADP EZ1 LP830 JP10 (CI-240RUH)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237PN4","2AVL4 A 40L ADP EZ1 LP835","2AVL4 A 40L ADP EZ1 LP835 (CI-237PN4)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["238G3R","2AVL4 A 40L MDR EZ1 LP830","2AVL4 A 40L MDR EZ1 LP830 (CI-238G3R)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237P35","2AVL4 A 40L MDR EZ1 LP835 CP","2AVL4 A 40L MDR EZ1 LP835 CP (CI-237P35)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["238KNX","2AVL4 A 40L MDR EZ1 LP835 N80","2AVL4 A 40L MDR EZ1 LP835 N80 (CI-238KNX)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236TVK","2AVL4 A 40L MDR EZ1 LP850","2AVL4 A 40L MDR EZ1 LP850 (CI-236TVK)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["238VN5","2AVL4 A 50L MDR EZ1 LP830","2AVL4 A 50L MDR EZ1 LP830 (CI-238VN5)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235TV6","2AVL4 A 50L MDR EZ1 LP835","2AVL4 A 50L MDR EZ1 LP835 (CI-235TV6)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235TUU","2AVL4 A 50L MDR EZ1 LP835 JP10","2AVL4 A 50L MDR EZ1 LP835 JP10 (CI-235TUU)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233ENA","2AVL4 A 50L MDR EZ1 LP835 N100 JP10","2AVL4 A 50L MDR EZ1 LP835 N100 JP10 (CI-233ENA)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237RHP","2AVL4 A 50L MDR EZ1 LP835 N80","2AVL4 A 50L MDR EZ1 LP835 N80 (CI-237RHP)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237MCL","2AVL4 A 50L MDR EZ1 LP835 N80 USPOM","2AVL4 A 50L MDR EZ1 LP835 N80 USPOM (CI-237MCL)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237MFJ","2AVL4 A 50L MDR EZ1 LP835 N80 USPOM JP10","2AVL4 A 50L MDR EZ1 LP835 N80 USPOM JP10 (CI-237MFJ)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237MFX","2AVL4 A 50L MDR EZ1 LP835 N80EMG USPOM","2AVL4 A 50L MDR EZ1 LP835 N80EMG USPOM (CI-237MFX)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237MGF","2AVL4 A 50L MDR EZ1 LP835 N80EMG USPOM JP10","2AVL4 A 50L MDR EZ1 LP835 N80EMG USPOM JP10 (CI-237MGF)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["245MH8","2AVL4 A 50L MDR EZ1 LP850","2AVL4 A 50L MDR EZ1 LP850 (CI-245MH8)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237WA4","2AVL4 A 50L MDR EZ1 PWS1836 LP835","2AVL4 A 50L MDR EZ1 PWS1836 LP835 (CI-237WA4)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234GT8","2AVL4 ST 30L ADP EZ1 LP830","2AVL4 ST 30L ADP EZ1 LP830 (CI-234GT8)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
[{"$f":"(LEFT((RIGHT(C1346,7)),6))","v":"236TN8"},{"$f":"LEFT(C1346,SEARCH(\"(CI-\",C1346)-2)","v":"2AVL4 ST 30L ADP EZ1 LP835"},"2AVL4 ST 30L ADP EZ1 LP835 (CI-236TN8)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236TNA","2AVL4 ST 30L ADP EZ1 LP835 JP10","2AVL4 ST 30L ADP EZ1 LP835 JP10 (CI-236TNA)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["240A3M","2AVL4 ST 30L ADP EZ1 LP835 N100","2AVL4 ST 30L ADP EZ1 LP835 N100 (CI-240A3M)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233UJY","2AVL4 ST 30L MDR EZ1 LP830","2AVL4 ST 30L MDR EZ1 LP830 (CI-233UJY)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["245R8M","2AVL4 ST 30L MDR EZ1 LP830 N100","2AVL4 ST 30L MDR EZ1 LP830 N100 (CI-245R8M)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["245RCL","2AVL4 ST 30L MDR EZ1 LP830 N100EMG","2AVL4 ST 30L MDR EZ1 LP830 N100EMG (CI-245RCL)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232CLK","2AVL4 ST 30L MDR EZ1 LP835","2AVL4 ST 30L MDR EZ1 LP835 (CI-232CLK)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232R7A","2AVL4 ST 30L MDR EZ1 LP835 JP10","2AVL4 ST 30L MDR EZ1 LP835 JP10 (CI-232R7A)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237U0U","2AVL4 ST 30L MDR EZ1 LP835 N100","2AVL4 ST 30L MDR EZ1 LP835 N100 (CI-237U0U)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237U13","2AVL4 ST 30L MDR EZ1 LP835 N100 JP10","2AVL4 ST 30L MDR EZ1 LP835 N100 JP10 (CI-237U13)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237X03","2AVL4 ST 30L SBL EZ1 LP840 N100","2AVL4 ST 30L SBL EZ1 LP840 N100 (CI-237X03)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["241PXW","2AVL4 ST 30L SBL EZ1 LP840 N100 JP10","2AVL4 ST 30L SBL EZ1 LP840 N100 JP10 (CI-241PXW)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235N8U","2AVL4 ST 40L ADP EZ1 LP835","2AVL4 ST 40L ADP EZ1 LP835 (CI-235N8U)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["240A3V","2AVL4 ST 40L ADP EZ1 LP835 N100","2AVL4 ST 40L ADP EZ1 LP835 N100 (CI-240A3V)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232WC7","2AVL4 ST 40L MDR EZ1 LP830","2AVL4 ST 40L MDR EZ1 LP830 (CI-232WC7)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232WC6","2AVL4 ST 40L MDR EZ1 LP830 JP10","2AVL4 ST 40L MDR EZ1 LP830 JP10 (CI-232WC6)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232P0M","2AVL4 ST 40L MDR EZ1 LP830 N100","2AVL4 ST 40L MDR EZ1 LP830 N100 (CI-232P0M)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230G00","2AVL4 ST 40L MDR EZ1 LP835","2AVL4 ST 40L MDR EZ1 LP835 (CI-230G00)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232P6P","2AVL4 ST 40L MDR EZ1 LP835 JP10","2AVL4 ST 40L MDR EZ1 LP835 JP10 (CI-232P6P)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230GGU","2AVL4 ST 40L MDR EZ1 LP835 N100","2AVL4 ST 40L MDR EZ1 LP835 N100 (CI-230GGU)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231EA8","2AVL4 ST 40L MDR EZ1 LP835 N100 JP10","2AVL4 ST 40L MDR EZ1 LP835 N100 JP10 (CI-231EA8)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230WNP","2AVL4 ST 40L MDR EZ1 LP835 N100EMG","2AVL4 ST 40L MDR EZ1 LP835 N100EMG (CI-230WNP)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236EV8","2AVL4 ST 40L MDR EZ1 LP835 N100EMG JP10","2AVL4 ST 40L MDR EZ1 LP835 N100EMG JP10 (CI-236EV8)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230R2L","2AVL4 ST 40L MDR EZ1 LP835 N80","2AVL4 ST 40L MDR EZ1 LP835 N80 (CI-230R2L)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230R2U","2AVL4 ST 40L MDR EZ1 LP835 N80 JP10","2AVL4 ST 40L MDR EZ1 LP835 N80 JP10 (CI-230R2U)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232L30","2AVL4 ST 40L MDR EZ1 LP835 N80EMG","2AVL4 ST 40L MDR EZ1 LP835 N80EMG (CI-232L30)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230G05","2AVL4 ST 40L MDR EZ1 LP840","2AVL4 ST 40L MDR EZ1 LP840 (CI-230G05)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231L3G","2AVL4 ST 40L MDR EZ1 LP840 JP10","2AVL4 ST 40L MDR EZ1 LP840 JP10 (CI-231L3G)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["229UHA","2AVL4 ST 40L MDR EZ1 LP840 N100","2AVL4 ST 40L MDR EZ1 LP840 N100 (CI-229UHA)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231TA6","2AVL4 ST 40L MDR EZ1 LP840 N100 JP10","2AVL4 ST 40L MDR EZ1 LP840 N100 JP10 (CI-231TA6)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["229UJP","2AVL4 ST 40L MDR EZ1 LP840 N100EMG","2AVL4 ST 40L MDR EZ1 LP840 N100EMG (CI-229UJP)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232H64","2AVL4 ST 40L MDR EZ1 LP840 N100EMG JP10","2AVL4 ST 40L MDR EZ1 LP840 N100EMG JP10 (CI-232H64)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236AVP","2AVL4 ST 40L MDR EZ1 PWS1836 LP835 N80","2AVL4 ST 40L MDR EZ1 PWS1836 LP835 N80 (CI-236AVP)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["245X3V","2AVL4 ST 40L SBL EZ1 LP835","2AVL4 ST 40L SBL EZ1 LP835 (CI-245X3V)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237WV7","2AVL4 ST 40L SBL EZ1 LP840 N100","2AVL4 ST 40L SBL EZ1 LP840 N100 (CI-237WV7)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237WUW","2AVL4 ST 40L SBL EZ1 LP840 N100EMG","2AVL4 ST 40L SBL EZ1 LP840 N100EMG (CI-237WUW)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["229UJG","2AVL4 ST 50L MDR EZ1 LP835","2AVL4 ST 50L MDR EZ1 LP835 (CI-229UJG)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232TYE","2AVL4 ST 50L MDR EZ1 LP835 JP10","2AVL4 ST 50L MDR EZ1 LP835 JP10 (CI-232TYE)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232JJN","2AVL4 ST 50L MDR EZ1 LP835 N100","2AVL4 ST 50L MDR EZ1 LP835 N100 (CI-232JJN)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232P6V","2AVL4 ST 50L MDR EZ1 LP835 N100 JP10","2AVL4 ST 50L MDR EZ1 LP835 N100 JP10 (CI-232P6V)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["232P04","2AVL4 ST 50L MDR EZ1 LP835 N100EMG","2AVL4 ST 50L MDR EZ1 LP835 N100EMG (CI-232P04)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231PJ1","2AVL4 ST 50L MDR EZ1 LP835 N80","2AVL4 ST 50L MDR EZ1 LP835 N80 (CI-231PJ1)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231RG6","2AVL4 ST 50L MDR EZ1 LP835 N80 JP10","2AVL4 ST 50L MDR EZ1 LP835 N80 JP10 (CI-231RG6)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["240ER8","2AVL4 ST 50L MDR EZ1 LP835 N80EMG","2AVL4 ST 50L MDR EZ1 LP835 N80EMG (CI-240ER8)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234W55","2AVL4 ST 50L MDR EZ1 LP840","2AVL4 ST 50L MDR EZ1 LP840 (CI-234W55)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234W5C","2AVL4 ST 50L MDR EZ1 LP840 JP10","2AVL4 ST 50L MDR EZ1 LP840 JP10 (CI-234W5C)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["237WVC","2AVL4 ST 50L SBL EZ1 LP840 N100","2AVL4 ST 50L SBL EZ1 LP840 N100 (CI-237WVC)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["241PYV","2AVL4 ST 50L SBL EZ1 LP840 N100 JP10","2AVL4 ST 50L SBL EZ1 LP840 N100 JP10 (CI-241PYV)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233TM4","2AVL4 ST A 30L ADP EZ1 LP840 N100","2AVL4 ST A 30L ADP EZ1 LP840 N100 (CI-233TM4)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233TKL","2AVL4 ST A 30L ADP EZ1 LP840 N100 JP10","2AVL4 ST A 30L ADP EZ1 LP840 N100 JP10 (CI-233TKL)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233P9Y","2AVL4 ST A 30L MDR EZ1 LP835","2AVL4 ST A 30L MDR EZ1 LP835 (CI-233P9Y)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236NM2","2AVL4 ST A 30L SBL EZ1 LP840 N100","2AVL4 ST A 30L SBL EZ1 LP840 N100 (CI-236NM2)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233JGR","2AVL4 ST A 40L MDR EZ1 LP830 JP10","2AVL4 ST A 40L MDR EZ1 LP830 JP10 (CI-233JGR)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231EY5","2AVL4 ST A 40L MDR EZ1 LP835","2AVL4 ST A 40L MDR EZ1 LP835 (CI-231EY5)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234V9J","2AVL4 ST A 40L MDR EZ1 LP835 JP10","2AVL4 ST A 40L MDR EZ1 LP835 JP10 (CI-234V9J)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231A62","2AVL4 ST A 40L MDR EZ1 LP835 N100","2AVL4 ST A 40L MDR EZ1 LP835 N100 (CI-231A62)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236YRC","2AVL4 ST A 40L MDR EZ1 LP835 N100 JP10","2AVL4 ST A 40L MDR EZ1 LP835 N100 JP10 (CI-236YRC)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231A5U","2AVL4 ST A 40L MDR EZ1 LP835 N100EMG","2AVL4 ST A 40L MDR EZ1 LP835 N100EMG (CI-231A5U)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231A8E","2AVL4 ST A 40L MDR EZ1 LP835 N80","2AVL4 ST A 40L MDR EZ1 LP835 N80 (CI-231A8E)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234UC1","2AVL4 ST A 40L MDR EZ1 LP835 N80 JP10","2AVL4 ST A 40L MDR EZ1 LP835 N80 JP10 (CI-234UC1)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231A8J","2AVL4 ST A 40L MDR EZ1 LP835 N80EMG","2AVL4 ST A 40L MDR EZ1 LP835 N80EMG (CI-231A8J)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230AHJ","2AVL4 ST A 40L MDR EZ1 LP840","2AVL4 ST A 40L MDR EZ1 LP840 (CI-230AHJ)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230NV3","2AVL4 ST A 40L MDR EZ1 LP840 N100","2AVL4 ST A 40L MDR EZ1 LP840 N100 (CI-230NV3)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230NW0","2AVL4 ST A 40L MDR EZ1 LP840 N100EMG","2AVL4 ST A 40L MDR EZ1 LP840 N100EMG (CI-230NW0)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
[{"$f":"(LEFT((RIGHT(C1410,7)),6))","v":"230U2L"},{"$f":"LEFT(C1410,SEARCH(\"(CI-\",C1410)-2)","v":"2AVL4 ST A 40L MDR EZ1 LP840 N80"},"2AVL4 ST A 40L MDR EZ1 LP840 N80 (CI-230U2L)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["230U2U","2AVL4 ST A 40L MDR EZ1 LP840 N80EMG","2AVL4 ST A 40L MDR EZ1 LP840 N80EMG (CI-230U2U)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["231L2M","2AVL4 ST A 40L SBL EZ1 LP835","2AVL4 ST A 40L SBL EZ1 LP835 (CI-231L2M)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236NMG","2AVL4 ST A 40L SBL EZ1 LP840 N100","2AVL4 ST A 40L SBL EZ1 LP840 N100 (CI-236NMG)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236AR6","2AVL4 ST A 50L MDR EZ1 LP835","2AVL4 ST A 50L MDR EZ1 LP835 (CI-236AR6)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["236ARF","2AVL4 ST A 50L MDR EZ1 LP835 JP10","2AVL4 ST A 50L MDR EZ1 LP835 JP10 (CI-236ARF)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233N2K","2AVL4 ST A 50L MDR EZ1 LP835 N100","2AVL4 ST A 50L MDR EZ1 LP835 N100 (CI-233N2K)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["233N44","2AVL4 ST A 50L MDR EZ1 LP835 N100EMG","2AVL4 ST A 50L MDR EZ1 LP835 N100EMG (CI-233N44)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["235UY8","2AVL4 ST A 50L SBL EZ1 LP840","2AVL4 ST A 50L SBL EZ1 LP840 (CI-235UY8)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234PLV","2AVL4 ST A 50L SBL EZ1 LP840 N100","2AVL4 ST A 50L SBL EZ1 LP840 N100 (CI-234PLV)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234PM4","2AVL4 ST A 50L SBL EZ1 LP840 N100 JP10","2AVL4 ST A 50L SBL EZ1 LP840 N100 JP10 (CI-234PM4)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234PM7","2AVL4 ST A 50L SBL EZ1 LP840 N100EMG","2AVL4 ST A 50L SBL EZ1 LP840 N100EMG (CI-234PM7)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["234PMP","2AVL4 ST A 50L SBL EZ1 LP840 N100EMG JP10","2AVL4 ST A 50L SBL EZ1 LP840 N100EMG JP10 (CI-234PMP)","PS1030","Remote mount only","ELA PSRME IC","3 Boards in parallel instructions","*239MR9"]
["241HJ1","AVL4 18L MDR EZ1 LP835 MMC JP20","AVL4 18L MDR EZ1 LP835 MMC JP20 (CI-241HJ1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239TNX","AVL4 18L MDR EZ1 LP835 N100","AVL4 18L MDR EZ1 LP835 N100 (CI-239TNX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239U0U","AVL4 18L MDR EZ1 LP835 N100 MMC JP20","AVL4 18L MDR EZ1 LP835 N100 MMC JP20 (CI-239U0U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240NUR","AVL4 18L MDR EZ1 LP840 N100","AVL4 18L MDR EZ1 LP840 N100 (CI-240NUR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240NK4","AVL4 18L MDR EZ1 LP840 N100 MMC JP20","AVL4 18L MDR EZ1 LP840 N100 MMC JP20 (CI-240NK4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236VCM","AVL4 18L MDR EZ1 LP850","AVL4 18L MDR EZ1 LP850 (CI-236VCM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["247RHT","AVL4 18L MDR EZ1 PWS1856LV LP840","AVL4 18L MDR EZ1 PWS1856LV LP840 (CI-247RHT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235URA","AVL4 18L SBL EZ1 LP835","AVL4 18L SBL EZ1 LP835 (CI-235URA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240TXW","AVL4 25L MDR EZ1 LP830 N100","AVL4 25L MDR EZ1 LP830 N100 (CI-240TXW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235U91","AVL4 25L MDR EZ1 LP835 N100","AVL4 25L MDR EZ1 LP835 N100 (CI-235U91)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233Y7X","AVL4 25L MDR EZ1 LP835 N80EMG","AVL4 25L MDR EZ1 LP835 N80EMG (CI-233Y7X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239U57","AVL4 25L MDR EZ1 PWS1836 LP835","AVL4 25L MDR EZ1 PWS1836 LP835 (CI-239U57)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241LPR","AVL4 25L MDR EZ1 PWS1856LV LP830","AVL4 25L MDR EZ1 PWS1856LV LP830 (CI-241LPR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239L27","AVL4 25L MDR EZ1 PWS1856LV LP835","AVL4 25L MDR EZ1 PWS1856LV LP835 (CI-239L27)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234YET","AVL4 25L SBL EZ1 LP835","AVL4 25L SBL EZ1 LP835 (CI-234YET)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234YEV","AVL4 25L SBL EZ1 LP835 N80EMG","AVL4 25L SBL EZ1 LP835 N80EMG (CI-234YEV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235F04","AVL4 ST 18L MDR EZ1 LP835","AVL4 ST 18L MDR EZ1 LP835 (CI-235F04)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236MCW","AVL4 ST 25L MDR EZ1 LP835","AVL4 ST 25L MDR EZ1 LP835 (CI-236MCW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229UUC","2BZL2 16L EZ1 LP835 LCT RFD180228","2BZL2 16L EZ1 LP835 LCT RFD180228 (CI-229UUC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229UU8","2BZL2 16L EZ1 LP835 RFD180228","2BZL2 16L EZ1 LP835 RFD180228 (CI-229UU8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["222G4V","2BZL2 24L D24 LP835","2BZL2 24L D24 LP835 (CI-222G4V)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["224GNF","2BZL2 24L D24 LP835 NATS","2BZL2 24L D24 LP835 NATS (CI-224GNF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["224GNG","2BZL2 24L D24 LP835 NATS JP32","2BZL2 24L D24 LP835 NATS JP32 (CI-224GNG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["223NTJ","2BZL2 24L D26 LP840 N100","2BZL2 24L D26 LP840 N100 (CI-223NTJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232EYY","2BZL2 24L EZ1 277 LCT QFC213GA LP835","2BZL2 24L EZ1 277 LCT QFC213GA LP835 (CI-232EYY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232KTM","2BZL2 24L EZ1 277 VLC LP835","2BZL2 24L EZ1 277 VLC LP835 (CI-232KTM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230J6R","2BZL2 24L EZ1 LP830","2BZL2 24L EZ1 LP830 (CI-230J6R)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225JJT","2BZL2 24L EZ1 LP835","2BZL2 24L EZ1 LP835 (CI-225JJT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225JK2","2BZL2 24L EZ1 LP835 N100","2BZL2 24L EZ1 LP835 N100 (CI-225JK2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225JJX","2BZL2 24L EZ1 LP835 N80","2BZL2 24L EZ1 LP835 N80 (CI-225JJX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226R9X","2BZL2 24L EZ1 LP840","2BZL2 24L EZ1 LP840 (CI-226R9X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227P77","2BZL2 24L EZ1 LP840 N100","2BZL2 24L EZ1 LP840 N100 (CI-227P77)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229R8L","2BZL2 24L EZ1 LP840 N80","2BZL2 24L EZ1 LP840 N80 (CI-229R8L)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232KYT","2BZL2 24L EZ1 PWS1836 LP835","2BZL2 24L EZ1 PWS1836 LP835 (CI-232KYT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225JX8","2BZL2 24L EZB LP835 N100","2BZL2 24L EZB LP835 N100 (CI-225JX8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225YMT","2BZL2 24L SLD LP835","2BZL2 24L SLD LP835 (CI-225YMT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229PTH","2BZL2 24L SLD LP840","2BZL2 24L SLD LP840 (CI-229PTH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230LUC","2BZL2 30L EZ1 LP830","2BZL2 30L EZ1 LP830 (CI-230LUC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233G10","2BZL2 30L EZ1 LP830 N100","2BZL2 30L EZ1 LP830 N100 (CI-233G10)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230A2T","2BZL2 30L EZ1 LP830 N80","2BZL2 30L EZ1 LP830 N80 (CI-230A2T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225JK4","2BZL2 30L EZ1 LP835","2BZL2 30L EZ1 LP835 (CI-225JK4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225JXL","2BZL2 30L EZ1 LP835 N100","2BZL2 30L EZ1 LP835 N100 (CI-225JXL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225JXJ","2BZL2 30L EZ1 LP835 N80","2BZL2 30L EZ1 LP835 N80 (CI-225JXJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228R1H","2BZL2 30L EZ1 LP840","2BZL2 30L EZ1 LP840 (CI-228R1H)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228F2R","2BZL2 30L EZ1 LP840 N100","2BZL2 30L EZ1 LP840 N100 (CI-228F2R)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233WJF","2BZL2 30L EZ1 LP840 N100 USPOM","2BZL2 30L EZ1 LP840 N100 USPOM (CI-233WJF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229GEV","2BZL2 30L EZ1 LP840 N80","2BZL2 30L EZ1 LP840 N80 (CI-229GEV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232P47","2BZL2 30L EZ1 PWS1836 LP835","2BZL2 30L EZ1 PWS1836 LP835 (CI-232P47)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233JH7","2BZL2 30L EZ1 PWS1836 LP840","2BZL2 30L EZ1 PWS1836 LP840 (CI-233JH7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231JKT","2BZL2 30L EZB LP835","2BZL2 30L EZB LP835 (CI-231JKT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225K67","2BZL2 30L EZB LP835 N100","2BZL2 30L EZB LP835 N100 (CI-225K67)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C1474,7)),6))","v":"229X3T"},{"$f":"LEFT(C1474,SEARCH(\"(CI-\",C1474)-2)","v":"2BZL2 30L EZB LP840"},"2BZL2 30L EZB LP840 (CI-229X3T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225YMX","2BZL2 30L SLD LP835","2BZL2 30L SLD LP835 (CI-225YMX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233J34","2BZL2 34L 277 EZ1 QFC311GA LP835 N100 NATS","2BZL2 34L 277 EZ1 QFC311GA LP835 N100 NATS (CI-233J34)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["221YUY","2BZL2 34L D36 LP835 N100","2BZL2 34L D36 LP835 N100 (CI-221YUY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["224THW","2BZL2 34L D36 LP835 USPOM","2BZL2 34L D36 LP835 USPOM (CI-224THW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226ULH","2BZL2 34L EZ1 LP830","2BZL2 34L EZ1 LP830 (CI-226ULH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226VEH","2BZL2 34L EZ1 LP830 N100","2BZL2 34L EZ1 LP830 N100 (CI-226VEH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228EM8","2BZL2 34L EZ1 LP830 N80","2BZL2 34L EZ1 LP830 N80 (CI-228EM8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225JK5","2BZL2 34L EZ1 LP835","2BZL2 34L EZ1 LP835 (CI-225JK5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225K6F","2BZL2 34L EZ1 LP835 N100","2BZL2 34L EZ1 LP835 N100 (CI-225K6F)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225K6E","2BZL2 34L EZ1 LP835 N80","2BZL2 34L EZ1 LP835 N80 (CI-225K6E)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226L1F","2BZL2 34L EZ1 LP840","2BZL2 34L EZ1 LP840 (CI-226L1F)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227JLU","2BZL2 34L EZ1 LP840 N100","2BZL2 34L EZ1 LP840 N100 (CI-227JLU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229L9G","2BZL2 34L EZ1 LP840 N80","2BZL2 34L EZ1 LP840 N80 (CI-229L9G)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229CHV","2BZL2 34L EZ1 LP840 RFD177386","2BZL2 34L EZ1 LP840 RFD177386 (CI-229CHV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231NX5","2BZL2 34L EZ1 PWS1836 LP835","2BZL2 34L EZ1 PWS1836 LP835 (CI-231NX5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230UF8","2BZL2 34L EZ1 PWS1836 LP835 N100","2BZL2 34L EZ1 PWS1836 LP835 N100 (CI-230UF8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230VME","2BZL2 34L EZ1 PWS1836 LP835 N100 USPOM","2BZL2 34L EZ1 PWS1836 LP835 N100 USPOM (CI-230VME)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231E80","2BZL2 34L EZB LP830","2BZL2 34L EZB LP830 (CI-231E80)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228JG6","2BZL2 34L EZB LP835","2BZL2 34L EZB LP835 (CI-228JG6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225K6L","2BZL2 34L EZB LP835 N100","2BZL2 34L EZB LP835 N100 (CI-225K6L)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228T92","2BZL2 34L EZB LP840","2BZL2 34L EZB LP840 (CI-228T92)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229HH6","2BZL2 34L EZB LP840 N100","2BZL2 34L EZB LP840 N100 (CI-229HH6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231E6R","2BZL2 34L SLD LP830","2BZL2 34L SLD LP830 (CI-231E6R)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225K6N","2BZL2 34L SLD LP835","2BZL2 34L SLD LP835 (CI-225K6N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232L37","2BZL2 34L SLD LP840","2BZL2 34L SLD LP840 (CI-232L37)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228XG4","2BZL2 NATS EZ1 LP840 RFD177386 LCT","2BZL2 NATS EZ1 LP840 RFD177386 LCT (CI-228XG4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227G2X","2BZL2 NATS EZ1 RFD163150 LCT","2BZL2 NATS EZ1 RFD163150 LCT (CI-227G2X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232G6M","2BZL4 120 EOHN QFC313GX VLC NATS JP16","2BZL4 120 EOHN QFC313GX VLC NATS JP16 (CI-232G6M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230RMG","2BZL4 277 QFC213GA LCT NATS","2BZL4 277 QFC213GA LCT NATS (CI-230RMG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230RMH","2BZL4 277 QFC213GA LCT NATS JP16","2BZL4 277 QFC213GA LCT NATS JP16 (CI-230RMH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230V8W","2BZL4 277 QFC213GA LCT NATS JP16 RFD183288","2BZL4 277 QFC213GA LCT NATS JP16 RFD183288 (CI-230V8W)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230V92","2BZL4 277 QFC213GA LCT NATS JP16 RFD183289","2BZL4 277 QFC213GA LCT NATS JP16 RFD183289 (CI-230V92)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230V8X","2BZL4 277 QFC213GA LCT NATS RFD183288","2BZL4 277 QFC213GA LCT NATS RFD183288 (CI-230V8X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233F26","2BZL4 277 QFC213GA LCT NATS RFD183289","2BZL4 277 QFC213GA LCT NATS RFD183289 (CI-233F26)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230VC6","2BZL4 277 QFC213GA N80 NATS","2BZL4 277 QFC213GA N80 NATS (CI-230VC6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227GHW","2BZL4 277 QFC213GA NATS","2BZL4 277 QFC213GA NATS (CI-227GHW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227GHM","2BZL4 277 QFC213GA NATS JP16","2BZL4 277 QFC213GA NATS JP16 (CI-227GHM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233JC2","2BZL4 277 QFC311GA N100 NATS","2BZL4 277 QFC311GA N100 NATS (CI-233JC2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233JE5","2BZL4 277 QFC311GB N100 NATS","2BZL4 277 QFC311GB N100 NATS (CI-233JE5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230RML","2BZL4 277 QFC313GX LCT NATS","2BZL4 277 QFC313GX LCT NATS (CI-230RML)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230RMK","2BZL4 277 QFC313GX LCT NATS JP16","2BZL4 277 QFC313GX LCT NATS JP16 (CI-230RMK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230UXW","2BZL4 277 QFC313GX LCT NATS JP16 RFD183288","2BZL4 277 QFC313GX LCT NATS JP16 RFD183288 (CI-230UXW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230V8T","2BZL4 277 QFC313GX LCT NATS RFD183288","2BZL4 277 QFC313GX LCT NATS RFD183288 (CI-230V8T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230V90","2BZL4 277 QFC313GX LCT NATS RFD183289","2BZL4 277 QFC313GX LCT NATS RFD183289 (CI-230V90)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227GH0","2BZL4 277 QFC313GX NATS","2BZL4 277 QFC313GX NATS (CI-227GH0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227GCE","2BZL4 277 QFC313GX NATS JP16","2BZL4 277 QFC313GX NATS JP16 (CI-227GCE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229KHU","2BZL4 40L 120 EZ1 QFC211GA LP835 N100","2BZL4 40L 120 EZ1 QFC211GA LP835 N100 (CI-229KHU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230T5N","2BZL4 40L EZ1 LP830","2BZL4 40L EZ1 LP830 (CI-230T5N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233G1G","2BZL4 40L EZ1 LP830 N100","2BZL4 40L EZ1 LP830 N100 (CI-233G1G)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233UF7","2BZL4 40L EZ1 LP830 N80","2BZL4 40L EZ1 LP830 N80 (CI-233UF7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225KKH","2BZL4 40L EZ1 LP835","2BZL4 40L EZ1 LP835 (CI-225KKH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225KL1","2BZL4 40L EZ1 LP835 N100","2BZL4 40L EZ1 LP835 N100 (CI-225KL1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225KKY","2BZL4 40L EZ1 LP835 N80","2BZL4 40L EZ1 LP835 N80 (CI-225KKY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228UV0","2BZL4 40L EZ1 LP840","2BZL4 40L EZ1 LP840 (CI-228UV0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226P6W","2BZL4 40L EZ1 LP840 N100","2BZL4 40L EZ1 LP840 N100 (CI-226P6W)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229UY0","2BZL4 40L EZ1 LP840 N100 USPOM","2BZL4 40L EZ1 LP840 N100 USPOM (CI-229UY0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226UYU","2BZL4 40L EZ1 LP840 N80","2BZL4 40L EZ1 LP840 N80 (CI-226UYU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228Y25","2BZL4 40L EZ1 PWS1836 LP830","2BZL4 40L EZ1 PWS1836 LP830 (CI-228Y25)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228AN4","2BZL4 40L EZ1 PWS1836 LP835","2BZL4 40L EZ1 PWS1836 LP835 (CI-228AN4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233NWY","2BZL4 40L EZ1 PWS1836 LP840","2BZL4 40L EZ1 PWS1836 LP840 (CI-233NWY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229Y6V","2BZL4 40L EZB LP835","2BZL4 40L EZB LP835 (CI-229Y6V)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225L1H","2BZL4 40L EZB LP835 NX","2BZL4 40L EZB LP835 NX (CI-225L1H)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232JUE","2BZL4 40L EZB LP840 N100","2BZL4 40L EZB LP840 N100 (CI-232JUE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C1538,7)),6))","v":"225KL5"},{"$f":"LEFT(C1538,SEARCH(\"(CI-\",C1538)-2)","v":"2BZL4 40L SLD LP835"},"2BZL4 40L SLD LP835 (CI-225KL5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231LJ9","2BZL4 40L SLD LP840","2BZL4 40L SLD LP840 (CI-231LJ9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231NWP","2BZL4 40L SLD PWS1846 LP835","2BZL4 40L SLD PWS1846 LP835 (CI-231NWP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229KHJ","2BZL4 48L 120 EZ1 QFC211GA LP835 N100","2BZL4 48L 120 EZ1 QFC211GA LP835 N100 (CI-229KHJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228GXT","2BZL4 48L 277 EZ1 GLR LP835","2BZL4 48L 277 EZ1 GLR LP835 (CI-228GXT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["223CHE","2BZL4 48L D46 LP835 N100","2BZL4 48L D46 LP835 N100 (CI-223CHE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228K6U","2BZL4 48L EZ1 LP830","2BZL4 48L EZ1 LP830 (CI-228K6U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229JLF","2BZL4 48L EZ1 LP830 N80","2BZL4 48L EZ1 LP830 N80 (CI-229JLF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225KT3","2BZL4 48L EZ1 LP835","2BZL4 48L EZ1 LP835 (CI-225KT3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227ATY","2BZL4 48L EZ1 LP835 JP16","2BZL4 48L EZ1 LP835 JP16 (CI-227ATY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225KT8","2BZL4 48L EZ1 LP835 N100","2BZL4 48L EZ1 LP835 N100 (CI-225KT8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225KT7","2BZL4 48L EZ1 LP835 N80","2BZL4 48L EZ1 LP835 N80 (CI-225KT7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225V4L","2BZL4 48L EZ1 LP840","2BZL4 48L EZ1 LP840 (CI-225V4L)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227JXH","2BZL4 48L EZ1 LP840 N100","2BZL4 48L EZ1 LP840 N100 (CI-227JXH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229HHL","2BZL4 48L EZ1 LP840 N80","2BZL4 48L EZ1 LP840 N80 (CI-229HHL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230FNK","2BZL4 48L EZ1 LP850 RFD181119","2BZL4 48L EZ1 LP850 RFD181119 (CI-230FNK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233JHE","2BZL4 48L EZ1 PWS1436 LP835 N80","2BZL4 48L EZ1 PWS1436 LP835 N80 (CI-233JHE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232K3U","2BZL4 48L EZ1 PWS1836 LP835","2BZL4 48L EZ1 PWS1836 LP835 (CI-232K3U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229GRH","2BZL4 48L EZ1 PWS1836 LP835 N100","2BZL4 48L EZ1 PWS1836 LP835 N100 (CI-229GRH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232K38","2BZL4 48L EZ1 PWS1846 LP835","2BZL4 48L EZ1 PWS1846 LP835 (CI-232K38)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225YE1","2BZL4 48L EZB LP835 N100","2BZL4 48L EZB LP835 N100 (CI-225YE1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225YE2","2BZL4 48L EZB LP835 NX","2BZL4 48L EZB LP835 NX (CI-225YE2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227YJE","2BZL4 48L EZB LP840","2BZL4 48L EZB LP840 (CI-227YJE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225KT9","2BZL4 48L SLD LP835","2BZL4 48L SLD LP835 (CI-225KT9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229PT3","2BZL4 48L SLD LP840","2BZL4 48L SLD LP840 (CI-229PT3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231NW9","2BZL4 48L SLD PWS1846 LP835","2BZL4 48L SLD PWS1846 LP835 (CI-231NW9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227K1Y","2BZL4 60L EZ1 LCT LP835 NATJ","2BZL4 60L EZ1 LCT LP835 NATJ (CI-227K1Y)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227FCW","2BZL4 60L EZ1 LP830","2BZL4 60L EZ1 LP830 (CI-227FCW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225KTC","2BZL4 60L EZ1 LP835","2BZL4 60L EZ1 LP835 (CI-225KTC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225KTN","2BZL4 60L EZ1 LP835 N100","2BZL4 60L EZ1 LP835 N100 (CI-225KTN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228CHR","2BZL4 60L EZ1 LP840","2BZL4 60L EZ1 LP840 (CI-228CHR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227J3N","2BZL4 60L EZ1 LP840 N100","2BZL4 60L EZ1 LP840 N100 (CI-227J3N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232NG3","2BZL4 60L EZ1 LP840 N100 SSQ","2BZL4 60L EZ1 LP840 N100 SSQ (CI-232NG3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233GJJ","2BZL4 60L EZ1 LP840 N80","2BZL4 60L EZ1 LP840 N80 (CI-233GJJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234F02","2BZL4 60L EZB LP830","2BZL4 60L EZB LP830 (CI-234F02)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233JGX","2BZL4 60L EZB LP835","2BZL4 60L EZB LP835 (CI-233JGX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233VWC","2BZL4 60L EZB LP840","2BZL4 60L EZB LP840 (CI-233VWC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229HHC","2BZL4 60L EZB LP840 N100","2BZL4 60L EZB LP840 N100 (CI-229HHC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229AH9","2BZL4 60L SLD LP830","2BZL4 60L SLD LP830 (CI-229AH9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229PTG","2BZL4 60L SLD LP840","2BZL4 60L SLD LP840 (CI-229PTG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228UC6","2BZL4 CTRL KIT RFD176545 NATS","2BZL4 CTRL KIT RFD176545 NATS (CI-228UC6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228TXX","2BZL4 CTRL KIT RFD176545 NATS JP18","2BZL4 CTRL KIT RFD176545 NATS JP18 (CI-228TXX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226H02","2BZL4 NATS EZ1 RFD163150 LCT","2BZL4 NATS EZ1 RFD163150 LCT (CI-226H02)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["219RXK","2BZL4 NATS RFD148228","2BZL4 NATS RFD148228 (CI-219RXK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["219RXJ","2BZL4 NATS RFD148228 JP16","2BZL4 NATS RFD148228 JP16 (CI-219RXJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["223G7H","2BZL4 NATS RFD148228 T100","2BZL4 NATS RFD148228 T100 (CI-223G7H)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["224G3U","2BZL4 NATS RFD163150","2BZL4 NATS RFD163150 (CI-224G3U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["224G3N","2BZL4 NATS RFD163150 JP16","2BZL4 NATS RFD163150 JP16 (CI-224G3N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["224XN3","2BZL4 NATS STK RFD163150","2BZL4 NATS STK RFD163150 (CI-224XN3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225TRR","2BZL2 24L 120 EZ1 LP835 N100 CS1WL10 SSQ","2BZL2 24L 120 EZ1 LP835 N100 CS1WL10 SSQ (CI-225TRR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225JXG","2BZL2 24L EDB LP835 NX","2BZL2 24L EDB LP835 NX (CI-225JXG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237TXR","2BZL2 24L EZ1 LP830 N100","2BZL2 24L EZ1 LP830 N100 (CI-237TXR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228UU0","2BZL2 24L EZ1 LP835 N100EMG","2BZL2 24L EZ1 LP835 N100EMG (CI-228UU0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["239EHU","2BZL2 24L EZ1 LP835 N80EMG","2BZL2 24L EZ1 LP835 N80EMG (CI-239EHU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225JJW","2BZL2 24L EZ1 LP835 NX","2BZL2 24L EZ1 LP835 NX (CI-225JJW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240VPL","2BZL2 24L EZ1 PWS1856LV LP830","2BZL2 24L EZ1 PWS1856LV LP830 (CI-240VPL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234YWK","2BZL2 24L EZ1 PWS1856LV LP835","2BZL2 24L EZ1 PWS1856LV LP835 (CI-234YWK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237URR","2BZL2 24L EZB LP835","2BZL2 24L EZB LP835 (CI-237URR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225JX6","2BZL2 24L EZB LP835 N80","2BZL2 24L EZB LP835 N80 (CI-225JX6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225JXA","2BZL2 24L EZB LP835 NX","2BZL2 24L EZB LP835 NX (CI-225JXA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225WXT","2BZL2 30L 120 EZ1 LP835 CS1WL10 SSQ","2BZL2 30L 120 EZ1 LP835 CS1WL10 SSQ (CI-225WXT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225TRJ","2BZL2 30L 120 EZ1 LP835 N100 CS1WL10 SSQ","2BZL2 30L 120 EZ1 LP835 N100 CS1WL10 SSQ (CI-225TRJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225K6A","2BZL2 30L EDB LP835 NX","2BZL2 30L EDB LP835 NX (CI-225K6A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228UTP","2BZL2 30L EZ1 LP835 N100EMG","2BZL2 30L EZ1 LP835 N100EMG (CI-228UTP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C1602,7)),6))","v":"225JXN"},{"$f":"LEFT(C1602,SEARCH(\"(CI-\",C1602)-2)","v":"2BZL2 30L EZ1 LP835 NX"},"2BZL2 30L EZ1 LP835 NX (CI-225JXN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237JPT","2BZL2 30L EZ1 PWS1856LV LP830","2BZL2 30L EZ1 PWS1856LV LP830 (CI-237JPT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["239GFT","2BZL2 30L EZ1 PWS1856LV LP835","2BZL2 30L EZ1 PWS1856LV LP835 (CI-239GFT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225K65","2BZL2 30L EZB LP835 N80","2BZL2 30L EZB LP835 N80 (CI-225K65)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225K69","2BZL2 30L EZB LP835 NX","2BZL2 30L EZB LP835 NX (CI-225K69)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237R20","2BZL2 30L EZB LP840 N80","2BZL2 30L EZB LP840 N80 (CI-237R20)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235R7V","2BZL2 30L SLD LP840","2BZL2 30L SLD LP840 (CI-235R7V)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240GVG","2BZL2 34L 120 EZ1 LP830 CS1WL10 SSQ","2BZL2 34L 120 EZ1 LP830 CS1WL10 SSQ (CI-240GVG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228H45","2BZL2 34L 120 EZ1 LP830 N100 CS1WL10 SSQ","2BZL2 34L 120 EZ1 LP830 N100 CS1WL10 SSQ (CI-228H45)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225TRE","2BZL2 34L 120 EZ1 LP835 N100 CS1WL10 SSQ","2BZL2 34L 120 EZ1 LP835 N100 CS1WL10 SSQ (CI-225TRE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229YHL","2BZL2 34L 120 EZ1 LP840 N100 CS1WL10 SSQ","2BZL2 34L 120 EZ1 LP840 N100 CS1WL10 SSQ (CI-229YHL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["222RLW","2BZL2 34L D36 LP835","2BZL2 34L D36 LP835 (CI-222RLW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225L1G","2BZL2 34L EDB LP835 NX","2BZL2 34L EDB LP835 NX (CI-225L1G)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234K66","2BZL2 34L EZ1 LP830 N100EMG","2BZL2 34L EZ1 LP830 N100EMG (CI-234K66)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228WET","2BZL2 34L EZ1 LP835 N100EMG","2BZL2 34L EZ1 LP835 N100EMG (CI-228WET)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229EHJ","2BZL2 34L EZ1 LP835 N80EMG","2BZL2 34L EZ1 LP835 N80EMG (CI-229EHJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225K6H","2BZL2 34L EZ1 LP835 NX","2BZL2 34L EZ1 LP835 NX (CI-225K6H)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237WYG","2BZL2 34L EZ1 LP835 USPOM","2BZL2 34L EZ1 LP835 USPOM (CI-237WYG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236J61","2BZL2 34L EZ1 LP840 USPOM","2BZL2 34L EZ1 LP840 USPOM (CI-236J61)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235RRN","2BZL2 34L EZ1 PWS1836 LP840","2BZL2 34L EZ1 PWS1836 LP840 (CI-235RRN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237XT4","2BZL2 34L EZ1 PWS1856LV LP835","2BZL2 34L EZ1 PWS1856LV LP835 (CI-237XT4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["245LY3","2BZL2 34L EZ1 PWS1856LV LP840","2BZL2 34L EZ1 PWS1856LV LP840 (CI-245LY3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225K6K","2BZL2 34L EZB LP835 N80","2BZL2 34L EZB LP835 N80 (CI-225K6K)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225L1F","2BZL2 34L EZB LP835 NX","2BZL2 34L EZB LP835 NX (CI-225L1F)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225L2X","2BZL4 40L EDB LP835 NX","2BZL4 40L EDB LP835 NX (CI-225L2X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239EKE","2BZL4 40L EZ1 LP835 N80EMG","2BZL4 40L EZ1 LP835 N80EMG (CI-239EKE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225KKJ","2BZL4 40L EZ1 LP835 NX","2BZL4 40L EZ1 LP835 NX (CI-225KKJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229UCP","2BZL4 40L EZ1 LP840 N100 USPOM DO NOT USE","2BZL4 40L EZ1 LP840 N100 USPOM DO NOT USE (CI-229UCP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236EEH","2BZL4 40L EZ1 LP840 N100EMG","2BZL4 40L EZ1 LP840 N100EMG (CI-236EEH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240XM4","2BZL4 40L EZ1 PWS1856LV LP830","2BZL4 40L EZ1 PWS1856LV LP830 (CI-240XM4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234YKC","2BZL4 40L EZ1 PWS1856LV LP835","2BZL4 40L EZ1 PWS1856LV LP835 (CI-234YKC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235NTC","2BZL4 40L EZ1 PWS1856LV LP840","2BZL4 40L EZ1 PWS1856LV LP840 (CI-235NTC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225L2U","2BZL4 40L EZB LP835 N100","2BZL4 40L EZB LP835 N100 (CI-225L2U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225L1V","2BZL4 40L EZB LP835 N80","2BZL4 40L EZB LP835 N80 (CI-225L1V)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238XYL","2BZL4 40L EZB LP840","2BZL4 40L EZB LP840 (CI-238XYL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225WXR","2BZL4 48L 120 EZ1 LP835 CS1WL10 SSQ","2BZL4 48L 120 EZ1 LP835 CS1WL10 SSQ (CI-225WXR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235UK9","2BZL4 48L 120 EZ1 LP840 N100 CS1WL10 SSQ","2BZL4 48L 120 EZ1 LP840 N100 CS1WL10 SSQ (CI-235UK9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225YL1","2BZL4 48L EDB LP835 NX","2BZL4 48L EDB LP835 NX (CI-225YL1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241HGP","2BZL4 48L EZ1 LP830 N100","2BZL4 48L EZ1 LP830 N100 (CI-241HGP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235XUE","2BZL4 48L EZ1 LP835 N100EMG","2BZL4 48L EZ1 LP835 N100EMG (CI-235XUE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225KT6","2BZL4 48L EZ1 LP835 NX","2BZL4 48L EZ1 LP835 NX (CI-225KT6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228WG4","2BZL4 48L EZ1 LP840 N100EMG","2BZL4 48L EZ1 LP840 N100EMG (CI-228WG4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236J60","2BZL4 48L EZ1 LP840 USPOM","2BZL4 48L EZ1 LP840 USPOM (CI-236J60)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235C97","2BZL4 48L EZ1 PWS1836 LP840","2BZL4 48L EZ1 PWS1836 LP840 (CI-235C97)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234YL0","2BZL4 48L EZ1 PWS1856LV LP835","2BZL4 48L EZ1 PWS1856LV LP835 (CI-234YL0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235NTJ","2BZL4 48L EZ1 PWS1856LV LP840","2BZL4 48L EZ1 PWS1856LV LP840 (CI-235NTJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225YC9","2BZL4 48L EZB LP835 N80","2BZL4 48L EZB LP835 N80 (CI-225YC9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235J20","2BZL4 48L EZB LP840 N100","2BZL4 48L EZB LP840 N100 (CI-235J20)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227HE0","2BZL4 60L 120 EZ1 LP835 CS1WL10 SSQ","2BZL4 60L 120 EZ1 LP835 CS1WL10 SSQ (CI-227HE0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["224MEW","2BZL4 60L D58 LP830 BLD","2BZL4 60L D58 LP830 BLD (CI-224MEW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225YL8","2BZL4 60L EDB LP835 NX","2BZL4 60L EDB LP835 NX (CI-225YL8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232WRN","2BZL4 60L EZ1 LP835 N100EMG","2BZL4 60L EZ1 LP835 N100EMG (CI-232WRN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225KTM","2BZL4 60L EZ1 LP835 N80","2BZL4 60L EZ1 LP835 N80 (CI-225KTM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239F5L","2BZL4 60L EZ1 LP835 N80EMG","2BZL4 60L EZ1 LP835 N80EMG (CI-239F5L)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225KTG","2BZL4 60L EZ1 LP835 NX","2BZL4 60L EZ1 LP835 NX (CI-225KTG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237XR6","2BZL4 60L EZ1 LP840 USPOM","2BZL4 60L EZ1 LP840 USPOM (CI-237XR6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240GLT","2BZL4 60L EZ1 PWS1836 LP835","2BZL4 60L EZ1 PWS1836 LP835 (CI-240GLT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237FLN","2BZL4 60L EZ1 PWS1836 LP840","2BZL4 60L EZ1 PWS1836 LP840 (CI-237FLN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234YVM","2BZL4 60L EZ1 PWS1856LV LP835","2BZL4 60L EZ1 PWS1856LV LP835 (CI-234YVM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235NUF","2BZL4 60L EZ1 PWS1856LV LP840","2BZL4 60L EZ1 PWS1856LV LP840 (CI-235NUF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225YL5","2BZL4 60L EZB LP835 N100","2BZL4 60L EZB LP835 N100 (CI-225YL5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225YL4","2BZL4 60L EZB LP835 N80","2BZL4 60L EZB LP835 N80 (CI-225YL4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225YL7","2BZL4 60L EZB LP835 NX","2BZL4 60L EZB LP835 NX (CI-225YL7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237J9R","2BZL4 60L EZB LP840 N100EMG","2BZL4 60L EZB LP840 N100EMG (CI-237J9R)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C1666,7)),6))","v":"237CFN"},{"$f":"LEFT(C1666,SEARCH(\"(CI-\",C1666)-2)","v":"2BZL4 60L EZB LP840 N80"},"2BZL4 60L EZB LP840 N80 (CI-237CFN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225KTW","2BZL4 60L SLD LP835","2BZL4 60L SLD LP835 (CI-225KTW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227HPR","2FSL2 20L EZ1 LP830","2FSL2 20L EZ1 LP830 (CI-227HPR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230A1P","2FSL2 20L EZ1 LP830 N80","2FSL2 20L EZ1 LP830 N80 (CI-230A1P)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["224P1A","2FSL2 20L EZ1 LP835","2FSL2 20L EZ1 LP835 (CI-224P1A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226L6V","2FSL2 20L EZ1 LP835 N100","2FSL2 20L EZ1 LP835 N100 (CI-226L6V)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228P44","2FSL2 20L EZ1 LP835 N80","2FSL2 20L EZ1 LP835 N80 (CI-228P44)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230NHM","2FSL2 20L EZ1 LP835 RFD182215","2FSL2 20L EZ1 LP835 RFD182215 (CI-230NHM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["224P1F","2FSL2 20L EZ1 LP840","2FSL2 20L EZ1 LP840 (CI-224P1F)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228J9T","2FSL2 20L EZ1 LP840 CP","2FSL2 20L EZ1 LP840 CP (CI-228J9T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226W42","2FSL2 20L EZ1 LP840 N100","2FSL2 20L EZ1 LP840 N100 (CI-226W42)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229PAK","2FSL2 20L EZ1 LP840 N80","2FSL2 20L EZ1 LP840 N80 (CI-229PAK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229UT9","2FSL2 20L EZ1 LP850","2FSL2 20L EZ1 LP850 (CI-229UT9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227GME","2FSL2 20L EZ1 LP850 N100","2FSL2 20L EZ1 LP850 N100 (CI-227GME)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225P03","2FSL2 20L EZ1 LP850 N80","2FSL2 20L EZ1 LP850 N80 (CI-225P03)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226V86","2FSL2 20L EZ1 PWS1836 LP835","2FSL2 20L EZ1 PWS1836 LP835 (CI-226V86)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228GK5","2FSL2 20L EZ1 PWS1836 LP835 N100","2FSL2 20L EZ1 PWS1836 LP835 N100 (CI-228GK5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226Y3M","2FSL2 20L EZ1 PWS1836 LP840","2FSL2 20L EZ1 PWS1836 LP840 (CI-226Y3M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231MMM","2FSL2 20L EZ1 PWS1836 LP840 N80","2FSL2 20L EZ1 PWS1836 LP840 N80 (CI-231MMM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234NV2","2FSL2 20L EZB LP830 N100","2FSL2 20L EZB LP830 N100 (CI-234NV2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230WXV","2FSL2 20L EZB LP835","2FSL2 20L EZB LP835 (CI-230WXV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228NKR","2FSL2 20L EZB LP835 N100","2FSL2 20L EZB LP835 N100 (CI-228NKR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229ML9","2FSL2 20L EZB LP840","2FSL2 20L EZB LP840 (CI-229ML9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232EJM","2FSL2 20L EZB PWS1856LV LP835","2FSL2 20L EZB PWS1856LV LP835 (CI-232EJM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234E3M","2FSL2 20L SLD LP835","2FSL2 20L SLD LP835 (CI-234E3M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225P0V","2FSL2 20L SLD LP840","2FSL2 20L SLD LP840 (CI-225P0V)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229KT2","2FSL2 20L SLD PWS1846 LP835","2FSL2 20L SLD PWS1846 LP835 (CI-229KT2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232W4N","2FSL2 20L SLD PWS1846 LP840","2FSL2 20L SLD PWS1846 LP840 (CI-232W4N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230UY8","2FSL2 33L 120 EZ1 GLR PWS1836 LP840","2FSL2 33L 120 EZ1 GLR PWS1836 LP840 (CI-230UY8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230EJJ","2FSL2 33L 120 EZ1 QFC211GA LP835","2FSL2 33L 120 EZ1 QFC211GA LP835 (CI-230EJJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234H2N","2FSL2 33L EDB LP840","2FSL2 33L EDB LP840 (CI-234H2N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234XW8","2FSL2 33L EOHN LP830","2FSL2 33L EOHN LP830 (CI-234XW8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229K76","2FSL2 33L EOHN LP840","2FSL2 33L EOHN LP840 (CI-229K76)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229TKU","2FSL2 33L EXB LP850","2FSL2 33L EXB LP850 (CI-229TKU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["224P3Y","2FSL2 33L EZ1 LP830","2FSL2 33L EZ1 LP830 (CI-224P3Y)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227CH9","2FSL2 33L EZ1 LP830 N100","2FSL2 33L EZ1 LP830 N100 (CI-227CH9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228RHG","2FSL2 33L EZ1 LP830 N80","2FSL2 33L EZ1 LP830 N80 (CI-228RHG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["224GPA","2FSL2 33L EZ1 LP835","2FSL2 33L EZ1 LP835 (CI-224GPA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226JH9","2FSL2 33L EZ1 LP835 CP","2FSL2 33L EZ1 LP835 CP (CI-226JH9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225NYU","2FSL2 33L EZ1 LP835 N100","2FSL2 33L EZ1 LP835 N100 (CI-225NYU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225KKV","2FSL2 33L EZ1 LP835 N80","2FSL2 33L EZ1 LP835 N80 (CI-225KKV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["224PY9","2FSL2 33L EZ1 LP835 SAMPLE AND CASE","2FSL2 33L EZ1 LP835 SAMPLE AND CASE (CI-224PY9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233NJY","2FSL2 33L EZ1 LP835 USPOM","2FSL2 33L EZ1 LP835 USPOM (CI-233NJY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["224NUR","2FSL2 33L EZ1 LP840","2FSL2 33L EZ1 LP840 (CI-224NUR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229FFT","2FSL2 33L EZ1 LP840 CP","2FSL2 33L EZ1 LP840 CP (CI-229FFT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225M30","2FSL2 33L EZ1 LP840 N100","2FSL2 33L EZ1 LP840 N100 (CI-225M30)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226F88","2FSL2 33L EZ1 LP840 N80","2FSL2 33L EZ1 LP840 N80 (CI-226F88)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227RWU","2FSL2 33L EZ1 LP840 RFD173863","2FSL2 33L EZ1 LP840 RFD173863 (CI-227RWU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232MFF","2FSL2 33L EZ1 LP840 USPOM","2FSL2 33L EZ1 LP840 USPOM (CI-232MFF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225R2E","2FSL2 33L EZ1 LP850","2FSL2 33L EZ1 LP850 (CI-225R2E)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230MY6","2FSL2 33L EZ1 LP850 N80","2FSL2 33L EZ1 LP850 N80 (CI-230MY6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227RHT","2FSL2 33L EZ1 PWS1836 LP830","2FSL2 33L EZ1 PWS1836 LP830 (CI-227RHT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233GL3","2FSL2 33L EZ1 PWS1836 LP830 N100","2FSL2 33L EZ1 PWS1836 LP830 N100 (CI-233GL3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225X3J","2FSL2 33L EZ1 PWS1836 LP835","2FSL2 33L EZ1 PWS1836 LP835 (CI-225X3J)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226EMR","2FSL2 33L EZ1 PWS1836 LP835 N100","2FSL2 33L EZ1 PWS1836 LP835 N100 (CI-226EMR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229PFE","2FSL2 33L EZ1 PWS1836 LP835 N100 USPOM","2FSL2 33L EZ1 PWS1836 LP835 N100 USPOM (CI-229PFE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229HH4","2FSL2 33L EZ1 PWS1836 LP835 N80","2FSL2 33L EZ1 PWS1836 LP835 N80 (CI-229HH4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226X47","2FSL2 33L EZ1 PWS1836 LP840","2FSL2 33L EZ1 PWS1836 LP840 (CI-226X47)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226EMY","2FSL2 33L EZ1 PWS1836 LP840 N100","2FSL2 33L EZ1 PWS1836 LP840 N100 (CI-226EMY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["224RX3","2FSL2 33L EZ1 PWS1836 LP840 N80","2FSL2 33L EZ1 PWS1836 LP840 N80 (CI-224RX3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231F86","2FSL2 33L EZ1 PWS1836 LP840 N80 USPOM","2FSL2 33L EZ1 PWS1836 LP840 N80 USPOM (CI-231F86)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227KNG","2FSL2 33L EZ1 PWS1846 LP835","2FSL2 33L EZ1 PWS1846 LP835 (CI-227KNG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232WEU","2FSL2 33L EZ1 PWS1846 LP835 N100","2FSL2 33L EZ1 PWS1846 LP835 N100 (CI-232WEU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226WNR","2FSL2 33L EZ1 PWS1846 LP840","2FSL2 33L EZ1 PWS1846 LP840 (CI-226WNR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C1730,7)),6))","v":"230M75"},{"$f":"LEFT(C1730,SEARCH(\"(CI-\",C1730)-2)","v":"2FSL2 33L EZ1 PWS1856LV LP835"},"2FSL2 33L EZ1 PWS1856LV LP835 (CI-230M75)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226X4L","2FSL2 33L EZ1 PWS1856LV LP840","2FSL2 33L EZ1 PWS1856LV LP840 (CI-226X4L)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227KX8","2FSL2 33L EZB LP830","2FSL2 33L EZB LP830 (CI-227KX8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231X1A","2FSL2 33L EZB LP830 N100","2FSL2 33L EZB LP830 N100 (CI-231X1A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226PV7","2FSL2 33L EZB LP835","2FSL2 33L EZB LP835 (CI-226PV7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225TGC","2FSL2 33L EZB LP835 N100","2FSL2 33L EZB LP835 N100 (CI-225TGC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225J4U","2FSL2 33L EZB LP835 N80","2FSL2 33L EZB LP835 N80 (CI-225J4U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233NVM","2FSL2 33L EZB LP840","2FSL2 33L EZB LP840 (CI-233NVM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227GMJ","2FSL2 33L EZB LP840 N100","2FSL2 33L EZB LP840 N100 (CI-227GMJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234VMP","2FSL2 33L LUTRON LP830 RFD191892","2FSL2 33L LUTRON LP830 RFD191892 (CI-234VMP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230M1R","2FSL2 33L SLD LP830","2FSL2 33L SLD LP830 (CI-230M1R)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226TU8","2FSL2 33L SLD LP835","2FSL2 33L SLD LP835 (CI-226TU8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228RC7","2FSL2 33L SLD LP840","2FSL2 33L SLD LP840 (CI-228RC7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231PCU","2FSL2 33L SLD LP935 RFD181990","2FSL2 33L SLD LP935 RFD181990 (CI-231PCU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232F6U","2FSL2 33L SLD LP935 RFD187480","2FSL2 33L SLD LP935 RFD187480 (CI-232F6U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228WYE","2FSL2 33L SLD PWS1846 LP835","2FSL2 33L SLD PWS1846 LP835 (CI-228WYE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233FAA","2FSL2 33L SLD PWS1846 LP840","2FSL2 33L SLD PWS1846 LP840 (CI-233FAA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230E6K","2FSL2 40L 277 EZ1 QFC213GA GLR LP840","2FSL2 40L 277 EZ1 QFC213GA GLR LP840 (CI-230E6K)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226Y6V","2FSL2 40L EZ1 LP830","2FSL2 40L EZ1 LP830 (CI-226Y6V)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233X0J","2FSL2 40L EZ1 LP830 CP","2FSL2 40L EZ1 LP830 CP (CI-233X0J)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228W98","2FSL2 40L EZ1 LP830 N100","2FSL2 40L EZ1 LP830 N100 (CI-228W98)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229WXC","2FSL2 40L EZ1 LP830 N80","2FSL2 40L EZ1 LP830 N80 (CI-229WXC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["224P1J","2FSL2 40L EZ1 LP835","2FSL2 40L EZ1 LP835 (CI-224P1J)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227E2C","2FSL2 40L EZ1 LP835 N100","2FSL2 40L EZ1 LP835 N100 (CI-227E2C)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226PR0","2FSL2 40L EZ1 LP835 N80","2FSL2 40L EZ1 LP835 N80 (CI-226PR0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228NX1","2FSL2 40L EZ1 LP835 USPOM","2FSL2 40L EZ1 LP835 USPOM (CI-228NX1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["224P1N","2FSL2 40L EZ1 LP840","2FSL2 40L EZ1 LP840 (CI-224P1N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225R2T","2FSL2 40L EZ1 LP840 N100","2FSL2 40L EZ1 LP840 N100 (CI-225R2T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231G3M","2FSL2 40L EZ1 LP840 N100 USPOM","2FSL2 40L EZ1 LP840 N100 USPOM (CI-231G3M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225KK3","2FSL2 40L EZ1 LP840 N80","2FSL2 40L EZ1 LP840 N80 (CI-225KK3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225PXR","2FSL2 40L EZ1 LP850","2FSL2 40L EZ1 LP850 (CI-225PXR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227FR6","2FSL2 40L EZ1 LP850 N100","2FSL2 40L EZ1 LP850 N100 (CI-227FR6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228A2M","2FSL2 40L EZ1 LP850 N80","2FSL2 40L EZ1 LP850 N80 (CI-228A2M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229JTL","2FSL2 40L EZ1 LP850 NA20","2FSL2 40L EZ1 LP850 NA20 (CI-229JTL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229G0M","2FSL2 40L EZ1 PWS1836 LP830","2FSL2 40L EZ1 PWS1836 LP830 (CI-229G0M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229J2M","2FSL2 40L EZ1 PWS1836 LP830 N100","2FSL2 40L EZ1 PWS1836 LP830 N100 (CI-229J2M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226Y6K","2FSL2 40L EZ1 PWS1836 LP835","2FSL2 40L EZ1 PWS1836 LP835 (CI-226Y6K)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228HYY","2FSL2 40L EZ1 PWS1836 LP835 N100","2FSL2 40L EZ1 PWS1836 LP835 N100 (CI-228HYY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229HMX","2FSL2 40L EZ1 PWS1836 LP835 UAL USPOM","2FSL2 40L EZ1 PWS1836 LP835 UAL USPOM (CI-229HMX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228U91","2FSL2 40L EZ1 PWS1836 LP840","2FSL2 40L EZ1 PWS1836 LP840 (CI-228U91)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228HGL","2FSL2 40L EZ1 PWS1836 LP840 N100","2FSL2 40L EZ1 PWS1836 LP840 N100 (CI-228HGL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232KWJ","2FSL2 40L EZ1 PWS1836 LP840 N80","2FSL2 40L EZ1 PWS1836 LP840 N80 (CI-232KWJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231FRU","2FSL2 40L EZ1 PWS1836 LP840 N80 USPOM","2FSL2 40L EZ1 PWS1836 LP840 N80 USPOM (CI-231FRU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231L4A","2FSL2 40L EZ1 PWS1846 LP835","2FSL2 40L EZ1 PWS1846 LP835 (CI-231L4A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232WE2","2FSL2 40L EZ1 PWS1846 LP835 N100","2FSL2 40L EZ1 PWS1846 LP835 N100 (CI-232WE2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230M7H","2FSL2 40L EZ1 PWS1856LV LP835","2FSL2 40L EZ1 PWS1856LV LP835 (CI-230M7H)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230GR2","2FSL2 40L EZB LP830","2FSL2 40L EZB LP830 (CI-230GR2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231RYP","2FSL2 40L EZB LP835","2FSL2 40L EZB LP835 (CI-231RYP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226AKF","2FSL2 40L EZB LP835 N100","2FSL2 40L EZB LP835 N100 (CI-226AKF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229TTN","2FSL2 40L EZB LP835 N80","2FSL2 40L EZB LP835 N80 (CI-229TTN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229GCH","2FSL2 40L EZB LP840","2FSL2 40L EZB LP840 (CI-229GCH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229PLH","2FSL2 40L EZB LP840 MB RFD178588","2FSL2 40L EZB LP840 MB RFD178588 (CI-229PLH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229R9G","2FSL2 40L EZB LP840 N80","2FSL2 40L EZB LP840 N80 (CI-229R9G)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230WA0","2FSL2 40L EZB PWS1836 LP835","2FSL2 40L EZB PWS1836 LP835 (CI-230WA0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229UEP","2FSL2 40L EZB PWS1836 LP840","2FSL2 40L EZB PWS1836 LP840 (CI-229UEP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232C9Y","2FSL2 40L SLD LP830","2FSL2 40L SLD LP830 (CI-232C9Y)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226WN4","2FSL2 40L SLD LP835","2FSL2 40L SLD LP835 (CI-226WN4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232NR1","2FSL2 40L SLD LP840","2FSL2 40L SLD LP840 (CI-232NR1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227TWJ","2FSL2 40L SLD PWS1846 LP835","2FSL2 40L SLD PWS1846 LP835 (CI-227TWJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232WVN","2FSL2 H 20L EZ1 LP840","2FSL2 H 20L EZ1 LP840 (CI-232WVN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229MKM","2FSL2 H 33L EZ1 LP830","2FSL2 H 33L EZ1 LP830 (CI-229MKM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231K5U","2FSL2 H 33L EZ1 LP835","2FSL2 H 33L EZ1 LP835 (CI-231K5U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233NRE","2FSL2 H 33L EZ1 LP835 N80","2FSL2 H 33L EZ1 LP835 N80 (CI-233NRE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232LJN","2FSL2 H 33L EZ1 LP840 N80","2FSL2 H 33L EZ1 LP840 N80 (CI-232LJN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C1794,7)),6))","v":"231J4K"},{"$f":"LEFT(C1794,SEARCH(\"(CI-\",C1794)-2)","v":"2FSL2 H 33L EZ1 PWS1836 LP835 N80"},"2FSL2 H 33L EZ1 PWS1836 LP835 N80 (CI-231J4K)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230TNU","2FSL2 H 40L EZ1 LP830","2FSL2 H 40L EZ1 LP830 (CI-230TNU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229MKA","2FSL2 H 40L EZ1 LP835","2FSL2 H 40L EZ1 LP835 (CI-229MKA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232FH8","2FSL2 H 40L EZ1 LP835 N80","2FSL2 H 40L EZ1 LP835 N80 (CI-232FH8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231W87","2FSL2 H 40L EZ1 LP840 N80","2FSL2 H 40L EZ1 LP840 N80 (CI-231W87)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228P80","2FSL4 30L EDB PWS1836 LP835","2FSL4 30L EDB PWS1836 LP835 (CI-228P80)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228EG7","2FSL4 30L EXB LP835","2FSL4 30L EXB LP835 (CI-228EG7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229YF3","2FSL4 30L EZ1 LP830","2FSL4 30L EZ1 LP830 (CI-229YF3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233W89","2FSL4 30L EZ1 LP830 N80","2FSL4 30L EZ1 LP830 N80 (CI-233W89)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["224P1V","2FSL4 30L EZ1 LP835","2FSL4 30L EZ1 LP835 (CI-224P1V)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228FXR","2FSL4 30L EZ1 LP835 N100","2FSL4 30L EZ1 LP835 N100 (CI-228FXR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230RH5","2FSL4 30L EZ1 LP835 N80","2FSL4 30L EZ1 LP835 N80 (CI-230RH5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["224P1Y","2FSL4 30L EZ1 LP840","2FSL4 30L EZ1 LP840 (CI-224P1Y)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227CAU","2FSL4 30L EZ1 LP840 N100","2FSL4 30L EZ1 LP840 N100 (CI-227CAU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227TC9","2FSL4 30L EZ1 LP840 N80","2FSL4 30L EZ1 LP840 N80 (CI-227TC9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234FPW","2FSL4 30L EZ1 LP840 USPOM","2FSL4 30L EZ1 LP840 USPOM (CI-234FPW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228EVE","2FSL4 30L EZ1 LP850","2FSL4 30L EZ1 LP850 (CI-228EVE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227HMK","2FSL4 30L EZ1 PWS1836 LP835","2FSL4 30L EZ1 PWS1836 LP835 (CI-227HMK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231FC6","2FSL4 30L EZ1 PWS1836 LP835 N80 USPOM","2FSL4 30L EZ1 PWS1836 LP835 N80 USPOM (CI-231FC6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231PGY","2FSL4 30L EZ1 PWS1836 LP840","2FSL4 30L EZ1 PWS1836 LP840 (CI-231PGY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229R8W","2FSL4 30L EZ1 PWS1836 LP840 N80","2FSL4 30L EZ1 PWS1836 LP840 N80 (CI-229R8W)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231FEK","2FSL4 30L EZ1 PWS1836 LP840 N80 USPOM","2FSL4 30L EZ1 PWS1836 LP840 N80 USPOM (CI-231FEK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233YEY","2FSL4 30L EZ1 PWS1856LV LP835","2FSL4 30L EZ1 PWS1856LV LP835 (CI-233YEY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233UW4","2FSL4 30L EZ1 PWS1856LV LP840","2FSL4 30L EZ1 PWS1856LV LP840 (CI-233UW4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228UWW","2FSL4 30L EZB LP835","2FSL4 30L EZB LP835 (CI-228UWW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227JH5","2FSL4 30L EZB LP835 N100","2FSL4 30L EZB LP835 N100 (CI-227JH5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229M6H","2FSL4 30L EZB LP840","2FSL4 30L EZB LP840 (CI-229M6H)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229KTA","2FSL4 30L EZB PWS1836 LP835","2FSL4 30L EZB PWS1836 LP835 (CI-229KTA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229T2Y","2FSL4 30L EZB PWS1836 LP850","2FSL4 30L EZB PWS1836 LP850 (CI-229T2Y)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230AMT","2FSL4 30L SLD LP830","2FSL4 30L SLD LP830 (CI-230AMT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229PK7","2FSL4 30L SLD LP835","2FSL4 30L SLD LP835 (CI-229PK7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226YVC","2FSL4 30L SLD LP840","2FSL4 30L SLD LP840 (CI-226YVC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232WF9","2FSL4 30L SLD PWS1846 LP840","2FSL4 30L SLD PWS1846 LP840 (CI-232WF9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228Y66","2FSL4 40L 120 EZ1 GLR LP840","2FSL4 40L 120 EZ1 GLR LP840 (CI-228Y66)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233WHA","2FSL4 40L 277 EZ1 GLR LP840","2FSL4 40L 277 EZ1 GLR LP840 (CI-233WHA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229ALK","2FSL4 40L 277 EZ1 QFC213GA GLR LP840","2FSL4 40L 277 EZ1 QFC213GA GLR LP840 (CI-229ALK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228N15","2FSL4 40L EDB PWS1836 LP835","2FSL4 40L EDB PWS1836 LP835 (CI-228N15)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229K78","2FSL4 40L EOHN LP840","2FSL4 40L EOHN LP840 (CI-229K78)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227TWR","2FSL4 40L EZ1 LP830","2FSL4 40L EZ1 LP830 (CI-227TWR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231AE9","2FSL4 40L EZ1 LP830 N100","2FSL4 40L EZ1 LP830 N100 (CI-231AE9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229G6M","2FSL4 40L EZ1 LP830 N80","2FSL4 40L EZ1 LP830 N80 (CI-229G6M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["224GR9","2FSL4 40L EZ1 LP835","2FSL4 40L EZ1 LP835 (CI-224GR9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225NFR","2FSL4 40L EZ1 LP835 N100","2FSL4 40L EZ1 LP835 N100 (CI-225NFR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226JRT","2FSL4 40L EZ1 LP835 N80","2FSL4 40L EZ1 LP835 N80 (CI-226JRT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230NHL","2FSL4 40L EZ1 LP835 RFD182090","2FSL4 40L EZ1 LP835 RFD182090 (CI-230NHL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229MYC","2FSL4 40L EZ1 LP835 USPOM","2FSL4 40L EZ1 LP835 USPOM (CI-229MYC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["224NUL","2FSL4 40L EZ1 LP840","2FSL4 40L EZ1 LP840 (CI-224NUL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["224W25","2FSL4 40L EZ1 LP840 N100","2FSL4 40L EZ1 LP840 N100 (CI-224W25)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231G3G","2FSL4 40L EZ1 LP840 N100 USPOM","2FSL4 40L EZ1 LP840 N100 USPOM (CI-231G3G)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225KKF","2FSL4 40L EZ1 LP840 N80","2FSL4 40L EZ1 LP840 N80 (CI-225KKF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227RWT","2FSL4 40L EZ1 LP840 RFD173863","2FSL4 40L EZ1 LP840 RFD173863 (CI-227RWT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229J7C","2FSL4 40L EZ1 LP840 USPOM","2FSL4 40L EZ1 LP840 USPOM (CI-229J7C)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225KFE","2FSL4 40L EZ1 LP850","2FSL4 40L EZ1 LP850 (CI-225KFE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229J2A","2FSL4 40L EZ1 LP850 N100","2FSL4 40L EZ1 LP850 N100 (CI-229J2A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229JTG","2FSL4 40L EZ1 LP850 NA20","2FSL4 40L EZ1 LP850 NA20 (CI-229JTG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227Y3X","2FSL4 40L EZ1 PWS1836 LP830","2FSL4 40L EZ1 PWS1836 LP830 (CI-227Y3X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231J61","2FSL4 40L EZ1 PWS1836 LP830 N100","2FSL4 40L EZ1 PWS1836 LP830 N100 (CI-231J61)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225MFA","2FSL4 40L EZ1 PWS1836 LP835","2FSL4 40L EZ1 PWS1836 LP835 (CI-225MFA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226EN0","2FSL4 40L EZ1 PWS1836 LP835 N100","2FSL4 40L EZ1 PWS1836 LP835 N100 (CI-226EN0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229PJN","2FSL4 40L EZ1 PWS1836 LP835 N100 USPOM","2FSL4 40L EZ1 PWS1836 LP835 N100 USPOM (CI-229PJN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229HGM","2FSL4 40L EZ1 PWS1836 LP835 N80","2FSL4 40L EZ1 PWS1836 LP835 N80 (CI-229HGM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226X4E","2FSL4 40L EZ1 PWS1836 LP840","2FSL4 40L EZ1 PWS1836 LP840 (CI-226X4E)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226EN3","2FSL4 40L EZ1 PWS1836 LP840 N100","2FSL4 40L EZ1 PWS1836 LP840 N100 (CI-226EN3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["224R46","2FSL4 40L EZ1 PWS1836 LP840 N80","2FSL4 40L EZ1 PWS1836 LP840 N80 (CI-224R46)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C1858,7)),6))","v":"230L7M"},{"$f":"LEFT(C1858,SEARCH(\"(CI-\",C1858)-2)","v":"2FSL4 40L EZ1 PWS1836 LP850"},"2FSL4 40L EZ1 PWS1836 LP850 (CI-230L7M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227Y3Y","2FSL4 40L EZ1 PWS1846 LP830","2FSL4 40L EZ1 PWS1846 LP830 (CI-227Y3Y)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225MFR","2FSL4 40L EZ1 PWS1846 LP835","2FSL4 40L EZ1 PWS1846 LP835 (CI-225MFR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232WUT","2FSL4 40L EZ1 PWS1846 LP835 N100","2FSL4 40L EZ1 PWS1846 LP835 N100 (CI-232WUT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225M3E","2FSL4 40L EZ1 PWS1846 LP840","2FSL4 40L EZ1 PWS1846 LP840 (CI-225M3E)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232EJR","2FSL4 40L EZ1 PWS1856LV LP835","2FSL4 40L EZ1 PWS1856LV LP835 (CI-232EJR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233X5N","2FSL4 40L EZ1 PWS1856LV LP840","2FSL4 40L EZ1 PWS1856LV LP840 (CI-233X5N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234C9U","2FSL4 40L EZ1 RRLA LP840","2FSL4 40L EZ1 RRLA LP840 (CI-234C9U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233Y4J","2FSL4 40L EZB LP830","2FSL4 40L EZB LP830 (CI-233Y4J)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231UJM","2FSL4 40L EZB LP835","2FSL4 40L EZB LP835 (CI-231UJM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227JKU","2FSL4 40L EZB LP835 N100","2FSL4 40L EZB LP835 N100 (CI-227JKU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229CGA","2FSL4 40L EZB LP835 N80","2FSL4 40L EZB LP835 N80 (CI-229CGA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231YH5","2FSL4 40L EZB LP840","2FSL4 40L EZB LP840 (CI-231YH5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231K5N","2FSL4 40L EZB LP840 N80","2FSL4 40L EZB LP840 N80 (CI-231K5N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229VGJ","2FSL4 40L EZB PWS1836 LP850","2FSL4 40L EZB PWS1836 LP850 (CI-229VGJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232CYA","2FSL4 40L SLD LP830","2FSL4 40L SLD LP830 (CI-232CYA)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["226MWR","2FSL4 40L SLD LP835","2FSL4 40L SLD LP835 (CI-226MWR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226PL1","2FSL4 40L SLD LP840","2FSL4 40L SLD LP840 (CI-226PL1)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MR9"]
["233XHA","2FSL4 40L SLD LP840 USPOM","2FSL4 40L SLD LP840 USPOM (CI-233XHA)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["227G71","2FSL4 40L SLD LP850","2FSL4 40L SLD LP850 (CI-227G71)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["228WYM","2FSL4 40L SLD PWS1846 LP835","2FSL4 40L SLD PWS1846 LP835 (CI-228WYM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232J3A","2FSL4 40L SLD PWS1846 LP840","2FSL4 40L SLD PWS1846 LP840 (CI-232J3A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230UYF","2FSL4 48L 120 EZ1 GLR PWS1836 LP840","2FSL4 48L 120 EZ1 GLR PWS1836 LP840 (CI-230UYF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230EK8","2FSL4 48L 120 EZ1 QFC211GA LP835","2FSL4 48L 120 EZ1 QFC211GA LP835 (CI-230EK8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231YGM","2FSL4 48L 277 EZ1 GLR LP840","2FSL4 48L 277 EZ1 GLR LP840 (CI-231YGM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233VNX","2FSL4 48L CONFIG L/D LP840 RFD176024","2FSL4 48L CONFIG L/D LP840 RFD176024 (CI-233VNX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234J7H","2FSL4 48L EDB LP840","2FSL4 48L EDB LP840 (CI-234J7H)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226GPY","2FSL4 48L EZ1 LP830","2FSL4 48L EZ1 LP830 (CI-226GPY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228E03","2FSL4 48L EZ1 LP830 N100","2FSL4 48L EZ1 LP830 N100 (CI-228E03)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["224P21","2FSL4 48L EZ1 LP835","2FSL4 48L EZ1 LP835 (CI-224P21)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225JX5","2FSL4 48L EZ1 LP835 N100","2FSL4 48L EZ1 LP835 N100 (CI-225JX5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226WNJ","2FSL4 48L EZ1 LP835 N80","2FSL4 48L EZ1 LP835 N80 (CI-226WNJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228NVR","2FSL4 48L EZ1 LP835 USPOM","2FSL4 48L EZ1 LP835 USPOM (CI-228NVR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["224P25","2FSL4 48L EZ1 LP840","2FSL4 48L EZ1 LP840 (CI-224P25)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225TGX","2FSL4 48L EZ1 LP840 N100","2FSL4 48L EZ1 LP840 N100 (CI-225TGX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226F8M","2FSL4 48L EZ1 LP840 N80","2FSL4 48L EZ1 LP840 N80 (CI-226F8M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226GWK","2FSL4 48L EZ1 LP850","2FSL4 48L EZ1 LP850 (CI-226GWK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228A2T","2FSL4 48L EZ1 LP850 N80","2FSL4 48L EZ1 LP850 N80 (CI-228A2T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226TP7","2FSL4 48L EZ1 PWS1836 LP830","2FSL4 48L EZ1 PWS1836 LP830 (CI-226TP7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225W9M","2FSL4 48L EZ1 PWS1836 LP835","2FSL4 48L EZ1 PWS1836 LP835 (CI-225W9M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230KY6","2FSL4 48L EZ1 PWS1836 LP835 N100","2FSL4 48L EZ1 PWS1836 LP835 N100 (CI-230KY6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229HH0","2FSL4 48L EZ1 PWS1836 LP835 N80","2FSL4 48L EZ1 PWS1836 LP835 N80 (CI-229HH0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228M0L","2FSL4 48L EZ1 PWS1836 LP840","2FSL4 48L EZ1 PWS1836 LP840 (CI-228M0L)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231WFR","2FSL4 48L EZ1 PWS1836 LP840 N100","2FSL4 48L EZ1 PWS1836 LP840 N100 (CI-231WFR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229R96","2FSL4 48L EZ1 PWS1836 LP840 N80","2FSL4 48L EZ1 PWS1836 LP840 N80 (CI-229R96)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231LN8","2FSL4 48L EZ1 PWS1836 LP850","2FSL4 48L EZ1 PWS1836 LP850 (CI-231LN8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226WNW","2FSL4 48L EZ1 PWS1846 LP840","2FSL4 48L EZ1 PWS1846 LP840 (CI-226WNW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230E8F","2FSL4 48L EZ1 PWS1856LV LP835","2FSL4 48L EZ1 PWS1856LV LP835 (CI-230E8F)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229GM8","2FSL4 48L EZ1 PWS1856LV LP835 SW14 RFD178398","2FSL4 48L EZ1 PWS1856LV LP835 SW14 RFD178398 (CI-229GM8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230E8K","2FSL4 48L EZ1 PWS1856LV LP840","2FSL4 48L EZ1 PWS1856LV LP840 (CI-230E8K)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232F66","2FSL4 48L EZ1 RRLC12S LP840","2FSL4 48L EZ1 RRLC12S LP840 (CI-232F66)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227P7L","2FSL4 48L EZB LP830","2FSL4 48L EZB LP830 (CI-227P7L)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232TJL","2FSL4 48L EZB LP835","2FSL4 48L EZB LP835 (CI-232TJL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231PH8","2FSL4 48L EZB LP835 N100","2FSL4 48L EZB LP835 N100 (CI-231PH8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229GCA","2FSL4 48L EZB LP835 N80","2FSL4 48L EZB LP835 N80 (CI-229GCA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232K0M","2FSL4 48L EZB LP840","2FSL4 48L EZB LP840 (CI-232K0M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229AW4","2FSL4 48L EZB LP850 N80","2FSL4 48L EZB LP850 N80 (CI-229AW4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229N48","2FSL4 48L EZB PWS1836 LP835","2FSL4 48L EZB PWS1836 LP835 (CI-229N48)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233F9W","2FSL4 48L EZB PWS1836 LP840","2FSL4 48L EZB PWS1836 LP840 (CI-233F9W)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234ECR","2FSL4 48L L/D LP835 RFD191309","2FSL4 48L L/D LP835 RFD191309 (CI-234ECR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233J5R","2FSL4 48L L/D LP840 RFD176024","2FSL4 48L L/D LP840 RFD176024 (CI-233J5R)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230AM4","2FSL4 48L SLD LP830","2FSL4 48L SLD LP830 (CI-230AM4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226THJ","2FSL4 48L SLD LP835","2FSL4 48L SLD LP835 (CI-226THJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227CRE","2FSL4 48L SLD LP840","2FSL4 48L SLD LP840 (CI-227CRE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C1922,7)),6))","v":"229PK3"},{"$f":"LEFT(C1922,SEARCH(\"(CI-\",C1922)-2)","v":"2FSL4 48L SLD LP850"},"2FSL4 48L SLD LP850 (CI-229PK3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226GE5","2FSL4 48L SLD PWS1846 LP835","2FSL4 48L SLD PWS1846 LP835 (CI-226GE5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228ERR","2FSL4 60L EDB LP835","2FSL4 60L EDB LP835 (CI-228ERR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227MU4","2FSL4 60L EZ1 LP830","2FSL4 60L EZ1 LP830 (CI-227MU4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233X0T","2FSL4 60L EZ1 LP830 CP","2FSL4 60L EZ1 LP830 CP (CI-233X0T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228W8X","2FSL4 60L EZ1 LP830 N100","2FSL4 60L EZ1 LP830 N100 (CI-228W8X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232EEP","2FSL4 60L EZ1 LP830 N80","2FSL4 60L EZ1 LP830 N80 (CI-232EEP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225KJV","2FSL4 60L EZ1 LP835","2FSL4 60L EZ1 LP835 (CI-225KJV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228RJV","2FSL4 60L EZ1 LP835 N100","2FSL4 60L EZ1 LP835 N100 (CI-228RJV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227GMM","2FSL4 60L EZ1 LP835 N80","2FSL4 60L EZ1 LP835 N80 (CI-227GMM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225X72","2FSL4 60L EZ1 LP840","2FSL4 60L EZ1 LP840 (CI-225X72)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227GML","2FSL4 60L EZ1 LP840 N100","2FSL4 60L EZ1 LP840 N100 (CI-227GML)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229T29","2FSL4 60L EZ1 LP840 N80","2FSL4 60L EZ1 LP840 N80 (CI-229T29)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225KH6","2FSL4 60L EZ1 LP850","2FSL4 60L EZ1 LP850 (CI-225KH6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228MYH","2FSL4 60L EZ1 LP850 N100","2FSL4 60L EZ1 LP850 N100 (CI-228MYH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227CMR","2FSL4 60L EZ1 PWS1836 LP830","2FSL4 60L EZ1 PWS1836 LP830 (CI-227CMR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227CMG","2FSL4 60L EZ1 PWS1836 LP830 N100","2FSL4 60L EZ1 PWS1836 LP830 N100 (CI-227CMG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228GU5","2FSL4 60L EZ1 PWS1836 LP835","2FSL4 60L EZ1 PWS1836 LP835 (CI-228GU5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233JAX","2FSL4 60L EZ1 PWS1836 LP835 N80","2FSL4 60L EZ1 PWS1836 LP835 N80 (CI-233JAX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226Y4J","2FSL4 60L EZ1 PWS1836 LP840","2FSL4 60L EZ1 PWS1836 LP840 (CI-226Y4J)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230YVM","2FSL4 60L EZ1 PWS1836 LP840 N100","2FSL4 60L EZ1 PWS1836 LP840 N100 (CI-230YVM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226WP1","2FSL4 60L EZ1 PWS1846 LP840","2FSL4 60L EZ1 PWS1846 LP840 (CI-226WP1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230LY0","2FSL4 60L EZ1 PWS1856LV LP835","2FSL4 60L EZ1 PWS1856LV LP835 (CI-230LY0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230GR4","2FSL4 60L EZB LP830","2FSL4 60L EZB LP830 (CI-230GR4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229W6H","2FSL4 60L EZB LP835","2FSL4 60L EZB LP835 (CI-229W6H)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226KY9","2FSL4 60L EZB LP835 N100","2FSL4 60L EZB LP835 N100 (CI-226KY9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226L21","2FSL4 60L EZB LP835 N80","2FSL4 60L EZB LP835 N80 (CI-226L21)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227VP1","2FSL4 60L EZB LP840","2FSL4 60L EZB LP840 (CI-227VP1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231FGH","2FSL4 60L SLD LP830","2FSL4 60L SLD LP830 (CI-231FGH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226U3P","2FSL4 60L SLD LP835","2FSL4 60L SLD LP835 (CI-226U3P)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226CNY","2FSL4 60L SLD LP840","2FSL4 60L SLD LP840 (CI-226CNY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230UJU","2FSL4 60L SLD LP850","2FSL4 60L SLD LP850 (CI-230UJU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234MTF","2FSL4 60L SLD PWS1846 LP835","2FSL4 60L SLD PWS1846 LP835 (CI-234MTF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226Y6P","2FSL4 60L SLD PWS1846 LP840","2FSL4 60L SLD PWS1846 LP840 (CI-226Y6P)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230CJX","2FSL4 72L EXB LP830","2FSL4 72L EXB LP830 (CI-230CJX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228CTG","2FSL4 72L EXB LP835","2FSL4 72L EXB LP835 (CI-228CTG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227WUL","2FSL4 72L EZ1 LP830","2FSL4 72L EZ1 LP830 (CI-227WUL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231L98","2FSL4 72L EZ1 LP830 N100","2FSL4 72L EZ1 LP830 N100 (CI-231L98)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234Y2W","2FSL4 72L EZ1 LP830 N80","2FSL4 72L EZ1 LP830 N80 (CI-234Y2W)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225X0V","2FSL4 72L EZ1 LP835","2FSL4 72L EZ1 LP835 (CI-225X0V)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228FWT","2FSL4 72L EZ1 LP835 N100","2FSL4 72L EZ1 LP835 N100 (CI-228FWT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227JMH","2FSL4 72L EZ1 LP835 N80","2FSL4 72L EZ1 LP835 N80 (CI-227JMH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225TC0","2FSL4 72L EZ1 LP840","2FSL4 72L EZ1 LP840 (CI-225TC0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227CMY","2FSL4 72L EZ1 LP840 N100","2FSL4 72L EZ1 LP840 N100 (CI-227CMY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229AC6","2FSL4 72L EZ1 LP840 N80","2FSL4 72L EZ1 LP840 N80 (CI-229AC6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234G7A","2FSL4 72L EZ1 LP840 USPOM","2FSL4 72L EZ1 LP840 USPOM (CI-234G7A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226L6L","2FSL4 72L EZ1 LP850","2FSL4 72L EZ1 LP850 (CI-226L6L)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228VTX","2FSL4 72L EZ1 LP850 N100","2FSL4 72L EZ1 LP850 N100 (CI-228VTX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228A3A","2FSL4 72L EZ1 LP850 N80","2FSL4 72L EZ1 LP850 N80 (CI-228A3A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227YGF","2FSL4 72L EZ1 PWS1836 LP830","2FSL4 72L EZ1 PWS1836 LP830 (CI-227YGF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229GCR","2FSL4 72L EZ1 PWS1836 LP835","2FSL4 72L EZ1 PWS1836 LP835 (CI-229GCR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232WUN","2FSL4 72L EZ1 PWS1836 LP835 N100","2FSL4 72L EZ1 PWS1836 LP835 N100 (CI-232WUN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233JCP","2FSL4 72L EZ1 PWS1836 LP835 N80","2FSL4 72L EZ1 PWS1836 LP835 N80 (CI-233JCP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228PVG","2FSL4 72L EZ1 PWS1836 LP840","2FSL4 72L EZ1 PWS1836 LP840 (CI-228PVG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229JX1","2FSL4 72L EZ1 PWS1836 LP840 N100","2FSL4 72L EZ1 PWS1836 LP840 N100 (CI-229JX1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228Y5N","2FSL4 72L EZ1 PWS1846 LP840 N80","2FSL4 72L EZ1 PWS1846 LP840 N80 (CI-228Y5N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230MGW","2FSL4 72L EZ1 PWS1856LV LP835","2FSL4 72L EZ1 PWS1856LV LP835 (CI-230MGW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232WF7","2FSL4 72L EZ1 PWS1856LV LP840","2FSL4 72L EZ1 PWS1856LV LP840 (CI-232WF7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230GR0","2FSL4 72L EZB LP830","2FSL4 72L EZB LP830 (CI-230GR0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230FEH","2FSL4 72L EZB LP835","2FSL4 72L EZB LP835 (CI-230FEH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232PU1","2FSL4 72L EZB LP840","2FSL4 72L EZB LP840 (CI-232PU1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228FFN","2FSL4 72L SLD LP835","2FSL4 72L SLD LP835 (CI-228FFN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226PKL","2FSL4 72L SLD LP840","2FSL4 72L SLD LP840 (CI-226PKL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230UHW","2FSL4 72L SLD LP850","2FSL4 72L SLD LP850 (CI-230UHW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C1986,7)),6))","v":"229Y99"},{"$f":"LEFT(C1986,SEARCH(\"(CI-\",C1986)-2)","v":"2FSL4 72L SLD PWS1846 LP835"},"2FSL4 72L SLD PWS1846 LP835 (CI-229Y99)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234KA1","2FSL4 72L SLD PWS1846 LP850","2FSL4 72L SLD PWS1846 LP850 (CI-234KA1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234TEF","2FSL4 CTRF 40L EZ1 LP840 RFD196040","2FSL4 CTRF 40L EZ1 LP840 RFD196040 (CI-234TEF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228XHR","2FSL4 H 30L EZ1 LP830","2FSL4 H 30L EZ1 LP830 (CI-228XHR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227XKX","2FSL4 H 30L EZ1 LP835","2FSL4 H 30L EZ1 LP835 (CI-227XKX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234JJV","2FSL4 H 30L EZ1 LP835 N100","2FSL4 H 30L EZ1 LP835 N100 (CI-234JJV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228UG0","2FSL4 H 30L EZ1 LP840","2FSL4 H 30L EZ1 LP840 (CI-228UG0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227JAT","2FSL4 H 40L EZ1 LP835","2FSL4 H 40L EZ1 LP835 (CI-227JAT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234JJL","2FSL4 H 40L EZ1 LP835 N100","2FSL4 H 40L EZ1 LP835 N100 (CI-234JJL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234JWM","2FSL4 H 40L EZ1 LP835 N80","2FSL4 H 40L EZ1 LP835 N80 (CI-234JWM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228UAG","2FSL4 H 40L EZ1 LP840","2FSL4 H 40L EZ1 LP840 (CI-228UAG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233FG5","2FSL4 H 40L EZ1 PWS1836 LP835","2FSL4 H 40L EZ1 PWS1836 LP835 (CI-233FG5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227RHE","2FSL4 H 48L EZ1 LP835","2FSL4 H 48L EZ1 LP835 (CI-227RHE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230W11","2FSL4 H 48L EZ1 LP835 N100","2FSL4 H 48L EZ1 LP835 N100 (CI-230W11)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232WJ9","2FSL4 H 48L EZ1 LP840","2FSL4 H 48L EZ1 LP840 (CI-232WJ9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237TUP","2FSL2 20L EZ1 LP830 N100","2FSL2 20L EZ1 LP830 N100 (CI-237TUP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230MJP","2FSL2 33L EZ1 LP835 N80EMG","2FSL2 33L EZ1 LP835 N80EMG (CI-230MJP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235HHR","2FSL2 33L EZB LP835 N80EMG","2FSL2 33L EZB LP835 N80EMG (CI-235HHR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235YNY","2FSL2 40L EZ1 PWS1836 LP835 USPOM","2FSL2 40L EZ1 PWS1836 LP835 USPOM (CI-235YNY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["239W60","2FSL2 H 33L EZ1 LP830 N100","2FSL2 H 33L EZ1 LP830 N100 (CI-239W60)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["238JLY","2FSL4 30L 277 EZ1 GLR PWS1856LV LP835","2FSL4 30L 277 EZ1 GLR PWS1856LV LP835 (CI-238JLY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236M6F","2FSL4 30L EZ1 PWS1856LV LP830","2FSL4 30L EZ1 PWS1856LV LP830 (CI-236M6F)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240JPK","2FSL4 40L EZ1 LP835 N100 USPOM","2FSL4 40L EZ1 LP835 N100 USPOM (CI-240JPK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236PWW","2FSL4 40L EZB PWS1836 LP835 N80","2FSL4 40L EZB PWS1836 LP835 N80 (CI-236PWW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232E93","2FSL4 48L EZ1 RRLA LP840","2FSL4 48L EZ1 RRLA LP840 (CI-232E93)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236FT7","2FSL4 60L EZ1 PWS1836 LP835 N100","2FSL4 60L EZ1 PWS1836 LP835 N100 (CI-236FT7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236YA7","2FSL4 72L EZ1 LP840 N80EMG","2FSL4 72L EZ1 LP840 N80EMG (CI-236YA7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236WNN","2FSL4 72L EZB LP840 N100","2FSL4 72L EZB LP840 N100 (CI-236WNN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235NJ3","2FSL4 H 48L EZ1 LP840 N100","2FSL4 H 48L EZ1 LP840 N100 (CI-235NJ3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229GT6","2GTL 2 20L A19 LP840 NX","2GTL 2 20L A19 LP840 NX (CI-229GT6)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["231U3Y","2GTL 2 20L EZ1 LP840 N80","2GTL 2 20L EZ1 LP840 N80 (CI-231U3Y)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228J4G","2GTL 2 20L FW PWS1836 LP840 NX","2GTL 2 20L FW PWS1836 LP840 NX (CI-228J4G)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["228E81","2GTL 2 20L PWS1836 LP840 PAF NX","2GTL 2 20L PWS1836 LP840 PAF NX (CI-228E81)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["233AHU","2GTL 2 20L SWL EZ1 PWS1836 LP840","2GTL 2 20L SWL EZ1 PWS1836 LP840 (CI-233AHU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234PG3","2GTL 2 33L A19 EZ1 LP840 USPOM","2GTL 2 33L A19 EZ1 LP840 USPOM (CI-234PG3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["223Y52","2GTL 2 33L A19 LP835 NX","2GTL 2 33L A19 LP835 NX (CI-223Y52)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234W4F","2GTL 2 33L EZ1 LP840 LATC","2GTL 2 33L EZ1 LP840 LATC (CI-234W4F)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233NAY","2GTL 2 33L EZ1 PWS1836 LP835 N100","2GTL 2 33L EZ1 PWS1836 LP835 N100 (CI-233NAY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234JRH","2GTL 2 33L FW 120 EZ1 GMF ABC LP835","2GTL 2 33L FW 120 EZ1 GMF ABC LP835 (CI-234JRH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225K2N","2GTL 2 33L FW A19 LP840 LATC NX","2GTL 2 33L FW A19 LP840 LATC NX (CI-225K2N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227CU5","2GTL 2 33L FW LP830 NX","2GTL 2 33L FW LP830 NX (CI-227CU5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229GJW","2GTL 2 33L FW PWS1836 LP835 NX","2GTL 2 33L FW PWS1836 LP835 NX (CI-229GJW)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["232L90","2GTL 2 33L FW SWL EZ1 LP835","2GTL 2 33L FW SWL EZ1 LP835 (CI-232L90)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227JCE","2GTL 2 33L LP840 LATC BLD","2GTL 2 33L LP840 LATC BLD (CI-227JCE)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["231PFM","2GTL 2 33L RW A19 EZ1 LP835","2GTL 2 33L RW A19 EZ1 LP835 (CI-231PFM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["223JN1","2GTL 2 33L RW LP835 NX","2GTL 2 33L RW LP835 NX (CI-223JN1)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["232JHE","2GTL 2 33L SWL 120 EZ1 GLR LP835 CP","2GTL 2 33L SWL 120 EZ1 GLR LP835 CP (CI-232JHE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["223NNV","2GTL 2 33L SWL LP840 NX","2GTL 2 33L SWL LP840 NX (CI-223NNV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228PWR","2GTL 2 37L FW ABC LP830 N80","2GTL 2 37L FW ABC LP830 N80 (CI-228PWR)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["225JU6","2GTL 2 37L FW SWL LP840 NX","2GTL 2 37L FW SWL LP840 NX (CI-225JU6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229EX9","2GTL 2 37L PWS1836 LP835 N80","2GTL 2 37L PWS1836 LP835 N80 (CI-229EX9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228VVJ","2GTL 2 37L SWL PWS1836 LP835 NX","2GTL 2 37L SWL PWS1836 LP835 NX (CI-228VVJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231LFX","2GTL 2 40L A19 SLD LP840 PAF","2GTL 2 40L A19 SLD LP840 PAF (CI-231LFX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232J83","2GTL 2 40L EZ1 LP835 USPOM","2GTL 2 40L EZ1 LP835 USPOM (CI-232J83)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230RW4","2GTL 2 40L EZ1 PWS1836 LP835","2GTL 2 40L EZ1 PWS1836 LP835 (CI-230RW4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230HRU","2GTL 2 40L FW A19 EZ1 ABC LP840","2GTL 2 40L FW A19 EZ1 ABC LP840 (CI-230HRU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231WTV","2GTL 2 40L RW EZ1 ABC LP840","2GTL 2 40L RW EZ1 ABC LP840 (CI-231WTV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230H26","2GTL 2 40L SWL EZ1 LP835","2GTL 2 40L SWL EZ1 LP835 (CI-230H26)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229EK2","2GTL 2 F 20L LP840 N100","2GTL 2 F 20L LP840 N100 (CI-229EK2)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["230JUH","2GTL 2 F 33L EZ1 LP840","2GTL 2 F 33L EZ1 LP840 (CI-230JUH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["224TJ2","2GTL 2 F 33L SWL LP840 NX","2GTL 2 F 33L SWL LP840 NX (CI-224TJ2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225V76","2GTL 2 F 37L LP840 NX","2GTL 2 F 37L LP840 NX (CI-225V76)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["233G70","2GTL 2 F 40L EZ1 LP850","2GTL 2 F 40L EZ1 LP850 (CI-233G70)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230LR3","2GTL 4 30L A19 EZ1 LP835","2GTL 4 30L A19 EZ1 LP835 (CI-230LR3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231U3U","2GTL 4 30L EZ1 LP840 N80","2GTL 4 30L EZ1 LP840 N80 (CI-231U3U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232TVL","2GTL 4 30L FW EZ1 LP840 N100","2GTL 4 30L FW EZ1 LP840 N100 (CI-232TVL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228M49","2GTL 4 30L LP835 NX USPOM","2GTL 4 30L LP835 NX USPOM (CI-228M49)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231JE8","2GTL 4 30L RW A19 EZ1 LP840","2GTL 4 30L RW A19 EZ1 LP840 (CI-231JE8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230A2R","2GTL 4 30L SWL EZ1 LP840","2GTL 4 30L SWL EZ1 LP840 (CI-230A2R)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232M48","2GTL 4 40L 277 EZ1 GLR LP835","2GTL 4 40L 277 EZ1 GLR LP835 (CI-232M48)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225X6W","2GTL 4 40L A19 277 GLR PWS1836 LP840 LATC NX","2GTL 4 40L A19 277 GLR PWS1836 LP840 LATC NX (CI-225X6W)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234R9X","2GTL 4 40L A19 EZ1 LP840 PAF","2GTL 4 40L A19 EZ1 LP840 PAF (CI-234R9X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233W3X","2GTL 4 40L EZ1 LP835 LATC","2GTL 4 40L EZ1 LP835 LATC (CI-233W3X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229XPV","2GTL 4 40L EZ1 LP850","2GTL 4 40L EZ1 LP850 (CI-229XPV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231T1P","2GTL 4 40L EZ1 PWS1836 LP835 PAF","2GTL 4 40L EZ1 PWS1836 LP835 PAF (CI-231T1P)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234N32","2GTL 4 40L EZ1 PWS1856LV LP840","2GTL 4 40L EZ1 PWS1856LV LP840 (CI-234N32)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234TF8","2GTL 4 40L FW A19 EZ1 LP840","2GTL 4 40L FW A19 EZ1 LP840 (CI-234TF8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232P6M","2GTL 4 40L FW EZ1 ABC LP840 N100","2GTL 4 40L FW EZ1 ABC LP840 N100 (CI-232P6M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229T5K","2GTL 4 40L FW LP840 PAF NX","2GTL 4 40L FW LP840 PAF NX (CI-229T5K)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225WF9","2GTL 4 40L LP835 N80","2GTL 4 40L LP835 N80 (CI-225WF9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233HNT","2GTL 4 40L RW 277 EZ1 GLR LP840","2GTL 4 40L RW 277 EZ1 GLR LP840 (CI-233HNT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233AJV","2GTL 4 40L RW EZ1 PWS1836 ABC LP835 PAF","2GTL 4 40L RW EZ1 PWS1836 ABC LP835 PAF (CI-233AJV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230E66","2GTL 4 40L SLD LP835","2GTL 4 40L SLD LP835 (CI-230E66)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230ECH","2GTL 4 40L SWL EZ1 LP840","2GTL 4 40L SWL EZ1 LP840 (CI-230ECH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["224P1W","2GTL 4 48L 120 GLR LP840 NX","2GTL 4 48L 120 GLR LP840 NX (CI-224P1W)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230MCL","2GTL 4 48L A12V EZ1 LP835 RFD172297","2GTL 4 48L A12V EZ1 LP835 RFD172297 (CI-230MCL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228MJA","2GTL 4 48L A19 LP835 N80","2GTL 4 48L A19 LP835 N80 (CI-228MJA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229UN1","2GTL 4 48L EZ1 LP835","2GTL 4 48L EZ1 LP835 (CI-229UN1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234E36","2GTL 4 48L EZ1 PWS1836 LP850","2GTL 4 48L EZ1 PWS1836 LP850 (CI-234E36)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234JUP","2GTL 4 48L FW A12125V EZ1 ABC LP850","2GTL 4 48L FW A12125V EZ1 ABC LP850 (CI-234JUP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231K4T","2GTL 4 48L FW A19 EZ1 LP835","2GTL 4 48L FW A19 EZ1 LP835 (CI-231K4T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228L19","2GTL 4 48L FW ABC LP835 PAF NX","2GTL 4 48L FW ABC LP835 PAF NX (CI-228L19)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234HUW","2GTL 4 48L FW EZ1 LP835 N80","2GTL 4 48L FW EZ1 LP835 N80 (CI-234HUW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234L90","2GTL 4 48L FW K12 EZ1 LP840 RFD189436","2GTL 4 48L FW K12 EZ1 LP840 RFD189436 (CI-234L90)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234U3T","2GTL 4 48L FW SWL EZ1 PWS1836 ABC LP835","2GTL 4 48L FW SWL EZ1 PWS1836 ABC LP835 (CI-234U3T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["222FYK","2GTL 4 48L LP835 NX","2GTL 4 48L LP835 NX (CI-222FYK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230YHY","2GTL 4 48L RN EZ1 LP840 N80","2GTL 4 48L RN EZ1 LP840 N80 (CI-230YHY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230C8J","2GTL 4 48L RW EZ1 LP840","2GTL 4 48L RW EZ1 LP840 (CI-230C8J)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232VUU","2GTL 4 48L RW EZ1 LP840 PAF N100","2GTL 4 48L RW EZ1 LP840 PAF N100 (CI-232VUU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230AVW","2GTL 4 48L SWL EZ1 LP840","2GTL 4 48L SWL EZ1 LP840 (CI-230AVW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["222T9G","2GTL 4 48L SWL LP840 NX","2GTL 4 48L SWL LP840 NX (CI-222T9G)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234UHK","2GTL 4 60L 277 EZ1 GMF LP835 N100","2GTL 4 60L 277 EZ1 GMF LP835 N100 (CI-234UHK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230NNJ","2GTL 4 60L A19 EZ1 LP840 JP18 RFD181785","2GTL 4 60L A19 EZ1 LP840 JP18 RFD181785 (CI-230NNJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225N8J","2GTL 4 60L A19 LP840 N80","2GTL 4 60L A19 LP840 N80 (CI-225N8J)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230AM6","2GTL 4 60L EZ1 LP850","2GTL 4 60L EZ1 LP850 (CI-230AM6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232WJA","2GTL 4 60L FN EZ1 LP835","2GTL 4 60L FN EZ1 LP835 (CI-232WJA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231U9C","2GTL 4 60L FW A19 EZ1 LP835","2GTL 4 60L FW A19 EZ1 LP835 (CI-231U9C)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233VGP","2GTL 4 60L FW EZ1 K20V ABC LP840 RFD191408","2GTL 4 60L FW EZ1 K20V ABC LP840 RFD191408 (CI-233VGP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["224VFJ","2GTL 4 60L FW LP840 ABC NX","2GTL 4 60L FW LP840 ABC NX (CI-224VFJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233JXN","2GTL 4 60L FW SLD PWS1846 ABC LP840","2GTL 4 60L FW SLD PWS1846 ABC LP840 (CI-233JXN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["222FAU","2GTL 4 60L LP835 NX RFD153314","2GTL 4 60L LP835 NX RFD153314 (CI-222FAU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227E5A","2GTL 4 60L LP850 N100","2GTL 4 60L LP850 N100 (CI-227E5A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226R6A","2GTL 4 60L RW A19 LP840 PAF NX","2GTL 4 60L RW A19 LP840 PAF NX (CI-226R6A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233C0A","2GTL 4 60L SWL EZ1 LP850","2GTL 4 60L SWL EZ1 LP850 (CI-233C0A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231FV2","2GTL 4 72L 277 EZ1 GLR LP840","2GTL 4 72L 277 EZ1 GLR LP840 (CI-231FV2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230RF8","2GTL 4 72L A19 EZ1 LP850 N100","2GTL 4 72L A19 EZ1 LP850 N100 (CI-230RF8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225PFT","2GTL 4 72L A19 LP850 N80","2GTL 4 72L A19 LP850 N80 (CI-225PFT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233EVY","2GTL 4 72L EZ1 LP835 DWAM","2GTL 4 72L EZ1 LP835 DWAM (CI-233EVY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230A3J","2GTL 4 72L EZ1 LP850","2GTL 4 72L EZ1 LP850 (CI-230A3J)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231FCK","2GTL 4 72L EZ1 PWS1836 LP850","2GTL 4 72L EZ1 PWS1836 LP850 (CI-231FCK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225ERX","2GTL 4 72L FW A19 ABC LP835 NX","2GTL 4 72L FW A19 ABC LP835 NX (CI-225ERX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233FHX","2GTL 4 72L FW EZ1 ABC LP850","2GTL 4 72L FW EZ1 ABC LP850 (CI-233FHX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225X6K","2GTL 4 72L FW LP835 NX","2GTL 4 72L FW LP835 NX (CI-225X6K)","PS1030","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MR9"]
["222EJJ","2GTL 4 72L LP835 NX","2GTL 4 72L LP835 NX (CI-222EJJ)","PS1030","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MR9"]
["222EY6","2GTL 4 72L LP850 NX","2GTL 4 72L LP850 NX (CI-222EY6)","PS1030","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MR9"]
["231PF7","2GTL 4 72L RW EZ1 LP835","2GTL 4 72L RW EZ1 LP835 (CI-231PF7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230T5P","2GTL 4 72L SLD LP835 PAF","2GTL 4 72L SLD LP835 PAF (CI-230T5P)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232W1X","2GTL 4 72L SWL EZ1 PWS1846 LP835 N100","2GTL 4 72L SWL EZ1 PWS1846 LP835 N100 (CI-232W1X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230NL1","2GTL 4 F 40L A19 EZ1 LP840","2GTL 4 F 40L A19 EZ1 LP840 (CI-230NL1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231PFK","2GTL 4 F 40L RW A19 EZ1 LP835","2GTL 4 F 40L RW A19 EZ1 LP835 (CI-231PFK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229Y54","2GTL 4 F 48L EZ1 LP835","2GTL 4 F 48L EZ1 LP835 (CI-229Y54)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231LMA","2GTL 4 F 48L SLD LP835","2GTL 4 F 48L SLD LP835 (CI-231LMA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225HFJ","2GTL 4 F 60L FW A19V ABC LP835 BLD","2GTL 4 F 60L FW A19V ABC LP835 BLD (CI-225HFJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229VVU","2GTL 4 F 60L RW A19 LP840 NX","2GTL 4 F 60L RW A19 LP840 NX (CI-229VVU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228MMK","2GTL 4 F 72L FW LP840 PAF NX","2GTL 4 F 72L FW LP840 PAF NX (CI-228MMK)","PS1030","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MR9"]
["228UAY","2GTL F 2 20L LP835 NX","2GTL F 2 20L LP835 NX (CI-228UAY)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["217NXV","2GTL2","2GTL2 (CI-217NXV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["224ULW","2GTL4 EZ1 LP840 RFD165301","2GTL4 EZ1 LP840 RFD165301 (CI-224ULW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230CW3","2GTL4 PLT","2GTL4 PLT (CI-230CW3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233WUP","2GTL4R 40L EZ1 LP835 J4","2GTL4R 40L EZ1 LP835 J4 (CI-233WUP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227YFT","2GTL4R 48L GOHN LP840 NAWL","2GTL4R 48L GOHN LP840 NAWL (CI-227YFT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232C3U","GTL 4 20L EZ1 LP850","GTL 4 20L EZ1 LP850 (CI-232C3U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233PF1","GTL 4 33L EZ1 LP850","GTL 4 33L EZ1 LP850 (CI-233PF1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233VFF","GTL 4 33L FW EZ1 LP840 PAF","GTL 4 33L FW EZ1 LP840 PAF (CI-233VFF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232TPE","GTL 4 40L EZ1 LP835 N100","GTL 4 40L EZ1 LP835 N100 (CI-232TPE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232RCG","GTL 4 40L SWL EZ1 LP835 N100","GTL 4 40L SWL EZ1 LP835 N100 (CI-232RCG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232JVG","GTL 4 40L SWL EZ1 LP840","GTL 4 40L SWL EZ1 LP840 (CI-232JVG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233WVT","GTL 4 48L SWL EZ1 PWS1436 LP840","GTL 4 48L SWL EZ1 PWS1436 LP840 (CI-233WVT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231K37","GTL F 4 33L EZ1 LP835 N100","GTL F 4 33L EZ1 LP835 N100 (CI-231K37)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232RC3","GTL F 4 40L A19 EZ1 LP835","GTL F 4 40L A19 EZ1 LP835 (CI-232RC3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231EGF","GTL F 4 40L SWL EZ1 LP840","GTL F 4 40L SWL EZ1 LP840 (CI-231EGF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232HHV","GTL F 4 48L RW EZ1 LP830","GTL F 4 48L RW EZ1 LP830 (CI-232HHV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234AE3","GTL4R 30L EZ1 LP835","GTL4R 30L EZ1 LP835 (CI-234AE3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240NK7","2GTL 2 20L EZ1 LP840 N100 MMC JP34","2GTL 2 20L EZ1 LP840 N100 MMC JP34 (CI-240NK7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240XC1","2GTL 2 20L EZ1 LP850 N100","2GTL 2 20L EZ1 LP850 N100 (CI-240XC1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240KJT","2GTL 2 20L FW EZ1 PWS1836 LP830","2GTL 2 20L FW EZ1 PWS1836 LP830 (CI-240KJT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240LH1","2GTL 2 20L RW EZ1 LP835","2GTL 2 20L RW EZ1 LP835 (CI-240LH1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["238PNY","2GTL 2 33L 120 EZ1 GMF LP840","2GTL 2 33L 120 EZ1 GMF LP840 (CI-238PNY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237YHL","2GTL 2 33L A12C EZ1 LP850","2GTL 2 33L A12C EZ1 LP850 (CI-237YHL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230EX3","2GTL 2 33L EZ1 LP835 CP USPOM","2GTL 2 33L EZ1 LP835 CP USPOM (CI-230EX3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236E7K","2GTL 2 33L EZ1 LP850 N100","2GTL 2 33L EZ1 LP850 N100 (CI-236E7K)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235K8P","2GTL 2 33L FW A12125V EZ1 LP835","2GTL 2 33L FW A12125V EZ1 LP835 (CI-235K8P)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["238ECL","2GTL 2 33L FW A12V EZ1 ABC LP835","2GTL 2 33L FW A12V EZ1 ABC LP835 (CI-238ECL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237R7A","2GTL 2 33L FW SLD ABC LP840","2GTL 2 33L FW SLD ABC LP840 (CI-237R7A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235V87","2GTL 2 33L RW A19 EZ1 LP840 N80","2GTL 2 33L RW A19 EZ1 LP840 N80 (CI-235V87)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["238NR7","2GTL 2 33L SLD LP840 LATC","2GTL 2 33L SLD LP840 LATC (CI-238NR7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237X31","2GTL 2 33L SWL SLD LP835","2GTL 2 33L SWL SLD LP835 (CI-237X31)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227AKW","2GTL 2 37L LP835 N100EMG","2GTL 2 37L LP835 N100EMG (CI-227AKW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["245MUL","2GTL 2 40L 120 EZ1 QFC213A LP835","2GTL 2 40L 120 EZ1 QFC213A LP835 (CI-245MUL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237N2A","2GTL 2 40L EZ1 LP850 N100 NOM","2GTL 2 40L EZ1 LP850 N100 NOM (CI-237N2A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["241C3L","2GTL 2 40L EZ1 PWS1436 LP835","2GTL 2 40L EZ1 PWS1436 LP835 (CI-241C3L)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["238U71","2GTL 2 40L FW A12125V EZ1 ABC LP840","2GTL 2 40L FW A12125V EZ1 ABC LP840 (CI-238U71)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235V6A","2GTL 2 40L FW EZ1 ABC LP830","2GTL 2 40L FW EZ1 ABC LP830 (CI-235V6A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236H8U","2GTL 2 40L FW SWL EZ1 ABC LP835 PAF","2GTL 2 40L FW SWL EZ1 ABC LP835 PAF (CI-236H8U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240EL7","2GTL 2 40L RW A19 SLD LP835","2GTL 2 40L RW A19 SLD LP835 (CI-240EL7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["251NKP","2GTL 2 40L SWL EZ1 PWS1846 LP835","2GTL 2 40L SWL EZ1 PWS1846 LP835 (CI-251NKP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236EU0","2GTL 4 30L A19 EZ1 LP835 N100EMG","2GTL 4 30L A19 EZ1 LP835 N100EMG (CI-236EU0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239EPV","2GTL 4 30L EZ1 PWS1836 LP850","2GTL 4 30L EZ1 PWS1836 LP850 (CI-239EPV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240L49","2GTL 4 30L EZ1 PWS1856LV LP830","2GTL 4 30L EZ1 PWS1856LV LP830 (CI-240L49)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240J3N","2GTL 4 30L FW EZ1 ABC LP840 N100","2GTL 4 30L FW EZ1 ABC LP840 N100 (CI-240J3N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236M3E","2GTL 4 30L RW A19 EZ1 LP840 N80","2GTL 4 30L RW A19 EZ1 LP840 N80 (CI-236M3E)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239F9V","2GTL 4 30L RW EZ1 LP840","2GTL 4 30L RW EZ1 LP840 (CI-239F9V)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238MEG","2GTL 4 30L SWL EZ1 PWS1846 LP835 PAF","2GTL 4 30L SWL EZ1 PWS1846 LP835 PAF (CI-238MEG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238V3P","2GTL 4 40L 277 EZ1 GMF PWS1836 LP835","2GTL 4 40L 277 EZ1 GMF PWS1836 LP835 (CI-238V3P)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237G63","2GTL 4 40L A19 EZ1 LP830","2GTL 4 40L A19 EZ1 LP830 (CI-237G63)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["247RTN","2GTL 4 40L EZ1 LP830 JP18","2GTL 4 40L EZ1 LP830 JP18 (CI-247RTN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236NHA","2GTL 4 40L EZ1 LP830 N100","2GTL 4 40L EZ1 LP830 N100 (CI-236NHA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235JC2","2GTL 4 40L EZ1 LP840 USPOM","2GTL 4 40L EZ1 LP840 USPOM (CI-235JC2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239W0A","2GTL 4 40L EZ1 PWS1836 LP840 PAF N80EMG USPOM","2GTL 4 40L EZ1 PWS1836 LP840 PAF N80EMG USPOM (CI-239W0A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235FWL","2GTL 4 40L FN A12125V EZ1 PWS1846 ABC LP835","2GTL 4 40L FN A12125V EZ1 PWS1846 ABC LP835 (CI-235FWL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C4098,7)),6))","v":"239UWG"},{"$f":"LEFT(C4098,SEARCH(\"(CI-\",C4098)-2)","v":"2GTL 4 40L FN SWL EZ1 PWS1856LV LP835"},"2GTL 4 40L FN SWL EZ1 PWS1856LV LP835 (CI-239UWG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236X02","2GTL 4 40L FW A12125V EZ1 PWS1856LV ABC LP840","2GTL 4 40L FW A12125V EZ1 PWS1856LV ABC LP840 (CI-236X02)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235T2E","2GTL 4 40L FW A19 EZ1 PWS1836 LP835 N80","2GTL 4 40L FW A19 EZ1 PWS1836 LP835 N80 (CI-235T2E)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240XVU","2GTL 4 40L FW EZ1 PWS1436 LP835 PAF","2GTL 4 40L FW EZ1 PWS1436 LP835 PAF (CI-240XVU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236PY1","2GTL 4 40L FW EZ1 PWS1836 ABC LP840","2GTL 4 40L FW EZ1 PWS1836 ABC LP840 (CI-236PY1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237XRK","2GTL 4 40L RN EZ1 LP835","2GTL 4 40L RN EZ1 LP835 (CI-237XRK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["249R0A","2GTL 4 40L RW EZ1 LP835 USPOM JP18","2GTL 4 40L RW EZ1 LP835 USPOM JP18 (CI-249R0A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239PE0","2GTL 4 40L SWL EZ1 LP835 N100","2GTL 4 40L SWL EZ1 LP835 N100 (CI-239PE0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245MFF","2GTL 4 48L 120 EZ1 QFC213A LP835 JP18","2GTL 4 48L 120 EZ1 QFC213A LP835 JP18 (CI-245MFF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["247RAV","2GTL 4 48L A19 EZ1 LP840 JP18","2GTL 4 48L A19 EZ1 LP840 JP18 (CI-247RAV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236G65","2GTL 4 48L A19V EZ1 LP840 PAF","2GTL 4 48L A19V EZ1 LP840 PAF (CI-236G65)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237FW4","2GTL 4 48L EZ1 LP850 N80","2GTL 4 48L EZ1 LP850 N80 (CI-237FW4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239VTJ","2GTL 4 48L EZ1 PWS1836 LP850 N100","2GTL 4 48L EZ1 PWS1836 LP850 N100 (CI-239VTJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239J7V","2GTL 4 48L FW A12125V EZ1 ABC LP830 N80","2GTL 4 48L FW A12125V EZ1 ABC LP830 N80 (CI-239J7V)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["251NNP","2GTL 4 48L FW A12V SLD ABC LP835","2GTL 4 48L FW A12V SLD ABC LP835 (CI-251NNP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["247PME","2GTL 4 48L FW A19 EZ1 PWS1836 LP840 USPOM","2GTL 4 48L FW A19 EZ1 PWS1836 LP840 USPOM (CI-247PME)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C4290,7)),6))","v":"238X6Y"},{"$f":"LEFT(C4290,SEARCH(\"(CI-\",C4290)-2)","v":"2GTL 4 48L FW EZ1 ABC LP835 LATC"},"2GTL 4 48L FW EZ1 ABC LP835 LATC (CI-238X6Y)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236M48","2GTL 4 48L FW EZ1 PWS1836 ABC LP835","2GTL 4 48L FW EZ1 PWS1836 ABC LP835 (CI-236M48)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236LFE","2GTL 4 48L FW SWL 277 EZ1 GLR LP835 PAF","2GTL 4 48L FW SWL 277 EZ1 GLR LP835 PAF (CI-236LFE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229NMW","2GTL 4 48L PWS1836 LP850 NX","2GTL 4 48L PWS1836 LP850 NX (CI-229NMW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239URR","2GTL 4 48L RW A19 EZ1 ABC LP835","2GTL 4 48L RW A19 EZ1 ABC LP835 (CI-239URR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C4354,7)),6))","v":"240TMY"},{"$f":"LEFT(C4354,SEARCH(\"(CI-\",C4354)-2)","v":"2GTL 4 48L SLD PWS1446 LP840 LATC"},"2GTL 4 48L SLD PWS1446 LP840 LATC (CI-240TMY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235FYM","2GTL 4 60L 277 EZ1 QFC211GA LP850","2GTL 4 60L 277 EZ1 QFC211GA LP850 (CI-235FYM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238MVA","2GTL 4 60L A19 EZ1 LP840 PAF","2GTL 4 60L A19 EZ1 LP840 PAF (CI-238MVA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239LJP","2GTL 4 60L EZ1 LP835 NPLT","2GTL 4 60L EZ1 LP835 NPLT (CI-239LJP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245UHL","2GTL 4 60L EZ1 LP850 JP18","2GTL 4 60L EZ1 LP850 JP18 (CI-245UHL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238XL1","2GTL 4 60L EZ1 PWS1836 LP840 USPOM","2GTL 4 60L EZ1 PWS1836 LP840 USPOM (CI-238XL1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240XTK","2GTL 4 60L FN A19 EZ1 LP830 N100","2GTL 4 60L FN A19 EZ1 LP830 N100 (CI-240XTK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245W09","2GTL 4 60L FW A12V EZ1 ABC LP835","2GTL 4 60L FW A12V EZ1 ABC LP835 (CI-245W09)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240WG3","2GTL 4 60L FW EZ1 PWS1236 ABC LP835","2GTL 4 60L FW EZ1 PWS1236 ABC LP835 (CI-240WG3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236M0T","2GTL 4 60L RW 120 SLD GLR LP840","2GTL 4 60L RW 120 SLD GLR LP840 (CI-236M0T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239U5G","2GTL 4 60L RW A19 EZ1 PWS1836 LP840","2GTL 4 60L RW A19 EZ1 PWS1836 LP840 (CI-239U5G)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236NP3","2GTL 4 60L SLD PWS1846 LP840","2GTL 4 60L SLD PWS1846 LP840 (CI-236NP3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237GV5","2GTL 4 72L 120 EZ1 GLR LP840","2GTL 4 72L 120 EZ1 GLR LP840 (CI-237GV5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237G5U","2GTL 4 72L A12125V EZ1 LP850","2GTL 4 72L A12125V EZ1 LP850 (CI-237G5U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["245VL6","2GTL 4 72L EZ1 LP840 N100EMG USPOM","2GTL 4 72L EZ1 LP840 N100EMG USPOM (CI-245VL6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["239JRW","2GTL 4 72L EZ1 PWS1846 LP840","2GTL 4 72L EZ1 PWS1846 LP840 (CI-239JRW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C4546,7)),6))","v":"245M32"},{"$f":"LEFT(C4546,SEARCH(\"(CI-\",C4546)-2)","v":"2GTL 4 72L FW A19 EZ1 PWS1836 ABC LP840"},"2GTL 4 72L FW A19 EZ1 PWS1836 ABC LP840 (CI-245M32)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225VLR","2GTL 4 72L LP835 N100EMG","2GTL 4 72L LP835 N100EMG (CI-225VLR)","PS1030","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MR9"]
["238AYH","2GTL 4 72L RW A19 EZ1 LP835 N100","2GTL 4 72L RW A19 EZ1 LP835 N100 (CI-238AYH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235XC6","2GTL 4 72L SLD PWS1846 LP840","2GTL 4 72L SLD PWS1846 LP840 (CI-235XC6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226FY8","2GTL 4 F 40L LP840 N100EMG","2GTL 4 F 40L LP840 N100EMG (CI-226FY8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234YXL","2GTL 4 F 48L FW EZ1 LP840","2GTL 4 F 48L FW EZ1 LP840 (CI-234YXL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241EK2","2GTL F 2 20L FW EZ1 LP850","2GTL F 2 20L FW EZ1 LP850 (CI-241EK2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237WFE","2GTL F 2 33L EZ1 LP840 N100","2GTL F 2 33L EZ1 LP840 N100 (CI-237WFE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240Y7K","2GTL F 2 40L A19 EZ1 LP850","2GTL F 2 40L A19 EZ1 LP850 (CI-240Y7K)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["241C2X","2GTL F 2 40L RW A19 EZ1 ABC LP840","2GTL F 2 40L RW A19 EZ1 ABC LP840 (CI-241C2X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["239C2Y","2GTL F 4 30L EZ1 LP835 N80","2GTL F 4 30L EZ1 LP835 N80 (CI-239C2Y)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241PFT","2GTL F 4 40L A19 EZ1 LP835","2GTL F 4 40L A19 EZ1 LP835 (CI-241PFT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237WF2","2GTL F 4 40L EZ1 LP840 N100","2GTL F 4 40L EZ1 LP840 N100 (CI-237WF2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245RR7","2GTL F 4 40L FW 277 EZ1 GLR ABC LP840","2GTL F 4 40L FW 277 EZ1 GLR ABC LP840 (CI-245RR7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240EV7","2GTL F 4 40L SWL EZ1 LP835","2GTL F 4 40L SWL EZ1 LP835 (CI-240EV7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241C3G","2GTL F 4 48L EZ1 PWS1436 LP835","2GTL F 4 48L EZ1 PWS1436 LP835 (CI-241C3G)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239HX3","2GTL F 4 48L FW EZ1 LP830","2GTL F 4 48L FW EZ1 LP830 (CI-239HX3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241ELR","2GTL F 4 60L EZ1 PWS1856LV LP830","2GTL F 4 60L EZ1 PWS1856LV LP830 (CI-241ELR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238EC7","2GTL F 4 60L FW EZ1 ABC LP840","2GTL F 4 60L FW EZ1 ABC LP840 (CI-238EC7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237MV4","2GTL F 4 72L A19 EZ1 LP830","2GTL F 4 72L A19 EZ1 LP830 (CI-237MV4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240Y1W","2GTL F 4 72L FW A12125V SLD PWS1846 ABCNG LP840","2GTL F 4 72L FW A12125V SLD PWS1846 ABCNG LP840 (CI-240Y1W)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237TE5","2GTL F 4 72L RW EZ1 LP840 CRM","2GTL F 4 72L RW EZ1 LP840 CRM (CI-237TE5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234TKW","2GTL2 A12 120 LP840","2GTL2 A12 120 LP840 (CI-234TKW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226FYM","2GTL2 SWL MVOLT","2GTL2 SWL MVOLT (CI-226FYM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230JNJ","2GTL2R 20L LP840 NAWL","2GTL2R 20L LP840 NAWL (CI-230JNJ)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["230M6R","2GTL2R 40L LP840 3RP","2GTL2R 40L LP840 3RP (CI-230M6R)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["241T06","2GTL4 5000LM PWS1836 LP835","2GTL4 5000LM PWS1836 LP835 (CI-241T06)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235GFV","2GTL4R 30L EZ1 LP850 J4","2GTL4R 30L EZ1 LP850 J4 (CI-235GFV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230VNK","2GTL4R 30L LP840 3RP","2GTL4R 30L LP840 3RP (CI-230VNK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230JXP","2GTL4R 40L LP840 3RP","2GTL4R 40L LP840 3RP (CI-230JXP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233YU9","2GTL4R 48L GTH250 LP840","2GTL4R 48L GTH250 LP840 (CI-233YU9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230JX9","2GTL4R 48L LP840 J4","2GTL4R 48L LP840 J4 (CI-230JX9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230JXT","2GTL4R 60L LP840 3RP","2GTL4R 60L LP840 3RP (CI-230JXT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245RNW","GTL 4 20L A19 EZ1 LP840","GTL 4 20L A19 EZ1 LP840 (CI-245RNW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237GJN","GTL 4 20L EZ1 PWS1856LV LP835","GTL 4 20L EZ1 PWS1856LV LP835 (CI-237GJN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["239P09","GTL 4 20L SWL EZ1 PWS1856LV LP835","GTL 4 20L SWL EZ1 PWS1856LV LP835 (CI-239P09)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237XUV","GTL 4 33L A19 SLD LP830","GTL 4 33L A19 SLD LP830 (CI-237XUV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236C59","GTL 4 33L FW A19 EZ1 ABC LP840 PAF","GTL 4 33L FW A19 EZ1 ABC LP840 PAF (CI-236C59)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["241KNN","GTL 4 33L SLD PWS1246 LP840","GTL 4 33L SLD PWS1246 LP840 (CI-241KNN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["238JKJ","GTL 4 33L SWL SLD LP835","GTL 4 33L SWL SLD LP835 (CI-238JKJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236K21","GTL 4 40L EZ1 PWS1836 LP835","GTL 4 40L EZ1 PWS1836 LP835 (CI-236K21)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237VAW","GTL 4 40L SWL EZ1 LP835 N80","GTL 4 40L SWL EZ1 LP835 N80 (CI-237VAW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["238CUX","GTL 4 48L FW A12125V EZ1 ABC LP840","GTL 4 48L FW A12125V EZ1 ABC LP840 (CI-238CUX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239N46","GTL 4 48L RW SWL EZ1 ABC LP840","GTL 4 48L RW SWL EZ1 ABC LP840 (CI-239N46)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245RP3","GTL F 4 20L FW 277 EZ1 GLR ABC LP840","GTL F 4 20L FW 277 EZ1 GLR ABC LP840 (CI-245RP3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237TMU","GTL F 4 33L EZ1 PWS1836 LP835 N80 CRE","GTL F 4 33L EZ1 PWS1836 LP835 N80 CRE (CI-237TMU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236C5N","GTL F 4 33L FW A19 EZ1 ABC LP840 PAF","GTL F 4 33L FW A19 EZ1 ABC LP840 PAF (CI-236C5N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["241X6P","GTL F 4 33L RW 277 EZ1 GLR LP835 CRM","GTL F 4 33L RW 277 EZ1 GLR LP835 CRM (CI-241X6P)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240U5E","GTL F 4 33L SWL SLD LP840","GTL F 4 33L SWL SLD LP840 (CI-240U5E)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237F7E","GTL F 4 40L FW EZ1 ABC LP840","GTL F 4 40L FW EZ1 ABC LP840 (CI-237F7E)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236E0W","GTL F 4 40L SWL EZ1 LP840 N80","GTL F 4 40L SWL EZ1 LP840 N80 (CI-236E0W)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240VKL","GTL F 4 48L FW EZ1 LP835 PAF USPOM","GTL F 4 48L FW EZ1 LP835 PAF USPOM (CI-240VKL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233L0F","GTL4R 20L LP835 SSQ","GTL4R 20L LP835 SSQ (CI-233L0F)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230PJ2","2RTL2 20L EZ1 LP835","2RTL2 20L EZ1 LP835 (CI-230PJ2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C5186,7)),6))","v":"233JY2"},{"$f":"LEFT(C5186,SEARCH(\"(CI-\",C5186)-2)","v":"2RTL2 20L EZ1 PWS1436 LP840"},"2RTL2 20L EZ1 PWS1436 LP840 (CI-233JY2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229XN6","2RTL2 24L D24 LP830 BLD","2RTL2 24L D24 LP830 BLD (CI-229XN6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["223H34","2RTL2 24L D24 LP835 NX RIF1","2RTL2 24L D24 LP835 NX RIF1 (CI-223H34)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226L68","2RTL2 33L D38 LP830 NX","2RTL2 33L D38 LP830 NX (CI-226L68)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["212JVJ","2RTL2 33L D38 LP835 N80 RFD101586","2RTL2 33L D38 LP835 N80 RFD101586 (CI-212JVJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["222G9P","2RTL2 33L D38 LP840 N100 SSQ","2RTL2 33L D38 LP840 N100 SSQ (CI-222G9P)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["214FY7","2RTL2 33L D38 LP850 N80","2RTL2 33L D38 LP850 N80 (CI-214FY7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227UV0","2RTL2 33L D38 PWS1846 LP835 BLD","2RTL2 33L D38 PWS1846 LP835 BLD (CI-227UV0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["207K0H","2RTL2 33L D45 LP835 N80 USPOM","2RTL2 33L D45 LP835 N80 USPOM (CI-207K0H)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230N8X","2RTL2 33L EZ1 LP835","2RTL2 33L EZ1 LP835 (CI-230N8X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230TLK","2RTL2 33L EZ1 LP840 N80","2RTL2 33L EZ1 LP840 N80 (CI-230TLK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234TFG","2RTL2 33L EZB LP835 N80","2RTL2 33L EZB LP835 N80 (CI-234TFG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234XRW","2RTL2 33L SLD PWS1846 LP840","2RTL2 33L SLD PWS1846 LP840 (CI-234XRW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231RJU","2RTL2 40L EZ1 LP850","2RTL2 40L EZ1 LP850 (CI-231RJU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226TGF","2RTL2 CAS 24L D24 LP835 BLD","2RTL2 CAS 24L D24 LP835 BLD (CI-226TGF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["209URM","2RTL2 CAS 33L D45 LP835 N100","2RTL2 CAS 33L D45 LP835 N100 (CI-209URM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234GUN","2RTL2R 20L EZ1 LP840","2RTL2R 20L EZ1 LP840 (CI-234GUN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["219W20","2RTL2R 32L D38 LP850 NX","2RTL2R 32L D38 LP850 NX (CI-219W20)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234RCH","2RTL2R 40L EZ1 LP840","2RTL2R 40L EZ1 LP840 (CI-234RCH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231RKV","2RTL2RT 33L EZB LP835 N100","2RTL2RT 33L EZB LP835 N100 (CI-231RKV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234FWU","2RTL4 30L EZ1 LP840 N100","2RTL4 30L EZ1 LP840 N100 (CI-234FWU)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
[{"$f":"(LEFT((RIGHT(C5442,7)),6))","v":"228T3M"},{"$f":"LEFT(C5442,SEARCH(\"(CI-\",C5442)-2)","v":"2RTL4 40L 120 D40 GMF LP835 NX"},"2RTL4 40L 120 D40 GMF LP835 NX (CI-228T3M)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["214HGE","2RTL4 40L D40 LP835 N100","2RTL4 40L D40 LP835 N100 (CI-214HGE)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["215GLX","2RTL4 40L D40 LP840 N100","2RTL4 40L D40 LP840 N100 (CI-215GLX)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["225X4M","2RTL4 40L D40 PWS1836 LP835 N100","2RTL4 40L D40 PWS1836 LP835 N100 (CI-225X4M)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["230P7P","2RTL4 40L EZ1 LP840","2RTL4 40L EZ1 LP840 (CI-230P7P)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["232T6K","2RTL4 40L EZ1 PWS1836 LP835","2RTL4 40L EZ1 PWS1836 LP835 (CI-232T6K)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["230W85","2RTL4 40L SLD LP840","2RTL4 40L SLD LP840 (CI-230W85)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["220G0N","2RTL4 48L 120 D49 GLR LP835 BLD","2RTL4 48L 120 D49 GLR LP835 BLD (CI-220G0N)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["233UF1","2RTL4 48L 277 EZ1 GLR LP840","2RTL4 48L 277 EZ1 GLR LP840 (CI-233UF1)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["210RNE","2RTL4 48L D49 LP835 N80","2RTL4 48L D49 LP835 N80 (CI-210RNE)","PS1030","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["225F9Y","2RTL4 48L D49 LP840 N100 USPOM","2RTL4 48L D49 LP840 N100 USPOM (CI-225F9Y)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["228NKH","2RTL4 48L D49 PWS1436 LP835 NX","2RTL4 48L D49 PWS1436 LP835 NX (CI-228NKH)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["227XMW","2RTL4 48L D49 PWS1846 LP835 N80","2RTL4 48L D49 PWS1846 LP835 N80 (CI-227XMW)","PS1030","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["227W14","2RTL4 48L EZ1 LP835 NX RFD174369","2RTL4 48L EZ1 LP835 NX RFD174369 (CI-227W14)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["233JW6","2RTL4 48L EZ1 PWS1846 LP835 N80","2RTL4 48L EZ1 PWS1846 LP835 N80 (CI-233JW6)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["230P7M","2RTL4 48L SLD LP840","2RTL4 48L SLD LP840 (CI-230P7M)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
[{"$f":"(LEFT((RIGHT(C5634,7)),6))","v":"232VLC"},{"$f":"LEFT(C5634,SEARCH(\"(CI-\",C5634)-2)","v":"2RTL4 60L EZ1 LP835 N100"},"2RTL4 60L EZ1 LP835 N100 (CI-232VLC)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["233A7G","2RTL4 60L EZB LP840","2RTL4 60L EZB LP840 (CI-233A7G)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["231TX6","2RTL4 72L EZ1 LP840","2RTL4 72L EZ1 LP840 (CI-231TX6)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["232PNM","2RTL4 CAS 40L EZ1 LP840 N100","2RTL4 CAS 40L EZ1 LP840 N100 (CI-232PNM)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["230ULF","2RTL4 CAS 48L EZ1 LP835","2RTL4 CAS 48L EZ1 LP835 (CI-230ULF)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["222FHX","2RTL4R 38L D43 LP835 BLD","2RTL4R 38L D43 LP835 BLD (CI-222FHX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228X81","2RTL4R 40L GZ1 LP840","2RTL4R 40L GZ1 LP840 (CI-228X81)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["215YHR","2RTL4R MG 43L D50 LP835 NX","2RTL4R MG 43L D50 LP835 NX (CI-215YHR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["220WVT","2RTL4RT 38L D43 LP850 N100","2RTL4RT 38L D43 LP850 N100 (CI-220WVT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["222FLH","2RTL4RT 44L D50 LP835 BLD N100","2RTL4RT 44L D50 LP835 BLD N100 (CI-222FLH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229UA1","2RTL4RT 48L EZ1 LP835 N100","2RTL4RT 48L EZ1 LP835 N100 (CI-229UA1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231NHF","2RTLX2 20L EZ1 LP835","2RTLX2 20L EZ1 LP835 (CI-231NHF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["209TXX","2RTLX2 32L D38 LP835 N80","2RTLX2 32L D38 LP835 N80 (CI-209TXX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["209TY0","2RTLX2 32L D38 LP840 NX","2RTLX2 32L D38 LP840 NX (CI-209TY0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232LJP","2RTLX2 40L EZ1 LP835","2RTLX2 40L EZ1 LP835 (CI-232LJP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["212NUM","2RTLX4 43L D49 LP835 N100","2RTLX4 43L D49 LP835 N100 (CI-212NUM)","PS1030","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["214EXC","2RTLX4 43L D49 LP840 N80","2RTLX4 43L D49 LP840 N80 (CI-214EXC)","PS1030","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["234R3M","2RTLX4 48L EZ1 LP850","2RTLX4 48L EZ1 LP850 (CI-234R3M)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["232U77","2RTLX4 72L EZ1 LP835","2RTLX4 72L EZ1 LP835 (CI-232U77)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["205UXM","RTL4 22L D25 LP835 N100","RTL4 22L D25 LP835 N100 (CI-205UXM)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series instructions","*239MRJ","*239MRC"]
["216UP7","RTL4 25L D24 LP835 NX PWS1836 RFD125001","RTL4 25L D24 LP835 NX PWS1836 RFD125001 (CI-216UP7)","PS1030","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["220LGC","RTL4 25L D24 LP850 N80","RTL4 25L D24 LP850 N80 (CI-220LGC)","PS1030","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["232N4C","RTL4 30L EZ1 LP840 N100","RTL4 30L EZ1 LP840 N100 (CI-232N4C)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series instructions","*239MRJ","*239MRC"]
["214M98","RTL4 40L D41 LP835 NX","RTL4 40L D41 LP835 NX (CI-214M98)","PS1030","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["220W5P","RTL4 40L D41 LP850 N100","RTL4 40L D41 LP850 N100 (CI-220W5P)","PS1030","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["230MVW","RTL4 40L EZ1 LP840","RTL4 40L EZ1 LP840 (CI-230MVW)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series instructions","*239MRJ","*239MRC"]
["234M10","RTL4 40L EZB LP835 N100","RTL4 40L EZB LP835 N100 (CI-234M10)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series instructions","*239MRJ","*239MRC"]
["234TFT","RTLX4 20L EZ1 LP835 USPOM","RTLX4 20L EZ1 LP835 USPOM (CI-234TFT)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series instructions","*239MRJ","*239MRC"]
["210TMK","RTLX4 24L D24 LP835 NX RFD94772","RTLX4 24L D24 LP835 NX RFD94772 (CI-210TMK)","PS1030","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR9","*239MR7"]
["234J2M","RTLX4 30L EZ1 LP835 MB RFD194141","RTLX4 30L EZ1 LP835 MB RFD194141 (CI-234J2M)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series instructions","*239MRJ","*239MRC"]
["231EK6","2RTL2 20L EZ1 LP840 N100EMG","2RTL2 20L EZ1 LP840 N100EMG (CI-231EK6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["219PKK","2RTL2 24L D24 LP840 N100EMG","2RTL2 24L D24 LP840 N100EMG (CI-219PKK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["204WPU","2RTL2 33L D45 LP835 N100 CS1WL10 SSQ","2RTL2 33L D45 LP835 N100 CS1WL10 SSQ (CI-204WPU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232PTP","2RTL2 33L EZ1 PWS1836 LP835 N80EMG","2RTL2 33L EZ1 PWS1836 LP835 N80EMG (CI-232PTP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237J77","2RTL2 40L EDB LP840","2RTL2 40L EDB LP840 (CI-237J77)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237TV7","2RTL2 40L EZB PWS1856LV LP835","2RTL2 40L EZB PWS1856LV LP835 (CI-237TV7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["238PE5","2RTL2 CAS 33L EZ1 LP840 N80EMG","2RTL2 CAS 33L EZ1 LP840 N80EMG (CI-238PE5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235WLF","2RTL2R 33L EZ1 LP835 N100EMG","2RTL2R 33L EZ1 LP835 N100EMG (CI-235WLF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C6082,7)),6))","v":"245V9A"},{"$f":"LEFT(C6082,SEARCH(\"(CI-\",C6082)-2)","v":"2RTL2RT 40L EZB LP840 N80"},"2RTL2RT 40L EZB LP840 N80 (CI-245V9A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236K80","2RTL4 40L 277 EZ1 QFC311GA LP835","2RTL4 40L 277 EZ1 QFC311GA LP835 (CI-236K80)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["224G3A","2RTL4 40L D40 LP835 N100EMG","2RTL4 40L D40 LP835 N100EMG (CI-224G3A)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["235RN8","2RTL4 40L EZB LP840 N100EMG","2RTL4 40L EZB LP840 N100EMG (CI-235RN8)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["215AHH","2RTL4 48L 277 D49 GLR LP840 N100EMG","2RTL4 48L 277 D49 GLR LP840 N100EMG (CI-215AHH)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["231C6C","2RTL4 48L EZ1 LP835 N100EMG","2RTL4 48L EZ1 LP835 N100EMG (CI-231C6C)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["239VY1","2RTL4 48L EZ1 PWS1856LV LP840","2RTL4 48L EZ1 PWS1856LV LP840 (CI-239VY1)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["237JAV","2RTL4 60L EZ1 LP840 USPOM","2RTL4 60L EZ1 LP840 USPOM (CI-237JAV)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["240UVN","2RTL4 72L EZ1 LP835 N80EMG","2RTL4 72L EZ1 LP835 N80EMG (CI-240UVN)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["232CA3","2RTL4 CAS 48L EZ1 LP840 N100EMG","2RTL4 CAS 48L EZ1 LP840 N100EMG (CI-232CA3)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["236N7M","2RTL4 CAS 48L EZ1 LP840 N80","2RTL4 CAS 48L EZ1 LP840 N80 (CI-236N7M)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["245VLU","2RTL4RT 48L EZ1 LP840 USPOM","2RTL4RT 48L EZ1 LP840 USPOM (CI-245VLU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["217TMU","2RTLX2 22L D26 LP835 NX USPOM","2RTLX2 22L D26 LP835 NX USPOM (CI-217TMU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["247R4X","2RTLX4 30L EZ1 LP830 N80","2RTLX4 30L EZ1 LP830 N80 (CI-247R4X)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["239RKC","2RTLX4 30L SLD LP840","2RTLX4 30L SLD LP840 (CI-239RKC)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["209U0L","2RTLX4 43L D48 LP840 N80","2RTLX4 43L D48 LP840 N80 (CI-209U0L)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
[{"$f":"(LEFT((RIGHT(C6274,7)),6))","v":"236N33"},{"$f":"LEFT(C6274,SEARCH(\"(CI-\",C6274)-2)","v":"2RTLX4 72L EZ1 LP835 N100"},"2RTLX4 72L EZ1 LP835 N100 (CI-236N33)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["235HJ7","RTL4 30L SLD LP835","RTL4 30L SLD LP835 (CI-235HJ7)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series instructions","*239MRJ","*239MRC"]
["245H2M","RTL4 30L SLD PWS1846 LP835","RTL4 30L SLD PWS1846 LP835 (CI-245H2M)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series instructions","*239MRJ","*239MRC"]
["245UK9","RTL4 48L EZ1 PWS1836 LP835","RTL4 48L EZ1 PWS1836 LP835 (CI-245UK9)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series instructions","*239MRJ","*239MRC"]
["235UPX","RTL4 60L EZ1 LP840","RTL4 60L EZ1 LP840 (CI-235UPX)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series instructions","*239MRJ","*239MRC"]
[{"$f":"(LEFT((RIGHT(C6338,7)),6))","v":"238GR8"},{"$f":"LEFT(C6338,SEARCH(\"(CI-\",C6338)-2)","v":"RTLX4 40L EZ1 LP830"},"RTLX4 40L EZ1 LP830 (CI-238GR8)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series instructions","*239MRJ","*239MRC"]
["238JLE","RTLX4 48L EZB LP830","RTLX4 48L EZB LP830 (CI-238JLE)","PS1050","6 inches minmum away from driver inside fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["214LFC","2SBSL2 33L FW D38 LP840 N100","2SBSL2 33L FW D38 LP840 N100 (CI-214LFC)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["211GXV","2SBSL2 33L RW D38 LP835 N80","2SBSL2 33L RW D38 LP835 N80 (CI-211GXV)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["216UPP","2SBSL4 46L RW D50 LP840 N100","2SBSL4 46L RW D50 LP840 N100 (CI-216UPP)","PS1030","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR9","*239MR7"]
["219K6P","2SBSL4 46L RW D50 LP840 N80","2SBSL4 46L RW D50 LP840 N80 (CI-219K6P)","PS1030","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR9","*239MR7"]
["233MYR","SBL4 30L EOHN LP835","SBL4 30L EOHN LP835 (CI-233MYR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232UY6","SBL4 40L EZ1 LP840","SBL4 40L EZ1 LP840 (CI-232UY6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230WEC","SBL4 LP840","SBL4 LP840 (CI-230WEC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235GHV","2SBSL2 33L FW EZ1 LP830","2SBSL2 33L FW EZ1 LP830 (CI-235GHV)","PS1050","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MR9","*239MRC"]
["232MP2","2SBSL2 33L RW 277 EZ1 LP840 N100 QFC313A","2SBSL2 33L RW 277 EZ1 LP840 N100 QFC313A (CI-232MP2)","PS1050","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MR9","*239MRC"]
["232MA4","2SBSL2 33L RW SLD LP840","2SBSL2 33L RW SLD LP840 (CI-232MA4)","PS1050","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MR9","*239MRC"]
["237PVA","2SBSL4 48L FW EZ1 LP840","2SBSL4 48L FW EZ1 LP840 (CI-237PVA)","PS1050","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MR9","*239MRC"]
["235XTP","2SBSL4 48L FW EZ1 LP850","2SBSL4 48L FW EZ1 LP850 (CI-235XTP)","PS1050","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MR9","*239MRC"]
["235KWP","2SBSLX2 40L FW EZ1 LP840","2SBSLX2 40L FW EZ1 LP840 (CI-235KWP)","PS1050","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MR9","*239MRC"]
["235Y5C","SBL4 30L EZ1 LP835 LSXRHL","SBL4 30L EZ1 LP835 LSXRHL (CI-235Y5C)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C6530,7)),6))","v":"235N24"},{"$f":"LEFT(C6530,SEARCH(\"(CI-\",C6530)-2)","v":"SBL4 40L EZ1 LP835 N100"},"SBL4 40L EZ1 LP835 N100 (CI-235N24)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235AER","SBL4 48L EZ1 LP830","SBL4 48L EZ1 LP830 (CI-235AER)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241GF8","SBL4 60L EZ1 LP840 USPOM","SBL4 60L EZ1 LP840 USPOM (CI-241GF8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234N3P","2TL2 20L FW A19 120 EZ1 GLR LP835","2TL2 20L FW A19 120 EZ1 GLR LP835 (CI-234N3P)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["217KJA","2TL2 33L FW A12 D38 LP840 N80","2TL2 33L FW A12 D38 LP840 N80 (CI-217KJA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["213AK6","2TL2 33L FW A12 D38 LP840 NX","2TL2 33L FW A12 D38 LP840 NX (CI-213AK6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232L0T","2TL2 33L FW A12 EZ1 PWS1436 LP835","2TL2 33L FW A12 EZ1 PWS1436 LP835 (CI-232L0T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["215CG8","2TL2 33L FW A12125 D38 LP840 NX","2TL2 33L FW A12125 D38 LP840 NX (CI-215CG8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231H66","2TL2 33L FW A12V D38 LP835 N100","2TL2 33L FW A12V D38 LP835 N100 (CI-231H66)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["217MF2","2TL2 33L FW A19 D38 ABCNG LP835 NX","2TL2 33L FW A19 D38 ABCNG LP835 NX (CI-217MF2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["213HE9","2TL2 33L FW A19 D38 LP835 NX","2TL2 33L FW A19 D38 LP835 NX (CI-213HE9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["219P0T","2TL2 33L FW A19 D38 LP850 NX","2TL2 33L FW A19 D38 LP850 NX (CI-219P0T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233LRH","2TL2 33L FW A19 EZ1 PWS1836 LP840","2TL2 33L FW A19 EZ1 PWS1836 LP840 (CI-233LRH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233Y78","2TL2 33L FW A19 EZ1 PWS1836 LP850","2TL2 33L FW A19 EZ1 PWS1836 LP850 (CI-233Y78)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231RA1","2TL2 33L FW MPL EZ1 LP835","2TL2 33L FW MPL EZ1 LP835 (CI-231RA1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["214JMT","2TL2 33L FW MWS D38 LP840 NX","2TL2 33L FW MWS D38 LP840 NX (CI-214JMT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231RA9","2TL2 33L FW MWS EZ1 LP830","2TL2 33L FW MWS EZ1 LP830 (CI-231RA9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["211T0M","2TL2 33L FW SBSQ D38 LP835 N80","2TL2 33L FW SBSQ D38 LP835 N80 (CI-211T0M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["215RW0","2TL2 33L FW SWL D38 LP840 NX","2TL2 33L FW SWL D38 LP840 NX (CI-215RW0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232N95","2TL2 33L FW SWL EZ1 LP850 NAEYB","2TL2 33L FW SWL EZ1 LP850 NAEYB (CI-232N95)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231T60","2TL2 33L RW A12 EZ1 LP835 N80","2TL2 33L RW A12 EZ1 LP835 N80 (CI-231T60)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228NPE","2TL2 33L RW A19 D38 ABCNG LP840 NX","2TL2 33L RW A19 D38 ABCNG LP840 NX (CI-228NPE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231NMM","2TL2 33L RW A19 EZ1 ABCNG LP840","2TL2 33L RW A19 EZ1 ABCNG LP840 (CI-231NMM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["223EP8","2TL2 33L RW MPL D38 PWS1836 LP835 NX","2TL2 33L RW MPL D38 PWS1836 LP835 NX (CI-223EP8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["220P47","2TL2 33L RW MWS D38 LP840 NX","2TL2 33L RW MWS D38 LP840 NX (CI-220P47)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["214CVL","2TL2 33L RW SWL D38 LP835 N100","2TL2 33L RW SWL D38 LP835 N100 (CI-214CVL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234LNG","2TL2 33L RW SWL EZ1 LP850","2TL2 33L RW SWL EZ1 LP850 (CI-234LNG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233KHH","2TL2 40L FW A12 SLD LP835","2TL2 40L FW A12 SLD LP835 (CI-233KHH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234EAR","2TL2 40L FW A19 EZB LP835 N80","2TL2 40L FW A19 EZB LP835 N80 (CI-234EAR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233HHU","2TL2 40L RW A12125 EZ1 LP835","2TL2 40L RW A12125 EZ1 LP835 (CI-233HHU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233M18","2TL4 40L FW A12125 EZ1 LP840","2TL4 40L FW A12125 EZ1 LP840 (CI-233M18)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232T1K","2TL4 40L RW A12 EZ1 LP840 N100","2TL4 40L RW A12 EZ1 LP840 N100 (CI-232T1K)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["224MFG","2TL4 46L FW A12 D50 ABC LP835 NX","2TL4 46L FW A12 D50 ABC LP835 NX (CI-224MFG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["214ETR","2TL4 46L FW A12 D50 LP840 N100","2TL4 46L FW A12 D50 LP840 N100 (CI-214ETR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["217FM4","2TL4 46L FW A12 D50 PWS1836 LP835 NX","2TL4 46L FW A12 D50 PWS1836 LP835 NX (CI-217FM4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["221JLT","2TL4 46L FW A12125 D50 LG LP840 NX","2TL4 46L FW A12125 D50 LG LP840 NX (CI-221JLT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["220JVW","2TL4 46L FW A12125 D50 PWS1836 LP840 NX","2TL4 46L FW A12125 D50 PWS1836 LP840 NX (CI-220JVW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229XN3","2TL4 46L FW A19 120 D50 GMF LP835 NX","2TL4 46L FW A19 120 D50 GMF LP835 NX (CI-229XN3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C6978,7)),6))","v":"211K5W"},{"$f":"LEFT(C6978,SEARCH(\"(CI-\",C6978)-2)","v":"2TL4 46L FW A19 D50 LP835 N100"},"2TL4 46L FW A19 D50 LP835 N100 (CI-211K5W)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225XY4","2TL4 46L FW A19 D50 PWS1836 LP850 NX","2TL4 46L FW A19 D50 PWS1836 LP850 NX (CI-225XY4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["219YLM","2TL4 46L FW MPL D50 LP840 N100","2TL4 46L FW MPL D50 LP840 N100 (CI-219YLM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["214LNH","2TL4 46L FW MWS D50 LP840 NX","2TL4 46L FW MWS D50 LP840 NX (CI-214LNH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228TE4","2TL4 46L FW SWL D50 LP830 NX","2TL4 46L FW SWL D50 LP830 NX (CI-228TE4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["213LV0","2TL4 46L FW SWL D50 LP840 NX","2TL4 46L FW SWL D50 LP840 NX (CI-213LV0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["223MTC","2TL4 46L RW A12 D50 LP850 N100","2TL4 46L RW A12 D50 LP850 N100 (CI-223MTC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["220VGJ","2TL4 46L RW A19 D50 LP835 BLD","2TL4 46L RW A19 D50 LP835 BLD (CI-220VGJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["216KHL","2TL4 46L RW MPL D50 LP850 NX","2TL4 46L RW MPL D50 LP850 NX (CI-216KHL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231EPW","2TL4 46L RW SWL D50 LP840 NX","2TL4 46L RW SWL D50 LP840 NX (CI-231EPW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232HWJ","2TL4 48L FW A12 EZ1 LP840 N80","2TL4 48L FW A12 EZ1 LP840 N80 (CI-232HWJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234JCL","2TL4 48L FW A12 SLD PWS1846 LP840","2TL4 48L FW A12 SLD PWS1846 LP840 (CI-234JCL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234N2K","2TL4 48L FW A12125 EZ1 LP840 N80","2TL4 48L FW A12125 EZ1 LP840 N80 (CI-234N2K)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229XJ2","2TL4 48L FW A19 EZ1 LP835","2TL4 48L FW A19 EZ1 LP835 (CI-229XJ2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231VT4","2TL4 48L FW A19 SLD LP840","2TL4 48L FW A19 SLD LP840 (CI-231VT4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232H08","2TL4 48L FW MWS EZ1 LP850","2TL4 48L FW MWS EZ1 LP850 (CI-232H08)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C7170,7)),6))","v":"232HJ3"},{"$f":"LEFT(C7170,SEARCH(\"(CI-\",C7170)-2)","v":"2TL4 48L FW SWL SLD PWS1846 LP840"},"2TL4 48L FW SWL SLD PWS1846 LP840 (CI-232HJ3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232M4Y","2TL4 48L RW SWL EZ1 LP835 N100","2TL4 48L RW SWL EZ1 LP835 N100 (CI-232M4Y)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234RVV","2TL4 60L FW A12125 EZ1 ABC LP840","2TL4 60L FW A12125 EZ1 ABC LP840 (CI-234RVV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232G23","2TL4 60L FW SWL EZ1 LP840","2TL4 60L FW SWL EZ1 LP840 (CI-232G23)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233YPY","2TL4 72L FW A12 EZB LP835","2TL4 72L FW A12 EZB LP835 (CI-233YPY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["209MEC","2TLED 36L D45 SSQ","2TLED 36L D45 SSQ (CI-209MEC)","PS1030","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MR9"]
["227GU0","2TLX2 33L FW A12 D38 LP850 NX USPOM","2TLX2 33L FW A12 D38 LP850 NX USPOM (CI-227GU0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229HVY","2TLX2 33L FW A19 D38 ABC LP835 N100","2TLX2 33L FW A19 D38 ABC LP835 N100 (CI-229HVY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232F77","2TLX2 33L FW A19 EZ1 LP840","2TLX2 33L FW A19 EZ1 LP840 (CI-232F77)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228WTH","2TLX2 33L RW MWS D38 LP835 NX","2TLX2 33L RW MWS D38 LP835 NX (CI-228WTH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234FHA","2TLX2 40L FW SWL EZ1 LP835","2TLX2 40L FW SWL EZ1 LP835 (CI-234FHA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234H0W","2TLX4 40L FW A19 EZ1 LP850","2TLX4 40L FW A19 EZ1 LP850 (CI-234H0W)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233NM2","2TLX4 40L RW A19 EZ1 LP840","2TLX4 40L RW A19 EZ1 LP840 (CI-233NM2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226EUW","2TLX4 46L FW A12 D50 LP850 NX","2TLX4 46L FW A12 D50 LP850 NX (CI-226EUW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228PAA","2TLX4 46L FW A19V D50 LP835 N80","2TLX4 46L FW A19V D50 LP835 N80 (CI-228PAA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["227U5A","2TLX4 46L RW A12 D50 LP840 NX","2TLX4 46L RW A12 D50 LP840 NX (CI-227U5A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231N60","2TLX4 48L FW A12 EZ1 LP840","2TLX4 48L FW A12 EZ1 LP840 (CI-231N60)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232V78","2TLX4 48L RW A19 EZ1 LP835","2TLX4 48L RW A19 EZ1 LP835 (CI-232V78)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233C96","2TLX4 60L FW A19 EZ1 LP840","2TLX4 60L FW A19 EZ1 LP840 (CI-233C96)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232JHK","TL4 30L FW A12 EZB LP840","TL4 30L FW A12 EZB LP840 (CI-232JHK)","PS1050","3 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["231RM5","TL4 40L FW A12 EZ1 LP835","TL4 40L FW A12 EZ1 LP835 (CI-231RM5)","PS1050","3 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
[{"$f":"(LEFT((RIGHT(C7426,7)),6))","v":"231V79"},{"$f":"LEFT(C7426,SEARCH(\"(CI-\",C7426)-2)","v":"TL4 40L FW A19 EZ1 LP840"},"TL4 40L FW A19 EZ1 LP840 (CI-231V79)","PS1050","3 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["232N9F","TL4 40L FW SWL EZ1 LP830 NAEYB","TL4 40L FW SWL EZ1 LP830 NAEYB (CI-232N9F)","PS1050","3 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["233MKV","TL4 40L RW A12 EZ1 LP835","TL4 40L RW A12 EZ1 LP835 (CI-233MKV)","PS1050","3 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["228CH4","TL4 43L FW A12 D46 LP835 NX USPOM","TL4 43L FW A12 D46 LP835 NX USPOM (CI-228CH4)","PS1050","3 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["226EWN","TL4 43L FW A19 D46 LP830 NX","TL4 43L FW A19 D46 LP830 NX (CI-226EWN)","PS1050","3 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["223AV4","TL4 43L FW A19 D46 PWS1836 LP840 N80","TL4 43L FW A19 D46 PWS1836 LP840 N80 (CI-223AV4)","PS1050","3 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["222PYH","TL4 43L FW SWL D46 LP835 NX","TL4 43L FW SWL D46 LP835 NX (CI-222PYH)","PS1050","3 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["224THT","TL4 43L RW A19 D46 LP835 N100 RFD155349","TL4 43L RW A19 D46 LP835 N100 RFD155349 (CI-224THT)","PS1050","3 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["232CLU","TL4 48L FW A12 EZ1 LP835 N100","TL4 48L FW A12 EZ1 LP835 N100 (CI-232CLU)","PS1050","3 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["229XAL","TL4 48L FW A19 EZ1 LP835","TL4 48L FW A19 EZ1 LP835 (CI-229XAL)","PS1050","3 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["234NLV","TL4 48L RW A19 EZ1 LP835 N100","TL4 48L RW A19 EZ1 LP835 N100 (CI-234NLV)","PS1050","3 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["232THV","TLX4 30L FW A12 EZ1 LP835","TLX4 30L FW A12 EZ1 LP835 (CI-232THV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231RLP","TLX4 40L FW A19 EZ1 LP840 N80","TLX4 40L FW A19 EZ1 LP840 N80 (CI-231RLP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229K7X","TLX4 43L FW A12 D46 LP840 N100","TLX4 43L FW A12 D46 LP840 N100 (CI-229K7X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228FYG","TLX4 43L FW A19 D46 LP850 NX","TLX4 43L FW A19 D46 LP850 NX (CI-228FYG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233JJV","TLX4 48L FW A12 EZ1 LP835","TLX4 48L FW A12 EZ1 LP835 (CI-233JJV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C7618,7)),6))","v":"233KMF"},{"$f":"LEFT(C7618,SEARCH(\"(CI-\",C7618)-2)","v":"TLX4 60L FW A19 EZ1 LP840"},"TLX4 60L FW A19 EZ1 LP840 (CI-233KMF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235HJC","2TL2 20L FW A12 EZ1 LP840 N100EMG","2TL2 20L FW A12 EZ1 LP840 N100EMG (CI-235HJC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240TGU","2TL2 20L FW A12125 EZ1 LP835","2TL2 20L FW A12125 EZ1 LP835 (CI-240TGU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237HAM","2TL2 20L RW A19 EZ1 PWS1836 LP830","2TL2 20L RW A19 EZ1 PWS1836 LP830 (CI-237HAM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237UG0","2TL2 33L FW A12 EZB LP840 N100EMG","2TL2 33L FW A12 EZB LP840 N100EMG (CI-237UG0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C7682,7)),6))","v":"240RFL"},{"$f":"LEFT(C7682,SEARCH(\"(CI-\",C7682)-2)","v":"2TL2 33L FW A12V EZ1 LP835"},"2TL2 33L FW A12V EZ1 LP835 (CI-240RFL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240RN0","2TL2 33L FW A19 EZ1 LP835 USPOM","2TL2 33L FW A19 EZ1 LP835 USPOM (CI-240RN0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238CUP","2TL2 33L FW A19 EZ1 PWS1856LV LG LP835","2TL2 33L FW A19 EZ1 PWS1856LV LG LP835 (CI-238CUP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240YWW","2TL2 33L FW MPL EZ1 PWS1836 LP840","2TL2 33L FW MPL EZ1 PWS1836 LP840 (CI-240YWW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241CV6","2TL2 33L FW SWL EZ1 LP840 N80","2TL2 33L FW SWL EZ1 LP840 N80 (CI-241CV6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239FMV","2TL2 33L FW SWL EZB LP835 N100","2TL2 33L FW SWL EZB LP835 N100 (CI-239FMV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235N57","2TL2 33L RW A19 EZ1 LP835 N80","2TL2 33L RW A19 EZ1 LP835 N80 (CI-235N57)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237PVN","2TL2 40L FW A12 EZ1 ABC LP830","2TL2 40L FW A12 EZ1 ABC LP830 (CI-237PVN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237PC6","2TL2 40L FW A12 EZ1 PWS1856LV LP835","2TL2 40L FW A12 EZ1 PWS1856LV LP835 (CI-237PC6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236U4F","2TL2 40L FW A12125 EZ1 LP840 N80","2TL2 40L FW A12125 EZ1 LP840 N80 (CI-236U4F)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239RWT","2TL2 40L FW A19 EZ1 PWS1836 LP835","2TL2 40L FW A19 EZ1 PWS1836 LP835 (CI-239RWT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238CVC","2TL2 40L FW MWS EZ1 LP835","2TL2 40L FW MWS EZ1 LP835 (CI-238CVC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237KT0","2TL2 40L FW SWL EZB ABCNG LP835 N80","2TL2 40L FW SWL EZB ABCNG LP835 N80 (CI-237KT0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241MM0","2TL2 40L RW A19 EZ1 PWS1856LV LP840","2TL2 40L RW A19 EZ1 PWS1856LV LP840 (CI-241MM0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245V6C","2TL2 40L RW SWL EZ1 LP850","2TL2 40L RW SWL EZ1 LP850 (CI-245V6C)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237GJ0","2TL4 30L FW A19 EZ1 LP835 N100","2TL4 30L FW A19 EZ1 LP835 N100 (CI-237GJ0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C7874,7)),6))","v":"238CV9"},{"$f":"LEFT(C7874,SEARCH(\"(CI-\",C7874)-2)","v":"2TL4 30L FW SWL EZ1 LP835"},"2TL4 30L FW SWL EZ1 LP835 (CI-238CV9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["243PCA","2TL4 30L RW A19 EZ1 LP840 N100","2TL4 30L RW A19 EZ1 LP840 N100 (CI-243PCA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236YR0","2TL4 40L FW A12 EZ1 LP840 N80EMG","2TL4 40L FW A12 EZ1 LP840 N80EMG (CI-236YR0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239E2M","2TL4 40L FW A12125 EZ1 LP830","2TL4 40L FW A12125 EZ1 LP830 (CI-239E2M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239U3T","2TL4 40L FW A19 EZ1 LP830","2TL4 40L FW A19 EZ1 LP830 (CI-239U3T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240J4C","2TL4 40L FW A19 EZB LP840","2TL4 40L FW A19 EZB LP840 (CI-240J4C)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236MYC","2TL4 40L FW MWS EZ1 LP840 N80","2TL4 40L FW MWS EZ1 LP840 N80 (CI-236MYC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245ULT","2TL4 40L RW A19 EZ1 PWS1856LV LP835","2TL4 40L RW A19 EZ1 PWS1856LV LP835 (CI-245ULT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232PTK","2TL4 48L FW A12 EZ1 LP835 N100EMG","2TL4 48L FW A12 EZ1 LP835 N100EMG (CI-232PTK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235XNU","2TL4 48L FW A12 EZB LP840","2TL4 48L FW A12 EZB LP840 (CI-235XNU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236ER3","2TL4 48L FW A12125 EZ1 PWS1836 LP835","2TL4 48L FW A12125 EZ1 PWS1836 LP835 (CI-236ER3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235HN9","2TL4 48L FW A19 EZ1 LP830 N80","2TL4 48L FW A19 EZ1 LP830 N80 (CI-235HN9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237V01","2TL4 48L FW A19 EZ1 PWS1836 LP830","2TL4 48L FW A19 EZ1 PWS1836 LP830 (CI-237V01)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["243P0Y","2TL4 48L FW MPL EZ1 LP840","2TL4 48L FW MPL EZ1 LP840 (CI-243P0Y)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239K3F","2TL4 48L FW SWL EZ1 ABC LP835","2TL4 48L FW SWL EZ1 ABC LP835 (CI-239K3F)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236X40","2TL4 48L RW SWL EZ1 LP835 N100EMG","2TL4 48L RW SWL EZ1 LP835 N100EMG (CI-236X40)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239LUU","2TL4 60L FW A12 EZ1 PWS1846 ABC LP835 N100EMG","2TL4 60L FW A12 EZ1 PWS1846 ABC LP835 N100EMG (CI-239LUU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236U4C","2TL4 60L FW A12125 EZ1 LP840 N80","2TL4 60L FW A12125 EZ1 LP840 N80 (CI-236U4C)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239P23","2TL4 60L FW A19V EZ1 ABC LP840","2TL4 60L FW A19V EZ1 ABC LP840 (CI-239P23)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240L0G","2TL4 60L RW A12 EZ1 LP840 N100","2TL4 60L RW A12 EZ1 LP840 N100 (CI-240L0G)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240UGR","2TL4 72L FW A12 EZ1 LP835 N80EMG","2TL4 72L FW A12 EZ1 LP835 N80EMG (CI-240UGR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239KWF","2TL4 72L FW A12V EZ1 ABC LP835","2TL4 72L FW A12V EZ1 ABC LP835 (CI-239KWF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235K9A","2TL4 72L FW A19 EZB LP835 N100","2TL4 72L FW A19 EZB LP835 N100 (CI-235K9A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235VGP","2TLX2 20L FW A19 EZ1 LP835","2TLX2 20L FW A19 EZ1 LP835 (CI-235VGP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236MNF","2TLX2 33L FW A12 EZ1 LP840 USPOM","2TLX2 33L FW A12 EZ1 LP840 USPOM (CI-236MNF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241CRV","2TLX2 33L RW A12 EZ1 LP835","2TLX2 33L RW A12 EZ1 LP835 (CI-241CRV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239W64","2TLX2 40L FW A12 EZB LP840","2TLX2 40L FW A12 EZB LP840 (CI-239W64)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235AHY","2TLX4 30L FW A12 EZ1 LP830","2TLX4 30L FW A12 EZ1 LP830 (CI-235AHY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240N1N","2TLX4 30L FW A19 EZ1 LP840","2TLX4 30L FW A19 EZ1 LP840 (CI-240N1N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237XTW","2TLX4 40L FW A12 EZB LP840","2TLX4 40L FW A12 EZB LP840 (CI-237XTW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245K1X","2TLX4 40L RW A19 EZ1 LP835 N100","2TLX4 40L RW A19 EZ1 LP835 N100 (CI-245K1X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237YVR","2TLX4 48L FW A12125V EZ1 LG LP840","2TLX4 48L FW A12125V EZ1 LG LP840 (CI-237YVR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236H4F","2TLX4 60L FW SWL EZ1 LP830","2TLX4 60L FW SWL EZ1 LP830 (CI-236H4F)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235UVX","2TLX4 72L FW A12 EZ1 LP850","2TLX4 72L FW A12 EZ1 LP850 (CI-235UVX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["247VMR","2TLX4 72L RW A12V EZ1 LP830 ABC","2TLX4 72L RW A12V EZ1 LP830 ABC (CI-247VMR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236NW9","TL4 20L FW A19 EZ1 LP840","TL4 20L FW A19 EZ1 LP840 (CI-236NW9)","PS1050","3 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["236LU6","TL4 20L RW A12 EZ1 LP835","TL4 20L RW A12 EZ1 LP835 (CI-236LU6)","PS1050","3 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["239E9G","TL4 30L FW A19 EZ1 LP830","TL4 30L FW A19 EZ1 LP830 (CI-239E9G)","PS1050","3 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["239LXM","TL4 30L FW MWS EZ1 PWS1836 LP835","TL4 30L FW MWS EZ1 PWS1836 LP835 (CI-239LXM)","PS1050","3 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["237AMP","TL4 40L FW A12 EZ1 LP840 N80EMG","TL4 40L FW A12 EZ1 LP840 N80EMG (CI-237AMP)","PS1050","3 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["236G6U","TL4 40L RW A12125 EZ1 LP840","TL4 40L RW A12125 EZ1 LP840 (CI-236G6U)","PS1050","3 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["237GWC","TL4 48L FW A12 EZ1 LP835 N80EMG","TL4 48L FW A12 EZ1 LP835 N80EMG (CI-237GWC)","PS1050","3 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["237UYF","TL4 48L RW A12 EZ1 LP840","TL4 48L RW A12 EZ1 LP840 (CI-237UYF)","PS1050","3 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["240LRV","TL4 60L FW MWS EZ1 LP840 N80","TL4 60L FW MWS EZ1 LP840 N80 (CI-240LRV)","PS1050","3 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["235AFL","TL4 F 40L FW A19 EZ1 LP840","TL4 F 40L FW A19 EZ1 LP840 (CI-235AFL)","PS1050","3 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["227YJ6","2VTL2 20L ADP EZ1 LP835 CP","2VTL2 20L ADP EZ1 LP835 CP (CI-227YJ6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225P14","2VTL2 20L ADP EZ1 LP840 N100","2VTL2 20L ADP EZ1 LP840 N100 (CI-225P14)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225HW6","2VTL2 20L ADP EZ1 PWS1836 LP835","2VTL2 20L ADP EZ1 PWS1836 LP835 (CI-225HW6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229TT6","2VTL2 20L ADP SLD PWS1846 LP835","2VTL2 20L ADP SLD PWS1846 LP835 (CI-229TT6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231L8P","2VTL2 33L ADP 277 EZ1 QFC313GX LP835 CLO NAKD","2VTL2 33L ADP 277 EZ1 QFC313GX LP835 CLO NAKD (CI-231L8P)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226PVC","2VTL2 33L ADP EZ1 LP835 N100 USPOM","2VTL2 33L ADP EZ1 LP835 N100 USPOM (CI-226PVC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230VW7","2VTL2 33L ADP EZ1 LP840 N100 DWAM","2VTL2 33L ADP EZ1 LP840 N100 DWAM (CI-230VW7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227UUX","2VTL2 33L ADP EZ1 PWS1836 LP830","2VTL2 33L ADP EZ1 PWS1836 LP830 (CI-227UUX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233LCT","2VTL2 33L ADP EZ1 PWS1836 LP850","2VTL2 33L ADP EZ1 PWS1836 LP850 (CI-233LCT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233NVE","2VTL2 33L ADP EZB LP830","2VTL2 33L ADP EZB LP830 (CI-233NVE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233U75","2VTL2 33L ADP EZB PWS1856LV LP830","2VTL2 33L ADP EZB PWS1856LV LP830 (CI-233U75)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["224VU3","2VTL2 40L ADP EZ1 LP840 N100","2VTL2 40L ADP EZ1 LP840 N100 (CI-224VU3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233GKN","2VTL2 40L ADP EZ1 PWS1436 LP835","2VTL2 40L ADP EZ1 PWS1436 LP835 (CI-233GKN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226PWY","2VTL2 40L ADP EZB LP830","2VTL2 40L ADP EZB LP830 (CI-226PWY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230GE8","2VTL2 40L ADP SLD LP830","2VTL2 40L ADP SLD LP830 (CI-230GE8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231HL5","2VTL2 H 40L ADP EZ1 LP830","2VTL2 H 40L ADP EZ1 LP830 (CI-231HL5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229HK9","2VTL2 H 40L ADP EZB LP835 N100","2VTL2 H 40L ADP EZB LP835 N100 (CI-229HK9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232PXP","2VTL2R 20L ADP EZ1 LP835 N80","2VTL2R 20L ADP EZ1 LP835 N80 (CI-232PXP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225EF2","2VTL2R 23L ADP D25 LP835 BLD","2VTL2R 23L ADP D25 LP835 BLD (CI-225EF2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232F24","2VTL2R 33L ADP EZ1 LP830 JP24","2VTL2R 33L ADP EZ1 LP830 JP24 (CI-232F24)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C8642,7)),6))","v":"228Y69"},{"$f":"LEFT(C8642,SEARCH(\"(CI-\",C8642)-2)","v":"2VTL2R 33L ADP EZ1 LP835 JP24"},"2VTL2R 33L ADP EZ1 LP835 JP24 (CI-228Y69)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234JJK","2VTL2R 40L ADP EZ1 LP840 N100","2VTL2R 40L ADP EZ1 LP840 N100 (CI-234JJK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228GG7","2VTL2RF 33L ADP GZ LP835","2VTL2RF 33L ADP GZ LP835 (CI-228GG7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229UAF","2VTL2RT 20L ADP GTH250 LP850","2VTL2RT 20L ADP GTH250 LP850 (CI-229UAF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["223TN3","2VTL2RT 23L ADP D25 LP840 NX","2VTL2RT 23L ADP D25 LP840 NX (CI-223TN3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226UN1","2VTL2RT 33L ADP D37 LP850 NX","2VTL2RT 33L ADP D37 LP850 NX (CI-226UN1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234TLV","2VTL2RT 33L ADP EZ1 LP850 JP24","2VTL2RT 33L ADP EZ1 LP850 JP24 (CI-234TLV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232PN5","2VTL4 30L ADP EZ1 LP830 N80","2VTL4 30L ADP EZ1 LP830 N80 (CI-232PN5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225A1U","2VTL4 30L ADP EZ1 LP835","2VTL4 30L ADP EZ1 LP835 (CI-225A1U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233JR8","2VTL4 30L ADP EZ1 PWS1856LV LP835","2VTL4 30L ADP EZ1 PWS1856LV LP835 (CI-233JR8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233FA3","2VTL4 40L ADP 120 EZ1 GMF LP835","2VTL4 40L ADP 120 EZ1 GMF LP835 (CI-233FA3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234C4M","2VTL4 40L ADP EZ1 LP835 MB RFD191137","2VTL4 40L ADP EZ1 LP835 MB RFD191137 (CI-234C4M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230WF5","2VTL4 40L ADP EZ1 LP840 N80 JP18 RFD181786","2VTL4 40L ADP EZ1 LP840 N80 JP18 RFD181786 (CI-230WF5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232T62","2VTL4 40L ADP EZ1 PWS1436 LP835 N100","2VTL4 40L ADP EZ1 PWS1436 LP835 N100 (CI-232T62)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225HFN","2VTL4 40L ADP EZ1 PWS1856LV LP840","2VTL4 40L ADP EZ1 PWS1856LV LP840 (CI-225HFN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225M69","2VTL4 48L ADP 277 EZ1 LP835 N100 GLR RFD151939","2VTL4 48L ADP 277 EZ1 LP835 N100 GLR RFD151939 (CI-225M69)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230VYK","2VTL4 48L ADP 277 EZ1 QFC211GA LP835","2VTL4 48L ADP 277 EZ1 QFC211GA LP835 (CI-230VYK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231MXW","2VTL4 48L ADP EZ1 LP840 N100 USPOM","2VTL4 48L ADP EZ1 LP840 N100 USPOM (CI-231MXW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231P6K","2VTL4 48L ADP EZ1 LP850 N80 USPOM","2VTL4 48L ADP EZ1 LP850 N80 USPOM (CI-231P6K)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226NFU","2VTL4 48L ADP EZ1 PWS1836 LP850 N80 USPOM","2VTL4 48L ADP EZ1 PWS1836 LP850 N80 USPOM (CI-226NFU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["224VCE","2VTL4 48L ADP EZB LP835","2VTL4 48L ADP EZB LP835 (CI-224VCE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228A3R","2VTL4 48L ADP SLD PWS1846 LP835","2VTL4 48L ADP SLD PWS1846 LP835 (CI-228A3R)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["226GPV","2VTL4 60L ADP EZ1 LP835 CP","2VTL4 60L ADP EZ1 LP835 CP (CI-226GPV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["231U89","2VTL4 60L ADP EZB LP835 N80","2VTL4 60L ADP EZB LP835 N80 (CI-231U89)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234KGU","2VTL4 60L ADP EZB LP850 N80","2VTL4 60L ADP EZB LP850 N80 (CI-234KGU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225XK3","2VTL4 72L ADP EZ1 LP835 N80 RRLC12S NAKD","2VTL4 72L ADP EZ1 LP835 N80 RRLC12S NAKD (CI-225XK3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230X12","2VTL4 72L ADP EZ1 PWS1436 LP835","2VTL4 72L ADP EZ1 PWS1436 LP835 (CI-230X12)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230KXG","2VTL4 72L ADP EZB LP835","2VTL4 72L ADP EZB LP835 (CI-230KXG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228C3H","2VTL4 72L ADP SLD PWS1846 LP835","2VTL4 72L ADP SLD PWS1846 LP835 (CI-228C3H)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225TH2","2VTL4 H 48L ADP EZ1 LP835","2VTL4 H 48L ADP EZ1 LP835 (CI-225TH2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229VLP","2VTL4 H 72L ADP EZ1 LP835","2VTL4 H 72L ADP EZ1 LP835 (CI-229VLP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["220YWJ","2VTL4R 39L ADP D43 LP835 N80 NAKD","2VTL4R 39L ADP D43 LP835 N80 NAKD (CI-220YWJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["221XL4","2VTL4R 39L ADP D43 LP835 N80 NAKD JP12","2VTL4R 39L ADP D43 LP835 N80 NAKD JP12 (CI-221XL4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230KMM","2VTL4R 40L ADP EZ1 LP840 JP12","2VTL4R 40L ADP EZ1 LP840 JP12 (CI-230KMM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229PEW","2VTL4R 40L ADP EZB LP835 JP12","2VTL4R 40L ADP EZB LP835 JP12 (CI-229PEW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230KM3","2VTL4R 40L ADP GZ LP840 JP12","2VTL4R 40L ADP GZ LP840 JP12 (CI-230KM3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["223AYX","2VTL4R 45L ADP D49 LP840 N80","2VTL4R 45L ADP D49 LP840 N80 (CI-223AYX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230WF0","2VTL4R 48L ADP EZ1 LP850","2VTL4R 48L ADP EZ1 LP850 (CI-230WF0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229KAK","2VTL4R 60L ADP EZ1 LP840","2VTL4R 60L ADP EZ1 LP840 (CI-229KAK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230CRN","2VTL4RT 30L ADP EZ1 LP840","2VTL4RT 30L ADP EZ1 LP840 (CI-230CRN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230CRW","2VTL4RT 30L ADP EZ1 LP840 JP12","2VTL4RT 30L ADP EZ1 LP840 JP12 (CI-230CRW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233GE6","2VTL4RT 40L ADP EZ1 LP830","2VTL4RT 40L ADP EZ1 LP830 (CI-233GE6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228XMV","2VTL4RT 40L ADP EZ1 LP840 N100 JP12","2VTL4RT 40L ADP EZ1 LP840 N100 JP12 (CI-228XMV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229PFP","2VTL4RT 40L ADP GZ LP840 JP12","2VTL4RT 40L ADP GZ LP840 JP12 (CI-229PFP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228FWH","2VTL4RT 45L ADP D49 LP840 N80","2VTL4RT 45L ADP D49 LP840 N80 (CI-228FWH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229L84","2VTL4RT 48L ADP EZ1 LP840 N100","2VTL4RT 48L ADP EZ1 LP840 N100 (CI-229L84)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229UAU","2VTL4RT 48L ADP GTH250 LP850","2VTL4RT 48L ADP GTH250 LP850 (CI-229UAU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234RAG","2VTL4RT 60L ADP GTH250 LP840 JP12","2VTL4RT 60L ADP GTH250 LP840 JP12 (CI-234RAG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228EU8","2VTLX2 20L ADP EZ1 LP830","2VTLX2 20L ADP EZ1 LP830 (CI-228EU8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231FP5","2VTLX2 33L ADP EZ1 LP840 N80","2VTLX2 33L ADP EZ1 LP840 N80 (CI-231FP5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228FU3","2VTLX2 40L ADP EZ1 LP835","2VTLX2 40L ADP EZ1 LP835 (CI-228FU3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226XRH","2VTLX4 24L ADP D24 LP835 NX","2VTLX4 24L ADP D24 LP835 NX (CI-226XRH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226FA5","2VTLX4 40L ADP D40 LP835 NX","2VTLX4 40L ADP D40 LP835 NX (CI-226FA5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234JG6","2VTLX4 40L ADP SLD LP835","2VTLX4 40L ADP SLD LP835 (CI-234JG6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230NLH","2VTLX4 48L ADP EZ1 LP835 USPOM","2VTLX4 48L ADP EZ1 LP835 USPOM (CI-230NLH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225M31","2VTLX4 72L ADP D75 LP850 NX","2VTLX4 72L ADP D75 LP850 NX (CI-225M31)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234T34","2VTLX4 72L ADP EZB LP835","2VTLX4 72L ADP EZB LP835 (CI-234T34)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231WGW","VTL4 20L ADP EZB LP835","VTL4 20L ADP EZB LP835 (CI-231WGW)","PS1050","6 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series instructions","*239MRJ","*239MRC"]
["229TTY","VTL4 40L ADP EZ1 LP835","VTL4 40L ADP EZ1 LP835 (CI-229TTY)","PS1050","6 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series instructions","*239MRJ","*239MRC"]
["231YH4","VTL4 40L ADP EZ1 LP935","VTL4 40L ADP EZ1 LP935 (CI-231YH4)","PS1050","6 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series instructions","*239MRJ","*239MRC"]
["232PRK","VTL4 48L ADP EZ1 LP835 CP","VTL4 48L ADP EZ1 LP835 CP (CI-232PRK)","PS1050","6 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series instructions","*239MRJ","*239MRC"]
["241HFE","2VTL2 20L ADP EZ1 LP835 MMC JP24","2VTL2 20L ADP EZ1 LP835 MMC JP24 (CI-241HFE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232NMV","2VTL2 20L ADP EZ1 LP840 N80EMG USPOM","2VTL2 20L ADP EZ1 LP840 N80EMG USPOM (CI-232NMV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235CUJ","2VTL2 20L ADPT EZ1 LP835 N100 NESPDT7","2VTL2 20L ADPT EZ1 LP835 N100 NESPDT7 (CI-235CUJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229GR6","2VTL2 33L ADP 120 EZB LP835 N100 CS1WL10 SSQ","2VTL2 33L ADP 120 EZB LP835 N100 CS1WL10 SSQ (CI-229GR6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["241G61","2VTL2 33L ADP EZ1 PWS1436 LP830","2VTL2 33L ADP EZ1 PWS1436 LP830 (CI-241G61)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236A7N","2VTL2 33L ADP EZB RRLA LP835","2VTL2 33L ADP EZB RRLA LP835 (CI-236A7N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235M7T","2VTL2 33L ADPT EZ1 LP835 N100 NESPDT7","2VTL2 33L ADPT EZ1 LP835 N100 NESPDT7 (CI-235M7T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235U1R","2VTL2 33L ADPT EZ1 PWS1836 LP835 MSD7ADCX","2VTL2 33L ADPT EZ1 PWS1836 LP835 MSD7ADCX (CI-235U1R)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230GNT","2VTL2 40L ADP EDB LP840","2VTL2 40L ADP EDB LP840 (CI-230GNT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226GLU","2VTL2 40L ADP EZ1 LP840 N100EMG","2VTL2 40L ADP EZ1 LP840 N100EMG (CI-226GLU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235CVT","2VTL2 40L ADP EZ1 PWS1856LV LP830","2VTL2 40L ADP EZ1 PWS1856LV LP830 (CI-235CVT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236KXE","2VTL2 40L ADP EZB RRLA LP835","2VTL2 40L ADP EZB RRLA LP835 (CI-236KXE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["238PA9","2VTL2 40L ADPT EZ1 LP850","2VTL2 40L ADPT EZ1 LP850 (CI-238PA9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["238HEE","2VTL2 H 33L ADP EZ1 LP835 N100EMG","2VTL2 H 33L ADP EZ1 LP835 N100EMG (CI-238HEE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231MLJ","2VTL2 H 40L ADP EZ1 LP835 N80EMG","2VTL2 H 40L ADP EZ1 LP835 N80EMG (CI-231MLJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237J64","2VTL2R 20L ADP EZ1 LP840 USPOM JP24","2VTL2R 20L ADP EZ1 LP840 USPOM JP24 (CI-237J64)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236VX2","2VTL2R 40L ADP EZ1 LP835 N100","2VTL2R 40L ADP EZ1 LP835 N100 (CI-236VX2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["238NF7","2VTL2RT 20L ADP EZ1 LP840 N100 JP24","2VTL2RT 20L ADP EZ1 LP840 N100 JP24 (CI-238NF7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235PLR","2VTL4 30L ADP 120 EZ1 GLR PWS1846 LP840","2VTL4 30L ADP 120 EZ1 GLR PWS1846 LP840 (CI-235PLR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237CCV","2VTL4 30L ADP EZ1 LP840 USPOM","2VTL4 30L ADP EZ1 LP840 USPOM (CI-237CCV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238F8C","2VTL4 30L ADPT EZ1 PWS1856LV LP835","2VTL4 30L ADPT EZ1 PWS1856LV LP835 (CI-238F8C)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239LHF","2VTL4 40L ADP EZ1 LP835 N100 MMC JP12","2VTL4 40L ADP EZ1 LP835 N100 MMC JP12 (CI-239LHF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["225LCF","2VTL4 40L ADP EZ1 LP835 N100EMG","2VTL4 40L ADP EZ1 LP835 N100EMG (CI-225LCF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235JT2","2VTL4 40L ADP EZB LP850","2VTL4 40L ADP EZB LP850 (CI-235JT2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235XC0","2VTL4 40L ADPT EZ1 LP835","2VTL4 40L ADPT EZ1 LP835 (CI-235XC0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235EUE","2VTL4 40L ADPT EZ1 LP835 N80 NESPDT7ADCX","2VTL4 40L ADPT EZ1 LP835 N80 NESPDT7ADCX (CI-235EUE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235CKR","2VTL4 48L ADP 120 EZ1 GLR LP835","2VTL4 48L ADP 120 EZ1 GLR LP835 (CI-235CKR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235E03","2VTL4 48L ADP EDB LP840","2VTL4 48L ADP EDB LP840 (CI-235E03)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235VG4","2VTL4 48L ADP EZ1 PWS1836 LP850 N100","2VTL4 48L ADP EZ1 PWS1836 LP850 N100 (CI-235VG4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235MUU","2VTL4 48L ADP EZB PWS1856LV LP840","2VTL4 48L ADP EZB PWS1856LV LP840 (CI-235MUU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237T29","2VTL4 48L ADPT EZ1 LP835 N80 NESPDT7ADCX","2VTL4 48L ADPT EZ1 LP835 N80 NESPDT7ADCX (CI-237T29)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240GMU","2VTL4 48L ADPT SLD PWS1846 LP835","2VTL4 48L ADPT SLD PWS1846 LP835 (CI-240GMU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["241VCX","2VTL4 60L ADP EZ1 PWS1836 LP835 N100","2VTL4 60L ADP EZ1 PWS1836 LP835 N100 (CI-241VCX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228ELX","2VTL4 60L ADP EZB LP840","2VTL4 60L ADP EZB LP840 (CI-228ELX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240XW1","2VTL4 60L ADPT EZ1 LP850","2VTL4 60L ADPT EZ1 LP850 (CI-240XW1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245JJ6","2VTL4 72L ADP 277 EZ1 GLR PWS1436 LP835 N100","2VTL4 72L ADP 277 EZ1 GLR PWS1436 LP835 N100 (CI-245JJ6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236C5T","2VTL4 72L ADP EZ1 LP850 N100EMG","2VTL4 72L ADP EZ1 LP850 N100EMG (CI-236C5T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239F92","2VTL4 H 30L ADP EZ1 PWS1856LV LP840","2VTL4 H 30L ADP EZ1 PWS1856LV LP840 (CI-239F92)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236FAV","2VTL4 H 40L ADP EZB LP835","2VTL4 H 40L ADP EZB LP835 (CI-236FAV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236L3A","2VTL4  H 40L ADP LE1 LP840","2VTL4  H 40L ADP LE1 LP840 (CI-236L3A)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235VW3","2VTL4R 40L ADP EZ1 LP835 N100 JP12","2VTL4R 40L ADP EZ1 LP835 N100 JP12 (CI-235VW3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238C1N","2VTL4R 60L ADP EZ1 LP830","2VTL4R 60L ADP EZ1 LP830 (CI-238C1N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["228VA3","2VTL4RT 40L ADP EZ1 LP840 N80 JP12","2VTL4RT 40L ADP EZ1 LP840 N80 JP12 (CI-228VA3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236ATL","2VTL4RT 60L ADP EZ1 LP835 JP12","2VTL4RT 60L ADP EZ1 LP835 JP12 (CI-236ATL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["237FMV","2VTLX2 33L ADP EZ1 LP850","2VTLX2 33L ADP EZ1 LP850 (CI-237FMV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237MR8","2VTLX4 40L ADP SLD LP840","2VTLX4 40L ADP SLD LP840 (CI-237MR8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240R2R","2VTLX4 60L ADP SLD LP830","2VTLX4 60L ADP SLD LP830 (CI-240R2R)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237LK6","VTL4 20L ADP EZ1 PWS1856LV LP835","VTL4 20L ADP EZ1 PWS1856LV LP835 (CI-237LK6)","PS1050","6 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series instructions","*239MRJ","*239MRC"]
["238HLW","VTL4 30L ADP EZ1 LP850","VTL4 30L ADP EZ1 LP850 (CI-238HLW)","PS1050","6 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series instructions","*239MRJ","*239MRC"]
["240P5R","VTL4 40L ADP EZ1 PWS1856LV LP835","VTL4 40L ADP EZ1 PWS1856LV LP835 (CI-240P5R)","PS1050","6 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series instructions","*239MRJ","*239MRC"]
["240HGW","VTL4 48L ADP EZB LP835","VTL4 48L ADP EZB LP835 (CI-240HGW)","PS1050","6 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series instructions","*239MRJ","*239MRC"]
["235XU2","VTL4 60L ADP EZB LP835","VTL4 60L ADP EZB LP835 (CI-235XU2)","PS1050","6 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series instructions","*239MRJ","*239MRC"]
["233TCK","LBL4 30L EOHN LP835","LBL4 30L EOHN LP835 (CI-233TCK)","PS1050","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["231LUW","LBL4 40L EZ1 LP850","LBL4 40L EZ1 LP850 (CI-231LUW)","PS1050","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["234RYL","LBL4 48L EZ1 LP840 LSXR10","LBL4 48L EZ1 LP840 LSXR10 (CI-234RYL)","PS1050","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["233NUM","LBL4 72L EOHN LP835","LBL4 72L EOHN LP835 (CI-233NUM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["217X9T","LBL4 LP840","LBL4 LP840 (CI-217X9T)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["234F3E","LBL4W 80L EOHN LP850","LBL4W 80L EOHN LP850 (CI-234F3E)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["238CCF","LBL2 20L EZ1 LP840 LSXRHL","LBL2 20L EZ1 LP840 LSXRHL (CI-238CCF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C10076,7)),6))","v":"241KP4"},{"$f":"LEFT(C10076,SEARCH(\"(CI-\",C10076)-2)","v":"LBL4 30L EZ1 LP830 N80"},"LBL4 30L EZ1 LP830 N80 (CI-241KP4)","PS1050","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["238YTJ","LBL4 40L EZ1 LP830 LSXR10","LBL4 40L EZ1 LP830 LSXR10 (CI-238YTJ)","PS1050","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["237NNW","LBL4 48L EZ1 LP850 N80","LBL4 48L EZ1 LP850 N80 (CI-237NNW)","PS1050","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ","*239MRC"]
["238G8L","LBL4 60L EZ1 LP850 LSXR10","LBL4 60L EZ1 LP850 LSXR10 (CI-238G8L)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235KXC","LBL4W 80L EZ1 LP830","LBL4W 80L EZ1 LP830 (CI-235KXC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232N0P","STL2 20L EZ1 LP835 DUP CODE","STL2 20L EZ1 LP835 DUP CODE (CI-232N0P)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233R8N","STL2 20L EZ1 LP840 N80","STL2 20L EZ1 LP840 N80 (CI-233R8N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227C36","STL2 20L EZB LP840 XADNS7","STL2 20L EZB LP840 XADNS7 (CI-227C36)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["217JV1","STL2 22L D26 LP835 N100 RFD123358","STL2 22L D26 LP835 N100 RFD123358 (CI-217JV1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["224HLL","STL2 22L D26 LP840 NX USPOM","STL2 22L D26 LP840 NX USPOM (CI-224HLL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232PT8","STL4 20L EZ1 LP840 DNA","STL4 20L EZ1 LP840 DNA (CI-232PT8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232AYG","STL4 30L EZ1 LP835 SC1","STL4 30L EZ1 LP835 SC1 (CI-232AYG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233YPK","STL4 30L EZB LP835 N80","STL4 30L EZB LP835 N80 (CI-233YPK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["218XXA","STL4 40L D40 LP835 N100","STL4 40L D40 LP835 N100 (CI-218XXA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["229AMA","STL4 40L D40 LP840 N100 USPOM","STL4 40L D40 LP840 N100 USPOM (CI-229AMA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230UYM","STL4 40L EZ1 LP830","STL4 40L EZ1 LP830 (CI-230UYM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C10268,7)),6))","v":"230M2X"},{"$f":"LEFT(C10268,SEARCH(\"(CI-\",C10268)-2)","v":"STL4 40L EZ1 LP835 N100"},"STL4 40L EZ1 LP835 N100 (CI-230M2X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233WWF","STL4 40L EZ1 LP840 DNA SC2","STL4 40L EZ1 LP840 DNA SC2 (CI-233WWF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232WLN","STL4 48L 277 EZ1 GLR LP840","STL4 48L 277 EZ1 GLR LP840 (CI-232WLN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["220H0U","STL4 48L D50 LP835 DNA BLD","STL4 48L D50 LP835 DNA BLD (CI-220H0U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["219GL1","STL4 48L D50 LP840 BLD","STL4 48L D50 LP840 BLD (CI-219GL1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C10332,7)),6))","v":"222FV2"},{"$f":"LEFT(C10332,SEARCH(\"(CI-\",C10332)-2)","v":"STL4 48L D50 LP840 NX RFD156301"},"STL4 48L D50 LP840 NX RFD156301 (CI-222FV2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["217XM8","STL4 48L D50 LP850 NX USPOM","STL4 48L D50 LP850 NX USPOM (CI-217XM8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["230W9K","STL4 48L EZ1 LP835 N100 SC1","STL4 48L EZ1 LP835 N100 SC1 (CI-230W9K)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233MM4","STL4 48L EZ1 LP840 LSXRHL","STL4 48L EZ1 LP840 LSXRHL (CI-233MM4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["233LP3","STL4 48L EZB LP835 DNA","STL4 48L EZB LP835 DNA (CI-233LP3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["234J2N","STL4 60L EZ1 LP840 SC1","STL4 60L EZ1 LP840 SC1 (CI-234J2N)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["245UM4","STL2 20L EZ1 LP840 NOM N80 SC1","STL2 20L EZ1 LP840 NOM N80 SC1 (CI-245UM4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237J4C","STL2 40L EZ1 LP835 LSXRHL SC1","STL2 40L EZ1 LP835 LSXRHL SC1 (CI-237J4C)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["247U9K","STL2 40L EZ1 LP840 N80 SC1","STL2 40L EZ1 LP840 N80 SC1 (CI-247U9K)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237U1K","STL4 20L EZ1 LP840 SC2","STL4 20L EZ1 LP840 SC2 (CI-237U1K)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239E8L","STL4 30L EZ1 LP830 N100","STL4 30L EZ1 LP830 N100 (CI-239E8L)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239WAG","STL4 30L EZ1 LP850 N100EMG","STL4 30L EZ1 LP850 N100EMG (CI-239WAG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["239LAN","STL4 40L EXA1 LP850","STL4 40L EXA1 LP850 (CI-239LAN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236TRX","STL4 40L EZB LP835 DNA","STL4 40L EZB LP835 DNA (CI-236TRX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["235VGH","STL4 48L EZ1 LP830 N100","STL4 48L EZ1 LP830 N100 (CI-235VGH)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236U4X","STL4 48L EZ1 LP840 N100 USPOM","STL4 48L EZ1 LP840 N100 USPOM (CI-236U4X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C10524,7)),6))","v":"236APY"},{"$f":"LEFT(C10524,SEARCH(\"(CI-\",C10524)-2)","v":"STL4 48L EZ1 LP850 LSXRHL SC1"},"STL4 48L EZ1 LP850 LSXRHL SC1 (CI-236APY)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["240KAT","STL4 60L EZ1 LP835 USPOM","STL4 60L EZ1 LP835 USPOM (CI-240KAT)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["236JRK","STL4 60L EZB LP830","STL4 60L EZB LP830 (CI-236JRK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series & 2 Boards in parallel instructions","*239MRJ"]
["232RJU","WL2 08L EZ1 LP835 N80 NES7","WL2 08L EZ1 LP835 N80 NES7 (CI-232RJU)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["226G9K","WL2 12L D13 277 LP835 NX GMF","WL2 12L D13 277 LP835 NX GMF (CI-226G9K)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["217F8R","WL2 12L D13 LP840 N100","WL2 12L D13 LP840 N100 (CI-217F8R)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["229A13","WL2 12L EZ1 LP830 DUP","WL2 12L EZ1 LP830 DUP (CI-229A13)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["225M9F","WL2 12L EZ1 LP835 DUP","WL2 12L EZ1 LP835 DUP (CI-225M9F)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["229P8J","WL2 12L EZ1 LP835 SC","WL2 12L EZ1 LP835 SC (CI-229P8J)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["229L6U","WL2 12L EZ1 LP840 N100 NES7 DIM10 DUP","WL2 12L EZ1 LP840 N100 NES7 DIM10 DUP (CI-229L6U)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["229L3E","WL2 12L EZ1 LP840 SC DUP","WL2 12L EZ1 LP840 SC DUP (CI-229L3E)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["233MT5","WL2 12L SLD LP835","WL2 12L SLD LP835 (CI-233MT5)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["224V3K","WL2 18L D20 LP835 N100 NES7ADCX","WL2 18L D20 LP835 N100 NES7ADCX (CI-224V3K)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["220P36","WL2 18L D20 LP840 N100 NESPDT7 DIM10 SC","WL2 18L D20 LP840 N100 NESPDT7 DIM10 SC (CI-220P36)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["221F29","WL2 18L D20 LP840 NX SC","WL2 18L D20 LP840 NX SC (CI-221F29)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["230JLE","WL2 18L EZ1 LP830 N80 NESPDT7","WL2 18L EZ1 LP830 N80 NESPDT7 (CI-230JLE)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["228LCE","WL2 18L EZ1 LP835 N100 NESPDT7 DUP","WL2 18L EZ1 LP835 N100 NESPDT7 DUP (CI-228LCE)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["231NXR","WL2 18L EZ1 LP840","WL2 18L EZ1 LP840 (CI-231NXR)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["230J4R","WL2 18L EZ1 LP840 N100 NES7 DIM50 SC","WL2 18L EZ1 LP840 N100 NES7 DIM50 SC (CI-230J4R)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["231P0V","WL2 18L EZ1 LP840 N80 NESPDT7 DIM50","WL2 18L EZ1 LP840 N80 NESPDT7 DIM50 (CI-231P0V)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["230ER3","WL2 18L EZ1 LP850 N100 NES7","WL2 18L EZ1 LP850 N100 NES7 (CI-230ER3)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
[{"$f":"(LEFT((RIGHT(C10780,7)),6))","v":"231F24"},{"$f":"LEFT(C10780,SEARCH(\"(CI-\",C10780)-2)","v":"WL2 22L EZ1 LP840 MSD7 DIM10 SC"},"WL2 22L EZ1 LP840 MSD7 DIM10 SC (CI-231F24)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["229U64","WL4 20L EZ1 LP830","WL4 20L EZ1 LP830 (CI-229U64)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231AP8","WL4 20L EZ1 LP835 N100 NES7 DIM50","WL4 20L EZ1 LP835 N100 NES7 DIM50 (CI-231AP8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232JWA","WL4 20L EZ1 LP840 MSD7 DIM10","WL4 20L EZ1 LP840 MSD7 DIM10 (CI-232JWA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["229MX2","WL4 20L EZ1 LP840 N100 NESPDT7 DIM10 SC","WL4 20L EZ1 LP840 N100 NESPDT7 DIM10 SC (CI-229MX2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233URA","WL4 20L EZ1 LP850 MSD7 DIM50","WL4 20L EZ1 LP850 MSD7 DIM50 (CI-233URA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["221TFC","WL4 25L D24 LP830 N100","WL4 25L D24 LP830 N100 (CI-221TFC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["215AF3","WL4 25L D24 LP835 N100","WL4 25L D24 LP835 N100 (CI-215AF3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["223LCG","WL4 25L D24 LP835 N100 NESPDT7 DIM50 SQC","WL4 25L D24 LP835 N100 NESPDT7 DIM50 SQC (CI-223LCG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["218KHW","WL4 25L D24 LP835 NIO LED LC N100 3V FW14 RFD138260","WL4 25L D24 LP835 NIO LED LC N100 3V FW14 RFD138260 (CI-218KHW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["215L4T","WL4 25L D24 LP840 N100 NES7 DIM10 USPOM","WL4 25L D24 LP840 N100 NES7 DIM10 USPOM (CI-215L4T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["225W4U","WL4 25L D24 LP840 N80 NES7 DIM50 USPOM","WL4 25L D24 LP840 N80 NES7 DIM50 USPOM (CI-225W4U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["221FTX","WL4 25L D24 LP840 N80 NESPDT7 DIM50 SC","WL4 25L D24 LP840 N80 NESPDT7 DIM50 SC (CI-221FTX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["219MN0","WL4 25L D24 LP850 N100 NES7ADCX DIM50","WL4 25L D24 LP850 N100 NES7ADCX DIM50 (CI-219MN0)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233L63","WL4 30L EZ1 LP830 N100 NES7ADCX DIM50","WL4 30L EZ1 LP830 N100 NES7ADCX DIM50 (CI-233L63)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["233J9X","WL4 30L EZ1 LP835 MSD7","WL4 30L EZ1 LP835 MSD7 (CI-233J9X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228P61","WL4 30L EZ1 LP835 N100 NESPDT7","WL4 30L EZ1 LP835 N100 NESPDT7 (CI-228P61)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232C2T","WL4 30L EZ1 LP835 SC RFD186875","WL4 30L EZ1 LP835 SC RFD186875 (CI-232C2T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234R4K","WL4 30L EZ1 LP840 N100 NES7 SC","WL4 30L EZ1 LP840 N100 NES7 SC (CI-234R4K)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232K9E","WL4 30L EZ1 LP840 N80 NES7 DIM50 SC","WL4 30L EZ1 LP840 N80 NES7 DIM50 SC (CI-232K9E)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234PVC","WL4 30L EZ1 LP840 XADNS7 DIM50","WL4 30L EZ1 LP840 XADNS7 DIM50 (CI-234PVC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232W29","WL4 30L EZB LP830 N100 NES7","WL4 30L EZB LP830 N100 NES7 (CI-232W29)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228HUA","WL4 30L SLD LP840","WL4 30L SLD LP840 (CI-228HUA)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230CUG","WL4 40L EZ1 LP830 N100 NESPDT7 DIM50","WL4 40L EZ1 LP830 N100 NESPDT7 DIM50 (CI-230CUG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228NN9","WL4 40L EZ1 LP835 N100 NES7 DIM10","WL4 40L EZ1 LP835 N100 NES7 DIM10 (CI-228NN9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["232Y0T","WL4 40L EZ1 LP835 N80 NESPDT7","WL4 40L EZ1 LP835 N80 NESPDT7 (CI-232Y0T)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231CCF","WL4 40L EZ1 LP840 MSD7 DIM10","WL4 40L EZ1 LP840 MSD7 DIM10 (CI-231CCF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228NA3","WL4 40L EZ1 LP840 N100 NES7ADCX DIM10","WL4 40L EZ1 LP840 N100 NES7ADCX DIM10 (CI-228NA3)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["231HH8","WL4 40L EZ1 LP840 N100 NESPDT7 DIM50 SC","WL4 40L EZ1 LP840 N100 NESPDT7 DIM50 SC (CI-231HH8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230VGX","WL4 40L EZ1 LP840 N80 NES7ADCX DIM50 SC","WL4 40L EZ1 LP840 N80 NES7ADCX DIM50 SC (CI-230VGX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227HEW","WL4 40L EZ1 LP840 SC","WL4 40L EZ1 LP840 SC (CI-227HEW)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["234HGU","WL4 40L EZ1 LP850 N100 NESPDT7","WL4 40L EZ1 LP850 N100 NESPDT7 (CI-234HGU)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230X58","WL4 40L EZB LP835 N100 NES7","WL4 40L EZB LP835 N100 NES7 (CI-230X58)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["216RHM","WL4 41L D43 LP835 N100","WL4 41L D43 LP835 N100 (CI-216RHM)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["222EAK","WL4 41L D43 LP835 N100 NES7ADCX DIM50 SC","WL4 41L D43 LP835 N100 NES7ADCX DIM50 SC (CI-222EAK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["220UPX","WL4 41L D43 LP835 N80 NES7 DIM50 SC","WL4 41L D43 LP835 N80 NES7 DIM50 SC (CI-220UPX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["216FM8","WL4 41L D43 LP835 NX","WL4 41L D43 LP835 NX (CI-216FM8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["223HYR","WL4 41L D43 LP840 N100 NES7ADCX DIM10 SC","WL4 41L D43 LP840 N100 NES7ADCX DIM10 SC (CI-223HYR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["218WLK","WL4 41L D43 LP840 N80","WL4 41L D43 LP840 N80 (CI-218WLK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["226YJL","WL4 41L D43 LP840 N80 NES7ADCX DIM10","WL4 41L D43 LP840 N80 NES7ADCX DIM10 (CI-226YJL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["223ER5","WL4 41L D43 LP840 SC RFD154852","WL4 41L D43 LP840 SC RFD154852 (CI-223ER5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235R0N","WL2 08L EZ1 LP840 MSD7 DIM10 SC","WL2 08L EZ1 LP840 MSD7 DIM10 SC (CI-235R0N)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["247RU2","WL2 08L EZ1 LP840 N100","WL2 08L EZ1 LP840 N100 (CI-247RU2)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["235GG5","WL2 12L EZ1 LP830 N100 NESPDT7 DIM50 SC","WL2 12L EZ1 LP830 N100 NESPDT7 DIM50 SC (CI-235GG5)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["240P3L","WL2 12L EZ1 LP835 MSD7 DIM50","WL2 12L EZ1 LP835 MSD7 DIM50 (CI-240P3L)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["233R80","WL2 12L EZ1 LP840 N80EMG","WL2 12L EZ1 LP840 N80EMG (CI-233R80)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["235J2L","WL2 12L EZB LP840 N100 NES7","WL2 12L EZB LP840 N100 NES7 (CI-235J2L)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["231NYM","WL2 18L EZ1 LP835 N100 NES7 SSQ CS1WL10","WL2 18L EZ1 LP835 N100 NES7 SSQ CS1WL10 (CI-231NYM)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["235U7V","WL2 18L EZ1 LP840 N100 NES7 SC","WL2 18L EZ1 LP840 N100 NES7 SC (CI-235U7V)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["240WV0","WL2 22L EZ1 LP830 N100 NES7 DIM10","WL2 22L EZ1 LP830 N100 NES7 DIM10 (CI-240WV0)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["239K2V","WL2 22L EZ1 LP830 N100 NESPDT7","WL2 22L EZ1 LP830 N100 NESPDT7 (CI-239K2V)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["236L8M","WL2 22L EZ1 LP835 XADS7","WL2 22L EZ1 LP835 XADS7 (CI-236L8M)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["238Y1V","WL2 22L EZ1 LP840 N80 NES7","WL2 22L EZ1 LP840 N80 NES7 (CI-238Y1V)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["226W5G","WL4 20L 120 EZ1 LP840 N100 NES7 DIM10 CS1WL10 SSQ","WL4 20L 120 EZ1 LP840 N100 NES7 DIM10 CS1WL10 SSQ (CI-226W5G)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C11420,7)),6))","v":"229K57"},{"$f":"LEFT(C11420,SEARCH(\"(CI-\",C11420)-2)","v":"WL4 20L EZ1 LP830 N100EMG"},"WL4 20L EZ1 LP830 N100EMG (CI-229K57)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235YM1","WL4 20L EZ1 LP835 N100EMG NES7 DIM10","WL4 20L EZ1 LP835 N100EMG NES7 DIM10 (CI-235YM1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235LU9","WL4 20L EZ1 LP840 N100 NESPDT7 SC","WL4 20L EZ1 LP840 N100 NESPDT7 SC (CI-235LU9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227K39","WL4 30L 120 EZ1 LP840 N100 NES7 DIM10 CS1WL10 SSQ","WL4 30L 120 EZ1 LP840 N100 NES7 DIM10 CS1WL10 SSQ (CI-227K39)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["227K4X","WL4 30L 120 EZ1 LP850 N100 NES7 DIM10 CS1WL10 SSQ","WL4 30L 120 EZ1 LP850 N100 NES7 DIM10 CS1WL10 SSQ (CI-227K4X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["235J2M","WL4 30L EZ1 LP835 N100 NESPDT7 SC","WL4 30L EZ1 LP835 N100 NESPDT7 SC (CI-235J2M)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["228P6X","WL4 30L EZ1 LP835 N80 NESPDT7 DIM10 SC","WL4 30L EZ1 LP835 N80 NESPDT7 DIM10 SC (CI-228P6X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["251N64","WL4 30L EZ1 LP840 N100 NESPDT7 DIM50 SC","WL4 30L EZ1 LP840 N100 NESPDT7 DIM50 SC (CI-251N64)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240L6C","WL4 30L EZ1 LP840 N80EMG","WL4 30L EZ1 LP840 N80EMG (CI-240L6C)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240XTN","WL4 30L EZB LP830","WL4 30L EZB LP830 (CI-240XTN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236KVP","WL4 40L 120 EZ1 LP840 CS1WL10 SSQ","WL4 40L 120 EZ1 LP840 CS1WL10 SSQ (CI-236KVP)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240LAG","WL4 40L EZ1 LP835 MSD7 DIM50 SC","WL4 40L EZ1 LP835 MSD7 DIM50 SC (CI-240LAG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["240KWX","WL4 40L EZ1 LP835 MSD7 SC","WL4 40L EZ1 LP835 MSD7 SC (CI-240KWX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["237VWJ","WL4 40L EZ1 LP835 N80EMG NESPDT7 DIM50","WL4 40L EZ1 LP835 N80EMG NESPDT7 DIM50 (CI-237VWJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["230HM4","WL4 40L EZ1 LP840 N100EMG NESPDT7 DIM10","WL4 40L EZ1 LP840 N100EMG NESPDT7 DIM10 (CI-230HM4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["239VTE","WL4 40L EZ1 LP840 N80EMG NESPDT7 DIM10 USPOM","WL4 40L EZ1 LP840 N80EMG NESPDT7 DIM10 USPOM (CI-239VTE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
[{"$f":"(LEFT((RIGHT(C11612,7)),6))","v":"234YM6"},{"$f":"LEFT(C11612,SEARCH(\"(CI-\",C11612)-2)","v":"WL4 40L EZ1 LP850 N100 NES7"},"WL4 40L EZ1 LP850 N100 NES7 (CI-234YM6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["245VHN","WL4 40L EZB LP840 N100EMG USPOM","WL4 40L EZB LP840 N100EMG USPOM (CI-245VHN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in series instructions","*239MRJ"]
["236XY6","HZL1D L48 7000LM FST MVOLT 40K 80CRI WH","HZL1D L48 7000LM FST MVOLT 40K 80CRI WH (CI-236XY6)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["234E4C","HZL1N L46 5000LM FST MVOLT 50K 80CRI SKGY","HZL1N L46 5000LM FST MVOLT 50K 80CRI SKGY (CI-234E4C)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["235JNU","HZL1N L46 7000LM FST MVOLT 40K 80CRI WH","HZL1N L46 7000LM FST MVOLT 40K 80CRI WH (CI-235JNU)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
[{"$f":"(LEFT((RIGHT(C11676,7)),6))","v":"229XF5"},{"$f":"LEFT(C11676,SEARCH(\"(CI-\",C11676)-2)","v":"HZL1N L48 5000LM FST MVOLT 35K 80CRI GALV"},"HZL1N L48 5000LM FST MVOLT 35K 80CRI GALV (CI-229XF5)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["236EFW","HZL1N L48 5000LM L/LENS MVOLT 30K 80CRI WH","HZL1N L48 5000LM L/LENS MVOLT 30K 80CRI WH (CI-236EFW)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["226TMX","HZL1N L48 7000LM FST MVOLT 40K 80CRI MB","HZL1N L48 7000LM FST MVOLT 40K 80CRI MB (CI-226TMX)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["230X3Y","HZL1N L48 7000LM FST MVOLT 50K 90CRI MB","HZL1N L48 7000LM FST MVOLT 50K 90CRI MB (CI-230X3Y)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["238U6W","HZL1D L24 2500LM FST MVOLT 50K 80CRI CS93BL MB","HZL1D L24 2500LM FST MVOLT 50K 80CRI CS93BL MB (CI-238U6W)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["238APU","HZL1D L48 3000LM FST MVOLT 35K 80CRI WH","HZL1D L48 3000LM FST MVOLT 35K 80CRI WH (CI-238APU)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["239UAG","HZL1D L48 7000LM FST MVOLT 40K 80CRI CS93W OUTEND WH","HZL1D L48 7000LM FST MVOLT 40K 80CRI CS93W OUTEND WH (CI-239UAG)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["238TVX","HZL1D L48 7000LM FST MVOLT 40K 80CRI MB","HZL1D L48 7000LM FST MVOLT 40K 80CRI MB (CI-238TVX)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["241XJ0","HZL1N L46 7000LM L/LENS MVOLT 40K 80CRI WH","HZL1N L46 7000LM L/LENS MVOLT 40K 80CRI WH (CI-241XJ0)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["245KUK","HZL1N L48 7000LM FST 120 30K 80CRI NPP16D SKGY","HZL1N L48 7000LM FST 120 30K 80CRI NPP16D SKGY (CI-245KUK)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["213RLX","ZL1 L24 1700L BDP LP830","ZL1 L24 1700L BDP LP830 (CI-213RLX)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["210AA5","ZL1 L24 1700L LP840","ZL1 L24 1700L LP840 (CI-210AA5)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["214YUX","ZL1 L24 2800L LP835","ZL1 L24 2800L LP835 (CI-214YUX)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["216EJV","ZL1 L24 3000L LP835 GALV","ZL1 L24 3000L LP835 GALV (CI-216EJV)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["214M92","ZL1 L46 2800L LP830","ZL1 L46 2800L LP830 (CI-214M92)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["210L4R","ZL1 L46 2800L LP835","ZL1 L46 2800L LP835 (CI-210L4R)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
[{"$f":"(LEFT((RIGHT(C11868,7)),6))","v":"211V8M"},{"$f":"LEFT(C11868,SEARCH(\"(CI-\",C11868)-2)","v":"ZL1 L46 6000L LP830"},"ZL1 L46 6000L LP830 (CI-211V8M)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["212A5F","ZL1 L48 2800L 120 CS1W LP840","ZL1 L48 2800L 120 CS1W LP840 (CI-212A5F)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["212MPU","ZL1 L48 2800L LP830","ZL1 L48 2800L LP830 (CI-212MPU)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["214WHJ","ZL1 L48 2800L LP840 SKGY","ZL1 L48 2800L LP840 SKGY (CI-214WHJ)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["214RJV","ZL1 L48 6000L 120 CS1W LP840","ZL1 L48 6000L 120 CS1W LP840 (CI-214RJV)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["221F0K","ZL1 L48 6000L LP830 MB","ZL1 L48 6000L LP830 MB (CI-221F0K)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["236GRM","ZL1D L24 1500LM FST MVOLT 30K 90CRI WH","ZL1D L24 1500LM FST MVOLT 30K 90CRI WH (CI-236GRM)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["232VT6","ZL1D L24 2500LM FST MVOLT 40K 80CRI WH","ZL1D L24 2500LM FST MVOLT 40K 80CRI WH (CI-232VT6)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["235V9L","ZL1D L48 3000LM FST MVOLT 40K 80CRI MB","ZL1D L48 3000LM FST MVOLT 40K 80CRI MB (CI-235V9L)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["237CJN","ZL1D L48 5000LM FST MVOLT 35K 80CRI PLR1LVG MB","ZL1D L48 5000LM FST MVOLT 35K 80CRI PLR1LVG MB (CI-237CJN)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["234XPE","ZL1D L48 5000LM FST MVOLT 50K 90CRI WH","ZL1D L48 5000LM FST MVOLT 50K 90CRI WH (CI-234XPE)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["235TX5","ZL1D L48 7000LM FST MVOLT 50K 80CRI WH","ZL1D L48 7000LM FST MVOLT 50K 80CRI WH (CI-235TX5)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["236T7G","ZL1F L24 3000LM MDD 120 35K 90CRI CS1W WH","ZL1F L24 3000LM MDD 120 35K 90CRI CS1W WH (CI-236T7G)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["236FNA","ZL1F L48 3000LM MDD MVOLT 35K 80CRI MB","ZL1F L48 3000LM MDD MVOLT 35K 80CRI MB (CI-236FNA)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["234XN2","ZL1F L48 4500LM MDD MVOLT 35K 80CRI WH","ZL1F L48 4500LM MDD MVOLT 35K 80CRI WH (CI-234XN2)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["235UY4","ZL1F L48 4500LM MDD MVOLT 50K 90CRI MB","ZL1F L48 4500LM MDD MVOLT 50K 90CRI MB (CI-235UY4)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["234T37","ZL1N L24 1500LM FST MVOLT 35K 80CRI PLR1LVG WH","ZL1N L24 1500LM FST MVOLT 35K 80CRI PLR1LVG WH (CI-234T37)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["237MT6","ZL1N L24 1500LM L/LENS MVOLT 30K 90CRI PLR1 MB","ZL1N L24 1500LM L/LENS MVOLT 30K 90CRI PLR1 MB (CI-237MT6)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["235EP9","ZL1N L24 1500LM L/LENS MVOLT 40K 90CRI WH","ZL1N L24 1500LM L/LENS MVOLT 40K 90CRI WH (CI-235EP9)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["223G5P","ZL1N L24 1700L LP835 NAKD","ZL1N L24 1700L LP835 NAKD (CI-223G5P)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["232M9C","ZL1N L24 2500LM FST MVOLT 35K 80CRI MB","ZL1N L24 2500LM FST MVOLT 35K 80CRI MB (CI-232M9C)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["235X0C","ZL1N L24 2500LM FST MVOLT 40K 80CRI PLR1 WH","ZL1N L24 2500LM FST MVOLT 40K 80CRI PLR1 WH (CI-235X0C)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["236GKM","ZL1N L24 2500LM L/LENS MVOLT 35K 80CRI PLR1 WH","ZL1N L24 2500LM L/LENS MVOLT 35K 80CRI PLR1 WH (CI-236GKM)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["229HAY","ZL1N L24 3000LM FST 120 40K 80CRI CS1W WH","ZL1N L24 3000LM FST 120 40K 80CRI CS1W WH (CI-229HAY)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["226KGT","ZL1N L24 3000LM FST MVOLT 40K 80CRI PLR1 WH","ZL1N L24 3000LM FST MVOLT 40K 80CRI PLR1 WH (CI-226KGT)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["231K1C","ZL1N L24 3000LM FST MVOLT 50K 80CRI PLR1G MB","ZL1N L24 3000LM FST MVOLT 50K 80CRI PLR1G MB (CI-231K1C)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["224WEH","ZL1N L24 3000LM L/LENS MVOLT 35K 80CRI BDP PLR22G WH","ZL1N L24 3000LM L/LENS MVOLT 35K 80CRI BDP PLR22G WH (CI-224WEH)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["223X1R","ZL1N L24 3000LM L/LENS MVOLT 40K 80CRI WH","ZL1N L24 3000LM L/LENS MVOLT 40K 80CRI WH (CI-223X1R)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["222NMH","ZL1N L24 3200L LP835","ZL1N L24 3200L LP835 (CI-222NMH)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["233E74","ZL1N L24 3500LM FST MVOLT 30K 90CRI GALV","ZL1N L24 3500LM FST MVOLT 30K 90CRI GALV (CI-233E74)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["236Y8C","ZL1N L24 3500LM FST MVOLT 40K 80CRI PLR1 WH","ZL1N L24 3500LM FST MVOLT 40K 80CRI PLR1 WH (CI-236Y8C)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["233KWN","ZL1N L24 3500LM FST MVOLT 50K 80CRI SKGY","ZL1N L24 3500LM FST MVOLT 50K 80CRI SKGY (CI-233KWN)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["222WTL","ZL1N L24 3600L L/LENS LP830","ZL1N L24 3600L L/LENS LP830 (CI-222WTL)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["234N25","ZL1N L46 3000LM FST MVOLT 30K 80CRI PLR1 WH","ZL1N L46 3000LM FST MVOLT 30K 80CRI PLR1 WH (CI-234N25)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["224AR1","ZL1N L46 3000LM FST MVOLT 35K 80CRI WH","ZL1N L46 3000LM FST MVOLT 35K 80CRI WH (CI-224AR1)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["229Y05","ZL1N L46 3000LM FST MVOLT 50K 80CRI WH","ZL1N L46 3000LM FST MVOLT 50K 80CRI WH (CI-229Y05)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["224C5F","ZL1N L46 3000LM L/LENS MVOLT 35K 80CRI WH","ZL1N L46 3000LM L/LENS MVOLT 35K 80CRI WH (CI-224C5F)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["223MV6","ZL1N L46 3200L L/LENS LP835","ZL1N L46 3200L L/LENS LP835 (CI-223MV6)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
[{"$f":"(LEFT((RIGHT(C12316,7)),6))","v":"227V2C"},{"$f":"LEFT(C12316,SEARCH(\"(CI-\",C12316)-2)","v":"ZL1N L46 5000LM FST MVOLT 30K 80CRI GALV"},"ZL1N L46 5000LM FST MVOLT 30K 80CRI GALV (CI-227V2C)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["224TVA","ZL1N L46 5000LM FST MVOLT 40K 80CRI WH","ZL1N L46 5000LM FST MVOLT 40K 80CRI WH (CI-224TVA)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["224R42","ZL1N L46 7000LM FST 120 40K 80CRI CS1W WH","ZL1N L46 7000LM FST 120 40K 80CRI CS1W WH (CI-224R42)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["224C60","ZL1N L46 7000LM L/LENS MVOLT 40K 80CRI WH","ZL1N L46 7000LM L/LENS MVOLT 40K 80CRI WH (CI-224C60)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["222WT8","ZL1N L46 7500L L/LENS LP840/DUP","ZL1N L46 7500L L/LENS LP840/DUP (CI-222WT8)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["228WGV","ZL1N L48 3000LM FST 120 40K 80CRI CS1W WH","ZL1N L48 3000LM FST 120 40K 80CRI CS1W WH (CI-228WGV)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["223WX2","ZL1N L48 3000LM FST 40K PLR1 WH","ZL1N L48 3000LM FST 40K PLR1 WH (CI-223WX2)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["224F44","ZL1N L48 3000LM FST MVOLT 30K 80CRI PLR1 WH","ZL1N L48 3000LM FST MVOLT 30K 80CRI PLR1 WH (CI-224F44)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["224RY9","ZL1N L48 3000LM FST MVOLT 35K 80CRI PLR1 WH","ZL1N L48 3000LM FST MVOLT 35K 80CRI PLR1 WH (CI-224RY9)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["232M9G","ZL1N L48 3000LM FST MVOLT 35K 90CRI PLR1 WH","ZL1N L48 3000LM FST MVOLT 35K 90CRI PLR1 WH (CI-232M9G)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["228PMK","ZL1N L48 3000LM FST MVOLT 40K 80CRI PLR1G MB","ZL1N L48 3000LM FST MVOLT 40K 80CRI PLR1G MB (CI-228PMK)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["229LPC","ZL1N L48 3000LM FST MVOLT 50K 80CRI PLR1LVG WH","ZL1N L48 3000LM FST MVOLT 50K 80CRI PLR1LVG WH (CI-229LPC)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["225EML","ZL1N L48 3000LM L/LENS MVOLT 30K 80CRI SKGY","ZL1N L48 3000LM L/LENS MVOLT 30K 80CRI SKGY (CI-225EML)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["224AR5","ZL1N L48 3000LM L/LENS MVOLT 35K 80CRI SKGY","ZL1N L48 3000LM L/LENS MVOLT 35K 80CRI SKGY (CI-224AR5)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["229R5F","ZL1N L48 3000LM L/LENS MVOLT 40K 80CRI PLR1G WH","ZL1N L48 3000LM L/LENS MVOLT 40K 80CRI PLR1G WH (CI-229R5F)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["223X1G","ZL1N L48 3000LM L/LENS MVOLT 40K WH USPOM","ZL1N L48 3000LM L/LENS MVOLT 40K WH USPOM (CI-223X1G)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
[{"$f":"(LEFT((RIGHT(C12508,7)),6))","v":"223R1N"},{"$f":"LEFT(C12508,SEARCH(\"(CI-\",C12508)-2)","v":"ZL1N L48 3200L L/LENS LP840 USPOM"},"ZL1N L48 3200L L/LENS LP840 USPOM (CI-223R1N)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["223HJX","ZL1N L48 4400L PLR1 LP840 SKGY","ZL1N L48 4400L PLR1 LP840 SKGY (CI-223HJX)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["234WR4","ZL1N L48 5000LM FST 347 40K 80CRI WH","ZL1N L48 5000LM FST 347 40K 80CRI WH (CI-234WR4)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["228YC8","ZL1N L48 5000LM FST MVOLT 35K 80CRI MB","ZL1N L48 5000LM FST MVOLT 35K 80CRI MB (CI-228YC8)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["234Y3L","ZL1N L48 5000LM FST MVOLT 35K 80CRI PLR22LVG MB","ZL1N L48 5000LM FST MVOLT 35K 80CRI PLR22LVG MB (CI-234Y3L)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["225A16","ZL1N L48 5000LM FST MVOLT 40K 80CRI PLR1 WH","ZL1N L48 5000LM FST MVOLT 40K 80CRI PLR1 WH (CI-225A16)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["230GCW","ZL1N L48 5000LM FST MVOLT 40K 80CRI PLR2A WH","ZL1N L48 5000LM FST MVOLT 40K 80CRI PLR2A WH (CI-230GCW)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["233NAA","ZL1N L48 5000LM FST MVOLT 40K 90CRI PLR1 WH","ZL1N L48 5000LM FST MVOLT 40K 90CRI PLR1 WH (CI-233NAA)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["226T1J","ZL1N L48 5000LM FST MVOLT 50K 80CRI SKGY","ZL1N L48 5000LM FST MVOLT 50K 80CRI SKGY (CI-226T1J)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["226XJA","ZL1N L48 5000LM L/LENS 277 35K 80CRI OCS WH","ZL1N L48 5000LM L/LENS 277 35K 80CRI OCS WH (CI-226XJA)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["225CCR","ZL1N L48 5000LM L/LENS MVOLT 35K 80CRI PLR1 WH","ZL1N L48 5000LM L/LENS MVOLT 35K 80CRI PLR1 WH (CI-225CCR)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["231ERT","ZL1N L48 5000LM L/LENS MVOLT 50K 90CRI SKGY","ZL1N L48 5000LM L/LENS MVOLT 50K 90CRI SKGY (CI-231ERT)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["222R9V","ZL1N L48 6600L 120 CS1W LP840","ZL1N L48 6600L 120 CS1W LP840 (CI-222R9V)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["232AMA","ZL1N L48 7000LM FST 277 35K 80CRI CS11W WH","ZL1N L48 7000LM FST 277 35K 80CRI CS11W WH (CI-232AMA)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["236F2P","ZL1N L48 7000LM FST MVOLT 30K 80CRI PLR1LVG WH","ZL1N L48 7000LM FST MVOLT 30K 80CRI PLR1LVG WH (CI-236F2P)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["226H7A","ZL1N L48 7000LM FST MVOLT 35K 80CRI PLR22G WH","ZL1N L48 7000LM FST MVOLT 35K 80CRI PLR22G WH (CI-226H7A)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["225XYT","ZL1N L48 7000LM FST MVOLT 40K 80CRI GALV","ZL1N L48 7000LM FST MVOLT 40K 80CRI GALV (CI-225XYT)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["228HCY","ZL1N L48 7000LM FST MVOLT 40K 80CRI WH USPOM","ZL1N L48 7000LM FST MVOLT 40K 80CRI WH USPOM (CI-228HCY)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["224N8Y","ZL1N L48 7000LM FST MVOLT 50K 80CRI WH","ZL1N L48 7000LM FST MVOLT 50K 80CRI WH (CI-224N8Y)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["224HFN","ZL1N L48 7000LM L/LENS MVOLT 35K 80CRI WH","ZL1N L48 7000LM L/LENS MVOLT 35K 80CRI WH (CI-224HFN)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["237L1H","ZL1N L48 7000LM L/LENS MVOLT 50K 80CRI GALV","ZL1N L48 7000LM L/LENS MVOLT 50K 80CRI GALV (CI-237L1H)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
[{"$f":"(LEFT((RIGHT(C12764,7)),6))","v":"223GLC"},{"$f":"LEFT(C12764,SEARCH(\"(CI-\",C12764)-2)","v":"ZL1N L48 7500L L/LENS 277 LP840 L/SNSR"},"ZL1N L48 7500L L/LENS 277 LP840 L/SNSR (CI-223GLC)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["238A41","ZL1D L24 1500LM FST MVOLT 35K 80CRI PLR1 WH","ZL1D L24 1500LM FST MVOLT 35K 80CRI PLR1 WH (CI-238A41)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["240LGK","ZL1D L24 3500LM FST MVOLT 40K 90CRI MB","ZL1D L24 3500LM FST MVOLT 40K 90CRI MB (CI-240LGK)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["241G77","ZL1D L48 3000LM FST MVOLT 30K 90CRI PLR1LVG WH","ZL1D L48 3000LM FST MVOLT 30K 90CRI PLR1LVG WH (CI-241G77)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["241GYW","ZL1D L48 3000LM FST MVOLT 40K 90CRI PLR1 WH","ZL1D L48 3000LM FST MVOLT 40K 90CRI PLR1 WH (CI-241GYW)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["245LEV","ZL1D L48 5000LM FST MVOLT 35K 80CRI PLR22 MB","ZL1D L48 5000LM FST MVOLT 35K 80CRI PLR22 MB (CI-245LEV)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["237RPY","ZL1D L48 7000LM FST MVOLT 40K 80CRI WH USPOM","ZL1D L48 7000LM FST MVOLT 40K 80CRI WH USPOM (CI-237RPY)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["240U1V","ZL1F L24 3000LM MDD MVOLT 50K 80CRI GALV","ZL1F L24 3000LM MDD MVOLT 50K 80CRI GALV (CI-240U1V)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["245M6N","ZL1F L48 3000LM MDD MVOLT 35K 80CRI SKGY","ZL1F L48 3000LM MDD MVOLT 35K 80CRI SKGY (CI-245M6N)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["239X3C","ZL1F L48 3000LM MDD MVOLT 50K 90CRI WH","ZL1F L48 3000LM MDD MVOLT 50K 90CRI WH (CI-239X3C)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["247RLV","ZL1F L48 4500LM MDD MVOLT 40K 80CRI PLR1LVG WH","ZL1F L48 4500LM MDD MVOLT 40K 80CRI PLR1LVG WH (CI-247RLV)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["237YV7","ZL1F L48 6000LM MDD MVOLT 30K 80CRI GALV","ZL1F L48 6000LM MDD MVOLT 30K 80CRI GALV (CI-237YV7)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["238RAV","ZL1F L48 6000LM MDD MVOLT 35K 90CRI PLR22 WH","ZL1F L48 6000LM MDD MVOLT 35K 90CRI PLR22 WH (CI-238RAV)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["238X4R","ZL1N L24 1500LM FST 120 40K 80CRI GLR WH","ZL1N L24 1500LM FST 120 40K 80CRI GLR WH (CI-238X4R)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["247R81","ZL1N L24 2500LM FST MVOLT 35K 80CRI PLR1LVG WH","ZL1N L24 2500LM FST MVOLT 35K 80CRI PLR1LVG WH (CI-247R81)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["230J5F","ZL1N L24 3000LM FST 277 40K 80CRI GLR PLR1 WH","ZL1N L24 3000LM FST 277 40K 80CRI GLR PLR1 WH (CI-230J5F)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
[{"$f":"(LEFT((RIGHT(C12956,7)),6))","v":"240AMY"},{"$f":"LEFT(C12956,SEARCH(\"(CI-\",C12956)-2)","v":"ZL1N L24 3500LM FST MVOLT 35K 90CRI MB"},"ZL1N L24 3500LM FST MVOLT 35K 90CRI MB (CI-240AMY)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["238N5N","ZL1N L24 3500LM FST MVOLT 50K 90CRI PLR22 WH","ZL1N L24 3500LM FST MVOLT 50K 90CRI PLR22 WH (CI-238N5N)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","1 Board instructions","*239MR4","*239MR0"]
["241LC3","ZL1N L46 3000LM FST MVOLT 35K 80CRI HC WH","ZL1N L46 3000LM FST MVOLT 35K 80CRI HC WH (CI-241LC3)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["238RNJ","ZL1N L46 3000LM SBL FST MVOLT 30K 80CRI WH","ZL1N L46 3000LM SBL FST MVOLT 30K 80CRI WH (CI-238RNJ)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["238J3K","ZL1N L46 5000LM SBL FST MVOLT 35K 90CRI GALV","ZL1N L46 5000LM SBL FST MVOLT 35K 90CRI GALV (CI-238J3K)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["238EPE","ZL1N L48 3000LM FST MVOLT 30K 90CRI MB","ZL1N L48 3000LM FST MVOLT 30K 90CRI MB (CI-238EPE)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["239RVE","ZL1N L48 3000LM SBL FST MVOLT 35K 80CRI PLR22LVG WH","ZL1N L48 3000LM SBL FST MVOLT 35K 80CRI PLR22LVG WH (CI-239RVE)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["237U8X","ZL1N L48 5000LM FST MVOLT 30K 90CRI MB","ZL1N L48 5000LM FST MVOLT 30K 90CRI MB (CI-237U8X)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["239WLL","ZL1N L48 5000LM FST MVOLT 40K 80CRI HC GALV","ZL1N L48 5000LM FST MVOLT 40K 80CRI HC GALV (CI-239WLL)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["238GA6","ZL1N L48 5000LM FST MVOLT 40K 90CRI PLR1 SKGY","ZL1N L48 5000LM FST MVOLT 40K 90CRI PLR1 SKGY (CI-238GA6)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["238MN6","ZL1N L48 5000LM L/LENS MVOLT 35K 80CRI MB","ZL1N L48 5000LM L/LENS MVOLT 35K 80CRI MB (CI-238MN6)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["247TE9","ZL1N L48 5000LM L/LENS MVOLT 50K 90CRI GALV","ZL1N L48 5000LM L/LENS MVOLT 50K 90CRI GALV (CI-247TE9)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["238EGW","ZL1N L48 7000LM FST MVOLT 40K 80CRI PLR2B WH","ZL1N L48 7000LM FST MVOLT 40K 80CRI PLR2B WH (CI-238EGW)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["238J2W","ZL1N L48 7000LM L/LENS 277 35K 80CRI GLR WH","ZL1N L48 7000LM L/LENS 277 35K 80CRI GLR WH (CI-238J2W)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MR4","*239MR0"]
["235UGR","TZL1D L96 10000LM FST MVOLT 30K 80CRI MB","TZL1D L96 10000LM FST MVOLT 30K 80CRI MB (CI-235UGR)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["235AL9","TZL1D L96 10000LM FST MVOLT 35K 90CRI PLR1 WH","TZL1D L96 10000LM FST MVOLT 35K 90CRI PLR1 WH (CI-235AL9)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["241PKH","TZL1D L96 10000LM FST MVOLT 40K 80CRI WH USPOM","TZL1D L96 10000LM FST MVOLT 40K 80CRI WH USPOM (CI-241PKH)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["236FM6","TZL1D L96 14000LM FST MVOLT 35K 80CRI PLR1LVG WH","TZL1D L96 14000LM FST MVOLT 35K 80CRI PLR1LVG WH (CI-236FM6)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["236ENE","TZL1D L96 14000LM FST MVOLT 50K 80CRI WH","TZL1D L96 14000LM FST MVOLT 50K 80CRI WH (CI-236ENE)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["238JMK","TZL1D L96 6000LM FST MVOLT 35K 90CRI MB","TZL1D L96 6000LM FST MVOLT 35K 90CRI MB (CI-238JMK)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["241G2H","TZL1D L96 6000LM FST MVOLT 50K 80CRI PLR33 WH","TZL1D L96 6000LM FST MVOLT 50K 80CRI PLR33 WH (CI-241G2H)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["234GUJ","TZL1F L96 12000LM MDD MVOLT 35K 80CRI PLR22LVG GALV","TZL1F L96 12000LM MDD MVOLT 35K 80CRI PLR22LVG GALV (CI-234GUJ)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["236PYF","TZL1F L96 6000LM MDD MVOLT 30K 80CRI PLR1G WH","TZL1F L96 6000LM MDD MVOLT 30K 80CRI PLR1G WH (CI-236PYF)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["234UTC","TZL1F L96 6000LM MDD MVOLT 40K 80CRI WH","TZL1F L96 6000LM MDD MVOLT 40K 80CRI WH (CI-234UTC)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["240NLA","TZL1F L96 9000LM MDD MVOLT 35K 80CRI GALV","TZL1F L96 9000LM MDD MVOLT 35K 80CRI GALV (CI-240NLA)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["241LXX","TZL1F L96 9000LM MDD MVOLT 40K 80CRI SKGY","TZL1F L96 9000LM MDD MVOLT 40K 80CRI SKGY (CI-241LXX)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["236HM7","TZL1F L96 9000LM MDD MVOLT 50K 90CRI WH","TZL1F L96 9000LM MDD MVOLT 50K 90CRI WH (CI-236HM7)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["231NMG","TZL1N L92 10000LM FST MVOLT 40K 80CRI PLR1G WH","TZL1N L92 10000LM FST MVOLT 40K 80CRI PLR1G WH (CI-231NMG)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["238V1K","TZL1N L92 14000LM FST MVOLT 30K 80CRI WH","TZL1N L92 14000LM FST MVOLT 30K 80CRI WH (CI-238V1K)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["227VW7","TZL1N L92 6000LM FST MVOLT 30K 80CRI PLR1 WH","TZL1N L92 6000LM FST MVOLT 30K 80CRI PLR1 WH (CI-227VW7)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["234UJ0","TZL1N L92 6000LM FST MVOLT 40K 80CRI PLR1 WH","TZL1N L92 6000LM FST MVOLT 40K 80CRI PLR1 WH (CI-234UJ0)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["224J9Y","TZL1N L92 6000LM L/LENS MVOLT 40K 80CRI WH","TZL1N L92 6000LM L/LENS MVOLT 40K 80CRI WH (CI-224J9Y)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["230UUR","TZL1N L96 10000LM FST 120 50K 80CRI CS1W WH","TZL1N L96 10000LM FST 120 50K 80CRI CS1W WH (CI-230UUR)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["236EFM","TZL1N L96 10000LM FST MVOLT 30K 80CRI PLR2BLVG WH","TZL1N L96 10000LM FST MVOLT 30K 80CRI PLR2BLVG WH (CI-236EFM)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["228YCA","TZL1N L96 10000LM FST MVOLT 35K 80CRI MB","TZL1N L96 10000LM FST MVOLT 35K 80CRI MB (CI-228YCA)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["234A8T","TZL1N L96 10000LM FST MVOLT 35K 80CRI PLR22 WH","TZL1N L96 10000LM FST MVOLT 35K 80CRI PLR22 WH (CI-234A8T)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["240UL3","TZL1N L96 10000LM FST MVOLT 35K 90CRI GALV","TZL1N L96 10000LM FST MVOLT 35K 90CRI GALV (CI-240UL3)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["228MPJ","TZL1N L96 10000LM FST MVOLT 40K 80CRI GALV","TZL1N L96 10000LM FST MVOLT 40K 80CRI GALV (CI-228MPJ)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
[{"$f":"(LEFT((RIGHT(C13404,7)),6))","v":"235NEF"},{"$f":"LEFT(C13404,SEARCH(\"(CI-\",C13404)-2)","v":"TZL1N L96 10000LM FST MVOLT 40K 80CRI PLR1LVG GALV"},"TZL1N L96 10000LM FST MVOLT 40K 80CRI PLR1LVG GALV (CI-235NEF)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["237JMW","TZL1N L96 10000LM FST MVOLT 40K 90CRI PLR1LVG WH USPOM","TZL1N L96 10000LM FST MVOLT 40K 90CRI PLR1LVG WH USPOM (CI-237JMW)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["234H1E","TZL1N L96 10000LM FST MVOLT 50K 80CRI PLR1LVG WH","TZL1N L96 10000LM FST MVOLT 50K 80CRI PLR1LVG WH (CI-234H1E)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["236L28","TZL1N L96 10000LM L/LENS MVOLT 30K 80CRI GALV","TZL1N L96 10000LM L/LENS MVOLT 30K 80CRI GALV (CI-236L28)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["237L2F","TZL1N L96 10000LM L/LENS MVOLT 35K 80CRI PLR1LVG WH","TZL1N L96 10000LM L/LENS MVOLT 35K 80CRI PLR1LVG WH (CI-237L2F)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["226RJK","TZL1N L96 10000LM L/LENS MVOLT 40K 80CRI MB","TZL1N L96 10000LM L/LENS MVOLT 40K 80CRI MB (CI-226RJK)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["233GKE","TZL1N L96 10000LM L/LENS MVOLT 50K 80CRI WH NAWT","TZL1N L96 10000LM L/LENS MVOLT 50K 80CRI WH NAWT (CI-233GKE)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["241CJW","TZL1N L96 10000LM SBL FST MVOLT 40K 80CRI MB","TZL1N L96 10000LM SBL FST MVOLT 40K 80CRI MB (CI-241CJW)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["229TCX","TZL1N L96 14000LM FST MVOLT 30K 80CRI SKGY","TZL1N L96 14000LM FST MVOLT 30K 80CRI SKGY (CI-229TCX)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["234JF8","TZL1N L96 14000LM FST MVOLT 40K 80CRI PLR1 MB","TZL1N L96 14000LM FST MVOLT 40K 80CRI PLR1 MB (CI-234JF8)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["238G0Y","TZL1N L96 14000LM FST MVOLT 40K 90CRI GALV","TZL1N L96 14000LM FST MVOLT 40K 90CRI GALV (CI-238G0Y)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["236MTX","TZL1N L96 14000LM FST MVOLT 50K 80CRI PLR22 WH","TZL1N L96 14000LM FST MVOLT 50K 80CRI PLR22 WH (CI-236MTX)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["233KW2","TZL1N L96 14000LM FST MVOLT 50K 90CRI PLR1 WH","TZL1N L96 14000LM FST MVOLT 50K 90CRI PLR1 WH (CI-233KW2)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["241JT9","TZL1N L96 14000LM L/LENS MVOLT 30K 80CRI MB","TZL1N L96 14000LM L/LENS MVOLT 30K 80CRI MB (CI-241JT9)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["229JWY","TZL1N L96 14000LM L/LENS MVOLT 40K 80CRI SKGY","TZL1N L96 14000LM L/LENS MVOLT 40K 80CRI SKGY (CI-229JWY)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["237V95","TZL1N L96 14000LM SBL FST MVOLT 35K 80CRI MB","TZL1N L96 14000LM SBL FST MVOLT 35K 80CRI MB (CI-237V95)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
[{"$f":"(LEFT((RIGHT(C13596,7)),6))","v":"239L9H"},{"$f":"LEFT(C13596,SEARCH(\"(CI-\",C13596)-2)","v":"TZL1N L96 6000LM FST MVOLT 30K 80CRI PLR1 SKGY"},"TZL1N L96 6000LM FST MVOLT 30K 80CRI PLR1 SKGY (CI-239L9H)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["234AVG","TZL1N L96 6000LM FST MVOLT 35K 80CRI PLR3A WH","TZL1N L96 6000LM FST MVOLT 35K 80CRI PLR3A WH (CI-234AVG)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["236CG9","TZL1N L96 6000LM FST MVOLT 35K 90CRI WH","TZL1N L96 6000LM FST MVOLT 35K 90CRI WH (CI-236CG9)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["224CAP","TZL1N L96 6000LM FST MVOLT 40K 80CRI PLR1LVG CRE WH NAFO","TZL1N L96 6000LM FST MVOLT 40K 80CRI PLR1LVG CRE WH NAFO (CI-224CAP)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["247RU5","TZL1N L96 6000LM FST MVOLT 40K 80CRI PLR2BG WH","TZL1N L96 6000LM FST MVOLT 40K 80CRI PLR2BG WH (CI-247RU5)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
[{"$f":"(LEFT((RIGHT(C13660,7)),6))","v":"224W39"},{"$f":"LEFT(C13660,SEARCH(\"(CI-\",C13660)-2)","v":"TZL1N L96 6000LM FST MVOLT 50K 80CRI PLR1 WH"},"TZL1N L96 6000LM FST MVOLT 50K 80CRI PLR1 WH (CI-224W39)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["235LRY","TZL1N L96 6000LM L/LENS MVOLT 30K 80CRI MB","TZL1N L96 6000LM L/LENS MVOLT 30K 80CRI MB (CI-235LRY)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["224F0V","TZL1N L96 6000LM L/LENS MVOLT 35K 80CRI MB","TZL1N L96 6000LM L/LENS MVOLT 35K 80CRI MB (CI-224F0V)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["224ARF","TZL1N L96 6000LM L/LENS MVOLT 40K 80CRI PLR1LVG WH","TZL1N L96 6000LM L/LENS MVOLT 40K 80CRI PLR1LVG WH (CI-224ARF)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["241GJY","TZL1N L96 6000LM SBL FST MVOLT 40K 80CRI WH USPOM","TZL1N L96 6000LM SBL FST MVOLT 40K 80CRI WH USPOM (CI-241GJY)","PS750L","4 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","4 Boards in parallel instructions","*239MR4","*239MR0"]
["225FEA","BRM9L HI 0/100 SSH U8 MVOLT EZB SCT LP835 C210 M4459A","BRM9L HI 0/100 SSH U8 MVOLT EZB SCT LP835 C210 M4459A (CI-225FEA)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["228N06","BRM9L HI 10/90 SSH U8 MVOLT ENNB ASC/B ADC2/M LP835 C110 M4595D","BRM9L HI 10/90 SSH U8 MVOLT ENNB ASC/B ADC2/M LP835 C110 M4595D (CI-228N06)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["226KU2","BRM9L HI 10/90 SSH U8 MVOLT EZB EC SCT LP835 C110","BRM9L HI 10/90 SSH U8 MVOLT EZB EC SCT LP835 C110 (CI-226KU2)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["226FLC","BRM9L HI 10/90 SSH U8 MVOLT EZB SCT LP840 C210","BRM9L HI 10/90 SSH U8 MVOLT EZB SCT LP840 C210 (CI-226FLC)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["226U55","BRM9L HI 20/80 SSH U4 MVOLT EZB SCT LP835 C110","BRM9L HI 20/80 SSH U4 MVOLT EZB SCT LP835 C110 (CI-226U55)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["227R85","BRM9L HI 20/80 SSH U8 MVOLT ENNB/E NSCT LP835 C210 LMES20","BRM9L HI 20/80 SSH U8 MVOLT ENNB/E NSCT LP835 C210 LMES20 (CI-227R85)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["226F5N","BRM9L HI 20/80 SSH U8 MVOLT EZB SCT LP840 C110","BRM9L HI 20/80 SSH U8 MVOLT EZB SCT LP840 C110 (CI-226F5N)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["225KHP","BRM9L HI 30/70 SSH U8 MVOLT EZB SCT LP835 C110","BRM9L HI 30/70 SSH U8 MVOLT EZB SCT LP835 C110 (CI-225KHP)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["224LTW","BRM9L HI 30/70 SSH U8 MVOLT EZB SCT LP835 C210","BRM9L HI 30/70 SSH U8 MVOLT EZB SCT LP835 C210 (CI-224LTW)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["228CMF","BRM9L HI 40/60 SSH U8 MVOLT EZB SCT LP840 C110","BRM9L HI 40/60 SSH U8 MVOLT EZB SCT LP840 C110 (CI-228CMF)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["225GJX","BRM9L HI 50/50 SSH U4 MVOLT EZB SCT LP840 C210 DU","BRM9L HI 50/50 SSH U4 MVOLT EZB SCT LP840 C210 DU (CI-225GJX)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
[{"$f":"(LEFT((RIGHT(C13852,7)),6))","v":"235VX1"},{"$f":"LEFT(C13852,SEARCH(\"(CI-\",C13852)-2)","v":"BRM9L HI 60/40 SSH U8 120 EZB SCT LP835 C210 ELH"},"BRM9L HI 60/40 SSH U8 120 EZB SCT LP835 C210 ELH (CI-235VX1)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["222R2R","BRM9L HI I4 120 EZB SCT ADC1/LE LP835 F1/24 PWRF C210 SSQ1 M4382A","BRM9L HI I4 120 EZB SCT ADC1/LE LP835 F1/24 PWRF C210 SSQ1 M4382A (CI-222R2R)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["226T2F","BRM9L HI SSH U4 MVOLT EZB EC SCT LP835 F2/36 PWRE C210 M4504A","BRM9L HI SSH U4 MVOLT EZB EC SCT LP835 F2/36 PWRE C210 M4504A (CI-226T2F)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["227HM6","BRM9L HI SSH U8 120 ENNB/E SCT PDT1/LR LP835 C210 M4489A","BRM9L HI SSH U8 120 ENNB/E SCT PDT1/LR LP835 C210 M4489A (CI-227HM6)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["226T2J","BRM9L HI SSH U8 MVOLT EZB EC/LR SCT LP835 F2/36 PWRE C210 M4504A","BRM9L HI SSH U8 MVOLT EZB EC/LR SCT LP835 F2/36 PWRE C210 M4504A (CI-226T2J)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["226T2K","BRM9L HI SSH U8 MVOLT EZB EC/LR SCT LP835 F2/36 PWRE C210 M4504B","BRM9L HI SSH U8 MVOLT EZB EC/LR SCT LP835 F2/36 PWRE C210 M4504B (CI-226T2K)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["227HAF","BRM9L LO 20/80 SSH U4 MVOLT ENNB/E NSCT LP835 C210","BRM9L LO 20/80 SSH U4 MVOLT ENNB/E NSCT LP835 C210 (CI-227HAF)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["226NG1","BRM9L LO 20/80 SSH U8 MVOLT ENNB/E SCT PDT1/R LP835 C210 LMES20 M446","BRM9L LO 20/80 SSH U8 MVOLT ENNB/E SCT PDT1/R LP835 C210 LMES20 M446 (CI-226NG1)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["223M5P","BRM9L LO 30/70 SSH U8 MVOLT EZB SCT LP835 C210 DU","BRM9L LO 30/70 SSH U8 MVOLT EZB SCT LP835 C210 DU (CI-223M5P)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["226K52","BRM9L LO 40/60 SSH U4 MVOLT EZB SCT LP835 C110 DU","BRM9L LO 40/60 SSH U4 MVOLT EZB SCT LP835 C110 DU (CI-226K52)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["224WX4","BRM9L LO 60/40 SSH U8 MVOLT EZB SCT LP830 C110 NYC M00045","BRM9L LO 60/40 SSH U8 MVOLT EZB SCT LP830 C110 NYC M00045 (CI-224WX4)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["226GT6","BRM9L LO SSH U4 MVOLT EZB EC SCT LP835 C110 DU M3797A","BRM9L LO SSH U4 MVOLT EZB EC SCT LP835 C110 DU M3797A (CI-226GT6)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["223XK3","BRM9L LO SSH U8 MVOLT EZB SCT LP840 C110","BRM9L LO SSH U8 MVOLT EZB SCT LP840 C110 (CI-223XK3)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["224RMJ","BRM9L LO SSH U8 MVOLT EZB SCT LP840 C210","BRM9L LO SSH U8 MVOLT EZB SCT LP840 C210 (CI-224RMJ)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["230R98","BRM9LQST HI 20/80 SSH U8 MVOLT EZB SCT LP840 C210","BRM9LQST HI 20/80 SSH U8 MVOLT EZB SCT LP840 C210 (CI-230R98)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["230TK2","BRM9LQST HI SSH U4 MVOLT EZB SCT LP835 C210 GMF","BRM9LQST HI SSH U4 MVOLT EZB SCT LP835 C210 GMF (CI-230TK2)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["235TA9","BRM9LQST LO 0/100 SSH U4 277 EZB SCT LP835 C210","BRM9LQST LO 0/100 SSH U4 277 EZB SCT LP835 C210 (CI-235TA9)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["230VJM","BRM9LQST LO 20/80 SSH U8 MVOLT EZB SCT LP835 C210","BRM9LQST LO 20/80 SSH U8 MVOLT EZB SCT LP835 C210 (CI-230VJM)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["234WNY","BRM9LUS HI 0/100 SSH U4 120 ENNBN SCT LP840 C202 LMES20","BRM9LUS HI 0/100 SSH U4 120 ENNBN SCT LP840 C202 LMES20 (CI-234WNY)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["233K3E","BRM9LUS HI 0/100 SSH U4 120 EZB SCT LP835 C210","BRM9LUS HI 0/100 SSH U4 120 EZB SCT LP835 C210 (CI-233K3E)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["236U5P","BRM9LUS HI 0/100 SSH U8 120 EZB EC/LR SCT LP830 C210 M3797E","BRM9LUS HI 0/100 SSH U8 120 EZB EC/LR SCT LP830 C210 M3797E (CI-236U5P)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["235LCC","BRM9LUS HI 0/100 SSH U8 120 EZB EL SCT LP840 C110","BRM9LUS HI 0/100 SSH U8 120 EZB EL SCT LP840 C110 (CI-235LCC)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["231YKF","BRM9LUS HI 0/100 SSH U8 MVOLT EZB SCT LP830 C210","BRM9LUS HI 0/100 SSH U8 MVOLT EZB SCT LP830 C210 (CI-231YKF)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["233H7X","BRM9LUS HI 10/90 SSH U4 120 EZB SCT LP830 C110","BRM9LUS HI 10/90 SSH U4 120 EZB SCT LP830 C110 (CI-233H7X)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["230VEV","BRM9LUS HI 10/90 SSH U4 MVOLT EZB EC SCT LP835 C210 DU","BRM9LUS HI 10/90 SSH U4 MVOLT EZB EC SCT LP835 C210 DU (CI-230VEV)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["235FUM","BRM9LUS HI 10/90 SSH U8 120 ENNB/E SCT ADC1/L LP835 C210","BRM9LUS HI 10/90 SSH U8 120 ENNB/E SCT ADC1/L LP835 C210 (CI-235FUM)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["236LRV","BRM9LUS HI 10/90 SSH U8 277 ENNB SCT PDT2/L LP840 C210","BRM9LUS HI 10/90 SSH U8 277 ENNB SCT PDT2/L LP840 C210 (CI-236LRV)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["229EPT","BRM9LUS HI 10/90 SSH U8 MVOLT EZB SCT LP835 C110 GMF","BRM9LUS HI 10/90 SSH U8 MVOLT EZB SCT LP835 C110 GMF (CI-229EPT)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["234WH0","BRM9LUS HI 20/80 SSH U4 120 EZB SCT LP835 C210 CSA","BRM9LUS HI 20/80 SSH U4 120 EZB SCT LP835 C210 CSA (CI-234WH0)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["234WH3","BRM9LUS HI 20/80 SSH U4 120 EZB SCT LP835 C210 CSA M4753A","BRM9LUS HI 20/80 SSH U4 120 EZB SCT LP835 C210 CSA M4753A (CI-234WH3)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["230FVW","BRM9LUS HI 20/80 SSH U4 MVOLT ENNB/E SCT LP835 C210 FC284449495","BRM9LUS HI 20/80 SSH U4 MVOLT ENNB/E SCT LP835 C210 FC284449495 (CI-230FVW)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["228NFH","BRM9LUS HI 20/80 SSH U4 MVOLT EZB SCT LP840 C110","BRM9LUS HI 20/80 SSH U4 MVOLT EZB SCT LP840 C110 (CI-228NFH)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["235K0G","BRM9LUS HI 20/80 SSH U8 120 EZB SCT LP835 C110 DU","BRM9LUS HI 20/80 SSH U8 120 EZB SCT LP835 C110 DU (CI-235K0G)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["232J49","BRM9LUS HI 20/80 SSH U8 277 EZB EC SCT LP835 C110","BRM9LUS HI 20/80 SSH U8 277 EZB EC SCT LP835 C110 (CI-232J49)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["236HNF","BRM9LUS HI 20/80 SSH U8 277 EZB SCT LP840 C110 GLR","BRM9LUS HI 20/80 SSH U8 277 EZB SCT LP840 C110 GLR (CI-236HNF)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["231H4N","BRM9LUS HI 20/80 SSH U8 MVOLT ENNB/E SCT PDT1/R LP835 C110 DU M4693A","BRM9LUS HI 20/80 SSH U8 MVOLT ENNB/E SCT PDT1/R LP835 C110 DU M4693A (CI-231H4N)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["230XWA","BRM9LUS HI 20/80 SSH U8 MVOLT EZB EC/L SCT ASC/B LP840 C210 ELS2","BRM9LUS HI 20/80 SSH U8 MVOLT EZB EC/L SCT ASC/B LP840 C210 ELS2 (CI-230XWA)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["228HXF","BRM9LUS HI 20/80 SSH U8 MVOLT EZB EC/L SCT LP840 C110 ELS2 M4458G","BRM9LUS HI 20/80 SSH U8 MVOLT EZB EC/L SCT LP840 C110 ELS2 M4458G (CI-228HXF)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["228HY2","BRM9LUS HI 20/80 SSH U8 MVOLT EZB SCT LP840 C110 M4458B","BRM9LUS HI 20/80 SSH U8 MVOLT EZB SCT LP840 C110 M4458B (CI-228HY2)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["234F1X","BRM9LUS HI 30/70 SSH U4 120 EZB SCT LP835 C110","BRM9LUS HI 30/70 SSH U4 120 EZB SCT LP835 C110 (CI-234F1X)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["235ER4","BRM9LUS HI 30/70 SSH U4 277 EZB EC SCT LP840 C210","BRM9LUS HI 30/70 SSH U4 277 EZB EC SCT LP840 C210 (CI-235ER4)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["231NMH","BRM9LUS HI 30/70 SSH U4 MVOLT EZB SCT LP830 C210","BRM9LUS HI 30/70 SSH U4 MVOLT EZB SCT LP830 C210 (CI-231NMH)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["232HU9","BRM9LUS HI 30/70 SSH U8 120 ENNBN/E SCT LP840 C210 LMES20","BRM9LUS HI 30/70 SSH U8 120 ENNBN/E SCT LP840 C210 LMES20 (CI-232HU9)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["234F9F","BRM9LUS HI 30/70 SSH U8 277 ENNB SCT ADC2/L LP840 C210","BRM9LUS HI 30/70 SSH U8 277 ENNB SCT ADC2/L LP840 C210 (CI-234F9F)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["230WMC","BRM9LUS HI 30/70 SSH U8 MVOLT EZB EC SCT LP835 C110","BRM9LUS HI 30/70 SSH U8 MVOLT EZB EC SCT LP835 C110 (CI-230WMC)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["230KXP","BRM9LUS HI 30/70 SSH U8 MVOLT EZB EC SCT LP835 C210","BRM9LUS HI 30/70 SSH U8 MVOLT EZB EC SCT LP835 C210 (CI-230KXP)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["230JG7","BRM9LUS HI 40/60 SSH U4 MVOLT EZB SCT LP830 C210 DU","BRM9LUS HI 40/60 SSH U4 MVOLT EZB SCT LP830 C210 DU (CI-230JG7)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["235KTU","BRM9LUS HI 40/60 SSH U8 277 EZB EC SCT LP835 C210 ELH","BRM9LUS HI 40/60 SSH U8 277 EZB EC SCT LP835 C210 ELH (CI-235KTU)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["236K9H","BRM9LUS HI 50/50 SSH U4 120 EZB SCT LP830 C110 DU","BRM9LUS HI 50/50 SSH U4 120 EZB SCT LP830 C110 DU (CI-236K9H)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["234ECH","BRM9LUS HI 50/50 SSH U8 120 ENNB/E SCT LP835 C210","BRM9LUS HI 50/50 SSH U8 120 ENNB/E SCT LP835 C210 (CI-234ECH)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["231JTT","BRM9LUS HI 50/50 SSH U8 MVOLT EZB SCT LP835 C210","BRM9LUS HI 50/50 SSH U8 MVOLT EZB SCT LP835 C210 (CI-231JTT)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["232X51","BRM9LUS HI 60/40 SSH U4 277 EZB SCT LP835 C110","BRM9LUS HI 60/40 SSH U4 277 EZB SCT LP835 C110 (CI-232X51)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["235VWW","BRM9LUS HI 60/40 SSH U8 120 ENNB/E EC SCT LP835 C210","BRM9LUS HI 60/40 SSH U8 120 ENNB/E EC SCT LP835 C210 (CI-235VWW)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["235LHC","BRM9LUS HI 60/40 SSH U8 277 ENNBN SCT LP840 C210 LMES20","BRM9LUS HI 60/40 SSH U8 277 ENNBN SCT LP840 C210 LMES20 (CI-235LHC)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["231XKR","BRM9LUS HI 60/40 SSH U8 MVOLT EZB SCT LP840 C110","BRM9LUS HI 60/40 SSH U8 MVOLT EZB SCT LP840 C110 (CI-231XKR)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["236F8M","BRM9LUS HI SSH U4 120 EZB EL SCT LP835 C210 DU","BRM9LUS HI SSH U4 120 EZB EL SCT LP835 C210 DU (CI-236F8M)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["232HUM","BRM9LUS HI SSH U4 120 EZB SCT LP835 C210","BRM9LUS HI SSH U4 120 EZB SCT LP835 C210 (CI-232HUM)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["234A30","BRM9LUS HI SSH U4 277 EZB EC SCT LP835 C210 ELS2","BRM9LUS HI SSH U4 277 EZB EC SCT LP835 C210 ELS2 (CI-234A30)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["229J42","BRM9LUS HI SSH U4 MVOLT ENNB/E EC SCT LP840 C110","BRM9LUS HI SSH U4 MVOLT ENNB/E EC SCT LP840 C110 (CI-229J42)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["228M2U","BRM9LUS HI SSH U4 MVOLT EZB SCT LP835 C110","BRM9LUS HI SSH U4 MVOLT EZB SCT LP835 C110 (CI-228M2U)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["234J81","BRM9LUS HI SSH U8 120 ENNBN/E EC SCT LP840 C210 LMES20","BRM9LUS HI SSH U8 120 ENNBN/E EC SCT LP840 C210 LMES20 (CI-234J81)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["232XXL","BRM9LUS HI SSH U8 120 EZB SCT LP835 C110","BRM9LUS HI SSH U8 120 EZB SCT LP835 C110 (CI-232XXL)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["234MPU","BRM9LUS HI SSH U8 277 EZB ASC/B LP835 C210 M4710B","BRM9LUS HI SSH U8 277 EZB ASC/B LP835 C210 M4710B (CI-234MPU)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["233NJL","BRM9LUS HI SSH U8 277 EZB EC/LR SCT LP835 C210 DU M4594A","BRM9LUS HI SSH U8 277 EZB EC/LR SCT LP835 C210 DU M4594A (CI-233NJL)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["234A31","BRM9LUS HI SSH U8 277 EZB SCT LP835 C210 ELS2","BRM9LUS HI SSH U8 277 EZB SCT LP835 C210 ELS2 (CI-234A31)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["229VP1","BRM9LUS HI SSH U8 MVOLT ENNB/E SCT LP835 C110","BRM9LUS HI SSH U8 MVOLT ENNB/E SCT LP835 C110 (CI-229VP1)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["228TF1","BRM9LUS HI SSH U8 MVOLT EZB SCT LP835 C210 DU","BRM9LUS HI SSH U8 MVOLT EZB SCT LP835 C210 DU (CI-228TF1)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["236C6G","BRM9LUS LO 0/100 SSH U4 120 EZB SCT LP830 C210","BRM9LUS LO 0/100 SSH U4 120 EZB SCT LP830 C210 (CI-236C6G)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["233UK1","BRM9LUS LO 0/100 SSH U8 277 ENNB/E SCT ADC1/L LP840 C110","BRM9LUS LO 0/100 SSH U8 277 ENNB/E SCT ADC1/L LP840 C110 (CI-233UK1)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["236TFE","BRM9LUS LO 10/90 SSH U4 120 ENNB/E SCT LP830 C210 DU","BRM9LUS LO 10/90 SSH U4 120 ENNB/E SCT LP830 C210 DU (CI-236TFE)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["232LYH","BRM9LUS LO 100/0 U8 120 EZB SCT LP830 C210 Z4519A","BRM9LUS LO 100/0 U8 120 EZB SCT LP830 C210 Z4519A (CI-232LYH)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["230GU4","BRM9LUS LO 20/80 SSH U4 MVOLT EZB SCT LP830 C210","BRM9LUS LO 20/80 SSH U4 MVOLT EZB SCT LP830 C210 (CI-230GU4)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["234NKR","BRM9LUS LO 20/80 SSH U8 120 EZB SCT LP840 C110","BRM9LUS LO 20/80 SSH U8 120 EZB SCT LP840 C110 (CI-234NKR)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["228W3P","BRM9LUS LO 20/80 SSH U8 MVOLT EZB SCT LP840 C110","BRM9LUS LO 20/80 SSH U8 MVOLT EZB SCT LP840 C110 (CI-228W3P)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["233XR5","BRM9LUS LO 30/70 SSH U4 277 EZB EC SCT LP835 C210","BRM9LUS LO 30/70 SSH U4 277 EZB EC SCT LP835 C210 (CI-233XR5)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["231G4N","BRM9LUS LO 30/70 SSH U4 MVOLT EZB SCT LP835 C099M RAL1035 DU","BRM9LUS LO 30/70 SSH U4 MVOLT EZB SCT LP835 C099M RAL1035 DU (CI-231G4N)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["233XRC","BRM9LUS LO 30/70 SSH U8 277 EZB EC SCT LP835 C210","BRM9LUS LO 30/70 SSH U8 277 EZB EC SCT LP835 C210 (CI-233XRC)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["232F0F","BRM9LUS LO 30/70 SSH U8 277 EZB SCT LP840 C210","BRM9LUS LO 30/70 SSH U8 277 EZB SCT LP840 C210 (CI-232F0F)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["231U62","BRM9LUS LO 40/60 SSH U4 MVOLT EZB ASC/B LP835 C210 M4710B","BRM9LUS LO 40/60 SSH U4 MVOLT EZB ASC/B LP835 C210 M4710B (CI-231U62)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["232KX2","BRM9LUS LO 40/60 SSH U8 277 ENNB/E SCT LP835 C110","BRM9LUS LO 40/60 SSH U8 277 ENNB/E SCT LP835 C110 (CI-232KX2)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["229YGR","BRM9LUS LO 40/60 SSH U8 MVOLT EZB SCT LP830 C110","BRM9LUS LO 40/60 SSH U8 MVOLT EZB SCT LP830 C110 (CI-229YGR)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["234FJ2","BRM9LUS LO 60/40 SSH U4 277 ENNBN/F SCT LP835 C210 DU LMES20 M4464A","BRM9LUS LO 60/40 SSH U4 277 ENNBN/F SCT LP835 C210 DU LMES20 M4464A (CI-234FJ2)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["236YX6","BRM9LUS LO 60/40 SSH U8 120 EZB SCT LP835 C210","BRM9LUS LO 60/40 SSH U8 120 EZB SCT LP835 C210 (CI-236YX6)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["234T3M","BRM9LUS LO 60/40 SSH U8 277 EZB SCT LP840 C110 USPOM","BRM9LUS LO 60/40 SSH U8 277 EZB SCT LP840 C110 USPOM (CI-234T3M)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["234J7T","BRM9LUS LO SSH U4 120 EZB SCT LP830 C210","BRM9LUS LO SSH U4 120 EZB SCT LP830 C210 (CI-234J7T)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["233TW4","BRM9LUS LO SSH U4 277 EZB SCT LP835 C210 DU","BRM9LUS LO SSH U4 277 EZB SCT LP835 C210 DU (CI-233TW4)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["235W9C","BRM9LUS LO SSH U8 277 EZB EC SCT LP835 C210","BRM9LUS LO SSH U8 277 EZB EC SCT LP835 C210 (CI-235W9C)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["230W7F","BRM9LUS LO SSH U8 MVOLT EZB SCT LP830 C210","BRM9LUS LO SSH U8 MVOLT EZB SCT LP830 C210 (CI-230W7F)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["222C2C","BRM9L HH U4 SSH MVOLT EZB SCT LP835 F1/24 C210 PWRF DL PLT M4030D","BRM9L HH U4 SSH MVOLT EZB SCT LP835 F1/24 C210 PWRF DL PLT M4030D (CI-222C2C)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["227YXK","BRM9L HI 30/70 SSH U8 MVOLT ENNB/E SCT PDT2/M LP840 C210 DU LMES20 M4466A","BRM9L HI 30/70 SSH U8 MVOLT ENNB/E SCT PDT2/M LP840 C210 DU LMES20 M4466A (CI-227YXK)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["226H22","BRM9L HI SSH U4 MVOLT EZB NSCT LP835 C210 N100E","BRM9L HI SSH U4 MVOLT EZB NSCT LP835 C210 N100E (CI-226H22)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["228G4U","BRM9L LO 10/90 SSH U4 MVOLT EZB SCT LP835 C210","BRM9L LO 10/90 SSH U4 MVOLT EZB SCT LP835 C210 (CI-228G4U)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["245W41","BRM9L QST U4 80CRI 35K ID1200LMF 0/100 DARK ZT 277 SCT C210 USPOM","BRM9L QST U4 80CRI 35K ID1200LMF 0/100 DARK ZT 277 SCT C210 USPOM (CI-245W41)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["241P1V","BRM9L QST U8 80CRI 35K ID1200LMF 20/80 DARK ZT 277 SCT C210 USPOM","BRM9L QST U8 80CRI 35K ID1200LMF 20/80 DARK ZT 277 SCT C210 USPOM (CI-241P1V)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["240L9E","BRM9L QST U8 80CRI 35K ID800LMF 20/80 DARK ZT 120 SCT C210 USPOM","BRM9L QST U8 80CRI 35K ID800LMF 20/80 DARK ZT 120 SCT C210 USPOM (CI-240L9E)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["240U52","BRM9L U4 80CRI 35K ID1200LMF 0/100 DARK ZT 120 SCT C202 USPOM","BRM9L U4 80CRI 35K ID1200LMF 0/100 DARK ZT 120 SCT C202 USPOM (CI-240U52)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["240K5G","BRM9L U4 80CRI 35K ID1200LMF 20/80 DARK NLIGHT/R 120 SCT C210 USPOM","BRM9L U4 80CRI 35K ID1200LMF 20/80 DARK NLIGHT/R 120 SCT C210 USPOM (CI-240K5G)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["241TV6","BRM9L U4 80CRI 35K ID1200LMF 20/80 MIN1 NLIGHT 120 SCT CL80 C210 USPOM","BRM9L U4 80CRI 35K ID1200LMF 20/80 MIN1 NLIGHT 120 SCT CL80 C210 USPOM (CI-241TV6)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["240MRU","BRM9L U4 80CRI 35K ID1200LMF 30/70 DARK ZT 277 SCT C210 USPOM","BRM9L U4 80CRI 35K ID1200LMF 30/70 DARK ZT 277 SCT C210 USPOM (CI-240MRU)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["239JTJ","BRM9L U4 80CRI 35K ID1200LMF 40/60 MIN1 NLIGHT 220/50HZ SCT CL80 C110 USPOM M4853A","BRM9L U4 80CRI 35K ID1200LMF 40/60 MIN1 NLIGHT 220/50HZ SCT CL80 C110 USPOM M4853A (CI-239JTJ)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["241P7X","BRM9L U4 80CRI 35K ID1200LMF 60/40 DARK ZT 277 SCT C210 USPOM","BRM9L U4 80CRI 35K ID1200LMF 60/40 DARK ZT 277 SCT C210 USPOM (CI-241P7X)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["239LVM","BRM9L U4 80CRI 35K ID1200LMF 70/30 DARK ZT 277 EC/R SCT C110","BRM9L U4 80CRI 35K ID1200LMF 70/30 DARK ZT 277 EC/R SCT C110 (CI-239LVM)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["239W58","BRM9L U4 80CRI 35K ID800LMF 10/90 DARK ZT 277 SCT C210 DU","BRM9L U4 80CRI 35K ID800LMF 10/90 DARK ZT 277 SCT C210 DU (CI-239W58)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["239LTV","BRM9L U4 80CRI 35K ID800LMF 50/50 DARK ZT 120 SCT C210 DU","BRM9L U4 80CRI 35K ID800LMF 50/50 DARK ZT 120 SCT C210 DU (CI-239LTV)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["240K5H","BRM9L U4 80CRI 35K ID800LMF 70/30 DARK ZT 277 SCT C110 USPOM","BRM9L U4 80CRI 35K ID800LMF 70/30 DARK ZT 277 SCT C110 USPOM (CI-240K5H)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["245X44","BRM9L U4 80CRI 40K ID1200LMF 20/80 DARK ZT 277 EC/R SCT C210 DU USPOM M3797A","BRM9L U4 80CRI 40K ID1200LMF 20/80 DARK ZT 277 EC/R SCT C210 DU USPOM M3797A (CI-245X44)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["247RHM","BRM9L U4 80CRI 40K ID1200LMF 40/60 DARK ZT 120 EC/R SCT C210 USPOM","BRM9L U4 80CRI 40K ID1200LMF 40/60 DARK ZT 120 EC/R SCT C210 USPOM (CI-247RHM)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["251R8Y","BRM9L U4 80CRI 40K ID1200LMF 70/30 DARK ZT 120 SCT C210 USPOM","BRM9L U4 80CRI 40K ID1200LMF 70/30 DARK ZT 120 SCT C210 USPOM (CI-251R8Y)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["239VHW","BRM9L U4 80CRI 40K ID800LMF 30/70 DARK ZT 277 SCT C210","BRM9L U4 80CRI 40K ID800LMF 30/70 DARK ZT 277 SCT C210 (CI-239VHW)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["240G8T","BRM9L U4 80CRI 50K ID1200LMF 30/70 DARK NLIGHT/R 120 SCT C210 DU USPOM M4581B","BRM9L U4 80CRI 50K ID1200LMF 30/70 DARK NLIGHT/R 120 SCT C210 DU USPOM M4581B (CI-240G8T)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["251P0Y","BRM9L U8 80CRI 30K ID1200LMF 0/100 DARK ZT 120 EC/LR SCT C210 USPOM","BRM9L U8 80CRI 30K ID1200LMF 0/100 DARK ZT 120 EC/LR SCT C210 USPOM (CI-251P0Y)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["240K6U","BRM9L U8 80CRI 35K ID1200LMF 20/80 DARK NLIGHT/R 120 SCT C210 USPOM","BRM9L U8 80CRI 35K ID1200LMF 20/80 DARK NLIGHT/R 120 SCT C210 USPOM (CI-240K6U)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["243P7R","BRM9L U8 80CRI 35K ID1200LMF 20/80 DARK ZT 120 SCT C210 USPOM","BRM9L U8 80CRI 35K ID1200LMF 20/80 DARK ZT 120 SCT C210 USPOM (CI-243P7R)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["240PU7","BRM9L U8 80CRI 35K ID1200LMF 20/80 MIN1 ZT 277 EC/L SCT C210 USPOM","BRM9L U8 80CRI 35K ID1200LMF 20/80 MIN1 ZT 277 EC/L SCT C210 USPOM (CI-240PU7)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["241PJT","BRM9L U8 80CRI 35K ID1200LMF 30/70 DARK ZT 120 SCT C110 USPOM","BRM9L U8 80CRI 35K ID1200LMF 30/70 DARK ZT 120 SCT C110 USPOM (CI-241PJT)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["239PMG","BRM9L U8 80CRI 35K ID1200LMF 60/40 DARK NLIGHT/R 277 SCT C210 DU","BRM9L U8 80CRI 35K ID1200LMF 60/40 DARK NLIGHT/R 277 SCT C210 DU (CI-239PMG)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["240K5C","BRM9L U8 80CRI 35K ID1200LMF 70/30 DARK ZT 120 EC/R SCT C210 USPOM","BRM9L U8 80CRI 35K ID1200LMF 70/30 DARK ZT 120 EC/R SCT C210 USPOM (CI-240K5C)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["239LV4","BRM9L U8 80CRI 35K ID1200LMF 70/30 DARK ZT 277 SCT C110","BRM9L U8 80CRI 35K ID1200LMF 70/30 DARK ZT 277 SCT C110 (CI-239LV4)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["241LG0","BRM9L U8 80CRI 35K ID800LMF 20/80 DARK ZT 120 SCT C110 OTM USPOM","BRM9L U8 80CRI 35K ID800LMF 20/80 DARK ZT 120 SCT C110 OTM USPOM (CI-241LG0)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["241H2M","BRM9L U8 80CRI 35K ID800LMF 50/50 DARK ZT 120 SCT C210 USPOM","BRM9L U8 80CRI 35K ID800LMF 50/50 DARK ZT 120 SCT C210 USPOM (CI-241H2M)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["239VWA","BRM9L U8 80CRI 35K ID800LMF 70/30 DARK ZT 120 SCT C210","BRM9L U8 80CRI 35K ID800LMF 70/30 DARK ZT 120 SCT C210 (CI-239VWA)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["241EC5","BRM9L U8 80CRI 40K ID1200LMF 20/80 DARK ZT 120 SCT C210 CSA USPOM","BRM9L U8 80CRI 40K ID1200LMF 20/80 DARK ZT 120 SCT C210 CSA USPOM (CI-241EC5)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["241KVU","BRM9L U8 80CRI 40K ID1200LMF 20/80 DARK ZT 277 SCT C210 USPOM","BRM9L U8 80CRI 40K ID1200LMF 20/80 DARK ZT 277 SCT C210 USPOM (CI-241KVU)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["241AJV","BRM9L U8 80CRI 40K ID1200LMF 70/30 DARK ZT 120 SCT C210 CSA USPOM","BRM9L U8 80CRI 40K ID1200LMF 70/30 DARK ZT 120 SCT C210 CSA USPOM (CI-241AJV)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["240G9L","BRM9L U8 80CRI 40K ID800LMF 20/80 DARK ZT 120 SCT C110 DU USPOM","BRM9L U8 80CRI 40K ID800LMF 20/80 DARK ZT 120 SCT C110 DU USPOM (CI-240G9L)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["241PYA","BRM9L U8 80CRI 40K ID800LMF 60/40 DARK ZT 277 SCT C110 USPOM","BRM9L U8 80CRI 40K ID800LMF 60/40 DARK ZT 277 SCT C110 USPOM (CI-241PYA)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["240FRR","BRM9L U8 80CRI 50K ID800LMF 70/30 DARK NLIGHT/R 120 SCT CL80 C210 DU USPOM M4581A","BRM9L U8 80CRI 50K ID800LMF 70/30 DARK NLIGHT/R 120 SCT CL80 C210 DU USPOM M4581A (CI-240FRR)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["237KC1","BRM9LUS HI 0/100 SSH U4 120 EZB SCT LP835 C110","BRM9LUS HI 0/100 SSH U4 120 EZB SCT LP835 C110 (CI-237KC1)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["238AX3","BRM9LUS HI 20/80 SSH U4 120 EZBN SCT LP835 C210","BRM9LUS HI 20/80 SSH U4 120 EZBN SCT LP835 C210 (CI-238AX3)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["238J2A","BRM9LUS HI 20/80 SSH U8 120 EZB SCT LP840 C202","BRM9LUS HI 20/80 SSH U8 120 EZB SCT LP840 C202 (CI-238J2A)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["231EYF","BRM9LUS HI 20/80 SSH U8 MVOLT ENNB SCT PDT1/RE LP835 C110 DU","BRM9LUS HI 20/80 SSH U8 MVOLT ENNB SCT PDT1/RE LP835 C110 DU (CI-231EYF)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["237X0K","BRM9LUS HI 40/60 SSH U8 277 ENNBN/E SCT LP840 C110 DU LMES20","BRM9LUS HI 40/60 SSH U8 277 ENNBN/E SCT LP840 C110 DU LMES20 (CI-237X0K)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["233X6W","BRM9LUS HI 50/50 SSH U8 120 EZB SCT LP835 C110","BRM9LUS HI 50/50 SSH U8 120 EZB SCT LP835 C110 (CI-233X6W)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["228K51","BRM9LUS HI 70/30 SSH U8 MVOLT EZB SCT LP835 C110 DO NOT USE INVALID","BRM9LUS HI 70/30 SSH U8 MVOLT EZB SCT LP835 C110 DO NOT USE INVALID (CI-228K51)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["238P5K","BRM9LUS HI SSH U4 277 EZB EC SCT LP835 C210 M3797A","BRM9LUS HI SSH U4 277 EZB EC SCT LP835 C210 M3797A (CI-238P5K)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["238TAF","BRM9LUS HI SSH U8 277 EZB EC/LR SCT LP830 C210 M3797E","BRM9LUS HI SSH U8 277 EZB EC/LR SCT LP830 C210 M3797E (CI-238TAF)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["237TV3","BRM9LUS LO 0/100 SSH U8 120 EZB SCT LP840 C110","BRM9LUS LO 0/100 SSH U8 120 EZB SCT LP840 C110 (CI-237TV3)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["236GLT","BRM9LUS LO 20/80 SSH U4 120 EZB SCT LP835 C210 DU","BRM9LUS LO 20/80 SSH U4 120 EZB SCT LP835 C210 DU (CI-236GLT)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["236VFP","BRM9LUS LO 20/80 SSH U8 277 EZB SCT LP840 C210","BRM9LUS LO 20/80 SSH U8 277 EZB SCT LP840 C210 (CI-236VFP)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["238LR4","BRM9LUS LO 60/40 SSH U8 277 EZB SCT LP835 C110 OTM","BRM9LUS LO 60/40 SSH U8 277 EZB SCT LP835 C110 OTM (CI-238LR4)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["237RRX","BRM9LUS LO SSH U8 120 ENNB/E SCT LP840 C210 CSA","BRM9LUS LO SSH U8 120 ENNB/E SCT LP840 C210 CSA (CI-237RRX)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["239YK8","BRM9LUS U4 80CRI 35K ID800LMF 0/100 DARK ZT 277 SCT C210","BRM9LUS U4 80CRI 35K ID800LMF 0/100 DARK ZT 277 SCT C210 (CI-239YK8)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["239MU9","BRM9LUS U8 80CRI 40K ID1200LMF 20/80 DARK ZT 277 SCT C110 USPOM","BRM9LUS U8 80CRI 40K ID1200LMF 20/80 DARK ZT 277 SCT C110 USPOM (CI-239MU9)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["226NGU","BRW9L HI SSH U8 MVOLT ENNB SCT LP835 C210 DU LMES20 M4466A","BRW9L HI SSH U8 MVOLT ENNB SCT LP835 C210 DU LMES20 M4466A (CI-226NGU)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["225LY8","BRW9L LO SSH U4 MVOLT EZB SCT LP835 C210","BRW9L LO SSH U4 MVOLT EZB SCT LP835 C210 (CI-225LY8)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["234TKV","BRW9LUS HI SSH U4 120 EZB SCT LP835 C210 DU","BRW9LUS HI SSH U4 120 EZB SCT LP835 C210 DU (CI-234TKV)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["228JP6","BRW9LUS HI SSH U4 MOVLT EZB SCT LP835 C210 PLT M4610A","BRW9LUS HI SSH U4 MOVLT EZB SCT LP835 C210 PLT M4610A (CI-228JP6)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["234T5N","BRW9LUS HI SSH U8 120 EZB SCT LP840 C210","BRW9LUS HI SSH U8 120 EZB SCT LP840 C210 (CI-234T5N)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["232RWG","BRW9LUS HI SSH U8 277 EZB SCT LP840 C110","BRW9LUS HI SSH U8 277 EZB SCT LP840 C110 (CI-232RWG)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["235HA4","BRW9LUS LO SSH U4 120 EZB EC SCT LP835 C110","BRW9LUS LO SSH U4 120 EZB EC SCT LP835 C110 (CI-235HA4)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["235E60","BRW9LUS LO SSH U8 277 EZB SCT LP830 C110 DU","BRW9LUS LO SSH U8 277 EZB SCT LP830 C110 DU (CI-235E60)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["239C8V","BRW9L U4 80CRI 35K ID600LMF DARK ZT 277 SCT C110 DU","BRW9L U4 80CRI 35K ID600LMF DARK ZT 277 SCT C110 DU (CI-239C8V)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["240WWU","BRW9L U8 80CRI 35K ID600LMF 40/60 DARK NLIGHT 120 SCT PDT/L C210 M4879A","BRW9L U8 80CRI 35K ID600LMF 40/60 DARK NLIGHT 120 SCT PDT/L C210 M4879A (CI-240WWU)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["237FXJ","BRW9LUS HI SSH U4 120 EZB SCT LP835 C210 CSA Z4799A","BRW9LUS HI SSH U4 120 EZB SCT LP835 C210 CSA Z4799A (CI-237FXJ)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["237YAJ","BRW9LUS LO SSH U4 120 EZB SCT LP835 C210","BRW9LUS LO SSH U4 120 EZB SCT LP835 C210 (CI-237YAJ)","PS730L","5 inches minimum away from driver inside the fixture or remote mount","ELA PSRME IC","2 Boards in parallel instructions","*239MPW","*239MPR"]
["232PR3","RD4M1 HI E8 120 EZB EC SCT LP840 F1/48 PWRE C032","RD4M1 HI E8 120 EZB EC SCT LP840 F1/48 PWRE C032 (CI-232PR3)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["235EKK","RD4M1 HI I4 277 EZB SCT LP830 F2/24 PWRF C032","RD4M1 HI I4 277 EZB SCT LP830 F2/24 PWRF C032 (CI-235EKK)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["232R99","RD4M1 HI S8 120 EZB SCT LP840 F1/48 PWRF C032","RD4M1 HI S8 120 EZB SCT LP840 F1/48 PWRF C032 (CI-232R99)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["236HV3","RD4MS HI E4 277 EZB SCT LP835 F2/96 C032","RD4MS HI E4 277 EZB SCT LP835 F2/96 C032 (CI-236HV3)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["236HT7","RD4MS HI I4 277 EZB SCT LP835 F2/96 PWRF C032","RD4MS HI I4 277 EZB SCT LP835 F2/96 PWRF C032 (CI-236HT7)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["236J17","RD4MS HI J8 277 EZB EC/LR SCT LP835 F2/96 C032 ELH","RD4MS HI J8 277 EZB EC/LR SCT LP835 F2/96 C032 ELH (CI-236J17)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["236XH4","RD4MS HI S4 277 EZB SCT LP835 F1/36 PWRF C110","RD4MS HI S4 277 EZB SCT LP835 F1/36 PWRF C110 (CI-236XH4)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["232LER","RD4MS LO ASO I4 277 EZB SCT LP840 F2/24 PWRF C110 BLK","RD4MS LO ASO I4 277 EZB SCT LP840 F2/24 PWRF C110 BLK (CI-232LER)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["235U13","RD4MS LO I4 277 ENNB/E SCT LP840 F2/48 PWRF C032","RD4MS LO I4 277 ENNB/E SCT LP840 F2/48 PWRF C032 (CI-235U13)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["232XA3","RD4MW HI I8 120 EZB SCT LP840 F1/24 PWRF C032","RD4MW HI I8 120 EZB SCT LP840 F1/24 PWRF C032 (CI-232XA3)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["235WRG","RD4W1 HI E4 277 EZB SCT LP835 C110","RD4W1 HI E4 277 EZB SCT LP835 C110 (CI-235WRG)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["236XYG","RD4WS HI I4 277 EZB SCT LP835 PWRF C110","RD4WS HI I4 277 EZB SCT LP835 PWRF C110 (CI-236XYG)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["233FXW","RDM1 HI E4 277 ENNBN/E SCT LP840 F1/48 C032 LMES20","RDM1 HI E4 277 ENNBN/E SCT LP840 F1/48 C032 LMES20 (CI-233FXW)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["236GVL","RDM1 HI E8 120 EZB SCT LP830 F1/72 C032","RDM1 HI E8 120 EZB SCT LP830 F1/72 C032 (CI-236GVL)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["233W1G","RDM1 HI I4 120 ENNBN/E SCT LP835 F2/24 PWRF C032 LMES20 M4451A","RDM1 HI I4 120 ENNBN/E SCT LP835 F2/24 PWRF C032 LMES20 M4451A (CI-233W1G)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["227UCC","RDM1 HI I8 MVOLT EZB SCT LP835 F1/36 PWRF C111","RDM1 HI I8 MVOLT EZB SCT LP835 F1/36 PWRF C111 (CI-227UCC)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["233MA7","RDM1 HI J8 120 EZB SCT LP835 F1A/48 C032","RDM1 HI J8 120 EZB SCT LP835 F1A/48 C032 (CI-233MA7)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["227UAH","RDM1 HI J8 MVOLT EZB SCT LP835 F1/36 C111","RDM1 HI J8 MVOLT EZB SCT LP835 F1/36 C111 (CI-227UAH)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["231NK7","RDM1 HI S8 MVOLT EZB SCT LP830 F2/72 PWRF C110","RDM1 HI S8 MVOLT EZB SCT LP830 F2/72 PWRF C110 (CI-231NK7)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["236WUK","RDM1 LO E8 120 EZB SCT LP835 F2/24 C099M 3116M","RDM1 LO E8 120 EZB SCT LP835 F2/24 C099M 3116M (CI-236WUK)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["228APN","RDM1 LO S8 MVOLT EZB SCT LP830 F1/24 PWRF C032","RDM1 LO S8 MVOLT EZB SCT LP830 F1/24 PWRF C032 (CI-228APN)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["232AEJ","RDMW HI E4 MVOLT EZBN SCT LP840 F2/36 C111","RDMW HI E4 MVOLT EZBN SCT LP840 F2/36 C111 (CI-232AEJ)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["233A6P","RDMW HI I8 120 EZB SCT LP835 F2/36 PWRF C111 BLK","RDMW HI I8 120 EZB SCT LP835 F2/36 PWRF C111 BLK (CI-233A6P)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["227U7N","RDMW HI J8 MVOLT EZB SCT LP835 F1/72 C111","RDMW HI J8 MVOLT EZB SCT LP835 F1/72 C111 (CI-227U7N)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["233ELT","RDMW HI S8 277 EZB SCT LP840 F1/48 PWRF C032","RDMW HI S8 277 EZB SCT LP840 F1/48 PWRF C032 (CI-233ELT)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["232R0H","RDMW LO E4 120 EZB SCT LP830 F2/36 C032","RDMW LO E4 120 EZB SCT LP830 F2/36 C032 (CI-232R0H)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["236XFM","RDMW LO I4 120 EZB SCT LP830 F1/24 PWRF C032","RDMW LO I4 120 EZB SCT LP830 F1/24 PWRF C032 (CI-236XFM)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["235TJV","RDMW LO I8 120 EZB SCT LP840 F1/24 PWRF C110","RDMW LO I8 120 EZB SCT LP840 F1/24 PWRF C110 (CI-235TJV)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["227EK9","RDMW LO S8 277 EZB SCT LP830 F2/96 PWRF C032","RDMW LO S8 277 EZB SCT LP830 F2/96 PWRF C032 (CI-227EK9)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["233W11","RDMW X9 LO J4 277 EZB SCT LP835 C099M RAL1035 Z4687B","RDMW X9 LO J4 277 EZB SCT LP835 C099M RAL1035 Z4687B (CI-233W11)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["233UP0","RDW1 HI I4 120 EZB SCT LP840 PWRF C032","RDW1 HI I4 120 EZB SCT LP840 PWRF C032 (CI-233UP0)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["229T0U","RDW1 HI I8 MVOLT ENNBN EC SCT LP835 PWRFE C032 LMES20","RDW1 HI I8 MVOLT ENNBN EC SCT LP835 PWRFE C032 LMES20 (CI-229T0U)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["228GV8","RDW1 LO E4 MVOLT EZB SCT LP830 C032","RDW1 LO E4 MVOLT EZB SCT LP830 C032 (CI-228GV8)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["228GVM","RDW1 LO I4 MVOLT EZB SCT LP830 PWRF C032","RDW1 LO I4 MVOLT EZB SCT LP830 PWRF C032 (CI-228GVM)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["232KJX","RDW1 LO J8 277 EZB SCT LP835 C032","RDW1 LO J8 277 EZB SCT LP835 C032 (CI-232KJX)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["237RFP","RD4M1 HI E4 277 EZB SCT LP830 F2/72 C110","RD4M1 HI E4 277 EZB SCT LP830 F2/72 C110 (CI-237RFP)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["237RG8","RD4M1 HI J8 277 EZB SCT LP830 F2/144 C110","RD4M1 HI J8 277 EZB SCT LP830 F2/144 C110 (CI-237RG8)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["227UM2","RD4M1 W40 E4 MVOLT EZB SCT LP835 F1/24 C032","RD4M1 W40 E4 MVOLT EZB SCT LP835 F1/24 C032 (CI-227UM2)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["230L4P","RD4M1 W40 I4 MVOLT ENNB EC SCT PDT2/R LP835 F1/24 PWRFE C110 M4675A","RD4M1 W40 I4 MVOLT ENNB EC SCT PDT2/R LP835 F1/24 PWRFE C110 M4675A (CI-230L4P)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["228KY2","RD4M1 W40 I8 MVOLT EZB SCT LP835 F2/48 PWRF C099M RAL3002","RD4M1 W40 I8 MVOLT EZB SCT LP835 F2/48 PWRF C099M RAL3002 (CI-228KY2)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["229LHN","RD4M1 W40 S4 MVOLT EZB SCT LP840 F2/72 PWRF C099G RAL1018","RD4M1 W40 S4 MVOLT EZB SCT LP840 F2/72 PWRF C099G RAL1018 (CI-229LHN)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["241K92","RD4M1L U8 80CRI 35K I400LMF DARK ZT 277 SCT F1/24A PWRF C032","RD4M1L U8 80CRI 35K I400LMF DARK ZT 277 SCT F1/24A PWRF C032 (CI-241K92)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["237A7L","RD4MS HI I4 120 EZB SCT LP840 F1/24 PWRF C032","RD4MS HI I4 120 EZB SCT LP840 F1/24 PWRF C032 (CI-237A7L)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["219HWH","RD4MS I8 120 D45 SCT ADC1/LE LP835 F1/24 C311 DL PLT SSQ1","RD4MS I8 120 D45 SCT ADC1/LE LP835 F1/24 C311 DL PLT SSQ1 (CI-219HWH)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["240TVK","RD4MS U4 80CRI 35K 800LMF DARK ZT 120 SCT F1/48A PWRF C032","RD4MS U4 80CRI 35K 800LMF DARK ZT 120 SCT F1/48A PWRF C032 (CI-240TVK)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["225Y6R","RD4MS W40 E4 MVOLT EZB SCT LP835 F2/36 C099G RAL9004","RD4MS W40 E4 MVOLT EZB SCT LP835 F2/36 C099G RAL9004 (CI-225Y6R)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["231G91","RD4MS W40 E8 MVOLT EZB SCT LP835 F1/72 C110","RD4MS W40 E8 MVOLT EZB SCT LP835 F1/72 C110 (CI-231G91)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["222A92","RD4MS W40 I4 MVOLT EZB SCT LP835 F1/144 PWRF C032","RD4MS W40 I4 MVOLT EZB SCT LP835 F1/144 PWRF C032 (CI-222A92)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["225Y6M","RD4MS W40 I8 MVOLT EZB EC SCT LP835 F2/36 PWRFE C099G RAL9004","RD4MS W40 I8 MVOLT EZB EC SCT LP835 F2/36 PWRFE C099G RAL9004 (CI-225Y6M)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["229WEL","RD4MS W40 J3 MVOLT EZB SCT LP835 F1/144 C032 Z4656A","RD4MS W40 J3 MVOLT EZB SCT LP835 F1/144 C032 Z4656A (CI-229WEL)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["229WAY","RD4MS W40 J6 MVOLT EZB SCT LP835 F1/144 C032 Z4656C","RD4MS W40 J6 MVOLT EZB SCT LP835 F1/144 C032 Z4656C (CI-229WAY)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["231CUR","RD4MS W40 S4 MVOLT EZB SCT LP830 F2/24 PWRF C032","RD4MS W40 S4 MVOLT EZB SCT LP830 F2/24 PWRF C032 (CI-231CUR)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["228P8X","RD4MS W40 S8 MVOLT EZB SCT LP835 F2/48 PWRF C110","RD4MS W40 S8 MVOLT EZB SCT LP835 F2/48 PWRF C110 (CI-228P8X)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["241KV5","RD4MSI U8 80CRI 35K 400LMF DARK ZT 277 SCT F2/48A C099G RAL3016 M4883B","RD4MSI U8 80CRI 35K 400LMF DARK ZT 277 SCT F2/48A C099G RAL3016 M4883B (CI-241KV5)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["241L1U","RD4MSI U8 80CRI 35K 400LMF DARK ZT 277 SCT F2/48A PWRF C099G RAL5002 M4883B","RD4MSI U8 80CRI 35K 400LMF DARK ZT 277 SCT F2/48A PWRF C099G RAL5002 M4883B (CI-241L1U)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["241N7Y","RD4MSL U8 80CRI 35K 400LMF DARK ZT 277 EC/L SCT F2/48A PWRFE C099G RAL5002 M4883A 88CAR","RD4MSL U8 80CRI 35K 400LMF DARK ZT 277 EC/L SCT F2/48A PWRFE C099G RAL5002 M4883A 88CAR (CI-241N7Y)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["241HEK","RD4MSL U8 80CRI 35K 400LMF DARK ZT 277 SCT F2/48A PWRF C099G RAL3016","RD4MSL U8 80CRI 35K 400LMF DARK ZT 277 SCT F2/48A PWRF C099G RAL3016 (CI-241HEK)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["240PH7","RD4MSR U4 80CRI 35K 800LMF ASO MIN1 ZT 120 SCT F2/36A C110","RD4MSR U4 80CRI 35K 800LMF ASO MIN1 ZT 120 SCT F2/36A C110 (CI-240PH7)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["251P05","RD4MSR U8 80CRI 35K 400LMF DARK ZT 277 SCT F1/24A C032","RD4MSR U8 80CRI 35K 400LMF DARK ZT 277 SCT F1/24A C032 (CI-251P05)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["238ME8","RD4MW HI S4 120 EZB SCT LP840 F2/48 PWRF C032","RD4MW HI S4 120 EZB SCT LP840 F2/48 PWRF C032 (CI-238ME8)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["237R9X","RDM1 HI E4 120 EZBN SCT LP835 F2/36 C110","RDM1 HI E4 120 EZBN SCT LP835 F2/36 C110 (CI-237R9X)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["227GPP","RDM1 HI S8 MVOLT EZB EC/L SCT LP835 F1/24 PWRFE C032 M4539A","RDM1 HI S8 MVOLT EZB EC/L SCT LP835 F1/24 PWRFE C032 M4539A (CI-227GPP)","PS1030","Remote mount only","ELA PSRME IC","1 Board instructions","*239MR9"]
["238G5L","RDM1 LO E4 277 EZB SCT LP830 F1/36 C032","RDM1 LO E4 277 EZB SCT LP830 F1/36 C032 (CI-238G5L)","PS1030","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MR9"]
["234HV7","SPM9L HI 0/100 U4 120 EZB SCT LP830 C032","SPM9L HI 0/100 U4 120 EZB SCT LP830 C032 (CI-234HV7)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["236H97","SPM9L HI 0/100 U8 120 ENNB/E SCT LP840 C032","SPM9L HI 0/100 U8 120 ENNB/E SCT LP840 C032 (CI-236H97)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["235RWT","SPM9L HI 20/80 U12 120 EZB EC SCT LP835 C111 DU","SPM9L HI 20/80 U12 120 EZB EC SCT LP835 C111 DU (CI-235RWT)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["233NWN","SPM9L HI 20/80 U4 120 ENNB/E SCT LP835 C111","SPM9L HI 20/80 U4 120 ENNB/E SCT LP835 C111 (CI-233NWN)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["235RWM","SPM9L HI 20/80 U4 120 EZB SCT LP835 C111 DU","SPM9L HI 20/80 U4 120 EZB SCT LP835 C111 DU (CI-235RWM)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["235LYY","SPM9L HI 20/80 U8 120 EZB EC/L SCT LP835 C111","SPM9L HI 20/80 U8 120 EZB EC/L SCT LP835 C111 (CI-235LYY)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["235LLV","SPM9L HI 30/70 I8 277 EZB SCT LP835 F2/48 PWRF C032 IND","SPM9L HI 30/70 I8 277 EZB SCT LP835 F2/48 PWRF C032 IND (CI-235LLV)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["236MGU","SPM9L HI 30/70 U12 120 EZB SCT LP830 C032","SPM9L HI 30/70 U12 120 EZB SCT LP830 C032 (CI-236MGU)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["232W7W","SPM9L HI 30/70 U8 277 ENNB/E EC/L SCT LP840 C032","SPM9L HI 30/70 U8 277 ENNB/E EC/L SCT LP840 C032 (CI-232W7W)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["234TUC","SPM9L HI 40/60 U12 120 EZB SCT LP840 C111","SPM9L HI 40/60 U12 120 EZB SCT LP840 C111 (CI-234TUC)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["235VA2","SPM9L HI 40/60 U8 120 EZB EC SCT LP835 C032 GMF DU","SPM9L HI 40/60 U8 120 EZB EC SCT LP835 C032 GMF DU (CI-235VA2)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["236CGC","SPM9L HI 40/60 U8 277 ENNB/E SCT PDT1/L LP835 C032 ELS2","SPM9L HI 40/60 U8 277 ENNB/E SCT PDT1/L LP835 C032 ELS2 (CI-236CGC)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["236P7A","SPM9L HI 50/50 I4 277 EZB SCT LP835 F1/24 PWRF C032 IND MCS","SPM9L HI 50/50 I4 277 EZB SCT LP835 F1/24 PWRF C032 IND MCS (CI-236P7A)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["234VGU","SPM9L HI 50/50 U4 120 EZB SCT LP835 C032","SPM9L HI 50/50 U4 120 EZB SCT LP835 C032 (CI-234VGU)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["234AGC","SPM9L HI 60/40 I8 120 EZB SCT LP840 F1/24 PWRF C032 IND","SPM9L HI 60/40 I8 120 EZB SCT LP840 F1/24 PWRF C032 IND (CI-234AGC)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["232U2J","SPM9L HI 60/40 U4 120 ENNB/E SCT LP835 C111","SPM9L HI 60/40 U4 120 ENNB/E SCT LP835 C111 (CI-232U2J)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["224PN4","SPM9L HI I4 WHR 120 EZB SCT ADC1/LE LP835 F1/24 PWRF C032 FEP SSQ1 M","SPM9L HI I4 WHR 120 EZB SCT ADC1/LE LP835 F1/24 PWRF C032 FEP SSQ1 M (CI-224PN4)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["234HP0","SPM9L HI U12 120 EZB SCT LP835 C111","SPM9L HI U12 120 EZB SCT LP835 C111 (CI-234HP0)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["233X65","SPM9L HI U4 120 ENNBN/E SCT ADC1/L LP830 C032 LMES20 IND SSQ1","SPM9L HI U4 120 ENNBN/E SCT ADC1/L LP830 C032 LMES20 IND SSQ1 (CI-233X65)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["236W1V","SPM9L HI U4 277 ENEB/E EC SCT LP835 C032 M4718A","SPM9L HI U4 277 ENEB/E EC SCT LP835 C032 M4718A (CI-236W1V)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["234Y4R","SPM9L HI U8 120 ENNB/E EC SCT LP830 C032","SPM9L HI U8 120 ENNB/E EC SCT LP830 C032 (CI-234Y4R)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["236AP2","SPM9L HI U8 120 EZB SCT LP835 C032 M3672C","SPM9L HI U8 120 EZB SCT LP835 C032 M3672C (CI-236AP2)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["234PPM","SPM9L HI U8 277 EZB EC/LR SCT LP835 C111 M4594E","SPM9L HI U8 277 EZB EC/LR SCT LP835 C111 M4594E (CI-234PPM)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["232N1V","SPM9L HI U8 277 EZB SCT LP835 C032","SPM9L HI U8 277 EZB SCT LP835 C032 (CI-232N1V)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["227TY9","SPM9L HI WHR 0/100 U8 MVOLT ENNB/E SCT LP840 C201 M4592A","SPM9L HI WHR 0/100 U8 MVOLT ENNB/E SCT LP840 C201 M4592A (CI-227TY9)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["230H1P","SPM9L HI WHR 20/80 I8 MVOLT SCT EZB LP840 PWRF F2/12 C111 IND","SPM9L HI WHR 20/80 I8 MVOLT SCT EZB LP840 PWRF F2/12 C111 IND (CI-230H1P)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["229XME","SPM9L HI WHR 20/80 U4 MVOLT EZB EC SCT LP835 C032","SPM9L HI WHR 20/80 U4 MVOLT EZB EC SCT LP835 C032 (CI-229XME)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["230R7J","SPM9L HI WHR 20/80 U8 MVOLT ENNB/E SCT LP835 C032","SPM9L HI WHR 20/80 U8 MVOLT ENNB/E SCT LP835 C032 (CI-230R7J)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["229FFJ","SPM9L HI WHR 20/80 U8 MVOLT EZB SCT LP840 C032","SPM9L HI WHR 20/80 U8 MVOLT EZB SCT LP840 C032 (CI-229FFJ)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["229W90","SPM9L HI WHR 30/70 U4 MVOLT EZB SCT LP835 C111","SPM9L HI WHR 30/70 U4 MVOLT EZB SCT LP835 C111 (CI-229W90)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["229TAK","SPM9L HI WHR 50/50 U12 MVOLT EZB SCT LP830 C032","SPM9L HI WHR 50/50 U12 MVOLT EZB SCT LP830 C032 (CI-229TAK)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["230M46","SPM9L HI WHR 50/50 U12 MVOLT EZB SCT LP830 C111","SPM9L HI WHR 50/50 U12 MVOLT EZB SCT LP830 C111 (CI-230M46)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["229TN3","SPM9L HI WHR U12 MVOLT ENNBN/E EC/M SCT PDT1/ML LP835 C032 LMES20 EL","SPM9L HI WHR U12 MVOLT ENNBN/E EC/M SCT PDT1/ML LP835 C032 LMES20 EL (CI-229TN3)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["225GCE","SPM9L HI WHR U4 MVOLT EZB SCT LP835 C032","SPM9L HI WHR U4 MVOLT EZB SCT LP835 C032 (CI-225GCE)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["228J83","SPM9L HI WHR U8 MVOLT EZB EC SCT LP835 C032","SPM9L HI WHR U8 MVOLT EZB EC SCT LP835 C032 (CI-228J83)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["224PLG","SPM9L HM I4 0/100 MVOLT EZB SCT ADC1/LE LP830 F1/12 PWRF C032 DL GMF","SPM9L HM I4 0/100 MVOLT EZB SCT ADC1/LE LP830 F1/12 PWRF C032 DL GMF (CI-224PLG)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["235V8N","SPM9L LO 0/100 U8 120 EZB SCT LP835 C032 ELS2","SPM9L LO 0/100 U8 120 EZB SCT LP835 C032 ELS2 (CI-235V8N)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["233FR5","SPM9L LO 20/80 U4 120 ENNB/F SCT PDT1/L LP830 C032","SPM9L LO 20/80 U4 120 ENNB/F SCT PDT1/L LP830 C032 (CI-233FR5)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["232M4A","SPM9L LO 20/80 U8 277 ENNBN/E PDT1/M SCT LP835 C032 LMES20","SPM9L LO 20/80 U8 277 ENNBN/E PDT1/M SCT LP835 C032 LMES20 (CI-232M4A)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["235K0J","SPM9L LO 20/80 U8 277 EZB EC SCT LP835 C111","SPM9L LO 20/80 U8 277 EZB EC SCT LP835 C111 (CI-235K0J)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["236TJN","SPM9L LO 50/50 U4 120 EZB SCT LP830 C111","SPM9L LO 50/50 U4 120 EZB SCT LP830 C111 (CI-236TJN)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["235L88","SPM9L LO 60/40 U4 120 EZB SCT LP840 C032 DU FC284528369","SPM9L LO 60/40 U4 120 EZB SCT LP840 C032 DU FC284528369 (CI-235L88)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["224PCT","SPM9L LO I4 WHR MVOLT EZB SCT LP835 F1/12 PWRF C032 PLT","SPM9L LO I4 WHR MVOLT EZB SCT LP835 F1/12 PWRF C032 PLT (CI-224PCT)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["234VAE","SPM9L LO U12 277 EZB SCT LP830 C032 DU M4594A","SPM9L LO U12 277 EZB SCT LP830 C032 DU M4594A (CI-234VAE)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["236X7H","SPM9L LO U8 120 EZB SCT LP835 C201","SPM9L LO U8 120 EZB SCT LP835 C201 (CI-236X7H)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["231VR6","SPM9L LO U8 MVOLT EZB SCT LP835 C032","SPM9L LO U8 MVOLT EZB SCT LP835 C032 (CI-231VR6)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["230N8P","SPM9L LO WHR 20/80 U8 MVOLT EZB EC/LR SCT LP830 C032","SPM9L LO WHR 20/80 U8 MVOLT EZB EC/LR SCT LP830 C032 (CI-230N8P)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["230N37","SPM9L LO WHR 20/80 U8 MVOLT EZB SCT LP830 C032","SPM9L LO WHR 20/80 U8 MVOLT EZB SCT LP830 C032 (CI-230N37)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["230R5K","SPM9L LO WHR 60/40 U8 MVOLT ENNB/E SCT LP840 C032","SPM9L LO WHR 60/40 U8 MVOLT ENNB/E SCT LP840 C032 (CI-230R5K)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["230Y7T","SPM9L LO WHR U8 MVOLT EZB SCT LP840 C032","SPM9L LO WHR U8 MVOLT EZB SCT LP840 C032 (CI-230Y7T)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["236FCN","SPW9L HI U4 120 EZB SCT LP840 C032","SPW9L HI U4 120 EZB SCT LP840 C032 (CI-236FCN)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["233ULF","SPW9L HI U8 120 EZB SCT LP840 C032 Z4745A","SPW9L HI U8 120 EZB SCT LP840 C032 Z4745A (CI-233ULF)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["229NML","SPW9L HI WHR U4 MVOLT EZB SCT LP840 C032","SPW9L HI WHR U4 MVOLT EZB SCT LP840 C032 (CI-229NML)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["230MXW","SPW9L LO WHR U4 MVOLT EZB SCT LP835 C032","SPW9L LO WHR U4 MVOLT EZB SCT LP835 C032 (CI-230MXW)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["238CXC","SPM9L HI 20/80 U12 120 ENNB/E SCT LP835 C111 CSA Z4507C","SPM9L HI 20/80 U12 120 ENNB/E SCT LP835 C111 CSA Z4507C (CI-238CXC)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["238GVH","SPM9L HI 20/80 U12 277 EZB EC/M SCT LP835 C111 M3797F","SPM9L HI 20/80 U12 277 EZB EC/M SCT LP835 C111 M3797F (CI-238GVH)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["238KKM","SPM9L HI 20/80 U8 120 EZB SCT LP835 C111 CSA","SPM9L HI 20/80 U8 120 EZB SCT LP835 C111 CSA (CI-238KKM)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["235LJW","SPM9L HI 30/70 I8 120 EZB SCT LP835 F2/48 PWRF C032 IND","SPM9L HI 30/70 I8 120 EZB SCT LP835 F2/48 PWRF C032 IND (CI-235LJW)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["237KWN","SPM9L HI 30/70 U4 120 EZB SCT LP840 C111 M4813A","SPM9L HI 30/70 U4 120 EZB SCT LP840 C111 M4813A (CI-237KWN)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["234P6K","SPM9L HI 40/60 U12 120 EZB SCT LP840 C032","SPM9L HI 40/60 U12 120 EZB SCT LP840 C032 (CI-234P6K)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["236PVX","SPM9L HI 60/40 U12 277 EZB SCT LP835 C032","SPM9L HI 60/40 U12 277 EZB SCT LP835 C032 (CI-236PVX)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["236MKK","SPM9L HI U12 120 ENNB SCT PDT2/ML LP840 C032","SPM9L HI U12 120 ENNB SCT PDT2/ML LP840 C032 (CI-236MKK)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["237TGP","SPM9L HI U8 277 ENNB/E SCT LP841 C099M SW6868","SPM9L HI U8 277 ENNB/E SCT LP841 C099M SW6868 (CI-237TGP)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["231JLN","SPM9L HI WHR 20/80 U8 MVOLT ENNB/E SCT LP835 C111 Z4507A","SPM9L HI WHR 20/80 U8 MVOLT ENNB/E SCT LP835 C111 Z4507A (CI-231JLN)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["238MK4","SPM9L LO 40/60 U4 277 EZB SCT LP835 C032","SPM9L LO 40/60 U4 277 EZB SCT LP835 C032 (CI-238MK4)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["239C15","SPM9L LO U12 120 EZB EC SCT LP835 C032","SPM9L LO U12 120 EZB EC SCT LP835 C032 (CI-239C15)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["235YE4","SPM9L LO U4 277 ENNB SCT PDT2/L LP835 C032 DU","SPM9L LO U4 277 ENNB SCT PDT2/L LP835 C032 DU (CI-235YE4)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["237VC3","SPM9L LO U8 277 ENNB/E SCT LP835 C032","SPM9L LO U8 277 ENNB/E SCT LP835 C032 (CI-237VC3)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["229CV2","SPM9L LO WHR 0/100 U4 MVOLT EZB SCT LP835 C032","SPM9L LO WHR 0/100 U4 MVOLT EZB SCT LP835 C032 (CI-229CV2)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["236FN0","SPW9L HI U4 277 EZB SCT LP840 C032","SPW9L HI U4 277 EZB SCT LP840 C032 (CI-236FN0)","PS730L","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MPW"]
["237FJL","2BLT2 20L ADP EZ1 LP850","2BLT2 20L ADP EZ1 LP850 (CI-237FJL)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["235RHF","2BLT2 33L ADP EZ1 LP830","2BLT2 33L ADP EZ1 LP830 (CI-235RHF)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["236Y7K","2BLT2 33L ADPT EZ1 LP835 MSDPDT7ADCX","2BLT2 33L ADPT EZ1 LP835 MSDPDT7ADCX (CI-236Y7K)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["235MMN","2BLT2 33L ADSM EZ1 LP835 N100 CS1WL10 SSQ","2BLT2 33L ADSM EZ1 LP835 N100 CS1WL10 SSQ (CI-235MMN)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["236P76","2BLT2 33L SDP EZ1 LP835","2BLT2 33L SDP EZ1 LP835 (CI-236P76)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["235RM6","2BLT2 33L SDSM EZ1 LP840","2BLT2 33L SDSM EZ1 LP840 (CI-235RM6)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["236VRA","2BLT2 40L ADP EZ1 LP835 N80EMG","2BLT2 40L ADP EZ1 LP835 N80EMG (CI-236VRA)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["236Y0J","2BLT2 40L ADPT EZ1 LP840 MSD7ADCX","2BLT2 40L ADPT EZ1 LP840 MSD7ADCX (CI-236Y0J)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["237AWN","2BLT2 40L ADSMT EZ1 LP940 N100","2BLT2 40L ADSMT EZ1 LP940 N100 (CI-237AWN)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["235YF3","2BLT2 40L SDSMT EZ1 LP840 N80 NES7","2BLT2 40L SDSMT EZ1 LP840 N80 NES7 (CI-235YF3)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["236CXK","2BLT4 30L ADPT EZ1 LP840 N100","2BLT4 30L ADPT EZ1 LP840 N100 (CI-236CXK)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["236L6U","2BLT4 40L ADP EZ1 LP840 N80","2BLT4 40L ADP EZ1 LP840 N80 (CI-236L6U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["237CXL","2BLT4 40L ADPT EZ1 LP835 IOSPW","2BLT4 40L ADPT EZ1 LP835 IOSPW (CI-237CXL)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["235XC2","2BLT4 40L ADSM EZ1 LP840","2BLT4 40L ADSM EZ1 LP840 (CI-235XC2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["237FVV","2BLT4 40L SDSM EZ1 LP835","2BLT4 40L SDSM EZ1 LP835 (CI-237FVV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["236RVR","2BLT4 48L ADP EZ1 LP830","2BLT4 48L ADP EZ1 LP830 (CI-236RVR)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["236P7X","2BLT4 48L ADP SLD LP835","2BLT4 48L ADP SLD LP835 (CI-236P7X)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["236M73","2BLT4 48L ADSM EZ1 LP835","2BLT4 48L ADSM EZ1 LP835 (CI-236M73)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["236CL1","2BLT4 48L SDSM EZ1 LP840 N100","2BLT4 48L SDSM EZ1 LP840 N100 (CI-236CL1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["237E8U","2BLT4 60LHE ADP EZ1 LP850","2BLT4 60LHE ADP EZ1 LP850 (CI-237E8U)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["236CWC","2BLT4 72L ADP EZ1 LP940","2BLT4 72L ADP EZ1 LP940 (CI-236CWC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["236TGE","2BLT4 85LHE ADP EZ1 LP840","2BLT4 85LHE ADP EZ1 LP840 (CI-236TGE)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["236PM6","BLT4 20L ADP EZ1 LP840","BLT4 20L ADP EZ1 LP840 (CI-236PM6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["236RW1","BLT4 40L ADP EZ1 LP830","BLT4 40L ADP EZ1 LP830 (CI-236RW1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["236XHC","BLT4 40L ADSM EZ1 LP840","BLT4 40L ADSM EZ1 LP840 (CI-236XHC)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["236J8X","BLT4 60LHE ADPT EZ1 LP840","BLT4 60LHE ADPT EZ1 LP840 (CI-236J8X)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["238E4A","2BLT2 20L ADPT EZ1 LP835 N100EMG NESPDT7","2BLT2 20L ADPT EZ1 LP835 N100EMG NESPDT7 (CI-238E4A)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["238CPH","2BLT2 20L ADSMT EZ1 LP830","2BLT2 20L ADSMT EZ1 LP830 (CI-238CPH)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["245P9R","2BLT2 33L ADP EZ1 LP835 USPOM","2BLT2 33L ADP EZ1 LP835 USPOM (CI-245P9R)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["239YMT","2BLT2 33L ADPT EZ1 LP830","2BLT2 33L ADPT EZ1 LP830 (CI-239YMT)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["241HN8","2BLT2 33L ADPT EZ1 LP835 NLTAIR RES7N","2BLT2 33L ADPT EZ1 LP835 NLTAIR RES7N (CI-241HN8)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["237HN5","2BLT2 33L ADPT EZ1 LP840 N100 NES7","2BLT2 33L ADPT EZ1 LP840 N100 NES7 (CI-237HN5)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["241G7X","2BLT2 33L ADPT EZ1 PWS1836 LP835 N80","2BLT2 33L ADPT EZ1 PWS1836 LP835 N80 (CI-241G7X)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["245W7N","2BLT2 33L ADSM EZ1 LP840","2BLT2 33L ADSM EZ1 LP840 (CI-245W7N)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["237LYM","2BLT2 33L SDPT EZ1 LP840","2BLT2 33L SDPT EZ1 LP840 (CI-237LYM)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["245W2W","2BLT2 40L ADP EZ1 LP840","2BLT2 40L ADP EZ1 LP840 (CI-245W2W)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["237JPE","2BLT2 40L ADPT EZ1 LP835 N100 NESPDT7","2BLT2 40L ADPT EZ1 LP835 N100 NESPDT7 (CI-237JPE)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["245LVG","2BLT2 40L ADPT EZ1 LP840 N80 NES7","2BLT2 40L ADPT EZ1 LP840 N80 NES7 (CI-245LVG)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["237VEP","2BLT2 40L ADPT EZ1 PWS1856LV LP935","2BLT2 40L ADPT EZ1 PWS1856LV LP935 (CI-237VEP)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["237XX4","2BLT2 40L ADSMT EZ1 LP840 N100","2BLT2 40L ADSMT EZ1 LP840 N100 (CI-237XX4)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["245P8M","2BLT2 40LHE ADP EZ1 LP840","2BLT2 40LHE ADP EZ1 LP840 (CI-245P8M)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["251RP2","2BLT2 40LHE ADPT EZ1 PWS1836 LP840 N80","2BLT2 40LHE ADPT EZ1 PWS1836 LP840 N80 (CI-251RP2)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["237T38","2BLT2 48LHE ADPT EZ1 LP840","2BLT2 48LHE ADPT EZ1 LP840 (CI-237T38)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["241VHR","2BLT2DR 33L ADP EZ1 LP835 SSQ","2BLT2DR 33L ADP EZ1 LP835 SSQ (CI-241VHR)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["240T1X","2BLT2R 33L ADPT EZ1 LP835 NLTAIR RES7N CS1WL10 SSQ","2BLT2R 33L ADPT EZ1 LP835 NLTAIR RES7N CS1WL10 SSQ (CI-240T1X)","PS1050","Remote mount only","ELA PSRME IC","1 Board instructions","*239MRJ"]
["243P39","2BLT4 30L ADP EZ1 LP835","2BLT4 30L ADP EZ1 LP835 (CI-243P39)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["238ECN","2BLT4 30L ADPT EZ1 LP835","2BLT4 30L ADPT EZ1 LP835 (CI-238ECN)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["240WR4","2BLT4 30L ADPT EZ1 LP840 N100 JP16","2BLT4 30L ADPT EZ1 LP840 N100 JP16 (CI-240WR4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["247VN7","2BLT4 30L ADPT EZ1 PWS1836 LP840 NLTAIR RES7Z","2BLT4 30L ADPT EZ1 PWS1836 LP840 NLTAIR RES7Z (CI-247VN7)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["239VMX","2BLT4 30L SDPT EZ1 PWS1856LV LP835","2BLT4 30L SDPT EZ1 PWS1856LV LP835 (CI-239VMX)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["251RL8","2BLT4 40L ADP EZ1 LP835 USPOM","2BLT4 40L ADP EZ1 LP835 USPOM (CI-251RL8)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["237W4C","2BLT4 40L ADPT EZ1 LP835","2BLT4 40L ADPT EZ1 LP835 (CI-237W4C)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["237YL4","2BLT4 40L ADPT EZ1 LP840 MSDPDT7ADCX","2BLT4 40L ADPT EZ1 LP840 MSDPDT7ADCX (CI-237YL4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["251REV","2BLT4 40L ADPT EZ1 LP840 NLTAIR RES7N USPOM","2BLT4 40L ADPT EZ1 LP840 NLTAIR RES7N USPOM (CI-251REV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["238VW9","2BLT4 40L ADPT EZ1 LP950","2BLT4 40L ADPT EZ1 LP950 (CI-238VW9)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["245WE1","2BLT4 40L ADSM EZ1 LP835 N100","2BLT4 40L ADSM EZ1 LP835 N100 (CI-245WE1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["247WJ4","2BLT4 40L ADSM EZ1 PWS1836 LP930","2BLT4 40L ADSM EZ1 PWS1836 LP930 (CI-247WJ4)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["235XC5","2BLT4 40L ADSMT EZ1 LP840 MSD7ADCX","2BLT4 40L ADSMT EZ1 LP840 MSD7ADCX (CI-235XC5)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["249RT6","2BLT4 40L SDSM EZ1 PWS1836 LP840","2BLT4 40L SDSM EZ1 PWS1836 LP840 (CI-249RT6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["251T80","2BLT4 48L ADP EZ1 LP935 CP","2BLT4 48L ADP EZ1 LP935 CP (CI-251T80)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["238T2R","2BLT4 48L ADPT EZ1 LP830","2BLT4 48L ADPT EZ1 LP830 (CI-238T2R)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["240LFA","2BLT4 48L ADPT EZ1 LP835 N80 NES7","2BLT4 48L ADPT EZ1 LP835 N80 NES7 (CI-240LFA)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["245T7R","2BLT4 48L ADPT EZ1 LP840 N100 NES7ADCX-","2BLT4 48L ADPT EZ1 LP840 N100 NES7ADCX- (CI-245T7R)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["238VWH","2BLT4 48L ADPT EZ1 LP950","2BLT4 48L ADPT EZ1 LP950 (CI-238VWH)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["245T81","2BLT4 48L ADSM EZ1 LP840","2BLT4 48L ADSM EZ1 LP840 (CI-245T81)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["247PPN","2BLT4 48L SDP EZ1 PWS1836 LP840","2BLT4 48L SDP EZ1 PWS1836 LP840 (CI-247PPN)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["249RH0","2BLT4 48L SDSMT EZ1 LP835 NLTAIR RES7Z","2BLT4 48L SDSMT EZ1 LP835 NLTAIR RES7Z (CI-249RH0)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["251T0C","2BLT4 60L ADP EZ1 LP835 N80","2BLT4 60L ADP EZ1 LP835 N80 (CI-251T0C)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["245N9F","2BLT4 60L ADPT EZ1 LP835 MSDPDT7ADCX","2BLT4 60L ADPT EZ1 LP835 MSDPDT7ADCX (CI-245N9F)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["237JPL","2BLT4 60L ADPT EZ1 LP840 N100 NESPDT7","2BLT4 60L ADPT EZ1 LP840 N100 NESPDT7 (CI-237JPL)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["241T6H","2BLT4 60L ADPT EZ1 LP950 N100 NESPDT7","2BLT4 60L ADPT EZ1 LP950 N100 NESPDT7 (CI-241T6H)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["247WKE","2BLT4 60L ADSM EZ1 LP835 USPOM JP16","2BLT4 60L ADSM EZ1 LP835 USPOM JP16 (CI-247WKE)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["239K69","2BLT4 60L SDPT EZ1 LP840 N100 NESPDT7","2BLT4 60L SDPT EZ1 LP840 N100 NESPDT7 (CI-239K69)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["247VNV","2BLT4 60LHE ADSMT EZ1 LP935 N100 NES7","2BLT4 60LHE ADSMT EZ1 LP935 N100 NES7 (CI-247VNV)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["238VX1","2BLT4 72L ADPT EZ1 LP830","2BLT4 72L ADPT EZ1 LP830 (CI-238VX1)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["241G0Y","2BLT4 72L SDSMT EZ1 LP840","2BLT4 72L SDSMT EZ1 LP840 (CI-241G0Y)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["247R51","2BLT4 A 60L ADPT EZ1 LP840 N80EMG","2BLT4 A 60L ADPT EZ1 LP840 N80EMG (CI-247R51)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["247RR6","2BLT4 TUWH PROR 60L ADSMT NLT NESPDT7","2BLT4 TUWH PROR 60L ADSMT NLT NESPDT7 (CI-247RR6)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["251T8G","2BLT4R 30L ADP EZ1 LP850 FAO","2BLT4R 30L ADP EZ1 LP850 FAO (CI-251T8G)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["247VE2","2BLT4R 40L ADSM EZ1 LP840","2BLT4R 40L ADSM EZ1 LP840 (CI-247VE2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["245UJG","2BLT4R 46L ADP LP835","2BLT4R 46L ADP LP835 (CI-245UJG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["251NEJ","2BLT4R 85LHE ADP EZ1 LP835","2BLT4R 85LHE ADP EZ1 LP835 (CI-251NEJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["245NCF","BLT4 20L ADPT EZ1 LP835 N80 NESPDT7","BLT4 20L ADPT EZ1 LP835 N80 NESPDT7 (CI-245NCF)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["240F9U","BLT4 30L SDPT EZ1 LP835 N100 NESPDT7","BLT4 30L SDPT EZ1 LP835 N100 NESPDT7 (CI-240F9U)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["239PLV","BLT4 40L ADPT EZ1 LP835 N100 NESPDT7","BLT4 40L ADPT EZ1 LP835 N100 NESPDT7 (CI-239PLV)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["245T83","BLT4 48L ADP EZ1 LP830","BLT4 48L ADP EZ1 LP830 (CI-245T83)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["245HW2","BLT4 48L SDSMT EZ1 LP835 N100","BLT4 48L SDSMT EZ1 LP835 N100 (CI-245HW2)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["245T3W","BLT4 60L SDPT EZ1 LP840-","BLT4 60L SDPT EZ1 LP840- (CI-245T3W)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["241NWW","IBG 12000LM HEF AFL ND MVOLT OZ10 40K 80CRI DWH","IBG 12000LM HEF AFL ND MVOLT OZ10 40K 80CRI DWH (CI-241NWW)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["241KA9","IBG 12000LM SEF AFL GND 120 OZ10 50K 80CRI MSI6XADL DSCXADL OUTCTR DNA","IBG 12000LM SEF AFL GND 120 OZ10 50K 80CRI MSI6XADL DSCXADL OUTCTR DNA (CI-241KA9)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["241E5U","IBG 12000LM SEF PCL WD MVOLT OZ10 40K 80CRI DWH","IBG 12000LM SEF PCL WD MVOLT OZ10 40K 80CRI DWH (CI-241E5U)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["241LK8","IBG 15000LM SEF AFL WD MVOLT OZ10 40K 80CRI DWH","IBG 15000LM SEF AFL WD MVOLT OZ10 40K 80CRI DWH (CI-241LK8)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["241EAE","IBG 18000LM HEF ACL ND MVOLT OZ10 40K 80CRI DWH","IBG 18000LM HEF ACL ND MVOLT OZ10 40K 80CRI DWH (CI-241EAE)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["243NW9","IBG 18000LM SEF AFL GND 120 OZ10 40K 80CRI CS1W NPP16D DWH","IBG 18000LM SEF AFL GND 120 OZ10 40K 80CRI CS1W NPP16D DWH (CI-243NW9)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["241WPL","IBG 18000LM SEF AFL ND 120 OZ10 50K 80CRI CS93W MSI6XADL DSCXADL DWH","IBG 18000LM SEF AFL ND 120 OZ10 50K 80CRI CS93W MSI6XADL DSCXADL DWH (CI-241WPL)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["241G90","IBG 18000LM SEF L/LENS GND MVOLT OZ10 50K 80CRI HA DWH","IBG 18000LM SEF L/LENS GND MVOLT OZ10 50K 80CRI HA DWH (CI-241G90)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["241A7U","IBG 24000LM HEF ACL WD 277 OZ10 50K 80CRI LAH0SZU DWH","IBG 24000LM HEF ACL WD 277 OZ10 50K 80CRI LAH0SZU DWH (CI-241A7U)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["241E01","IBG 24000LM SEF AFL GND 277 OZ10 40K 80CRI OCS DWH","IBG 24000LM SEF AFL GND 277 OZ10 40K 80CRI OCS DWH (CI-241E01)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["243P1V","IBG 24000LM SEF AFL GND MVOLT OZ10 40K 80CRI WGX DWH","IBG 24000LM SEF AFL GND MVOLT OZ10 40K 80CRI WGX DWH (CI-243P1V)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["241MUV","IBG 24000LM SEF PFL GND MVOLT OZ10 50K 80CRI DWH","IBG 24000LM SEF PFL GND MVOLT OZ10 50K 80CRI DWH (CI-241MUV)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["241G9Y","IBG 30000LM SEF AFL WD MVOLT OZ10 35K 80CRI OUTCTR DNA","IBG 30000LM SEF AFL WD MVOLT OZ10 35K 80CRI OUTCTR DNA (CI-241G9Y)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["241P19","IBG 36000LM SEF AFL GND 120 OZ10 40K 80CRI XAD WGX DWH","IBG 36000LM SEF AFL GND 120 OZ10 40K 80CRI XAD WGX DWH (CI-241P19)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["241UAR","IBG 48000LM SEF ACL ND MVOLT OZ10 40K 80CRI DWH","IBG 48000LM SEF ACL ND MVOLT OZ10 40K 80CRI DWH (CI-241UAR)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["241EGA","IBG 60000LM HEF AFL GND MVOLT OZ10 40K 80CRI HA DWH","IBG 60000LM HEF AFL GND MVOLT OZ10 40K 80CRI HA DWH (CI-241EGA)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["241MVU","IBG 60000LM SEF AFL WD MVOLT OZ10 50K 80CRI DWH","IBG 60000LM SEF AFL WD MVOLT OZ10 50K 80CRI DWH (CI-241MVU)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["241WPE","IBG 8000LM SEF AFL WD MVOLT OZ10 50K 80CRI DWH","IBG 8000LM SEF AFL WD MVOLT OZ10 50K 80CRI DWH (CI-241WPE)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["241R0U","IBGN 24000LM SEF AFL ND 277 OZ10 50K 80CRI CS11WL10 LCOZU DWH","IBGN 24000LM SEF AFL ND 277 OZ10 50K 80CRI CS11WL10 LCOZU DWH (CI-241R0U)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["249PHT","IBG 12000LM SEF AFL GND 277 OZ10 40K 80CRI OCS DWH","IBG 12000LM SEF AFL GND 277 OZ10 40K 80CRI OCS DWH (CI-249PHT)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["245U7M","IBG 12000LM SEF PFL FD MVOLT OZ10 50K 80CRI DWH","IBG 12000LM SEF PFL FD MVOLT OZ10 50K 80CRI DWH (CI-245U7M)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["247WTC","IBG 15000LM HEF AFL WD MVOLT OZ10 50K 80CRI DWH","IBG 15000LM HEF AFL WD MVOLT OZ10 50K 80CRI DWH (CI-247WTC)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["245NW1","IBG 15000LM SEF ACL GND 277 OZ10 50K 80CRI LAOZU DWH","IBG 15000LM SEF ACL GND 277 OZ10 50K 80CRI LAOZU DWH (CI-245NW1)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["245K2G","IBG 15000LM SEF AFL GND 277 OZ10 40K 80CRI LAOZU DWH","IBG 15000LM SEF AFL GND 277 OZ10 40K 80CRI LAOZU DWH (CI-245K2G)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["245VN4","IBG 15000LM SEF AFL GND MVOLT OZ10 50K 80CRI CS93W DNA","IBG 15000LM SEF AFL GND MVOLT OZ10 50K 80CRI CS93W DNA (CI-245VN4)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["245V58","IBG 15000LM SEF AFL WD 277 OZ10 50K 80CRI LCH0SZU DWH","IBG 15000LM SEF AFL WD 277 OZ10 50K 80CRI LCH0SZU DWH (CI-245V58)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["245K46","IBG 18000LM HEF ACL GND 277 OZ10 40K 80CRI CS11W DWH","IBG 18000LM HEF ACL GND 277 OZ10 40K 80CRI CS11W DWH (CI-245K46)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["245M57","IBG 18000LM SEF ACL GND MVOLT OZ10 40K 80CRI DWH","IBG 18000LM SEF ACL GND MVOLT OZ10 40K 80CRI DWH (CI-245M57)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["245HAK","IBG 18000LM SEF AFL GND 277 OZ10 50K 80CRI CS11W DWH","IBG 18000LM SEF AFL GND 277 OZ10 50K 80CRI CS11W DWH (CI-245HAK)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["245MF1","IBG 18000LM SEF AFL GND MVOLT OZ10 50K 70CRI DWH","IBG 18000LM SEF AFL GND MVOLT OZ10 50K 70CRI DWH (CI-245MF1)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["247PGT","IBG 18000LM SEF AFL WD MVOLT OZ10 40K 80CRI HA DWH","IBG 18000LM SEF AFL WD MVOLT OZ10 40K 80CRI HA DWH (CI-247PGT)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["247T7H","IBG 24000LM HEF PFL GND MVOLT OZ10 40K 80CRI DWH","IBG 24000LM HEF PFL GND MVOLT OZ10 40K 80CRI DWH (CI-247T7H)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["245VXN","IBG 24000LM SEF ACL GND MVOLT OZ10 50K 80CRI DWH","IBG 24000LM SEF ACL GND MVOLT OZ10 50K 80CRI DWH (CI-245VXN)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["247RHA","IBG 24000LM SEF AFL GND 208 OZ10 50K 80CRI CS43W DWH","IBG 24000LM SEF AFL GND 208 OZ10 50K 80CRI CS43W DWH (CI-247RHA)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["247V74","IBG 24000LM SEF AFL GND 277 OZ10 50K 80CRI CS11WL10 LAOZU DWH","IBG 24000LM SEF AFL GND 277 OZ10 50K 80CRI CS11WL10 LAOZU DWH (CI-247V74)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["245K4F","IBG 24000LM SEF AFL GND MVOLT OZ10 50K 80CRI WGX DWH","IBG 24000LM SEF AFL GND MVOLT OZ10 50K 80CRI WGX DWH (CI-245K4F)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["245MMM","IBG 24000LM SEF L/LENS GND MVOLT OZ10 40K 80CRI DWH","IBG 24000LM SEF L/LENS GND MVOLT OZ10 40K 80CRI DWH (CI-245MMM)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["249RU6","IBG 30000LM HEF AFL GND 277 OZ10 40K 70CRI IMP DWH","IBG 30000LM HEF AFL GND 277 OZ10 40K 70CRI IMP DWH (CI-249RU6)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["249PJF","IBG 30000LM SEF AFL GND MVOLT OZ10 35K 80CRI DWH","IBG 30000LM SEF AFL GND MVOLT OZ10 35K 80CRI DWH (CI-249PJF)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["245MN7","IBG 30000LM SEF AFL WD MVOLT OZ10 50K 90CRI DWH","IBG 30000LM SEF AFL WD MVOLT OZ10 50K 90CRI DWH (CI-245MN7)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["245RKL","IBG 36000LM SEF ACL WD MVOLT OZ10 50K 80CRI DWH","IBG 36000LM SEF ACL WD MVOLT OZ10 50K 80CRI DWH (CI-245RKL)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["251P6H","IBG 48000LM SEF ACL GND 277 OZ10 50K 80CRI CS11WL10 DWH","IBG 48000LM SEF ACL GND 277 OZ10 50K 80CRI CS11WL10 DWH (CI-251P6H)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["245RJR","IBG 48000LM SEF AFL GND 277 OZ10 50K 80CRI CS11WL15 DWH","IBG 48000LM SEF AFL GND 277 OZ10 50K 80CRI CS11WL15 DWH (CI-245RJR)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["245RK0","IBG 60000LM HEF ACL GND MVOLT OZ10 50K 90CRI DWH","IBG 60000LM HEF ACL GND MVOLT OZ10 50K 90CRI DWH (CI-245RK0)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["247W6K","IBG 8000LM SEF AFL FD MVOLT OZ10 40K 90CRI DWH","IBG 8000LM SEF AFL FD MVOLT OZ10 40K 90CRI DWH (CI-247W6K)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["245K1N","IBG 8000LM SEF AFL ND MVOLT OZ10 40K 80CRI DWH","IBG 8000LM SEF AFL ND MVOLT OZ10 40K 80CRI DWH (CI-245K1N)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["247RXW","IBGN 18000LM SEF AFL GND 277 OZ10 40K 80CRI LAOZU WGX DWH","IBGN 18000LM SEF AFL GND 277 OZ10 40K 80CRI LAOZU WGX DWH (CI-247RXW)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["247PXR","IBGN 18000LM SEF AFL GND MVOLT OZ10 50K 80CRI IMP DWH","IBGN 18000LM SEF AFL GND MVOLT OZ10 50K 80CRI IMP DWH (CI-247PXR)","PS30250","Remote mount only","None","PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","*251PT0"]
["247P2G","IBGN 24000LM SEF AFL WD MVOLT OZ10 40K 80CRI HA DWH","IBGN 24000LM SEF AFL WD MVOLT OZ10 40K 80CRI HA DWH (CI-247P2G)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["245J9V","IBGN 30000LM SEF L/LENS FD 277 OZ10 50K 70CRI OCS LCM0SZU DWH","IBGN 30000LM SEF L/LENS FD 277 OZ10 50K 70CRI OCS LCM0SZU DWH (CI-245J9V)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["236CU6","ICO 30/05 4 60D 120 EZB HSG U","ICO 30/05 4 60D 120 EZB HSG U (CI-236CU6)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235HVK","ICO 30/10 4 25D 120 EZB HSG U","ICO 30/10 4 25D 120 EZB HSG U (CI-235HVK)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236F92","ICO 30/15 4 50D 120 EDXB HSG U OS","ICO 30/15 4 50D 120 EDXB HSG U OS (CI-236F92)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235C1A","ICO 30/15 4 50D 120 EZB HSG U OS","ICO 30/15 4 50D 120 EZB HSG U OS (CI-235C1A)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237JMT","ICO 30/20 4 65D 277 EZB HSG U","ICO 30/20 4 65D 277 EZB HSG U (CI-237JMT)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["230N75","ICO 30/20 6 45D 120 EDXB HSG U OS","ICO 30/20 6 45D 120 EDXB HSG U OS (CI-230N75)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236MT0","ICO 30/25 4 30D 120 EZB HSG U","ICO 30/25 4 30D 120 EZB HSG U (CI-236MT0)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233LM5","ICO 30/30 4 60D 120 EDXB HSG U","ICO 30/30 4 60D 120 EDXB HSG U (CI-233LM5)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239T1W","ICO 30/30 6 40D 120 EDXB SF HSG U","ICO 30/30 6 40D 120 EDXB SF HSG U (CI-239T1W)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["229Y31","ICO 30/30 6 60D 277 EZB HSG U OS","ICO 30/30 6 60D 277 EZB HSG U OS (CI-229Y31)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["232U5J","ICO 30/40 6 65D 120 EZB HSG U OS","ICO 30/40 6 65D 120 EZB HSG U OS (CI-232U5J)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233FCU","ICO 30/40 6 70D 120 EZB HSG U OS","ICO 30/40 6 70D 120 EZB HSG U OS (CI-233FCU)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237TX5","ICO 30/60 6 30D 120 EZB HSG U OS","ICO 30/60 6 30D 120 EZB HSG U OS (CI-237TX5)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233EAH","ICO 30/60 6 60D 120 EZB HSG U OS","ICO 30/60 6 60D 120 EZB HSG U OS (CI-233EAH)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["228V0C","ICO 30/65 6 40D 120 EDXB HSG U OS","ICO 30/65 6 40D 120 EDXB HSG U OS (CI-228V0C)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239AY3","ICO 35/05 4 30D 277 EZB HSG U","ICO 35/05 4 30D 277 EZB HSG U (CI-239AY3)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234PLK","ICO 35/07 4 15D 277 EZB HSG U","ICO 35/07 4 15D 277 EZB HSG U (CI-234PLK)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["232J2K","ICO 35/10 4 45D 120 EZB HSG U","ICO 35/10 4 45D 120 EZB HSG U (CI-232J2K)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238HCH","ICO 35/15 4 60D 120 EDXB HSG U","ICO 35/15 4 60D 120 EDXB HSG U (CI-238HCH)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235THF","ICO 35/15 4 60D 120 EZB HSG U","ICO 35/15 4 60D 120 EZB HSG U (CI-235THF)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["231RNE","ICO 35/20 6 20D 277 EZB NPS80EZ HSG U OS","ICO 35/20 6 20D 277 EZB NPS80EZ HSG U OS (CI-231RNE)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237A7E","ICO 35/20 6 40D 120 EZB NPS80EZER HSG U OS","ICO 35/20 6 40D 120 EZB NPS80EZER HSG U OS (CI-237A7E)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["230N1J","ICO 35/20 6 60D 120 EZB HSG U OS","ICO 35/20 6 60D 120 EZB HSG U OS (CI-230N1J)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238HCE","ICO 35/25 4 60D 120 EDXB HSG U OS","ICO 35/25 4 60D 120 EDXB HSG U OS (CI-238HCE)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239N7N","ICO 35/25 6 60D 120 EZB HSG U","ICO 35/25 6 60D 120 EZB HSG U (CI-239N7N)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237C1M","ICO 35/30 4 30D 277 EZB HSG U OS","ICO 35/30 4 30D 277 EZB HSG U OS (CI-237C1M)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235P77","ICO 35/30 6 45D 120 EZB SF HSG U OS","ICO 35/30 6 45D 120 EZB SF HSG U OS (CI-235P77)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["230W4H","ICO 35/30 6 45D 277 EZB HSG U OS","ICO 35/30 6 45D 277 EZB HSG U OS (CI-230W4H)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239HPU","ICO 35/35 6 60D 277 EZB HSG U","ICO 35/35 6 60D 277 EZB HSG U (CI-239HPU)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238X1Y","ICO 35/40 6 30D 277 EZ1 HSG U","ICO 35/40 6 30D 277 EZ1 HSG U (CI-238X1Y)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["229M0M","ICO 35/40 6 60D 277 EZB HSG U OS","ICO 35/40 6 60D 277 EZB HSG U OS (CI-229M0M)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235AJT","ICO 35/45 6 60D 120 EZB HSG U OS","ICO 35/45 6 60D 120 EZB HSG U OS (CI-235AJT)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234W4U","ICO 35/50 6 35D 120 EDXB HSG U OS","ICO 35/50 6 35D 120 EDXB HSG U OS (CI-234W4U)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233W73","ICO 35/50 6 60D 120 EZB HSG U OS","ICO 35/50 6 60D 120 EZB HSG U OS (CI-233W73)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["229F34","ICO 35/60 6 45D 120 EZB HSG U OS","ICO 35/60 6 45D 120 EZB HSG U OS (CI-229F34)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["229RW0","ICO 35/60 6 45D 120 EZB SF HSG U OS","ICO 35/60 6 45D 120 EZB SF HSG U OS (CI-229RW0)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["229TXT","ICO 35/65 6 30D 120 EZB HSG U OS","ICO 35/65 6 30D 120 EZB HSG U OS (CI-229TXT)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233V38","ICO 40/07 4 45D 120 EZB HSG U","ICO 40/07 4 45D 120 EZB HSG U (CI-233V38)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237YKE","ICO 40/15 4 40D 120 EZB HSG U","ICO 40/15 4 40D 120 EZB HSG U (CI-237YKE)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237G97","ICO 40/20 4FL 65D 120 EZB HSG U","ICO 40/20 4FL 65D 120 EZB HSG U (CI-237G97)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236F8C","ICO 40/20 6 70D 120 EDXB HSG U OS","ICO 40/20 6 70D 120 EDXB HSG U OS (CI-236F8C)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233FH8","ICO 40/25 6 40D 277 EZB HSG U OS","ICO 40/25 6 40D 277 EZB HSG U OS (CI-233FH8)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["230N1U","ICO 40/30 6 40D 277 EZB HSG U OS","ICO 40/30 6 40D 277 EZB HSG U OS (CI-230N1U)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239JPR","ICO 40/30 6 45D 120 EZB HSG U","ICO 40/30 6 45D 120 EZB HSG U (CI-239JPR)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238HFL","ICO 40/35 6 45D 277 EZB SF HSG USPOM U OS","ICO 40/35 6 45D 277 EZB SF HSG USPOM U OS (CI-238HFL)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["228Y8X","ICO 40/40 6 60D 120 EZB HSG U OS","ICO 40/40 6 60D 120 EZB HSG U OS (CI-228Y8X)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["232GUV","ICO 40/45 6 40D 277 EZB HSG U OS","ICO 40/45 6 40D 277 EZB HSG U OS (CI-232GUV)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["232E69","ICO 40/50 6 20D 277 EZB HSG U OS","ICO 40/50 6 20D 277 EZB HSG U OS (CI-232E69)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239TJ6","ICO 40/50 6 65D 120 EZB HSG U","ICO 40/50 6 65D 120 EZB HSG U (CI-239TJ6)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239J2E","ICO 40/60 6 40D 120 EZB NPS80EZ HSG U","ICO 40/60 6 40D 120 EZB NPS80EZ HSG U (CI-239J2E)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239EEX","ICO 40/65 6 30D 277 EZ1 HSG USPOM U","ICO 40/65 6 30D 277 EZ1 HSG USPOM U (CI-239EEX)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239LTK","ICO 40/65 6 40D 120 EZ10 HSG U","ICO 40/65 6 40D 120 EZ10 HSG U (CI-239LTK)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239M2U","ICO ADJ 27/30 6 45D 120 EZB HSG U","ICO ADJ 27/30 6 45D 120 EZB HSG U (CI-239M2U)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237AET","ICO ADJ 30/07 4 30D 120 EZB HSG U","ICO ADJ 30/07 4 30D 120 EZB HSG U (CI-237AET)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["230EHM","ICO ADJ 30/10 4 30D 120 EZB HSG U OS","ICO ADJ 30/10 4 30D 120 EZB HSG U OS (CI-230EHM)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236V5K","ICO ADJ 30/12 4 50D 120 EZB HSG U OS","ICO ADJ 30/12 4 50D 120 EZB HSG U OS (CI-236V5K)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235HTY","ICO ADJ 30/20 4 35D 120 EZB HSG U OS","ICO ADJ 30/20 4 35D 120 EZB HSG U OS (CI-235HTY)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234MRW","ICO ADJ 30/20 4 45D 120 EZB HSG U","ICO ADJ 30/20 4 45D 120 EZB HSG U (CI-234MRW)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239GYP","ICO ADJ 30/25 4 30D 277 EZ1 HSG U","ICO ADJ 30/25 4 30D 277 EZ1 HSG U (CI-239GYP)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["230H3E","ICO ADJ 30/30 6 55D 120 EZB HSG U OS","ICO ADJ 30/30 6 55D 120 EZB HSG U OS (CI-230H3E)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239TN0","ICO ADJ 30/60 6 40D 120 EZB HSG U","ICO ADJ 30/60 6 40D 120 EZB HSG U (CI-239TN0)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234TXN","ICO ADJ 35/10 4 40D 277 EZB HSG U","ICO ADJ 35/10 4 40D 277 EZB HSG U (CI-234TXN)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238GX7","ICO ADJ 35/15 4 35D 120 EZB SF NPS80EZ HSG U OS","ICO ADJ 35/15 4 35D 120 EZB SF NPS80EZ HSG U OS (CI-238GX7)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239MGY","ICO ADJ 35/20 4 25D 277 EZ10 HSG U OS","ICO ADJ 35/20 4 25D 277 EZ10 HSG U OS (CI-239MGY)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234HCN","ICO ADJ 35/20 6 30D 120 EZB HSG U OS","ICO ADJ 35/20 6 30D 120 EZB HSG U OS (CI-234HCN)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237A67","ICO ADJ 35/25 4 15D 277 EZB HSG U OS","ICO ADJ 35/25 4 15D 277 EZB HSG U OS (CI-237A67)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237LCV","ICO ADJ 35/30 6 20D 120 EZB HSG U OS","ICO ADJ 35/30 6 20D 120 EZB HSG U OS (CI-237LCV)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236FNU","ICO ADJ 35/35 6 40D 120 EZB NPS80EZ HSG U OS","ICO ADJ 35/35 6 40D 120 EZB NPS80EZ HSG U OS (CI-236FNU)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238REK","ICO ADJ 35/60 6 35D 120 EDXB HSG U OS","ICO ADJ 35/60 6 35D 120 EDXB HSG U OS (CI-238REK)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239F38","ICO ADJ 40/15 4 35D 120 EZ1 HSG U","ICO ADJ 40/15 4 35D 120 EZ1 HSG U (CI-239F38)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236EX6","ICO ADJ 40/20 6 55D 277 EZB HSG U OS","ICO ADJ 40/20 6 55D 277 EZB HSG U OS (CI-236EX6)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235N88","ICO ADJ 40/30 6 40D 120 EZB NPS80EZ HSG U OS","ICO ADJ 40/30 6 40D 120 EZB NPS80EZ HSG U OS (CI-235N88)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237FP6","ICO SQ 27/15 4 25D 120 EZB HSG U OS","ICO SQ 27/15 4 25D 120 EZB HSG U OS (CI-237FP6)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239F23","ICO SQ 27/65 6 40D 120 EZB HSG U","ICO SQ 27/65 6 40D 120 EZB HSG U (CI-239F23)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238XKC","ICO SQ 30/20 4 40D 120 EDXB HSG U","ICO SQ 30/20 4 40D 120 EDXB HSG U (CI-238XKC)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238XKE","ICO SQ 30/30 6 30D 120 EDXB HSG U","ICO SQ 30/30 6 30D 120 EDXB HSG U (CI-238XKE)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235PNC","ICO SQ 35/10 4 45D 120 EZB HSG U","ICO SQ 35/10 4 45D 120 EZB HSG U (CI-235PNC)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234NJY","ICO SQ 35/25 4 60D 120 EZB HSG U OS","ICO SQ 35/25 4 60D 120 EZB HSG U OS (CI-234NJY)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["229M50","ICO SQ 35/30 6 40D 277 EZB HSG U OS","ICO SQ 35/30 6 40D 277 EZB HSG U OS (CI-229M50)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239NVT","ICO SQ 35/60 6 40D 277 EZB HSG U","ICO SQ 35/60 6 40D 277 EZB HSG U (CI-239NVT)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237GCW","ICO SQ 40/15 4 35D 277 EZB HSG U","ICO SQ 40/15 4 35D 277 EZB HSG U (CI-237GCW)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237FM4","ICO SQ 40/30 4 45D 120 EZB HSG U","ICO SQ 40/30 4 45D 120 EZB HSG U (CI-237FM4)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235ACW","ICO SQ 40/50 6 70D 277 EZB HSG U OS","ICO SQ 40/50 6 70D 277 EZB HSG U OS (CI-235ACW)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235VYP","ICO SQADJ 30/15 4 25D 120 EDXB HSG U","ICO SQADJ 30/15 4 25D 120 EDXB HSG U (CI-235VYP)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237P9T","ICO SQADJ 35/20 4 15D 120 EZB HSG U SSQ OS","ICO SQADJ 35/20 4 15D 120 EZB HSG U SSQ OS (CI-237P9T)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236V6P","ICO SQADJ 40/25 4 45D 277 EZB HSG U","ICO SQADJ 40/25 4 45D 277 EZB HSG U (CI-236V6P)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["230TU9","MSL 10000LM L/LV MVOLT GZ10 35K 90CRI WH","MSL 10000LM L/LV MVOLT GZ10 35K 90CRI WH (CI-230TU9)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["226CUJ","MSL 3L CLO LP840","MSL 3L CLO LP840 (CI-226CUJ)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["231FYT","MSL 4000LM L/LV 120 GZ10 40K 80CRI LAOZU WH","MSL 4000LM L/LV 120 GZ10 40K 80CRI LAOZU WH (CI-231FYT)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["228KUW","MSL 4000LM L/LV 277 EZ1 50K 80CRI GLR WH","MSL 4000LM L/LV 277 EZ1 50K 80CRI GLR WH (CI-228KUW)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["234F3W","MSL 4000LM L/LV MVOLT EZ1 40K 80CRI PLR1LVG CRM WH","MSL 4000LM L/LV MVOLT EZ1 40K 80CRI PLR1LVG CRM WH (CI-234F3W)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["228V5V","MSL 4000LM L/LV MVOLT GZ10 35K 80CRI WH","MSL 4000LM L/LV MVOLT GZ10 35K 80CRI WH (CI-228V5V)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["227U72","MSL 4000LM MVOLT EZ1 35K 90CRI","MSL 4000LM MVOLT EZ1 35K 90CRI (CI-227U72)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["229NE4","MSL 4000LM SBL MVOLT EZ1 50K 80CRI WH","MSL 4000LM SBL MVOLT EZ1 50K 80CRI WH (CI-229NE4)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["231PN5","MSL 4000LM SBL MVOLT GZ10 50K 80CRI WH","MSL 4000LM SBL MVOLT GZ10 50K 80CRI WH (CI-231PN5)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["221UXG","MSL 4L LP840 CS1W 120 SSQ2","MSL 4L LP840 CS1W 120 SSQ2 (CI-221UXG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["228WH0","MSL 8000LM L/LV 120 GZ10 40K 90CRI CS1W WH","MSL 8000LM L/LV 120 GZ10 40K 90CRI CS1W WH (CI-228WH0)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["233UYA","MSL 8000LM L/LV MVOLT GZ10 40K 80CRI CS93W WH","MSL 8000LM L/LV MVOLT GZ10 40K 80CRI CS93W WH (CI-233UYA)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["232R4Y","TMSL 16000LM L/LV 120 GZ10 40K 80CRI CS3W WH","TMSL 16000LM L/LV 120 GZ10 40K 80CRI CS3W WH (CI-232R4Y)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["230RNA","TMSL 16000LM L/LV MVOLT GZ10 50K 80CRI WH","TMSL 16000LM L/LV MVOLT GZ10 50K 80CRI WH (CI-230RNA)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["226HXU","TMSL 16L LP840 PLR1LVG CRE","TMSL 16L LP840 PLR1LVG CRE (CI-226HXU)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["237FG3","TMSL 8000LM L/LV 120 GZ10 40K 80CRI CS1W PLR1LVG CRM WH","TMSL 8000LM L/LV 120 GZ10 40K 80CRI CS1W PLR1LVG CRM WH (CI-237FG3)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["233VE3","TMSL 8000LM L/LV 480 GZ10 40K 80CRI WH","TMSL 8000LM L/LV 480 GZ10 40K 80CRI WH (CI-233VE3)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["233VPH","TMSL 8000LM L/LV MVOLT EZ1 50K 80CRI WH","TMSL 8000LM L/LV MVOLT EZ1 50K 80CRI WH (CI-233VPH)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["231UL6","TMSL 8000LM L/LV MVOLT GZ10 40K 80CRI CS93W WH","TMSL 8000LM L/LV MVOLT GZ10 40K 80CRI CS93W WH (CI-231UL6)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["237C2L","TMSL 8000LM L/LV MVOLT GZ10 50K 90CRI CS93W PLR1G CRM WH","TMSL 8000LM L/LV MVOLT GZ10 50K 90CRI CS93W PLR1G CRM WH (CI-237C2L)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["232JGU","TMSL 8000LM SBL 277 GZ10 40K 90CRI GMF CRE WH","TMSL 8000LM SBL 277 GZ10 40K 90CRI GMF CRE WH (CI-232JGU)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["231E5E","TMSL 8000LM SBL MVOLT GZ10 40K 80CRI WH","TMSL 8000LM SBL MVOLT GZ10 40K 80CRI WH (CI-231E5E)","PS1050","Remote mount only","ELA PSRME IC","4 Boards in parallel instructions","*239MRJ"]
["227UGG","TMSL 8L LP850 CRM","TMSL 8L LP850 CRM (CI-227UGG)","PS1050","Remote mount only","ELA PSRME IC","2 Boards in parallel instructions","*239MRJ"]
["234MPP","EVO 27/10 4 WD MVOLT EZB HSG","EVO 27/10 4 WD MVOLT EZB HSG (CI-234MPP)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236CE6","EVO 27/10 6 WD MVOLT EZ1 CRI90 HSG","EVO 27/10 6 WD MVOLT EZ1 CRI90 HSG (CI-236CE6)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234HN9","EVO 27/15 4 WD MVOLT EDXB HSG","EVO 27/15 4 WD MVOLT EDXB HSG (CI-234HN9)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235NRK","EVO 27/15 6 MWD 120 ECOS2 HSG","EVO 27/15 6 MWD 120 ECOS2 HSG (CI-235NRK)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237X5M","EVO 27/20 4 MWD MVOLT EZ1 CRI90 HSG","EVO 27/20 4 MWD MVOLT EZ1 CRI90 HSG (CI-237X5M)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236CNP","EVO 27/20 6 MD MVOLT EZB HSG","EVO 27/20 6 MD MVOLT EZB HSG (CI-236CNP)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234WAH","EVO 27/20 6 WD MVOLT EZ1 HSG","EVO 27/20 6 WD MVOLT EZ1 HSG (CI-234WAH)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238G41","EVO 27/25 8 WD 120 EZ1 HSG","EVO 27/25 8 WD 120 EZ1 HSG (CI-238G41)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237KU0","EVO 27/35 6 MWD MVOLT EZ1 HSG","EVO 27/35 6 MWD MVOLT EZ1 HSG (CI-237KU0)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["230E59","EVO 30/06 4 120 AZ10 HSG GEN2","EVO 30/06 4 120 AZ10 HSG GEN2 (CI-230E59)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235U5U","EVO 30/07 4 WD 347 EZ1 HSG CSA","EVO 30/07 4 WD 347 EZ1 HSG CSA (CI-235U5U)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239FP6","EVO 30/10 4 MD 277 EZB NPS80EZER HSG","EVO 30/10 4 MD 277 EZB NPS80EZER HSG (CI-239FP6)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233LCV","EVO 30/10 4 MWD MVOLT EZ1 HSG","EVO 30/10 4 MWD MVOLT EZ1 HSG (CI-233LCV)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233X6C","EVO 30/10 4 WD MVOLT EZ1 HSG","EVO 30/10 4 WD MVOLT EZ1 HSG (CI-233X6C)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233KVM","EVO 30/10 6 MD MVOLT EZ1 HSG","EVO 30/10 6 MD MVOLT EZ1 HSG (CI-233KVM)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234PXK","EVO 30/10 6 WD 120 EZ1 SF HSG","EVO 30/10 6 WD 120 EZ1 SF HSG (CI-234PXK)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238HPH","EVO 30/15 4 MWD 120 EZB NPS80EZ HSG","EVO 30/15 4 MWD 120 EZB NPS80EZ HSG (CI-238HPH)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239J5G","EVO 30/15 4 WD 120 EZ1 NPS80EZ HSG USPOM","EVO 30/15 4 WD 120 EZ1 NPS80EZ HSG USPOM (CI-239J5G)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235RU9","EVO 30/15 6 MD 120 EZ1 NPS80EZ HSG","EVO 30/15 6 MD 120 EZ1 NPS80EZ HSG (CI-235RU9)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233R3E","EVO 30/15 6 MD MVOLT EZB HSG","EVO 30/15 6 MD MVOLT EZB HSG (CI-233R3E)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238CKW","EVO 30/15 6 MWD MVOLT EZ10 HSG","EVO 30/15 6 MWD MVOLT EZ10 HSG (CI-238CKW)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["230AAP","EVO 30/18 6 MVOLT AZ10 HSG GEN2","EVO 30/18 6 MVOLT AZ10 HSG GEN2 (CI-230AAP)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239MHE","EVO 30/20 4 MWD 120 EZB SF HSG","EVO 30/20 4 MWD 120 EZB SF HSG (CI-239MHE)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237WLR","EVO 30/20 4FL WD MVOLT EZ1 HSG","EVO 30/20 4FL WD MVOLT EZ1 HSG (CI-237WLR)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237AY2","EVO 30/20 6 WD 120 EZ1 SF HSG","EVO 30/20 6 WD 120 EZ1 SF HSG (CI-237AY2)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236UFK","EVO 30/25 4 MD MVOLT EZ1 HSG","EVO 30/25 4 MD MVOLT EZ1 HSG (CI-236UFK)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238JUT","EVO 30/25 6 MD 277 ECOS3 HSG","EVO 30/25 6 MD 277 ECOS3 HSG (CI-238JUT)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233KRA","EVO 30/25 6 MWD MVOLT EZB HSG","EVO 30/25 6 MWD MVOLT EZB HSG (CI-233KRA)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238LM7","EVO 30/25 8 MD 120 EZ1 NPS80EZ HSG","EVO 30/25 8 MD 120 EZ1 NPS80EZ HSG (CI-238LM7)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238PVU","EVO 30/25 8 VND 277 EZ1 HSG","EVO 30/25 8 VND 277 EZ1 HSG (CI-238PVU)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238KCJ","EVO 30/30 6 MD MVOLT EZ10 HSG","EVO 30/30 6 MD MVOLT EZ10 HSG (CI-238KCJ)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235GWA","EVO 30/30 6 WD MVOLT EZB HSG","EVO 30/30 6 WD MVOLT EZB HSG (CI-235GWA)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236C1M","EVO 30/40 6 MD MVOLT EZ1 HSG","EVO 30/40 6 MD MVOLT EZ1 HSG (CI-236C1M)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237PLT","EVO 35/07 4 MD 120 EZ1 NPS80EZ HSG","EVO 35/07 4 MD 120 EZ1 NPS80EZ HSG (CI-237PLT)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["232XYA","EVO 35/07 4 MWD MVOLT EZ1 HSG","EVO 35/07 4 MWD MVOLT EZ1 HSG (CI-232XYA)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["216XM7","EVO 35/10 4 120 ECOS3 HSG GEN2","EVO 35/10 4 120 ECOS3 HSG GEN2 (CI-216XM7)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237RX7","EVO 35/10 4 MD MVOLT EZ1 CRI90 HSG","EVO 35/10 4 MD MVOLT EZ1 CRI90 HSG (CI-237RX7)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234XHK","EVO 35/10 4 MWD 277 EZ1 NPS80EZ HSG","EVO 35/10 4 MWD 277 EZ1 NPS80EZ HSG (CI-234XHK)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234XG7","EVO 35/10 4 WD 120 EZ1 SF HSG","EVO 35/10 4 WD 120 EZ1 SF HSG (CI-234XG7)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233JUU","EVO 35/10 4 WD MVOLT EZB HSG","EVO 35/10 4 WD MVOLT EZB HSG (CI-233JUU)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238LAG","EVO 35/10 6 MD 347 EZ1 NPS80EZ HSG CSA","EVO 35/10 6 MD 347 EZ1 NPS80EZ HSG CSA (CI-238LAG)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238XER","EVO 35/10 6 MWD 120 ECOS3 HSG","EVO 35/10 6 MWD 120 ECOS3 HSG (CI-238XER)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234E5F","EVO 35/10 6 MWD 277 EZ1 NPS80EZ HSG","EVO 35/10 6 MWD 277 EZ1 NPS80EZ HSG (CI-234E5F)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233CYT","EVO 35/10 6 MWD MVOLT EZ1 HSG","EVO 35/10 6 MWD MVOLT EZ1 HSG (CI-233CYT)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234V36","EVO 35/10 6 WD 277 EZ1 NPS80EZ HSG","EVO 35/10 6 WD 277 EZ1 NPS80EZ HSG (CI-234V36)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["224MUU","EVO 35/14 4 120 ECOS2 HSG GEN2","EVO 35/14 4 120 ECOS2 HSG GEN2 (CI-224MUU)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236TX3","EVO 35/15 4 MD 277 EZ1 NPS80EZER HSG","EVO 35/15 4 MD 277 EZ1 NPS80EZER HSG (CI-236TX3)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["232YKJ","EVO 35/15 4 MVOLT EZ1 HSG","EVO 35/15 4 MVOLT EZ1 HSG (CI-232YKJ)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234RJ4","EVO 35/15 4 WD 277 EZB NPS80EZ HSG","EVO 35/15 4 WD 277 EZB NPS80EZ HSG (CI-234RJ4)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["232VTN","EVO 35/15 6  MVOLT EZ1 HSG","EVO 35/15 6  MVOLT EZ1 HSG (CI-232VTN)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233P6P","EVO 35/15 6 MD 277 ECOS3 HSG","EVO 35/15 6 MD 277 ECOS3 HSG (CI-233P6P)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234KLV","EVO 35/15 6 MD MVOLT EDXB HSG","EVO 35/15 6 MD MVOLT EDXB HSG (CI-234KLV)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237FG8","EVO 35/15 6 MWD 120 EZ1 SF HSG CP","EVO 35/15 6 MWD 120 EZ1 SF HSG CP (CI-237FG8)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237J1A","EVO 35/15 6 MWD 347 EZ1 CRI90 HSG CSA","EVO 35/15 6 MWD 347 EZ1 CRI90 HSG CSA (CI-237J1A)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233LGJ","EVO 35/15 6 VND MVOLT EZ1 HSG","EVO 35/15 6 VND MVOLT EZ1 HSG (CI-233LGJ)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235GAC","EVO 35/15 6 WD MVOLT EZ1 CRI90 HSG","EVO 35/15 6 WD MVOLT EZ1 CRI90 HSG (CI-235GAC)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234J2K","EVO 35/20 4 MD 277 AZ10 NPP16D HSG GEN2","EVO 35/20 4 MD 277 AZ10 NPP16D HSG GEN2 (CI-234J2K)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235LMH","EVO 35/20 4 MWD 120 EZ1 NPS80EZER HSG","EVO 35/20 4 MWD 120 EZ1 NPS80EZER HSG (CI-235LMH)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238LGU","EVO 35/20 4 WD 120 ECOS3 HSG","EVO 35/20 4 WD 120 ECOS3 HSG (CI-238LGU)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233TKN","EVO 35/20 4 WD MVOLT EZB HSG","EVO 35/20 4 WD MVOLT EZB HSG (CI-233TKN)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235YY1","EVO 35/20 6 MD 120 EZ1 NPS80EZER HSG","EVO 35/20 6 MD 120 EZ1 NPS80EZER HSG (CI-235YY1)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239FKK","EVO 35/20 6 MD 277 EZ10 SF HSG","EVO 35/20 6 MD 277 EZ10 SF HSG (CI-239FKK)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233FCP","EVO 35/20 6 MVOLT EZ1 HSG","EVO 35/20 6 MVOLT EZ1 HSG (CI-233FCP)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233X7F","EVO 35/20 6 MWD 120 EZB NPS80EZ HSG","EVO 35/20 6 MWD 120 EZB NPS80EZ HSG (CI-233X7F)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["232WTC","EVO 35/20 6 ND MVOLT EZ1 HSG","EVO 35/20 6 ND MVOLT EZ1 HSG (CI-232WTC)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235JPF","EVO 35/20 6 WD 277 EZ1 SF HSG","EVO 35/20 6 WD 277 EZ1 SF HSG (CI-235JPF)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233G1W","EVO 35/20 6 WD MVOLT EZB HSG","EVO 35/20 6 WD MVOLT EZB HSG (CI-233G1W)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235KFA","EVO 35/20 8 MD 277 EZ1 NPS80EZ HSG","EVO 35/20 8 MD 277 EZ1 NPS80EZ HSG (CI-235KFA)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237T93","EVO 35/20 8 MWD 120 EZ1 SF HSG","EVO 35/20 8 MWD 120 EZ1 SF HSG (CI-237T93)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239TMW","EVO 35/20 8 WD 120 EZ10 HSG","EVO 35/20 8 WD 120 EZ10 HSG (CI-239TMW)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235L4K","EVO 35/25 4 WD MVOLT EZ1 HSG","EVO 35/25 4 WD MVOLT EZ1 HSG (CI-235L4K)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239G37","EVO 35/25 6 MD 120 EZ1 SF HSG","EVO 35/25 6 MD 120 EZ1 SF HSG (CI-239G37)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235VNM","EVO 35/25 6 MWD 277 ECOS3 HSG","EVO 35/25 6 MWD 277 ECOS3 HSG (CI-235VNM)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238U3V","EVO 35/25 6 ND 120 EZ1 SF HSG","EVO 35/25 6 ND 120 EZ1 SF HSG (CI-238U3V)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236CAK","EVO 35/25 6 WD 277 EZ1 NPS80EZER HSG","EVO 35/25 6 WD 277 EZ1 NPS80EZER HSG (CI-236CAK)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239ULH","EVO 35/25 8 MWD 120 EZ10 HSG","EVO 35/25 8 MWD 120 EZ10 HSG (CI-239ULH)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236A2F","EVO 35/25 8 WD 277 EZ1 SF HSG","EVO 35/25 8 WD 277 EZ1 SF HSG (CI-236A2F)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233YKY","EVO 35/30 4 WD MVOLT EZ1 HSG","EVO 35/30 4 WD MVOLT EZ1 HSG (CI-233YKY)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239TKR","EVO 35/30 6 MWD 120 EZ1 HSG CP","EVO 35/30 6 MWD 120 EZ1 HSG CP (CI-239TKR)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239TKY","EVO 35/30 6 VND MVOLT EZB HSG","EVO 35/30 6 VND MVOLT EZB HSG (CI-239TKY)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238UWT","EVO 35/30 8 MD 120 EZ1 CRI90 HSG","EVO 35/30 8 MD 120 EZ1 CRI90 HSG (CI-238UWT)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238RGT","EVO 35/30 8 VND 120 EZ1 HSG","EVO 35/30 8 VND 120 EZ1 HSG (CI-238RGT)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236RXF","EVO 35/35 6 MD MVOLT EZB HSG","EVO 35/35 6 MD MVOLT EZB HSG (CI-236RXF)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238MKJ","EVO 35/40 6 ND 277 EZB NPS80EZ HSG","EVO 35/40 6 ND 277 EZB NPS80EZ HSG (CI-238MKJ)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["232VX3","EVO 35/45 6 MWD MVOLT EZ1 HSG","EVO 35/45 6 MWD MVOLT EZ1 HSG (CI-232VX3)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237RNY","EVO 35/45 6 WD 277 EZB SF HSG","EVO 35/45 6 WD 277 EZB SF HSG (CI-237RNY)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234ERU","EVO 40/07 4 MWD 120 EZ1 NPS80EZ HSG","EVO 40/07 4 MWD 120 EZ1 NPS80EZ HSG (CI-234ERU)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237PL1","EVO 40/07 4FL MD MVOLT EZB HSG","EVO 40/07 4FL MD MVOLT EZB HSG (CI-237PL1)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236F4V","EVO 40/10 4 MD MVOLT EZ1 CRI90 HSG","EVO 40/10 4 MD MVOLT EZ1 CRI90 HSG (CI-236F4V)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238XH5","EVO 40/10 4FL MD MVOLT EZ1 HSG","EVO 40/10 4FL MD MVOLT EZ1 HSG (CI-238XH5)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238HMJ","EVO 40/10 6 MD 277 EZB NPS80EZ CRI90 HSG","EVO 40/10 6 MD 277 EZB NPS80EZ CRI90 HSG (CI-238HMJ)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235YX8","EVO 40/10 6 MWD 120 EZB NPS80EZ HSG","EVO 40/10 6 MWD 120 EZB NPS80EZ HSG (CI-235YX8)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238XKH","EVO 40/10 6 MWD MVOLT EZ10 HSG","EVO 40/10 6 MWD MVOLT EZ10 HSG (CI-238XKH)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238UM3","EVO 40/10 6 WD MVOLT EZ10 HSG","EVO 40/10 6 WD MVOLT EZ10 HSG (CI-238UM3)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236VE9","EVO 40/15 4 MD MVOLT EZ1 HSG USPOM","EVO 40/15 4 MD MVOLT EZ1 HSG USPOM (CI-236VE9)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233NUK","EVO 40/15 4 MWD MVOLT EZ1 HSG","EVO 40/15 4 MWD MVOLT EZ1 HSG (CI-233NUK)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235J0K","EVO 40/15 6 MD 120 EZ1 SF HSG","EVO 40/15 6 MD 120 EZ1 SF HSG (CI-235J0K)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239EY6","EVO 40/15 6 MWD 120 EZ1 SF CRI90 HSG","EVO 40/15 6 MWD 120 EZ1 SF CRI90 HSG (CI-239EY6)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235LLX","EVO 40/15 6 MWD 277 EZB NPS80EZ HSG","EVO 40/15 6 MWD 277 EZB NPS80EZ HSG (CI-235LLX)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239J77","EVO 40/15 6 ND 120 EZ1 SF HSG","EVO 40/15 6 ND 120 EZ1 SF HSG (CI-239J77)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237FJA","EVO 40/15 6 WD 277 EZB NPS80EZER HSG","EVO 40/15 6 WD 277 EZB NPS80EZER HSG (CI-237FJA)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236JN1","EVO 40/20 4 MD 277 EZ1 NPS80EZ HSG","EVO 40/20 4 MD 277 EZ1 NPS80EZ HSG (CI-236JN1)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236GMX","EVO 40/20 4 MWD 277 EZ1 NPS80EZ HSG","EVO 40/20 4 MWD 277 EZ1 NPS80EZ HSG (CI-236GMX)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235T8H","EVO 40/20 4 WD 347 EZ1 HSG CSA","EVO 40/20 4 WD 347 EZ1 HSG CSA (CI-235T8H)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236MVV","EVO 40/20 6 MD 277 EZ1 NPS80EZ HSG","EVO 40/20 6 MD 277 EZ1 NPS80EZ HSG (CI-236MVV)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234PG0","EVO 40/20 6 MWD 277 ECOS3 HSG","EVO 40/20 6 MWD 277 ECOS3 HSG (CI-234PG0)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234WXX","EVO 40/20 6 MWD MVOLT EZ1 HSG ST3 USPOM","EVO 40/20 6 MWD MVOLT EZ1 HSG ST3 USPOM (CI-234WXX)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236W91","EVO 40/20 6 WD 277 EZ1 NPS80EZER HSG","EVO 40/20 6 WD 277 EZ1 NPS80EZER HSG (CI-236W91)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235C0K","EVO 40/20 6 WD MVOLT EZB HSG","EVO 40/20 6 WD MVOLT EZB HSG (CI-235C0K)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234PXG","EVO 40/20 8 MWD 120 EZ1 HSG USPOM","EVO 40/20 8 MWD 120 EZ1 HSG USPOM (CI-234PXG)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233GUW","EVO 40/20 8 WD 120 EZ1 HSG","EVO 40/20 8 WD 120 EZ1 HSG (CI-233GUW)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239J44","EVO 40/25 4 MD 277 EZ1 NPS80EZ HSG","EVO 40/25 4 MD 277 EZ1 NPS80EZ HSG (CI-239J44)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237M34","EVO 40/25 6 MD 277 EZB NPS80EZ HSG","EVO 40/25 6 MD 277 EZB NPS80EZ HSG (CI-237M34)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233U2C","EVO 40/25 6 MWD MVOLT EZ1 HSG","EVO 40/25 6 MWD MVOLT EZ1 HSG (CI-233U2C)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239J3X","EVO 40/25 6 ND 277 EZ1 NPS80EZER HSG","EVO 40/25 6 ND 277 EZ1 NPS80EZER HSG (CI-239J3X)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234EJR","EVO 40/25 8 WD 120 EZ1 HSG","EVO 40/25 8 WD 120 EZ1 HSG (CI-234EJR)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239E05","EVO 40/30 4 WD 120 EZ1 SF HSG","EVO 40/30 4 WD 120 EZ1 SF HSG (CI-239E05)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237RPW","EVO 40/30 6 MD MVOLT EZ1 HSG USPOM","EVO 40/30 6 MD MVOLT EZ1 HSG USPOM (CI-237RPW)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236RVU","EVO 40/30 6 WD 347 EZ1 SF HSG CSA","EVO 40/30 6 WD 347 EZ1 SF HSG CSA (CI-236RVU)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238TEJ","EVO 40/30 8 MD 120 EZ1 SF HSG","EVO 40/30 8 MD 120 EZ1 SF HSG (CI-238TEJ)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239M1E","EVO 40/30 8 MWD 120 EZ10 HSG","EVO 40/30 8 MWD 120 EZ10 HSG (CI-239M1E)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235MPF","EVO 40/35 6 MD MVOLT EZ1 HSG","EVO 40/35 6 MD MVOLT EZ1 HSG (CI-235MPF)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234PC1","EVO 40/35 6 MWD 347 EZ1 HSG CSA","EVO 40/35 6 MWD 347 EZ1 HSG CSA (CI-234PC1)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234GYX","EVO 40/40 6 WD MVOLT EZ1 HSG","EVO 40/40 6 WD MVOLT EZ1 HSG (CI-234GYX)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239M1G","EVO 40/45 6 MWD MVOLT EZ10 HSG","EVO 40/45 6 MWD MVOLT EZ10 HSG (CI-239M1G)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["223CG9","EVO 41/18 4 WD 277 HSG GEN2","EVO 41/18 4 WD 277 HSG GEN2 (CI-223CG9)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["230A11","EVO 41/29 8 277 AZ10 HSG","EVO 41/29 8 277 AZ10 HSG (CI-230A11)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["232VHA","EVO 4AR LSS TRIM U","EVO 4AR LSS TRIM U (CI-232VHA)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["220KWV","EVO 4ARFL LD TRIM U","EVO 4ARFL LD TRIM U (CI-220KWV)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233LEH","EVO 4PR LSS TRIM U","EVO 4PR LSS TRIM U (CI-233LEH)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["232YKF","EVO 4PR LSS TRW TRIM U","EVO 4PR LSS TRW TRIM U (CI-232YKF)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["217AL9","EVO 6AR LD TRW TRIM USPOM U","EVO 6AR LD TRW TRIM USPOM U (CI-217AL9)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["217ALG","EVO 6AR LS TRW TRIM U","EVO 6AR LS TRW TRIM U (CI-217ALG)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["216XEW","EVO 6AR TRIM NATS U","EVO 6AR TRIM NATS U (CI-216XEW)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236JPC","EVO 6BR DECO TRIM U","EVO 6BR DECO TRIM U (CI-236JPC)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["221U9J","EVO 6DFR TRIM USPOM U","EVO 6DFR TRIM USPOM U (CI-221U9J)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["217AM3","EVO 6PR LD TRIM U","EVO 6PR LD TRIM U (CI-217AM3)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233TJ9","EVO 6WTR LSS TRIM U","EVO 6WTR LSS TRIM U (CI-233TJ9)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235RU7","EVO 6WTR LSS TRW TRIM U","EVO 6WTR LSS TRW TRIM U (CI-235RU7)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["216XAP","EVO 8AR TRIM U","EVO 8AR TRIM U (CI-216XAP)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238EXN","EVO 8PR LSS TRIM U","EVO 8PR LSS TRIM U (CI-238EXN)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238X32","EVO CYL 27/10 6AR ND LS MVOLT EZ1 ACC DBL","EVO CYL 27/10 6AR ND LS MVOLT EZ1 ACC DBL (CI-238X32)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234R2L","EVO CYL 27/15 6AR WD LSS MVOLT EZ1 FCM DBL","EVO CYL 27/15 6AR WD LSS MVOLT EZ1 FCM DBL (CI-234R2L)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239GWR","EVO CYL 27/25 6AR MWD LSS 120 ECOS2 PM DMB","EVO CYL 27/25 6AR MWD LSS 120 ECOS2 PM DMB (CI-239GWR)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239EH7","EVO CYL 27/30 6AR MD LSS 120 ECOS2 PM DDB","EVO CYL 27/30 6AR MD LSS 120 ECOS2 PM DDB (CI-239EH7)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237FA8","EVO CYL 30/10 6AR MD LS MVOLT EDAB PM DWHG","EVO CYL 30/10 6AR MD LS MVOLT EDAB PM DWHG (CI-237FA8)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239FWJ","EVO CYL 30/10 6AR MD LSS MVOLT EZ1 ACC DWHG","EVO CYL 30/10 6AR MD LSS MVOLT EZ1 ACC DWHG (CI-239FWJ)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237NXF","EVO CYL 30/15 6AR MWD LSS MVOLT EZ1 ACC CRI90 DGC","EVO CYL 30/15 6AR MWD LSS MVOLT EZ1 ACC CRI90 DGC (CI-237NXF)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237MG1","EVO CYL 30/15 6BR WD 277 EZ1 PM SF DGC","EVO CYL 30/15 6BR WD 277 EZ1 PM SF DGC (CI-237MG1)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234TY4","EVO CYL 30/20 6AR MD LS MVOLT EZ1 ACC180 DNA","EVO CYL 30/20 6AR MD LS MVOLT EZ1 ACC180 DNA (CI-234TY4)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
[{"$f":"(LEFT((RIGHT(C22044,7)),6))","v":"235X5P"},{"$f":"LEFT(C22044,SEARCH(\"(CI-\",C22044)-2)","v":"EVO CYL 30/20 6AR MWD LD MVOLT EZ1 FCM DBL"},"EVO CYL 30/20 6AR MWD LD MVOLT EZ1 FCM DBL (CI-235X5P)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236J38","EVO CYL 30/20 6AR WD LSS MVOLT EZ1 FCM DWHG","EVO CYL 30/20 6AR WD LSS MVOLT EZ1 FCM DWHG (CI-236J38)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234KL8","EVO CYL 30/20 8AR MD LD MVOLT EZ1 PM DWHG","EVO CYL 30/20 8AR MD LD MVOLT EZ1 PM DWHG (CI-234KL8)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235EVM","EVO CYL 30/25 6AR WD LD MVOLT EZ1 PM DBL","EVO CYL 30/25 6AR WD LD MVOLT EZ1 PM DBL (CI-235EVM)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239FHU","EVO CYL 30/25 6AR WD LD MVOLT EZB PM DGC","EVO CYL 30/25 6AR WD LD MVOLT EZB PM DGC (CI-239FHU)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237ENJ","EVO CYL 30/30 6AR MD LSS MVOLT EZ1 ACC180 DBL","EVO CYL 30/30 6AR MD LSS MVOLT EZ1 ACC180 DBL (CI-237ENJ)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235TAH","EVO CYL 30/30 8AR MWD LD MVOLT EZ1 FCM DNA","EVO CYL 30/30 8AR MWD LD MVOLT EZ1 FCM DNA (CI-235TAH)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237FLM","EVO CYL 30/30 8WR MD MVOLT EZ1 FCM DWHG","EVO CYL 30/30 8WR MD MVOLT EZ1 FCM DWHG (CI-237FLM)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236CY2","EVO CYL 30/35 6AR WD LSS MVOLT EZ1 PM DWHG","EVO CYL 30/35 6AR WD LSS MVOLT EZ1 PM DWHG (CI-236CY2)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236JTG","EVO CYL 30/45 6AR MWD LD MVOLT EZ1 PM DWHG","EVO CYL 30/45 6AR MWD LD MVOLT EZ1 PM DWHG (CI-236JTG)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235V4L","EVO CYL 30/45 6AR WD LSS MVOLT EZB ACC DDB","EVO CYL 30/45 6AR WD LSS MVOLT EZB ACC DDB (CI-235V4L)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238YX1","EVO CYL 35/10 6AR MD LSS MVOLT EZB PM DWHG USPOM","EVO CYL 35/10 6AR MD LSS MVOLT EZB PM DWHG USPOM (CI-238YX1)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239AFA","EVO CYL 35/10 6AR MWD LD MVOLT EZ1 ACC DWHG","EVO CYL 35/10 6AR MWD LD MVOLT EZ1 ACC DWHG (CI-239AFA)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238AK5","EVO CYL 35/10 6AR WD LS MVOLT EZ1 PM DBL","EVO CYL 35/10 6AR WD LS MVOLT EZ1 PM DBL (CI-238AK5)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238NVV","EVO CYL 35/10 6BR WD MVOLT EZ1 PM DBL","EVO CYL 35/10 6BR WD MVOLT EZ1 PM DBL (CI-238NVV)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237RFL","EVO CYL 35/15 6AR MD LD MVOLT EZ1 FCM DBL","EVO CYL 35/15 6AR MD LD MVOLT EZ1 FCM DBL (CI-237RFL)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
[{"$f":"(LEFT((RIGHT(C22236,7)),6))","v":"235MW0"},{"$f":"LEFT(C22236,SEARCH(\"(CI-\",C22236)-2)","v":"EVO CYL 35/15 6AR MD LSS MVOLT EZ1 ACC DBL"},"EVO CYL 35/15 6AR MD LSS MVOLT EZ1 ACC DBL (CI-235MW0)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236JTJ","EVO CYL 35/15 6AR MWD LS MVOLT EZ1 ACC DWHG","EVO CYL 35/15 6AR MWD LS MVOLT EZ1 ACC DWHG (CI-236JTJ)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235WMG","EVO CYL 35/15 6AR MWD LSS MVOLT EZ1 WM DDB","EVO CYL 35/15 6AR MWD LSS MVOLT EZ1 WM DDB (CI-235WMG)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239A62","EVO CYL 35/15 6BR MWD MVOLT EZ1 FCM DBL","EVO CYL 35/15 6BR MWD MVOLT EZ1 FCM DBL (CI-239A62)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235FWC","EVO CYL 35/15 6BR MWD MVOLT EZ1 FCM DWHG","EVO CYL 35/15 6BR MWD MVOLT EZ1 FCM DWHG (CI-235FWC)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
[{"$f":"(LEFT((RIGHT(C22300,7)),6))","v":"237V97"},{"$f":"LEFT(C22300,SEARCH(\"(CI-\",C22300)-2)","v":"EVO CYL 35/20 6AR MD LD MVOLT EZ1 PM DDB"},"EVO CYL 35/20 6AR MD LD MVOLT EZ1 PM DDB (CI-237V97)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233TC4","EVO CYL 35/20 6AR MD LSS MVOLT EZ1 FCM DBL","EVO CYL 35/20 6AR MD LSS MVOLT EZ1 FCM DBL (CI-233TC4)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238YLU","EVO CYL 35/20 6AR MD LSS MVOLT EZ10 WM DWHG","EVO CYL 35/20 6AR MD LSS MVOLT EZ10 WM DWHG (CI-238YLU)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238CWU","EVO CYL 35/20 6AR MWD LSS MVOLT EZ1 ACC DBL","EVO CYL 35/20 6AR MWD LSS MVOLT EZ1 ACC DBL (CI-238CWU)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237L1A","EVO CYL 35/20 6AR MWD LSS MVOLT EZB ACC180 DWHG","EVO CYL 35/20 6AR MWD LSS MVOLT EZB ACC180 DWHG (CI-237L1A)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235WM3","EVO CYL 35/20 6AR WD LS MVOLT EZ1 WM DWHG","EVO CYL 35/20 6AR WD LS MVOLT EZ1 WM DWHG (CI-235WM3)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236XL7","EVO CYL 35/20 6WTR WD LSS MVOLT EZ1 ACC180 DWHG","EVO CYL 35/20 6WTR WD LSS MVOLT EZ1 ACC180 DWHG (CI-236XL7)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235GUL","EVO CYL 35/20 8AR MWD LSS MVOLT EZ1 ACC DWHG","EVO CYL 35/20 8AR MWD LSS MVOLT EZ1 ACC DWHG (CI-235GUL)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235GY6","EVO CYL 35/25 6AR MD LSS MVOLT EZ1 PM DWHG","EVO CYL 35/25 6AR MD LSS MVOLT EZ1 PM DWHG (CI-235GY6)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236JLG","EVO CYL 35/25 6AR MWD LSS MVOLT EZ1 FCM DBL","EVO CYL 35/25 6AR MWD LSS MVOLT EZ1 FCM DBL (CI-236JLG)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239T47","EVO CYL 35/25 6AR WD LD MVOLT EZ1 ACC DWHG","EVO CYL 35/25 6AR WD LD MVOLT EZ1 ACC DWHG (CI-239T47)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238XEC","EVO CYL 35/25 6BR MWD MVOLT ECOS3 PM DBL","EVO CYL 35/25 6BR MWD MVOLT ECOS3 PM DBL (CI-238XEC)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237MK2","EVO CYL 35/25 8AR MWD LSS MVOLT EZ1 FCM DWHG","EVO CYL 35/25 8AR MWD LSS MVOLT EZ1 FCM DWHG (CI-237MK2)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237EMP","EVO CYL 35/25 8BR WD MVOLT EZ1 FCM DBL","EVO CYL 35/25 8BR WD MVOLT EZ1 FCM DBL (CI-237EMP)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238YX8","EVO CYL 35/30 6AR MD LSS MVOLT EZ1 ACC DBL","EVO CYL 35/30 6AR MD LSS MVOLT EZ1 ACC DBL (CI-238YX8)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233WXT","EVO CYL 35/30 6AR MWD LSS MVOLT EZ1 ACC DWHG","EVO CYL 35/30 6AR MWD LSS MVOLT EZ1 ACC DWHG (CI-233WXT)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
[{"$f":"(LEFT((RIGHT(C22492,7)),6))","v":"236PXW"},{"$f":"LEFT(C22492,SEARCH(\"(CI-\",C22492)-2)","v":"EVO CYL 35/30 8AR MD LS MVOLT EZ1 FCM DWHG"},"EVO CYL 35/30 8AR MD LS MVOLT EZ1 FCM DWHG (CI-236PXW)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236E3W","EVO CYL 35/30 8AR MWD LSS MVOLT EZ1 PM DWHG USPOM","EVO CYL 35/30 8AR MWD LSS MVOLT EZ1 PM DWHG USPOM (CI-236E3W)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239T6M","EVO CYL 35/30 8AR WD LS MVOLT EZB PM DWHG","EVO CYL 35/30 8AR WD LS MVOLT EZB PM DWHG (CI-239T6M)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237V7T","EVO CYL 35/35 6AR MWD LSS MVOLT EZ1 FCM DWHG","EVO CYL 35/35 6AR MWD LSS MVOLT EZ1 FCM DWHG (CI-237V7T)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239F1Y","EVO CYL 35/40 6AR MD LD MVOLT EZ10 ACC DWH","EVO CYL 35/40 6AR MD LD MVOLT EZ10 ACC DWH (CI-239F1Y)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236JKC","EVO CYL 35/40 6AR WD LS MVOLT EZ1 ACC DWH","EVO CYL 35/40 6AR WD LS MVOLT EZ1 ACC DWH (CI-236JKC)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238NA8","EVO CYL 35/45 6AR ND LSS MVOLT EZ1 ACC DWHG","EVO CYL 35/45 6AR ND LSS MVOLT EZ1 ACC DWHG (CI-238NA8)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238HUY","EVO CYL 40/10 6AR MD LS MVOLT EZ1 FCM DWHG","EVO CYL 40/10 6AR MD LS MVOLT EZ1 FCM DWHG (CI-238HUY)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237EK1","EVO CYL 40/15 6AR MD LD MVOLT EZ1 PM DWHG","EVO CYL 40/15 6AR MD LD MVOLT EZ1 PM DWHG (CI-237EK1)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239LP0","EVO CYL 40/15 6AR MWD LSS MVOLT EZ1 ACC180 DNA","EVO CYL 40/15 6AR MWD LSS MVOLT EZ1 ACC180 DNA (CI-239LP0)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239M1K","EVO CYL 40/15 6BRW MVOLT EZ1 PM DBL","EVO CYL 40/15 6BRW MVOLT EZ1 PM DBL (CI-239M1K)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238HUW","EVO CYL 40/20 6AR MD LS MVOLT EZ1 PM DBL","EVO CYL 40/20 6AR MD LS MVOLT EZ1 PM DBL (CI-238HUW)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238HMK","EVO CYL 40/20 6AR MD LSS MVOLT EZ1 FCM DBL","EVO CYL 40/20 6AR MD LSS MVOLT EZ1 FCM DBL (CI-238HMK)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237YNH","EVO CYL 40/20 6AR MWD LSS MVOLT EZ1 WM DDB","EVO CYL 40/20 6AR MWD LSS MVOLT EZ1 WM DDB (CI-237YNH)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235GVU","EVO CYL 40/20 6PR WD LD MVOLT EZ1 WM DDB","EVO CYL 40/20 6PR WD LD MVOLT EZ1 WM DDB (CI-235GVU)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237V39","EVO CYL 40/20 8AR MD LSS 120 EZ1 ACC NPS80EZ DWHG","EVO CYL 40/20 8AR MD LSS 120 EZ1 ACC NPS80EZ DWHG (CI-237V39)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239TCH","EVO CYL 40/25 6AR MD LSS MVOLT EZ1 ACC DWH","EVO CYL 40/25 6AR MD LSS MVOLT EZ1 ACC DWH (CI-239TCH)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238HP7","EVO CYL 40/25 8AR WD LSS 277 EZ1 FCM NPS80EZER DDB","EVO CYL 40/25 8AR WD LSS 277 EZ1 FCM NPS80EZER DDB (CI-238HP7)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238ENG","EVO CYL 40/30 6AR MD LSS MVOLT EZ1 PM DBL","EVO CYL 40/30 6AR MD LSS MVOLT EZ1 PM DBL (CI-238ENG)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238KXX","EVO CYL 40/30 6BR MWD MVOLT EZ1 FCM DWHG","EVO CYL 40/30 6BR MWD MVOLT EZ1 FCM DWHG (CI-238KXX)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236WWJ","EVO CYL 40/30 8AR MWD LD MVOLT EZ1 PM DNA","EVO CYL 40/30 8AR MWD LD MVOLT EZ1 PM DNA (CI-236WWJ)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235KLM","EVO CYL 40/30 8AR WD LSS MVOLT EZ1 ACC DWHG","EVO CYL 40/30 8AR WD LSS MVOLT EZ1 ACC DWHG (CI-235KLM)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235PNE","EVO CYL 40/40 6AR MD LS MVOLT EZ1 FCM DWHG","EVO CYL 40/40 6AR MD LS MVOLT EZ1 FCM DWHG (CI-235PNE)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238C3L","EVO CYL 40/45 6AR MD LD 120 EZ1 PM NPS80EZ DWHG","EVO CYL 40/45 6AR MD LD 120 EZ1 PM NPS80EZ DWHG (CI-238C3L)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["229TXP","EVO CYL 41/22 6AR WD MVOLT WM DWHG GEN2","EVO CYL 41/22 6AR WD MVOLT WM DWHG GEN2 (CI-229TXP)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["220WK9","EVO LW 30/10 6AR TRIM U","EVO LW 30/10 6AR TRIM U (CI-220WK9)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238TEG","EVO LW 30/14 6AR LD TRW TRIM U","EVO LW 30/14 6AR LD TRW TRIM U (CI-238TEG)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["225FE6","EVO LW 30/20 4AR LD TRIM U","EVO LW 30/20 4AR LD TRIM U (CI-225FE6)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["224K9E","EVO LW 30/22 6AR TRW TRIM U","EVO LW 30/22 6AR TRW TRIM U (CI-224K9E)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["221ERF","EVO LW 35/10 6AR LD TRW TRIM U","EVO LW 35/10 6AR LD TRW TRIM U (CI-221ERF)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["224XUM","EVO LW 35/14 4AR TRW TRIM U","EVO LW 35/14 4AR TRW TRIM U (CI-224XUM)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235THE","EVO LW 35/18 4AR LS TRW TRIM U","EVO LW 35/18 4AR LS TRW TRIM U (CI-235THE)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["221G87","EVO LW 35/20 4AR TRIM U","EVO LW 35/20 4AR TRIM U (CI-221G87)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["231FCG","EVO LW 4 120 EZB HSG","EVO LW 4 120 EZB HSG (CI-231FCG)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["232KTR","EVO LW 4 277 EZB HSG","EVO LW 4 277 EZB HSG (CI-232KTR)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["224HM1","EVO LW 41/14 6AR TRIM U","EVO LW 41/14 6AR TRIM U (CI-224HM1)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["218W07","EVO LW 41/18 6AR TRW TRIM U","EVO LW 41/18 6AR TRW TRIM U (CI-218W07)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238PW9","EVO LW 6 120 EZ1 NPS80EZ HSG","EVO LW 6 120 EZ1 NPS80EZ HSG (CI-238PW9)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236H1G","EVO LW 6 277 AZ10 HSG NATS","EVO LW 6 277 AZ10 HSG NATS (CI-236H1G)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239CHA","EVO R 27/07 4 MWD MVOLT EZ10 HSG","EVO R 27/07 4 MWD MVOLT EZ10 HSG (CI-239CHA)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239HHM","EVO R 27/20 6 MWD MVOLT EZB HSG","EVO R 27/20 6 MWD MVOLT EZB HSG (CI-239HHM)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236KUX","EVO R 30/15 4 WD MVOLT EZ1 HSG","EVO R 30/15 4 WD MVOLT EZ1 HSG (CI-236KUX)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236EX2","EVO R 30/20 6 WD 347 EZ1 HSG CSA","EVO R 30/20 6 WD 347 EZ1 HSG CSA (CI-236EX2)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238MJC","EVO R 35/10 4 MWD MVOLT EZ10 HSG","EVO R 35/10 4 MWD MVOLT EZ10 HSG (CI-238MJC)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238PTM","EVO R 35/10 6 MWD MVOLT EZ10 HSG","EVO R 35/10 6 MWD MVOLT EZ10 HSG (CI-238PTM)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238EYR","EVO R 35/15 6 MWD MVOLT EZ10 HSG","EVO R 35/15 6 MWD MVOLT EZ10 HSG (CI-238EYR)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237RUA","EVO R 35/20 4 WD MVOLT EZB HSG","EVO R 35/20 4 WD MVOLT EZB HSG (CI-237RUA)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235C91","EVO R 35/20 8 MD 277 EZ1 HSG","EVO R 35/20 8 MD 277 EZ1 HSG (CI-235C91)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235KCP","EVO R 35/25 6 WD MVOLT EZ1 HSG","EVO R 35/25 6 WD MVOLT EZ1 HSG (CI-235KCP)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235MHT","EVO R 40/10 6 MWD MVOLT EZ1 HSG","EVO R 40/10 6 MWD MVOLT EZ1 HSG (CI-235MHT)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236RUN","EVO R 40/20 6 MWD MVOLT EDXB HSG","EVO R 40/20 6 MWD MVOLT EDXB HSG (CI-236RUN)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239C6L","EVO R 40/20 8 WD 277 EZ1 RRLA HSG","EVO R 40/20 8 WD 277 EZ1 RRLA HSG (CI-239C6L)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234P2K","EVO R 40/30 8 MD 277 EZ1 HSG","EVO R 40/30 8 MD 277 EZ1 HSG (CI-234P2K)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237MWJ","EVO SQ 27/15 4 120 EZ1 NPS80EZ HSG","EVO SQ 27/15 4 120 EZ1 NPS80EZ HSG (CI-237MWJ)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
[{"$f":"(LEFT((RIGHT(C23132,7)),6))","v":"237WPG"},{"$f":"LEFT(C23132,SEARCH(\"(CI-\",C23132)-2)","v":"EVO SQ 27/20 4 MVOLT EZ1 CRI90 HSG"},"EVO SQ 27/20 4 MVOLT EZ1 CRI90 HSG (CI-237WPG)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234KL9","EVO SQ 30/07 4 MVOLT EZ1 HSG","EVO SQ 30/07 4 MVOLT EZ1 HSG (CI-234KL9)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235UH2","EVO SQ 30/10 6 277 EZ1 NPS80EZ HSG","EVO SQ 30/10 6 277 EZ1 NPS80EZ HSG (CI-235UH2)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237FAF","EVO SQ 30/20 6 120 ECOS2 HSG","EVO SQ 30/20 6 120 ECOS2 HSG (CI-237FAF)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238W6A","EVO SQ 30/30 6 MVOLT EZB CRI90 HSG","EVO SQ 30/30 6 MVOLT EZB CRI90 HSG (CI-238W6A)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235K32","EVO SQ 35/07 4 MVOLT EZB HSG","EVO SQ 35/07 4 MVOLT EZB HSG (CI-235K32)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236KFH","EVO SQ 35/10 4 277 EZ1 NPS80EZER HSG","EVO SQ 35/10 4 277 EZ1 NPS80EZER HSG (CI-236KFH)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234YJV","EVO SQ 35/10 6 120 EZ1 SF HSG","EVO SQ 35/10 6 120 EZ1 SF HSG (CI-234YJV)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["217GTL","EVO SQ 35/14 4 277 HSG GEN2","EVO SQ 35/14 4 277 HSG GEN2 (CI-217GTL)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235E2J","EVO SQ 35/15 4 277 EZ1 NPS80EZER HSG","EVO SQ 35/15 4 277 EZ1 NPS80EZER HSG (CI-235E2J)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234KLA","EVO SQ 35/15 6 347 EZ1 HSG CSA","EVO SQ 35/15 6 347 EZ1 HSG CSA (CI-234KLA)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233R3V","EVO SQ 35/20 4 MVOLT EZ1 HSG","EVO SQ 35/20 4 MVOLT EZ1 HSG (CI-233R3V)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["230JLK","EVO SQ 35/22 6 277 AZ10 HSG GEN2","EVO SQ 35/22 6 277 AZ10 HSG GEN2 (CI-230JLK)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235K36","EVO SQ 35/25 6 MVOLT EZB HSG","EVO SQ 35/25 6 MVOLT EZB HSG (CI-235K36)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233C57","EVO SQ 35/35 6 MVOLT EZ1 HSG","EVO SQ 35/35 6 MVOLT EZ1 HSG (CI-233C57)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234R7P","EVO SQ 40/10 4 MVOLT EZ1 CRI90 HSG","EVO SQ 40/10 4 MVOLT EZ1 CRI90 HSG (CI-234R7P)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234N33","EVO SQ 40/10 6 MVOLT EZB HSG","EVO SQ 40/10 6 MVOLT EZB HSG (CI-234N33)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238XEU","EVO SQ 40/15 6 MVOLT EZ1 CRI90 HSG","EVO SQ 40/15 6 MVOLT EZ1 CRI90 HSG (CI-238XEU)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233MFV","EVO SQ 40/20 4 MVOLT EZ1 HSG","EVO SQ 40/20 4 MVOLT EZ1 HSG (CI-233MFV)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235Y2M","EVO SQ 40/30 4 MVOLT EZB HSG","EVO SQ 40/30 4 MVOLT EZB HSG (CI-235Y2M)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238MRG","EVO SQ 4AR LSS TRIM U SSQ","EVO SQ 4AR LSS TRIM U SSQ (CI-238MRG)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
[{"$f":"(LEFT((RIGHT(C23388,7)),6))","v":"221AJ2"},{"$f":"LEFT(C23388,SEARCH(\"(CI-\",C23388)-2)","v":"EVO SQ 4BR TRIM U"},"EVO SQ 4BR TRIM U (CI-221AJ2)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239A5C","EVO SQ 4FL U SSQ","EVO SQ 4FL U SSQ (CI-239A5C)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["222RRV","EVO SQ 6AR LD TRW TRIM U","EVO SQ 6AR LD TRW TRIM U (CI-222RRV)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233PVY","EVO SQ 6ARFL LSS TRIM U","EVO SQ 6ARFL LSS TRIM U (CI-233PVY)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["218CKX","EVO SQ 6WR TRIM U","EVO SQ 6WR TRIM U (CI-218CKX)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234YRN","EVO SQ TUWH ATMR/18 4 120 DMX HSG","EVO SQ TUWH ATMR/18 4 120 DMX HSG (CI-234YRN)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234Y7Y","EVO SQLW 30/15 4 277 ECOS3 HSG","EVO SQLW 30/15 4 277 ECOS3 HSG (CI-234Y7Y)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["237HWR","EVO SQLW 35/10 4 277 ECOS3 HSG","EVO SQLW 35/10 4 277 ECOS3 HSG (CI-237HWR)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234PUC","EVO SQLW 35/15 4 120 ECOS3 HSG","EVO SQLW 35/15 4 120 ECOS3 HSG (CI-234PUC)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239J92","EVO SQLW 35/20 4 MVOLT EZ1 RRLA HSG","EVO SQLW 35/20 4 MVOLT EZ1 RRLA HSG (CI-239J92)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238RHG","EVO SQLW 35/25 6 MVOLT EZ10 HSG","EVO SQLW 35/25 6 MVOLT EZ10 HSG (CI-238RHG)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["236NV5","EVO SQLW 40/20 4 MVOLT EZ1 HSG","EVO SQLW 40/20 4 MVOLT EZ1 HSG (CI-236NV5)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235KAC","EVO SQLW 4ARFL LD TRIM U","EVO SQLW 4ARFL LD TRIM U (CI-235KAC)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235JCA","EVO SQLW 4WTR LSS TRBL TRIM U","EVO SQLW 4WTR LSS TRBL TRIM U (CI-235JCA)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["239MRL","EVO WDIM HALR/10 4 WD 120 DMX HSG","EVO WDIM HALR/10 4 WD 120 DMX HSG (CI-239MRL)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234E0L","EVO WW 4AR LSS TRW TRIM U","EVO WW 4AR LSS TRW TRIM U (CI-234E0L)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
[{"$f":"(LEFT((RIGHT(C23580,7)),6))","v":"217EUP"},{"$f":"LEFT(C23580,SEARCH(\"(CI-\",C23580)-2)","v":"EVO WW 4WR TRIM U"},"EVO WW 4WR TRIM U (CI-217EUP)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234PY6","EVO WW 6AR LSS TRW TRIM USPOM U","EVO WW 6AR LSS TRW TRIM USPOM U (CI-234PY6)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["220UEY","EVO WW 8AR LD TRIM U","EVO WW 8AR LD TRIM U (CI-220UEY)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["217EWA","EVO WW 8WR TRIM U","EVO WW 8WR TRIM U (CI-217EWA)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["235NPP","LDN6 27/06 120 EZ1 HSG OS","LDN6 27/06 120 EZ1 HSG OS (CI-235NPP)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["226V13","LDN6 27/15 120 HSG OS","LDN6 27/15 120 HSG OS (CI-226V13)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["231H2X","LDN6 30/10 277 EZ1 HSG OS","LDN6 30/10 277 EZ1 HSG OS (CI-231H2X)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["228UL2","LDN6 30/20 120 EZ1 HSG OS","LDN6 30/20 120 EZ1 HSG OS (CI-228UL2)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["224H19","LDN6 35/06 120 HSG OS","LDN6 35/06 120 HSG OS (CI-224H19)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["230W2G","LDN6 35/10 120 NPS80EZ HSG OS","LDN6 35/10 120 NPS80EZ HSG OS (CI-230W2G)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["230PML","LDN6 35/10 277 NPS80EZ HSG OS","LDN6 35/10 277 NPS80EZ HSG OS (CI-230PML)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["234AKR","LDN6 35/15 120 HSG NAGB OS","LDN6 35/15 120 HSG NAGB OS (CI-234AKR)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["227T00","LDN6 35/20 120 EZ1 HSG OS","LDN6 35/20 120 EZ1 HSG OS (CI-227T00)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["238HP2","LDN6 35/20 277 EZ1 NPS80EZER HSG OS","LDN6 35/20 277 EZ1 NPS80EZER HSG OS (CI-238HP2)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["232W51","LDN6 40/06 277 EZ1 NPS80EZ HSG OS","LDN6 40/06 277 EZ1 NPS80EZ HSG OS (CI-232W51)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["226MVR","LDN6 40/15 120 HSG OS","LDN6 40/15 120 HSG OS (CI-226MVR)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["230X2F","LDN6 40/15 277 SF HSG OS","LDN6 40/15 277 SF HSG OS (CI-230X2F)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["233J3U","LDN6 40/20 277 SF HSG OS","LDN6 40/20 277 SF HSG OS (CI-233J3U)","PS1050DL","Remote mount only","None","1 Board instructions-DL","*251PRK"]
["217HX6","IBH 11L MVOLT","IBH 11L MVOLT (CI-217HX6)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237XAV","IBH 12000LM L/LENS MD 120 OZ10 40K 80CRI CS3W WH","IBH 12000LM L/LENS MD 120 OZ10 40K 80CRI CS3W WH (CI-237XAV)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237FPW","IBH 12000LM L/LENS MD 277 OZ10 40K 80CRI MSI360D WH","IBH 12000LM L/LENS MD 277 OZ10 40K 80CRI MSI360D WH (CI-237FPW)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["231NE5","IBH 12000LM L/LENS MD MVOLT GZ10 50K 70CRI WH","IBH 12000LM L/LENS MD MVOLT GZ10 50K 70CRI WH (CI-231NE5)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237VKT","IBH 12000LM L/LENS MD MVOLT OZ10 50K 80CRI WH","IBH 12000LM L/LENS MD MVOLT OZ10 50K 80CRI WH (CI-237VKT)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["228T3V","IBH 12000LM SD080 MD 120 GZ10 40K 70CRI LAOZU WH","IBH 12000LM SD080 MD 120 GZ10 40K 70CRI LAOZU WH (CI-228T3V)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["228E32","IBH 12000LM SD080 MD 120 GZ10 40K 80CRI CS1W WH","IBH 12000LM SD080 MD 120 GZ10 40K 80CRI CS1W WH (CI-228E32)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["230THF","IBH 12000LM SD080 MD 120 GZ10 50K 70CRI CS3W WH","IBH 12000LM SD080 MD 120 GZ10 50K 70CRI CS3W WH (CI-230THF)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["230XPE","IBH 12000LM SD080 MD 120 GZ10 50K 80CRI CS3W WH","IBH 12000LM SD080 MD 120 GZ10 50K 80CRI CS3W WH (CI-230XPE)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["238GF0","IBH 12000LM SD080 MD 120 OZ10 40K 70CRI CS3W WH OUTCTR","IBH 12000LM SD080 MD 120 OZ10 40K 70CRI CS3W WH OUTCTR (CI-238GF0)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237GGP","IBH 12000LM SD080 MD 120 OZ10 50K 70CRI LAH0SZU MB","IBH 12000LM SD080 MD 120 OZ10 50K 70CRI LAH0SZU MB (CI-237GGP)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["235AXM","IBH 12000LM SD080 MD 208 GZ10 50K 80CRI LAOZU WH","IBH 12000LM SD080 MD 208 GZ10 50K 80CRI LAOZU WH (CI-235AXM)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["233E6A","IBH 12000LM SD080 MD 277 GZ10 40K 70CRI LAM0SZU WH","IBH 12000LM SD080 MD 277 GZ10 40K 70CRI LAM0SZU WH (CI-233E6A)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["235P60","IBH 12000LM SD080 MD 277 GZ10 50K 70CRI CS93W NPP16D WH OUTCTR","IBH 12000LM SD080 MD 277 GZ10 50K 70CRI CS93W NPP16D WH OUTCTR (CI-235P60)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["234F35","IBH 12000LM SD080 MD 277 GZ10 50K 80CRI LAOZU WH","IBH 12000LM SD080 MD 277 GZ10 50K 80CRI LAOZU WH (CI-234F35)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237U2M","IBH 12000LM SD080 MD 277 OZ10 40K 80CRI LAOZU WH","IBH 12000LM SD080 MD 277 OZ10 40K 80CRI LAOZU WH (CI-237U2M)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237MAJ","IBH 12000LM SD080 MD 277 OZ10 50K 70CRI CS11W WH","IBH 12000LM SD080 MD 277 OZ10 50K 70CRI CS11W WH (CI-237MAJ)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["239KCL","IBH 12000LM SD080 MD 347 OZ10 50K 70CRI CS93W NMSI360 WH","IBH 12000LM SD080 MD 347 OZ10 50K 70CRI CS93W NMSI360 WH (CI-239KCL)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["228C6N","IBH 12000LM SD080 MD MVOLT GZ10 40K 70CRI MB","IBH 12000LM SD080 MD MVOLT GZ10 40K 70CRI MB (CI-228C6N)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["235VU9","IBH 12000LM SD080 MD MVOLT GZ10 40K 80CRI WH USPOM","IBH 12000LM SD080 MD MVOLT GZ10 40K 80CRI WH USPOM (CI-235VU9)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
[{"$f":"(LEFT((RIGHT(C24028,7)),6))","v":"237GVP"},{"$f":"LEFT(C24028,SEARCH(\"(CI-\",C24028)-2)","v":"IBH 12000LM SD080 MD MVOLT OZ10 30K 70CRI WH"},"IBH 12000LM SD080 MD MVOLT OZ10 30K 70CRI WH (CI-237GVP)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237GVX","IBH 12000LM SD080 MD MVOLT OZ10 40K 80CRI WH OUTCTR","IBH 12000LM SD080 MD MVOLT OZ10 40K 80CRI WH OUTCTR (CI-237GVX)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["238M51","IBH 12000LM SD080 MD MVOLT OZ10 50K 80CRI CS93W WH","IBH 12000LM SD080 MD MVOLT OZ10 50K 80CRI CS93W WH (CI-238M51)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237WG7","IBH 12000LM SD080 ND 277 OZ10 40K 70CRI LAOZU WH WGX USPOM","IBH 12000LM SD080 ND 277 OZ10 40K 70CRI LAOZU WH WGX USPOM (CI-237WG7)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["236V0H","IBH 12000LM SD080 ND MVOLT GZ10 50K 80CRI CS93W WH","IBH 12000LM SD080 ND MVOLT GZ10 50K 80CRI CS93W WH (CI-236V0H)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["235XNV","IBH 15000LM L/LENS MD 120 GZ10 40K 80CRI LAG0SZU WH","IBH 15000LM L/LENS MD 120 GZ10 40K 80CRI LAG0SZU WH (CI-235XNV)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["239MP4","IBH 15000LM L/LENS MD 120 OZ10 50K 70CRI CS3W WH","IBH 15000LM L/LENS MD 120 OZ10 50K 70CRI CS3W WH (CI-239MP4)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["234YU5","IBH 15000LM L/LENS MD 277 GZ10 40K 70CRI LAOZU WH","IBH 15000LM L/LENS MD 277 GZ10 40K 70CRI LAOZU WH (CI-234YU5)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237J9X","IBH 15000LM L/LENS MD 480 OZ10 50K 70CRI LCM0SZU WH","IBH 15000LM L/LENS MD 480 OZ10 50K 70CRI LCM0SZU WH (CI-237J9X)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["235WV4","IBH 15000LM L/LENS ND MVOLT GZ10 50K 70CRI WH","IBH 15000LM L/LENS ND MVOLT GZ10 50K 70CRI WH (CI-235WV4)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["235Y7A","IBH 15000LM L/LENS ND MVOLT GZ10 50K 80CRI WH","IBH 15000LM L/LENS ND MVOLT GZ10 50K 80CRI WH (CI-235Y7A)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["236A7C","IBH 15000LM SD080 MD 120 GZ10 50K 80CRI XPW WH WGX","IBH 15000LM SD080 MD 120 GZ10 50K 80CRI XPW WH WGX (CI-236A7C)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237PF8","IBH 15000LM SD080 MD 120 OZ10 40K 70CRI LCOZU WH","IBH 15000LM SD080 MD 120 OZ10 40K 70CRI LCOZU WH (CI-237PF8)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["238AKR","IBH 15000LM SD080 MD 120 OZ10 50K 80CRI CS1W WH","IBH 15000LM SD080 MD 120 OZ10 50K 80CRI CS1W WH (CI-238AKR)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237MJ1","IBH 15000LM SD080 MD 240 OZ10 50K 80CRI CS43W LAOZU WH","IBH 15000LM SD080 MD 240 OZ10 50K 80CRI CS43W LAOZU WH (CI-237MJ1)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["235KJG","IBH 15000LM SD080 MD 277 GZ10 40K 80CRI CS93W LAOZU WH","IBH 15000LM SD080 MD 277 GZ10 40K 80CRI CS93W LAOZU WH (CI-235KJG)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
[{"$f":"(LEFT((RIGHT(C24220,7)),6))","v":"238Y0R"},{"$f":"LEFT(C24220,SEARCH(\"(CI-\",C24220)-2)","v":"IBH 15000LM SD080 MD 277 OZ10 40K 80CRI CS11W NPP16D WH"},"IBH 15000LM SD080 MD 277 OZ10 40K 80CRI CS11W NPP16D WH (CI-238Y0R)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["234UT4","IBH 15000LM SD080 MD MVOLT GZ10 40K 70CRI MB","IBH 15000LM SD080 MD MVOLT GZ10 40K 70CRI MB (CI-234UT4)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["228NV3","IBH 15000LM SD080 MD MVOLT GZ10 40K 70CRI WH","IBH 15000LM SD080 MD MVOLT GZ10 40K 70CRI WH (CI-228NV3)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237CLY","IBH 15000LM SD080 MD MVOLT OZ10 40K 70CRI WH WGX","IBH 15000LM SD080 MD MVOLT OZ10 40K 70CRI WH WGX (CI-237CLY)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["239K0V","IBH 15000LM SD080 MD MVOLT OZ10 50K 80CRI CS93W WH","IBH 15000LM SD080 MD MVOLT OZ10 50K 80CRI CS93W WH (CI-239K0V)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
[{"$f":"(LEFT((RIGHT(C24284,7)),6))","v":"236H29"},{"$f":"LEFT(C24284,SEARCH(\"(CI-\",C24284)-2)","v":"IBH 15000LM SD080 ND 277 GZ10 50K 70CRI CS11W WH"},"IBH 15000LM SD080 ND 277 GZ10 50K 70CRI CS11W WH (CI-236H29)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["235F2C","IBH 15000LM SD080 ND MVOLT GZ10 50K 70CRI WH","IBH 15000LM SD080 ND MVOLT GZ10 50K 70CRI WH (CI-235F2C)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["235NT7","IBH 18000LM L/LENS MD 120 GZ10 40K 80CRI LAM0SZU WH","IBH 18000LM L/LENS MD 120 GZ10 40K 80CRI LAM0SZU WH (CI-235NT7)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["232VG0","IBH 18000LM L/LENS MD 277 GZ10 50K 70CRI LAOZU WH","IBH 18000LM L/LENS MD 277 GZ10 50K 70CRI LAOZU WH (CI-232VG0)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["236NJU","IBH 18000LM L/LENS MD MVOLT GZ10 40K 70CRI RRLAB WH WGX","IBH 18000LM L/LENS MD MVOLT GZ10 40K 70CRI RRLAB WH WGX (CI-236NJU)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["230HE9","IBH 18000LM L/LENS MD MVOLT GZ10 40K 70CRI WH","IBH 18000LM L/LENS MD MVOLT GZ10 40K 70CRI WH (CI-230HE9)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["239M0A","IBH 18000LM L/LENS ND 120 OZ10 50K 70CRI XAD WH","IBH 18000LM L/LENS ND 120 OZ10 50K 70CRI XAD WH (CI-239M0A)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239CAR","IBH 18000LM L/LENS ND 347 OZ10 40K 70CRI LCOTD WH","IBH 18000LM L/LENS ND 347 OZ10 40K 70CRI LCOTD WH (CI-239CAR)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235V33","IBH 18000LM SD080 MD 120 GZ10 40K 70CRI CS3W LAOZU WH","IBH 18000LM SD080 MD 120 GZ10 40K 70CRI CS3W LAOZU WH (CI-235V33)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["236R78","IBH 18000LM SD080 MD 120 GZ10 40K 70CRI NMSI360D WH OUTCTR","IBH 18000LM SD080 MD 120 GZ10 40K 70CRI NMSI360D WH OUTCTR (CI-236R78)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["230AU6","IBH 18000LM SD080 MD 120 GZ10 50K 70CRI CS1W WH","IBH 18000LM SD080 MD 120 GZ10 50K 70CRI CS1W WH (CI-230AU6)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["238U0J","IBH 18000LM SD080 MD 120 OZ10 35K 80CRI CS3W WH","IBH 18000LM SD080 MD 120 OZ10 35K 80CRI CS3W WH (CI-238U0J)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239GVH","IBH 18000LM SD080 MD 120 OZ10 40K 80CRI LAM0SZU WH","IBH 18000LM SD080 MD 120 OZ10 40K 80CRI LAM0SZU WH (CI-239GVH)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237GJV","IBH 18000LM SD080 MD 120 OZ10 40K 80CRI LAOZU WH","IBH 18000LM SD080 MD 120 OZ10 40K 80CRI LAOZU WH (CI-237GJV)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234YVJ","IBH 18000LM SD080 MD 277 GZ10 40K 70CRI CS11W LAOZU WH","IBH 18000LM SD080 MD 277 GZ10 40K 70CRI CS11W LAOZU WH (CI-234YVJ)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["227WJL","IBH 18000LM SD080 MD 277 GZ10 40K 70CRI LAOZU WH","IBH 18000LM SD080 MD 277 GZ10 40K 70CRI LAOZU WH (CI-227WJL)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
[{"$f":"(LEFT((RIGHT(C24476,7)),6))","v":"228EJW"},{"$f":"LEFT(C24476,SEARCH(\"(CI-\",C24476)-2)","v":"IBH 18000LM SD080 MD 277 GZ10 40K 80CRI NMSI360D WH"},"IBH 18000LM SD080 MD 277 GZ10 40K 80CRI NMSI360D WH (CI-228EJW)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["234VCX","IBH 18000LM SD080 MD 277 GZ10 50K 70CRI OCS LAOZU WH","IBH 18000LM SD080 MD 277 GZ10 50K 70CRI OCS LAOZU WH (CI-234VCX)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["238H93","IBH 18000LM SD080 MD 277 OZ10 40K 70CRI CS11W MSI360 WH","IBH 18000LM SD080 MD 277 OZ10 40K 70CRI CS11W MSI360 WH (CI-238H93)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239F8N","IBH 18000LM SD080 MD 277 OZ10 40K 70CRI NPP16D WH","IBH 18000LM SD080 MD 277 OZ10 40K 70CRI NPP16D WH (CI-239F8N)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238H0N","IBH 18000LM SD080 MD 277 OZ10 50K 70CRI LAOZU WH","IBH 18000LM SD080 MD 277 OZ10 50K 70CRI LAOZU WH (CI-238H0N)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238EMT","IBH 18000LM SD080 MD 277 OZ10 50K 80CRI CS11W LAOZU WH","IBH 18000LM SD080 MD 277 OZ10 50K 80CRI CS11W LAOZU WH (CI-238EMT)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["229P4L","IBH 18000LM SD080 MD MVOLT GZ10 40K 80CRI MB","IBH 18000LM SD080 MD MVOLT GZ10 40K 80CRI MB (CI-229P4L)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["227XRN","IBH 18000LM SD080 MD MVOLT GZ10 50K 80CRI WH WGX","IBH 18000LM SD080 MD MVOLT GZ10 50K 80CRI WH WGX (CI-227XRN)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["239P7F","IBH 18000LM SD080 MD MVOLT OZ10 40K 70CRI CS93WL10 WH","IBH 18000LM SD080 MD MVOLT OZ10 40K 70CRI CS93WL10 WH (CI-239P7F)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237C7U","IBH 18000LM SD080 MD MVOLT OZ10 40K 80CRI WH","IBH 18000LM SD080 MD MVOLT OZ10 40K 80CRI WH (CI-237C7U)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237YCE","IBH 18000LM SD080 ND 120 OZ10 40K 80CRI CS3W LCOZU WH","IBH 18000LM SD080 ND 120 OZ10 40K 80CRI CS3W LCOZU WH (CI-237YCE)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239U6A","IBH 18000LM SD080 ND 277 OZ10 40K 70CRI SPD WH","IBH 18000LM SD080 ND 277 OZ10 40K 70CRI SPD WH (CI-239U6A)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237VP2","IBH 18000LM SD080 ND MVOLT OZ10 40K 70CRI CS93W WH","IBH 18000LM SD080 ND MVOLT OZ10 40K 70CRI CS93W WH (CI-237VP2)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237CRX","IBH 18000LM SD080 ND MVOLT OZ10 40K 70CRI WH","IBH 18000LM SD080 ND MVOLT OZ10 40K 70CRI WH (CI-237CRX)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235HEC","IBH 24000LM L/LENS MD 208 GZ10 50K 70CRI CS43W WH","IBH 24000LM L/LENS MD 208 GZ10 50K 70CRI CS43W WH (CI-235HEC)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["234A8N","IBH 24000LM L/LENS MD 277 GZ10 50K 80CRI LAPZU WH","IBH 24000LM L/LENS MD 277 GZ10 50K 80CRI LAPZU WH (CI-234A8N)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237WWM","IBH 24000LM L/LENS MD 277 OZ10 50K 70CRI CS11WL10 LAH0SZU WH","IBH 24000LM L/LENS MD 277 OZ10 50K 70CRI CS11WL10 LAH0SZU WH (CI-237WWM)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["236KEG","IBH 24000LM L/LENS MD MVOLT GZ10 40K 70CRI CS93WL12 WH","IBH 24000LM L/LENS MD MVOLT GZ10 40K 70CRI CS93WL12 WH (CI-236KEG)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237TH1","IBH 24000LM L/LENS MD MVOLT OZ10 40K 80CRI WH WGX","IBH 24000LM L/LENS MD MVOLT OZ10 40K 80CRI WH WGX (CI-237TH1)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["239JHC","IBH 24000LM L/LENS ND 120 OZ10 40K 90CRI CS3W WH","IBH 24000LM L/LENS ND 120 OZ10 40K 90CRI CS3W WH (CI-239JHC)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237N6L","IBH 24000LM L/LENS ND MVOLT OZ10 40K 80CRI WH","IBH 24000LM L/LENS ND MVOLT OZ10 40K 80CRI WH (CI-237N6L)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["238J38","IBH 24000LM L/LENS ND MVOLT OZ10 50K 70CRI WH","IBH 24000LM L/LENS ND MVOLT OZ10 50K 70CRI WH (CI-238J38)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237W7T","IBH 24000LM SD080 MD 120 OZ10 40K 70CRI CS93W LAPZU WH","IBH 24000LM SD080 MD 120 OZ10 40K 70CRI CS93W LAPZU WH (CI-237W7T)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237PK6","IBH 24000LM SD080 MD 120 OZ10 50K 80CRI NPP16D WH WGX","IBH 24000LM SD080 MD 120 OZ10 50K 80CRI NPP16D WH WGX (CI-237PK6)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["233J7R","IBH 24000LM SD080 MD 277 GZ10 40K 70CRI CS11W LAOZU WH","IBH 24000LM SD080 MD 277 GZ10 40K 70CRI CS11W LAOZU WH (CI-233J7R)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["230AN3","IBH 24000LM SD080 MD 277 GZ10 40K 70CRI LCM0SZU WH","IBH 24000LM SD080 MD 277 GZ10 40K 70CRI LCM0SZU WH (CI-230AN3)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["230R3U","IBH 24000LM SD080 MD 277 GZ10 40K 80CRI LAOZU WH","IBH 24000LM SD080 MD 277 GZ10 40K 80CRI LAOZU WH (CI-230R3U)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["234V0Y","IBH 24000LM SD080 MD 277 GZ10 50K 70CRI LAOTU CS11W WH","IBH 24000LM SD080 MD 277 GZ10 50K 70CRI LAOTU CS11W WH (CI-234V0Y)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["235AWN","IBH 24000LM SD080 MD 277 GZ10 50K 80CRI OCS10 LAOZU WH","IBH 24000LM SD080 MD 277 GZ10 50K 80CRI OCS10 LAOZU WH (CI-235AWN)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237JTE","IBH 24000LM SD080 MD 277 OZ10 40K 80CRI CS11W WH WGX","IBH 24000LM SD080 MD 277 OZ10 40K 80CRI CS11W WH WGX (CI-237JTE)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["238WRU","IBH 24000LM SD080 MD 277 OZ10 50K 70CRI LCOZU WH","IBH 24000LM SD080 MD 277 OZ10 50K 70CRI LCOZU WH (CI-238WRU)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["238U6K","IBH 24000LM SD080 MD 347 OZ10 40K 70CRI CS93W LAOZU WH","IBH 24000LM SD080 MD 347 OZ10 40K 70CRI CS93W LAOZU WH (CI-238U6K)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["238VMW","IBH 24000LM SD080 MD 480 OZ10 50K 80CRI OCS10 LAH0SZU WH","IBH 24000LM SD080 MD 480 OZ10 50K 80CRI OCS10 LAH0SZU WH (CI-238VMW)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["228YGX","IBH 24000LM SD080 MD MVOLT GZ10 40K 80CRI WH WGX","IBH 24000LM SD080 MD MVOLT GZ10 40K 80CRI WH WGX (CI-228YGX)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["238N3M","IBH 24000LM SD080 MD MVOLT OZ10 30K 80CRI WH","IBH 24000LM SD080 MD MVOLT OZ10 30K 80CRI WH (CI-238N3M)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237ETF","IBH 24000LM SD080 MD MVOLT OZ10 40K 80CRI CS93W WH","IBH 24000LM SD080 MD MVOLT OZ10 40K 80CRI CS93W WH (CI-237ETF)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["238T66","IBH 24000LM SD080 MD MVOLT OZ10 50K 80CRI CS93W WH","IBH 24000LM SD080 MD MVOLT OZ10 50K 80CRI CS93W WH (CI-238T66)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["236JL1","IBH 24000LM SD080 ND 277 GZ10 40K 70CRI LAOZU WH","IBH 24000LM SD080 ND 277 GZ10 40K 70CRI LAOZU WH (CI-236JL1)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["239M5C","IBH 24000LM SD080 ND 277 OZ10 50K 80CRI LAPZU WH","IBH 24000LM SD080 ND 277 OZ10 50K 80CRI LAPZU WH (CI-239M5C)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["239NNW","IBH 24000LM SD080 ND MVOLT OZ10 50K 70CRI WH","IBH 24000LM SD080 ND MVOLT OZ10 50K 70CRI WH (CI-239NNW)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237RW5","IBH 30000LM L/LENS MD 120 OZ10 50K 70CRI MSI6XADL DSCXADL WH","IBH 30000LM L/LENS MD 120 OZ10 50K 70CRI MSI6XADL DSCXADL WH (CI-237RW5)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237F54","IBH 30000LM L/LENS MD 277 OZ10 50K 70CRI LAOTU WH","IBH 30000LM L/LENS MD 277 OZ10 50K 70CRI LAOTU WH (CI-237F54)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237E8J","IBH 30000LM L/LENS MD MVOLT OZ10 50K 80CRI WH","IBH 30000LM L/LENS MD MVOLT OZ10 50K 80CRI WH (CI-237E8J)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237JR6","IBH 30000LM L/LENS ND 347 OZ10 40K 70CRI CS93W LAOZU WH","IBH 30000LM L/LENS ND 347 OZ10 40K 70CRI CS93W LAOZU WH (CI-237JR6)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["239G12","IBH 30000LM PCL125 ND 277 OZ10 40K 80CRI LAM0STU WH","IBH 30000LM PCL125 ND 277 OZ10 40K 80CRI LAM0STU WH (CI-239G12)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["239G17","IBH 30000LM SD080 MD 120 OZ10 40K 80CRI NMSI360 WH WGX","IBH 30000LM SD080 MD 120 OZ10 40K 80CRI NMSI360 WH WGX (CI-239G17)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["233TW0","IBH 30000LM SD080 MD 277 GZ10 50K 80CRI CS93W LCOTU WH","IBH 30000LM SD080 MD 277 GZ10 50K 80CRI CS93W LCOTU WH (CI-233TW0)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["238J34","IBH 30000LM SD080 MD 277 OZ10 40K 80CRI CS11W WH WGX","IBH 30000LM SD080 MD 277 OZ10 40K 80CRI CS11W WH WGX (CI-238J34)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237LHK","IBH 30000LM SD080 MD 277 OZ10 50K 70CRI CS93WL10 LAH0SZU WH","IBH 30000LM SD080 MD 277 OZ10 50K 70CRI CS93WL10 LAH0SZU WH (CI-237LHK)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["227WRC","IBH 30000LM SD080 MD MVOLT GZ10 40K 80CRI WH","IBH 30000LM SD080 MD MVOLT GZ10 40K 80CRI WH (CI-227WRC)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["238L2F","IBH 30000LM SD080 MD MVOLT OZ10 35K 90CRI WH WGX","IBH 30000LM SD080 MD MVOLT OZ10 35K 90CRI WH WGX (CI-238L2F)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237RVV","IBH 30000LM SD080 MD MVOLT OZ10 50K 70CRI WH","IBH 30000LM SD080 MD MVOLT OZ10 50K 70CRI WH (CI-237RVV)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["238K4J","IBH 30000LM SD080 ND 480 OZ10 50K 80CRI OCS10 LAH0SZU WH","IBH 30000LM SD080 ND 480 OZ10 50K 80CRI OCS10 LAH0SZU WH (CI-238K4J)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["238H12","IBH 30000LM SD080 ND MVOLT OZ10 50K 80CRI CS93W WH","IBH 30000LM SD080 ND MVOLT OZ10 50K 80CRI CS93W WH (CI-238H12)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237LM9","IBH 36000LM SD080 MD 277 OZ10 40K 70CRI CS11W WH WGX","IBH 36000LM SD080 MD 277 OZ10 40K 70CRI CS11W WH WGX (CI-237LM9)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["239JTG","IBH 36000LM SD080 MD MVOLT OZ10 40K 90CRI WH","IBH 36000LM SD080 MD MVOLT OZ10 40K 90CRI WH (CI-239JTG)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["238MMT","IBH 36000LM SD080 ND 277 OZ10 40K 80CRI OCS15 LAOZU WH","IBH 36000LM SD080 ND 277 OZ10 40K 80CRI OCS15 LAOZU WH (CI-238MMT)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["235VRT","IBH 9000LM L/LENS MD 120 GZ10 50K 80CRI CS1W WH","IBH 9000LM L/LENS MD 120 GZ10 50K 80CRI CS1W WH (CI-235VRT)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["238ETR","IBH 9000LM L/LENS MD 277 OZ10 40K 80CRI LAOZU WH","IBH 9000LM L/LENS MD 277 OZ10 40K 80CRI LAOZU WH (CI-238ETR)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237EPY","IBH 9000LM L/LENS MD MVOLT OZ10 35K 70CRI WH","IBH 9000LM L/LENS MD MVOLT OZ10 35K 70CRI WH (CI-237EPY)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["230F6N","IBH 9000LM SD080 MD 120 GZ10 40K 70CRI CS3W WH","IBH 9000LM SD080 MD 120 GZ10 40K 70CRI CS3W WH (CI-230F6N)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["231A29","IBH 9000LM SD080 MD 120 GZ10 40K 80CRI LAOZU WH","IBH 9000LM SD080 MD 120 GZ10 40K 80CRI LAOZU WH (CI-231A29)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237UR9","IBH 9000LM SD080 MD 120 OZ10 40K 70CRI LAOZU WH","IBH 9000LM SD080 MD 120 OZ10 40K 70CRI LAOZU WH (CI-237UR9)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["234VUL","IBH 9000LM SD080 MD 277 GZ10 50K 80CRI LCPZU WH","IBH 9000LM SD080 MD 277 GZ10 50K 80CRI LCPZU WH (CI-234VUL)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237PH9","IBH 9000LM SD080 MD 277 OZ10 50K 80CRI CS11W WH","IBH 9000LM SD080 MD 277 OZ10 50K 80CRI CS11W WH (CI-237PH9)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["232C2U","IBH 9000LM SD080 MD MVOLT GZ10 40K 80CRI WH WGX","IBH 9000LM SD080 MD MVOLT GZ10 40K 80CRI WH WGX (CI-232C2U)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237F3N","IBH 9000LM SD080 MD MVOLT OZ10 40K 70CRI MB","IBH 9000LM SD080 MD MVOLT OZ10 40K 70CRI MB (CI-237F3N)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["239F2X","IBH 9000LM SD080 MD MVOLT OZ10 40K 80CRI CS93W WH WGX","IBH 9000LM SD080 MD MVOLT OZ10 40K 80CRI CS93W WH WGX (CI-239F2X)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["236WLC","IBH 9000LM SD080 MD MVOLT OZ10 50K 80CRI WH","IBH 9000LM SD080 MD MVOLT OZ10 50K 80CRI WH (CI-236WLC)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["234GWE","IBH 9000LM SD080 ND MVOLT GZ10 50K 70CRI WH","IBH 9000LM SD080 ND MVOLT GZ10 50K 70CRI WH (CI-234GWE)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["237VVF","IBHST 18000LM SD080 MD MVOLT GZ10 40K 70CRI WH","IBHST 18000LM SD080 MD MVOLT GZ10 40K 70CRI WH (CI-237VVF)","PS30250","Remote mount only","None","PS30250@250VDC_2 Boards in parallel Instructions","*251PT0"]
["223TJ2","IBL 12L ND 277 LP750 DLC MSIPED NAAA","IBL 12L ND 277 LP750 DLC MSIPED NAAA (CI-223TJ2)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["231NK6","IBL 12L ND LP835","IBL 12L ND LP835 (CI-231NK6)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["235NC7","IBL 12L ND SD125 277 LP740 DLC MSE360","IBL 12L ND SD125 277 LP740 DLC MSE360 (CI-235NC7)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["232YFP","IBL 12L ND SD125 LP750 DLC WGX","IBL 12L ND SD125 LP750 DLC WGX (CI-232YFP)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["230GWG","IBL 12L WD 120 CS93W LP740 DLC LAOZU","IBL 12L WD 120 CS93W LP740 DLC LAOZU (CI-230GWG)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["237TV5","IBL 12L WD 120 LP840 LCH0SZU","IBL 12L WD 120 LP840 LCH0SZU (CI-237TV5)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["218L7W","IBL 12L WD 277 CS93W LP740 DLC MSE360","IBL 12L WD 277 CS93W LP740 DLC MSE360 (CI-218L7W)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["239JX2","IBL 12L WD ACL LP740 DWH DLC WGX","IBL 12L WD ACL LP740 DWH DLC WGX (CI-239JX2)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["239HML","IBL 12L WD LP850 DWH","IBL 12L WD LP850 DWH (CI-239HML)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["219A9H","IBL 12L WD SD125 120 CS3W LP740 DWH DLC","IBL 12L WD SD125 120 CS3W LP740 DWH DLC (CI-219A9H)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["228JMP","IBL 12L WD SD125 120 LP740 DLC NPP16D","IBL 12L WD SD125 120 LP740 DLC NPP16D (CI-228JMP)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["226VMW","IBL 12L WD SD125 277 CS11W LP740 DLC","IBL 12L WD SD125 277 CS11W LP740 DLC (CI-226VMW)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["228JN9","IBL 12L WD SD125 277 LP750 DLC NPP16D","IBL 12L WD SD125 277 LP750 DLC NPP16D (CI-228JN9)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["235Y1J","IBL 12L WD SD125 CS93W LP750 DWH DLC","IBL 12L WD SD125 CS93W LP750 DWH DLC (CI-235Y1J)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["220K86","IBL 12L WD SD125 LP740 DLC WGX","IBL 12L WD SD125 LP740 DLC WGX (CI-220K86)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["232HTK","IBL 12L WD SD125 LP840 DWH WGX","IBL 12L WD SD125 LP840 DWH WGX (CI-232HTK)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["238GFU","IBL 18L ND 277 LP740 DLC LAM0SZU","IBL 18L ND 277 LP740 DLC LAM0SZU (CI-238GFU)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239XCW","IBL 18L ND 277 OCS LP750 DLC LCOZU","IBL 18L ND 277 OCS LP750 DLC LCOZU (CI-239XCW)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["218E81","IBL 18L ND LP740 DWH DLC","IBL 18L ND LP740 DWH DLC (CI-218E81)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237M04","IBL 18L ND LP850 NOM","IBL 18L ND LP850 NOM (CI-237M04)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
[{"$f":"(LEFT((RIGHT(C25564,7)),6))","v":"239A6Y"},{"$f":"LEFT(C25564,SEARCH(\"(CI-\",C25564)-2)","v":"IBL 18L ND SD125 277 CS93W LP840 LCH0SZU"},"IBL 18L ND SD125 277 CS93W LP840 LCH0SZU (CI-239A6Y)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235WUC","IBL 18L ND SD125 277 LP840 LCM0SZU","IBL 18L ND SD125 277 LP840 LCM0SZU (CI-235WUC)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["214AUC","IBL 18L ND SD125 LP740 DLC","IBL 18L ND SD125 LP740 DLC (CI-214AUC)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["222A74","IBL 18L WD 120 CS3W LP740 DLC","IBL 18L WD 120 CS3W LP740 DLC (CI-222A74)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236MRK","IBL 18L WD 240 LP750 DLC MSI360","IBL 18L WD 240 LP750 DLC MSI360 (CI-236MRK)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
[{"$f":"(LEFT((RIGHT(C25628,7)),6))","v":"238JWV"},{"$f":"LEFT(C25628,SEARCH(\"(CI-\",C25628)-2)","v":"IBL 18L WD 277 IMP LP740 DLC LCOZU WGX"},"IBL 18L WD 277 IMP LP740 DLC LCOZU WGX (CI-238JWV)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239WH8","IBL 18L WD 277 LP740 DLC MSE360 WGX","IBL 18L WD 277 LP740 DLC MSE360 WGX (CI-239WH8)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["230HT2","IBL 18L WD 277 LP840 LAOZU","IBL 18L WD 277 LP840 LAOZU (CI-230HT2)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["223JNJ","IBL 18L WD 480 CS97W LP750 DLC","IBL 18L WD 480 CS97W LP750 DLC (CI-223JNJ)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["219E1G","IBL 18L WD CS93WL10 LP750 DLC","IBL 18L WD CS93WL10 LP750 DLC (CI-219E1G)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["221Y72","IBL 18L WD LP740 DWH DLC WGX","IBL 18L WD LP740 DWH DLC WGX (CI-221Y72)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["228T2R","IBL 18L WD LP850 DWH","IBL 18L WD LP850 DWH (CI-228T2R)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235T7E","IBL 18L WD SD125 120 LP840 DWH NPP16D WGX","IBL 18L WD SD125 120 LP840 DWH NPP16D WGX (CI-235T7E)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239MPY","IBL 18L WD SD125 277 CS93W LP750 DLC LAOZU","IBL 18L WD SD125 277 CS93W LP750 DLC LAOZU (CI-239MPY)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239M6V","IBL 18L WD SD125 277 LP740 DLC NMSI360D WGX","IBL 18L WD SD125 277 LP740 DLC NMSI360D WGX (CI-239M6V)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235REX","IBL 18L WD SD125 277 LP840 LAOZU","IBL 18L WD SD125 277 LP840 LAOZU (CI-235REX)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["232W01","IBL 18L WD SD125 CS93W LP740 DLC WGX","IBL 18L WD SD125 CS93W LP740 DLC WGX (CI-232W01)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236G01","IBL 18L WD SD125 CS93W LP850","IBL 18L WD SD125 CS93W LP850 (CI-236G01)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["215RH0","IBL 18L WD SD125 LP740 DWH DLC","IBL 18L WD SD125 LP740 DWH DLC (CI-215RH0)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["226T6M","IBL 18L WD SD125 LP840","IBL 18L WD SD125 LP840 (CI-226T6M)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235JRK","IBL 24L ND 277 CS11W LP750 DLC LAOZV","IBL 24L ND 277 CS11W LP750 DLC LAOZV (CI-235JRK)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
[{"$f":"(LEFT((RIGHT(C25820,7)),6))","v":"234P4R"},{"$f":"LEFT(C25820,SEARCH(\"(CI-\",C25820)-2)","v":"IBL 24L ND 277 LP750 DLC NMSI"},"IBL 24L ND 277 LP750 DLC NMSI (CI-234P4R)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235UME","IBL 24L ND 277 OCS10 LP740 DLC","IBL 24L ND 277 OCS10 LP740 DLC (CI-235UME)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["218TJ5","IBL 24L ND 480 OCS LP740 DLC","IBL 24L ND 480 OCS LP740 DLC (CI-218TJ5)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["214RFM","IBL 24L ND CS93W LP750 DLC","IBL 24L ND CS93W LP750 DLC (CI-214RFM)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239HMT","IBL 24L ND LP740 DWH DLC WGX","IBL 24L ND LP740 DWH DLC WGX (CI-239HMT)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239K54","IBL 24L ND SD125 120 CS93W LP740 DLC MSI","IBL 24L ND SD125 120 CS93W LP740 DLC MSI (CI-239K54)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238V3X","IBL 24L ND SD125 277 CS11W LP840 LCOZU","IBL 24L ND SD125 277 CS11W LP840 LCOZU (CI-238V3X)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["221W7A","IBL 24L ND SD125 CS93W LP740 DLC","IBL 24L ND SD125 CS93W LP740 DLC (CI-221W7A)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["214ALV","IBL 24L ND SD125 LP750 DLC","IBL 24L ND SD125 LP750 DLC (CI-214ALV)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238K2Y","IBL 24L ND SD125 RRLA LP840","IBL 24L ND SD125 RRLA LP840 (CI-238K2Y)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["227L3N","IBL 24L WD 120 CS1W LP850","IBL 24L WD 120 CS1W LP850 (CI-227L3N)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235XAK","IBL 24L WD 120 CS93W LP750 DLC LAOZU","IBL 24L WD 120 CS93W LP750 DLC LAOZU (CI-235XAK)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["217TE6","IBL 24L WD 120 LP740 DLC MSE360","IBL 24L WD 120 LP740 DLC MSE360 (CI-217TE6)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238MYA","IBL 24L WD 120 LP740 DWH DLC MSE360","IBL 24L WD 120 LP740 DWH DLC MSE360 (CI-238MYA)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["227MJW","IBL 24L WD 120 LP750 DLC LAOZU","IBL 24L WD 120 LP750 DLC LAOZU (CI-227MJW)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236AC5","IBL 24L WD 120 LP750 DLC LAOZU USPOM","IBL 24L WD 120 LP750 DLC LAOZU USPOM (CI-236AC5)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["222YHH","IBL 24L WD 120 LP750 DLC MSE360","IBL 24L WD 120 LP750 DLC MSE360 (CI-222YHH)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235XR4","IBL 24L WD 120 LP835 MSE360","IBL 24L WD 120 LP835 MSE360 (CI-235XR4)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235GC6","IBL 24L WD 120 LP840 NPP16D","IBL 24L WD 120 LP840 NPP16D (CI-235GC6)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234RL9","IBL 24L WD 120 LP850 LAH0SZU","IBL 24L WD 120 LP850 LAH0SZU (CI-234RL9)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234R48","IBL 24L WD 120 OCS LP840 DWH","IBL 24L WD 120 OCS LP840 DWH (CI-234R48)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235VRV","IBL 24L WD 208 CS93WL12 LP750 DLC LAOZU","IBL 24L WD 208 CS93WL12 LP750 DLC LAOZU (CI-235VRV)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["220C4K","IBL 24L WD 240 CS43W LP750 DLC","IBL 24L WD 240 CS43W LP750 DLC (CI-220C4K)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["233G9Y","IBL 24L WD 240 CS43W LP750 DLC LBH0SZU","IBL 24L WD 240 CS43W LP750 DLC LBH0SZU (CI-233G9Y)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["214UYN","IBL 24L WD 277 CS11W LP740 DLC","IBL 24L WD 277 CS11W LP740 DLC (CI-214UYN)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["214WW2","IBL 24L WD 277 CS11W LP750 DLC","IBL 24L WD 277 CS11W LP750 DLC (CI-214WW2)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235F1U","IBL 24L WD 277 CS11W LP750 DLC LAH0SZU","IBL 24L WD 277 CS11W LP750 DLC LAH0SZU (CI-235F1U)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["231E6H","IBL 24L WD 277 CS11W LP750 DLC LAOZU","IBL 24L WD 277 CS11W LP750 DLC LAOZU (CI-231E6H)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["223K93","IBL 24L WD 277 CS11W LP750 DLC MSE360","IBL 24L WD 277 CS11W LP750 DLC MSE360 (CI-223K93)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
[{"$f":"(LEFT((RIGHT(C25948,7)),6))","v":"222G70"},{"$f":"LEFT(C25948,SEARCH(\"(CI-\",C25948)-2)","v":"IBL 24L WD 277 CS11W LP750 DLC MSI360"},"IBL 24L WD 277 CS11W LP750 DLC MSI360 (CI-222G70)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["229W29","IBL 24L WD 277 CS11W LP840 LAOZU","IBL 24L WD 277 CS11W LP840 LAOZU (CI-229W29)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238LEM","IBL 24L WD 277 CS11W LP850 MSE360","IBL 24L WD 277 CS11W LP850 MSE360 (CI-238LEM)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["224JYC","IBL 24L WD 277 CS11WL10 LP750 DLC","IBL 24L WD 277 CS11WL10 LP750 DLC (CI-224JYC)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239APW","IBL 24L WD 277 CS11WL10 LP840 LAOZU","IBL 24L WD 277 CS11WL10 LP840 LAOZU (CI-239APW)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239RT3","IBL 24L WD 277 CS11WL10 LP850 LCOZU","IBL 24L WD 277 CS11WL10 LP850 LCOZU (CI-239RT3)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["226YE9","IBL 24L WD 277 CS11WL15 LP750 DLC","IBL 24L WD 277 CS11WL15 LP750 DLC (CI-226YE9)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235N8W","IBL 24L WD 277 CS11WL15 LP850 LAPZU","IBL 24L WD 277 CS11WL15 LP850 LAPZU (CI-235N8W)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236JY7","IBL 24L WD 277 CS11WL15 LP850 LCOZU","IBL 24L WD 277 CS11WL15 LP850 LCOZU (CI-236JY7)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["216TFJ","IBL 24L WD 277 CS11WL20 LP740 DLC","IBL 24L WD 277 CS11WL20 LP740 DLC (CI-216TFJ)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235KPJ","IBL 24L WD 277 CS7WL10 LP750 DLC","IBL 24L WD 277 CS7WL10 LP750 DLC (CI-235KPJ)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235M5V","IBL 24L WD 277 CS7WL15 LP850","IBL 24L WD 277 CS7WL15 LP850 (CI-235M5V)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235LP6","IBL 24L WD 277 CS93W LP750 DLC LAM06TU","IBL 24L WD 277 CS93W LP750 DLC LAM06TU (CI-235LP6)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235L7M","IBL 24L WD 277 CS93W LP750 DLC LBOTU","IBL 24L WD 277 CS93W LP750 DLC LBOTU (CI-235L7M)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239HKW","IBL 24L WD 277 CS93W LP850 MSE360 WGX","IBL 24L WD 277 CS93W LP850 MSE360 WGX (CI-239HKW)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["221CJC","IBL 24L WD 277 GLR LP740 DLC","IBL 24L WD 277 GLR LP740 DLC (CI-221CJC)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["227C6E","IBL 24L WD 277 IMP LP740 DLC WGX","IBL 24L WD 277 IMP LP740 DLC WGX (CI-227C6E)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238WA6","IBL 24L WD 277 IMP LP740 DWH DLC MSE360 WGX","IBL 24L WD 277 IMP LP740 DWH DLC MSE360 WGX (CI-238WA6)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["226JXC","IBL 24L WD 277 IMP LP750 DLC","IBL 24L WD 277 IMP LP750 DLC (CI-226JXC)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238V3F","IBL 24L WD 277 LP740 DLC LAM0SZU","IBL 24L WD 277 LP740 DLC LAM0SZU (CI-238V3F)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["226LK6","IBL 24L WD 277 LP740 DLC LAOZU","IBL 24L WD 277 LP740 DLC LAOZU (CI-226LK6)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235TNK","IBL 24L WD 277 LP740 DLC LAPZU","IBL 24L WD 277 LP740 DLC LAPZU (CI-235TNK)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235R91","IBL 24L WD 277 LP740 DLC LCOZU","IBL 24L WD 277 LP740 DLC LCOZU (CI-235R91)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["218YMH","IBL 24L WD 277 LP740 DLC MSE360","IBL 24L WD 277 LP740 DLC MSE360 (CI-218YMH)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["230T3G","IBL 24L WD 277 LP740 DLC MSE360 WGX","IBL 24L WD 277 LP740 DLC MSE360 WGX (CI-230T3G)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["215WCP","IBL 24L WD 277 LP740 DLC MSI360","IBL 24L WD 277 LP740 DLC MSI360 (CI-215WCP)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["225VFJ","IBL 24L WD 277 LP740 DLC MSI360D","IBL 24L WD 277 LP740 DLC MSI360D (CI-225VFJ)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235GR1","IBL 24L WD 277 LP750 DLC LAH0SZU","IBL 24L WD 277 LP750 DLC LAH0SZU (CI-235GR1)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["226GUJ","IBL 24L WD 277 LP750 DLC LAOZU","IBL 24L WD 277 LP750 DLC LAOZU (CI-226GUJ)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["226HVU","IBL 24L WD 277 LP750 DLC MSE360","IBL 24L WD 277 LP750 DLC MSE360 (CI-226HVU)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["214VPT","IBL 24L WD 277 LP750 DLC MSI360","IBL 24L WD 277 LP750 DLC MSI360 (CI-214VPT)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238H1P","IBL 24L WD 277 LP835 NPP16D WGX","IBL 24L WD 277 LP835 NPP16D WGX (CI-238H1P)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235LRN","IBL 24L WD 277 LP840 DWH LAOZU","IBL 24L WD 277 LP840 DWH LAOZU (CI-235LRN)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["229X6N","IBL 24L WD 277 LP840 LAM0SZU","IBL 24L WD 277 LP840 LAM0SZU (CI-229X6N)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["220L7M","IBL 24L WD 277 OCS LP740 DLC","IBL 24L WD 277 OCS LP740 DLC (CI-220L7M)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237JWL","IBL 24L WD 277 OCS LP740 DLC LAOZU","IBL 24L WD 277 OCS LP740 DLC LAOZU (CI-237JWL)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["222T9W","IBL 24L WD 277 OCS LP750 DLC","IBL 24L WD 277 OCS LP750 DLC (CI-222T9W)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["233G3V","IBL 24L WD 277 OCS LP750 DLC LAH0SZU","IBL 24L WD 277 OCS LP750 DLC LAH0SZU (CI-233G3V)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["222TAF","IBL 24L WD 277 OCS LP750 DLC MSE360","IBL 24L WD 277 OCS LP750 DLC MSE360 (CI-222TAF)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234V04","IBL 24L WD 277 OCS LP750 DLC NPP16D","IBL 24L WD 277 OCS LP750 DLC NPP16D (CI-234V04)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237JWJ","IBL 24L WD 277 OCS10 LP740 DLC LAOZU","IBL 24L WD 277 OCS10 LP740 DLC LAOZU (CI-237JWJ)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["223LRH","IBL 24L WD 277 OCS10 LP750 DLC","IBL 24L WD 277 OCS10 LP750 DLC (CI-223LRH)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["226GPJ","IBL 24L WD 277 OCS10 LP750 DLC MSI360","IBL 24L WD 277 OCS10 LP750 DLC MSI360 (CI-226GPJ)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["226FC5","IBL 24L WD 277 OCS4CL10 LP750 DWH DLC","IBL 24L WD 277 OCS4CL10 LP750 DWH DLC (CI-226FC5)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237C5P","IBL 24L WD 347 LP735 MSE360","IBL 24L WD 347 LP735 MSE360 (CI-237C5P)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239RXW","IBL 24L WD 480 CS97W LP740 DWH DLC","IBL 24L WD 480 CS97W LP740 DWH DLC (CI-239RXW)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["221KML","IBL 24L WD 480 CS97W LP750 DLC","IBL 24L WD 480 CS97W LP750 DLC (CI-221KML)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234Y2H","IBL 24L WD 480 GLR LP740 DLC","IBL 24L WD 480 GLR LP740 DLC (CI-234Y2H)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239WKG","IBL 24L WD 480 IMP LP750 DLC","IBL 24L WD 480 IMP LP750 DLC (CI-239WKG)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["226VWM","IBL 24L WD 480 LP740 DLC","IBL 24L WD 480 LP740 DLC (CI-226VWM)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["228F97","IBL 24L WD 480 LP750 DLC USPOM","IBL 24L WD 480 LP750 DLC USPOM (CI-228F97)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["232WPP","IBL 24L WD 480 OCS LP740 DLC","IBL 24L WD 480 OCS LP740 DLC (CI-232WPP)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237JG7","IBL 24L WD 480 OCS LP840","IBL 24L WD 480 OCS LP840 (CI-237JG7)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234PA1","IBL 24L WD 480 OCS10 LP740 DLC LAM0SZU","IBL 24L WD 480 OCS10 LP740 DLC LAM0SZU (CI-234PA1)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["223LRT","IBL 24L WD 480 OCS10 LP750 DLC","IBL 24L WD 480 OCS10 LP750 DLC (CI-223LRT)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236C12","IBL 24L WD 480 OCS10 LP750 DLC LAM0SZU","IBL 24L WD 480 OCS10 LP750 DLC LAM0SZU (CI-236C12)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239JXM","IBL 24L WD ACL 277 LP740 DWH DLC LAOZU WGX","IBL 24L WD ACL 277 LP740 DWH DLC LAOZU WGX (CI-239JXM)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239JXK","IBL 24L WD ACL LP740 DWH DLC WGX","IBL 24L WD ACL LP740 DWH DLC WGX (CI-239JXK)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["214W8R","IBL 24L WD CS93W LP740 DLC","IBL 24L WD CS93W LP740 DLC (CI-214W8R)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["216WU3","IBL 24L WD CS93W LP750 DLC","IBL 24L WD CS93W LP750 DLC (CI-216WU3)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["217MJY","IBL 24L WD CS93W LP750 DLC WGX","IBL 24L WD CS93W LP750 DLC WGX (CI-217MJY)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235V3F","IBL 24L WD CS93W LP840 DWH","IBL 24L WD CS93W LP840 DWH (CI-235V3F)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["219E18","IBL 24L WD CS93WL10 LP750 DLC","IBL 24L WD CS93WL10 LP750 DLC (CI-219E18)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235VTM","IBL 24L WD CS93WL12 LP750 DLC","IBL 24L WD CS93WL12 LP750 DLC (CI-235VTM)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
[{"$f":"(LEFT((RIGHT(C26012,7)),6))","v":"228X3V"},{"$f":"LEFT(C26012,SEARCH(\"(CI-\",C26012)-2)","v":"IBL 24L WD IMP LP740 DLC WGX"},"IBL 24L WD IMP LP740 DLC WGX (CI-228X3V)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["220TFR","IBL 24L WD IMP LP750 DLC","IBL 24L WD IMP LP750 DLC (CI-220TFR)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["227MTM","IBL 24L WD LP735","IBL 24L WD LP735 (CI-227MTM)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["213VRU","IBL 24L WD LP740 DLC","IBL 24L WD LP740 DLC (CI-213VRU)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236UX2","IBL 24L WD LP740 DLC DWH","IBL 24L WD LP740 DLC DWH (CI-236UX2)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237EHX","IBL 24L WD LP740 DLC DWH WGX","IBL 24L WD LP740 DLC DWH WGX (CI-237EHX)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236WFX","IBL 24L WD LP740 DLC NOM","IBL 24L WD LP740 DLC NOM (CI-236WFX)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["215NXG","IBL 24L WD LP740 DLC WGX","IBL 24L WD LP740 DLC WGX (CI-215NXG)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["221MLR","IBL 24L WD LP740 DWH DLC","IBL 24L WD LP740 DWH DLC (CI-221MLR)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["225PTM","IBL 24L WD LP740 DWH DLC WGX","IBL 24L WD LP740 DWH DLC WGX (CI-225PTM)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["213VVK","IBL 24L WD LP750 DLC","IBL 24L WD LP750 DLC (CI-213VVK)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234U67","IBL 24L WD LP750 DLC NOM","IBL 24L WD LP750 DLC NOM (CI-234U67)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["221GH8","IBL 24L WD LP750 DLC OUTCTR","IBL 24L WD LP750 DLC OUTCTR (CI-221GH8)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["216TXG","IBL 24L WD LP750 DLC WGX","IBL 24L WD LP750 DLC WGX (CI-216TXG)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["215VYG","IBL 24L WD LP750 DWH DLC","IBL 24L WD LP750 DWH DLC (CI-215VYG)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["226HL0","IBL 24L WD LP835","IBL 24L WD LP835 (CI-226HL0)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235EN1","IBL 24L WD LP835 DWH","IBL 24L WD LP835 DWH (CI-235EN1)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["226L5H","IBL 24L WD LP840","IBL 24L WD LP840 (CI-226L5H)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["231YYF","IBL 24L WD LP840 DWH","IBL 24L WD LP840 DWH (CI-231YYF)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239XE5","IBL 24L WD LP840 NOM","IBL 24L WD LP840 NOM (CI-239XE5)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234RF0","IBL 24L WD LP840 USPOM","IBL 24L WD LP840 USPOM (CI-234RF0)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["226JY1","IBL 24L WD LP840 WGX","IBL 24L WD LP840 WGX (CI-226JY1)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["226P3J","IBL 24L WD LP850","IBL 24L WD LP850 (CI-226P3J)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["225WMN","IBL 24L WD LP850 DWH","IBL 24L WD LP850 DWH (CI-225WMN)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["229AY7","IBL 24L WD LP850 USPOM","IBL 24L WD LP850 USPOM (CI-229AY7)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["214TA6","IBL 24L WD SD125 120 CS1W LP740 DLC","IBL 24L WD SD125 120 CS1W LP740 DLC (CI-214TA6)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["222FP6","IBL 24L WD SD125 120 CS1W LP740 DLC WGX","IBL 24L WD SD125 120 CS1W LP740 DLC WGX (CI-222FP6)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235E3Y","IBL 24L WD SD125 120 CS1W LP840","IBL 24L WD SD125 120 CS1W LP840 (CI-235E3Y)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235LRE","IBL 24L WD SD125 120 CS3W LP740 DWH DLC WGX","IBL 24L WD SD125 120 CS3W LP740 DWH DLC WGX (CI-235LRE)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239U74","IBL 24L WD SD125 120 CS93W LP740 DWH DLC NPP16D","IBL 24L WD SD125 120 CS93W LP740 DWH DLC NPP16D (CI-239U74)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238MFF","IBL 24L WD SD125 120 CS93W LP840 DWH LAM0SZU","IBL 24L WD SD125 120 CS93W LP840 DWH LAM0SZU (CI-238MFF)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237UXC","IBL 24L WD SD125 120 CS93W LP840 LAOZU","IBL 24L WD SD125 120 CS93W LP840 LAOZU (CI-237UXC)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237WNX","IBL 24L WD SD125 120 GLR LP740 DWH DLC","IBL 24L WD SD125 120 GLR LP740 DWH DLC (CI-237WNX)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237HG7","IBL 24L WD SD125 120 LP735 NPP16D","IBL 24L WD SD125 120 LP735 NPP16D (CI-237HG7)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235TNH","IBL 24L WD SD125 120 LP735 NPP16D WGX","IBL 24L WD SD125 120 LP735 NPP16D WGX (CI-235TNH)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237M5Y","IBL 24L WD SD125 120 LP740 DLC LAOZU","IBL 24L WD SD125 120 LP740 DLC LAOZU (CI-237M5Y)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235N5J","IBL 24L WD SD125 120 LP740 DLC LCOZU","IBL 24L WD SD125 120 LP740 DLC LCOZU (CI-235N5J)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["214RER","IBL 24L WD SD125 120 LP740 DLC MSE360","IBL 24L WD SD125 120 LP740 DLC MSE360 (CI-214RER)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236UX1","IBL 24L WD SD125 120 LP740 DLC NMSI360D","IBL 24L WD SD125 120 LP740 DLC NMSI360D (CI-236UX1)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["225VT4","IBL 24L WD SD125 120 LP740 DLC NPP16D","IBL 24L WD SD125 120 LP740 DLC NPP16D (CI-225VT4)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["227WKH","IBL 24L WD SD125 120 LP740 DLC NPP16D WGX","IBL 24L WD SD125 120 LP740 DLC NPP16D WGX (CI-227WKH)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["225TK2","IBL 24L WD SD125 120 LP740 DWH DLC NPP16D WGX","IBL 24L WD SD125 120 LP740 DWH DLC NPP16D WGX (CI-225TK2)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["221NH0","IBL 24L WD SD125 120 LP740 DWH DLC OUTCTR MSE360","IBL 24L WD SD125 120 LP740 DWH DLC OUTCTR MSE360 (CI-221NH0)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239JXP","IBL 24L WD SD125 120 LP835 LAPZU","IBL 24L WD SD125 120 LP835 LAPZU (CI-239JXP)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234P4L","IBL 24L WD SD125 120 LP835 NPP16D","IBL 24L WD SD125 120 LP835 NPP16D (CI-234P4L)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237Y3F","IBL 24L WD SD125 120 LP840 DWH MSI360D","IBL 24L WD SD125 120 LP840 DWH MSI360D (CI-237Y3F)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236XW5","IBL 24L WD SD125 120 LP840 LAM0SZU","IBL 24L WD SD125 120 LP840 LAM0SZU (CI-236XW5)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238WAJ","IBL 24L WD SD125 120 LP840 NPP16D WGX","IBL 24L WD SD125 120 LP840 NPP16D WGX (CI-238WAJ)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235R8T","IBL 24L WD SD125 120 LP850 NPP16D WGX","IBL 24L WD SD125 120 LP850 NPP16D WGX (CI-235R8T)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["233V3A","IBL 24L WD SD125 120 LP850 OUTCTR LAOZU WGX","IBL 24L WD SD125 120 LP850 OUTCTR LAOZU WGX (CI-233V3A)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["221KP7","IBL 24L WD SD125 208 LP740 DLC MSI360","IBL 24L WD SD125 208 LP740 DLC MSI360 (CI-221KP7)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237HFT","IBL 24L WD SD125 277 CS11W LP735","IBL 24L WD SD125 277 CS11W LP735 (CI-237HFT)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236A9R","IBL 24L WD SD125 277 CS11W LP735 DWH NPP16D WGX","IBL 24L WD SD125 277 CS11W LP735 DWH NPP16D WGX (CI-236A9R)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["216CCW","IBL 24L WD SD125 277 CS11W LP740 DLC","IBL 24L WD SD125 277 CS11W LP740 DLC (CI-216CCW)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["233J8J","IBL 24L WD SD125 277 CS11W LP740 DLC WGX","IBL 24L WD SD125 277 CS11W LP740 DLC WGX (CI-233J8J)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238HE4","IBL 24L WD SD125 277 CS11W LP740 DWH DLC LAOZU","IBL 24L WD SD125 277 CS11W LP740 DWH DLC LAOZU (CI-238HE4)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["228MYW","IBL 24L WD SD125 277 CS11W LP740 DWH DLC WGX","IBL 24L WD SD125 277 CS11W LP740 DWH DLC WGX (CI-228MYW)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["214RCT","IBL 24L WD SD125 277 CS11W LP750 DLC","IBL 24L WD SD125 277 CS11W LP750 DLC (CI-214RCT)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239F0Y","IBL 24L WD SD125 277 CS11W LP835","IBL 24L WD SD125 277 CS11W LP835 (CI-239F0Y)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["230RY7","IBL 24L WD SD125 277 CS11W LP840","IBL 24L WD SD125 277 CS11W LP840 (CI-230RY7)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["231JKX","IBL 24L WD SD125 277 CS11W LP850","IBL 24L WD SD125 277 CS11W LP850 (CI-231JKX)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["222EAL","IBL 24L WD SD125 277 CS11WL10 LP740 DLC","IBL 24L WD SD125 277 CS11WL10 LP740 DLC (CI-222EAL)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["224U47","IBL 24L WD SD125 277 CS11WL10 LP740 DWH DLC MSI360","IBL 24L WD SD125 277 CS11WL10 LP740 DWH DLC MSI360 (CI-224U47)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234V1T","IBL 24L WD SD125 277 CS11WL10 LP750 DLC NPP16D","IBL 24L WD SD125 277 CS11WL10 LP750 DLC NPP16D (CI-234V1T)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
[{"$f":"(LEFT((RIGHT(C26076,7)),6))","v":"236AFY"},{"$f":"LEFT(C26076,SEARCH(\"(CI-\",C26076)-2)","v":"IBL 24L WD SD125 277 CS11WL15 LP840"},"IBL 24L WD SD125 277 CS11WL15 LP840 (CI-236AFY)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235N8L","IBL 24L WD SD125 277 CS11WL15 LP850 LAPZU","IBL 24L WD SD125 277 CS11WL15 LP850 LAPZU (CI-235N8L)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["230C0X","IBL 24L WD SD125 277 CS93W LP740 DLC LAOZU DWH WGX","IBL 24L WD SD125 277 CS93W LP740 DLC LAOZU DWH WGX (CI-230C0X)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239WKT","IBL 24L WD SD125 277 CS93W LP750 DLC NPP16D OUTCTR","IBL 24L WD SD125 277 CS93W LP750 DLC NPP16D OUTCTR (CI-239WKT)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237VVY","IBL 24L WD SD125 277 CS93W LP840 DWH LAOZU","IBL 24L WD SD125 277 CS93W LP840 DWH LAOZU (CI-237VVY)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238A7R","IBL 24L WD SD125 277 CS93W LP850 MSE360 DWH","IBL 24L WD SD125 277 CS93W LP850 MSE360 DWH (CI-238A7R)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["232PJW","IBL 24L WD SD125 277 CS93WL10 LP840 NPP16D","IBL 24L WD SD125 277 CS93WL10 LP840 NPP16D (CI-232PJW)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234Y39","IBL 24L WD SD125 277 CS93WL12 LP740 DLC MSE360 USPOM","IBL 24L WD SD125 277 CS93WL12 LP740 DLC MSE360 USPOM (CI-234Y39)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236KK7","IBL 24L WD SD125 277 GLR LP740 DLC LAOZU WGX","IBL 24L WD SD125 277 GLR LP740 DLC LAOZU WGX (CI-236KK7)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["226XXC","IBL 24L WD SD125 277 GLR LP740 DLC WGX","IBL 24L WD SD125 277 GLR LP740 DLC WGX (CI-226XXC)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237TVK","IBL 24L WD SD125 277 GLR LP840 DWH WGX","IBL 24L WD SD125 277 GLR LP840 DWH WGX (CI-237TVK)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239X3N","IBL 24L WD SD125 277 LP740 DLC LAM0SZU","IBL 24L WD SD125 277 LP740 DLC LAM0SZU (CI-239X3N)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["229L6G","IBL 24L WD SD125 277 LP740 DLC LAOZU","IBL 24L WD SD125 277 LP740 DLC LAOZU (CI-229L6G)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["217YYP","IBL 24L WD SD125 277 LP740 DLC MSI360","IBL 24L WD SD125 277 LP740 DLC MSI360 (CI-217YYP)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234RYR","IBL 24L WD SD125 277 LP740 DLC NMSI360D","IBL 24L WD SD125 277 LP740 DLC NMSI360D (CI-234RYR)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["231Y3K","IBL 24L WD SD125 277 LP740 DLC NPP16D WGX","IBL 24L WD SD125 277 LP740 DLC NPP16D WGX (CI-231Y3K)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238LFH","IBL 24L WD SD125 277 LP750 DLC LAH0SZU","IBL 24L WD SD125 277 LP750 DLC LAH0SZU (CI-238LFH)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234P4F","IBL 24L WD SD125 277 LP750 DLC LAM0SZU","IBL 24L WD SD125 277 LP750 DLC LAM0SZU (CI-234P4F)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234KVE","IBL 24L WD SD125 277 LP750 DLC LAOZU","IBL 24L WD SD125 277 LP750 DLC LAOZU (CI-234KVE)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["228T45","IBL 24L WD SD125 277 LP750 DLC MSE360","IBL 24L WD SD125 277 LP750 DLC MSE360 (CI-228T45)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["218G5C","IBL 24L WD SD125 277 LP750 DLC MSI360","IBL 24L WD SD125 277 LP750 DLC MSI360 (CI-218G5C)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["223KKL","IBL 24L WD SD125 277 LP750 DLC MSI360PED","IBL 24L WD SD125 277 LP750 DLC MSI360PED (CI-223KKL)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238HCV","IBL 24L WD SD125 277 LP750 DLC NMSI360 WGX","IBL 24L WD SD125 277 LP750 DLC NMSI360 WGX (CI-238HCV)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236LH9","IBL 24L WD SD125 277 LP835 LAM0SZU","IBL 24L WD SD125 277 LP835 LAM0SZU (CI-236LH9)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238V40","IBL 24L WD SD125 277 LP835 LAPZU","IBL 24L WD SD125 277 LP835 LAPZU (CI-238V40)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["229F3Y","IBL 24L WD SD125 277 LP840 LAOZU","IBL 24L WD SD125 277 LP840 LAOZU (CI-229F3Y)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["229PHF","IBL 24L WD SD125 277 LP840 LCPZU","IBL 24L WD SD125 277 LP840 LCPZU (CI-229PHF)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239WHU","IBL 24L WD SD125 277 LP840 MSI6XADL DSCXADL WGX","IBL 24L WD SD125 277 LP840 MSI6XADL DSCXADL WGX (CI-239WHU)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236GXM","IBL 24L WD SD125 277 LP840 NPP16D WGX","IBL 24L WD SD125 277 LP840 NPP16D WGX (CI-236GXM)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239PF2","IBL 24L WD SD125 277 LP850 NMSI","IBL 24L WD SD125 277 LP850 NMSI (CI-239PF2)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239PF9","IBL 24L WD SD125 277 LP850 NMSI360","IBL 24L WD SD125 277 LP850 NMSI360 (CI-239PF9)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239F1G","IBL 24L WD SD125 277 LP850 NPP16D WGX","IBL 24L WD SD125 277 LP850 NPP16D WGX (CI-239F1G)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["227TP1","IBL 24L WD SD125 277 OCS LP740 DLC NPP16D","IBL 24L WD SD125 277 OCS LP740 DLC NPP16D (CI-227TP1)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238V3T","IBL 24L WD SD125 277 OCS LP840","IBL 24L WD SD125 277 OCS LP840 (CI-238V3T)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238WR5","IBL 24L WD SD125 277 OCS LP850","IBL 24L WD SD125 277 OCS LP850 (CI-238WR5)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238V3U","IBL 24L WD SD125 277 OCS LP850 LAOZU","IBL 24L WD SD125 277 OCS LP850 LAOZU (CI-238V3U)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236NKN","IBL 24L WD SD125 277 OCS10 LP750 DLC MSE360","IBL 24L WD SD125 277 OCS10 LP750 DLC MSE360 (CI-236NKN)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235EEH","IBL 24L WD SD125 277 OCS10 LP840 DWH LAH0SZU","IBL 24L WD SD125 277 OCS10 LP840 DWH LAH0SZU (CI-235EEH)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["223VYG","IBL 24L WD SD125 347 CS93W LP740 DLC MSI360","IBL 24L WD SD125 347 CS93W LP740 DLC MSI360 (CI-223VYG)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234R4F","IBL 24L WD SD125 347 LP740 DLC MSE360","IBL 24L WD SD125 347 LP740 DLC MSE360 (CI-234R4F)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["229WMF","IBL 24L WD SD125 347 LP740 DLC NPP16D","IBL 24L WD SD125 347 LP740 DLC NPP16D (CI-229WMF)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239M71","IBL 24L WD SD125 347 LP740 DWH DLC LCPZU","IBL 24L WD SD125 347 LP740 DWH DLC LCPZU (CI-239M71)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["218TJ1","IBL 24L WD SD125 480 CS97W LP750 DLC","IBL 24L WD SD125 480 CS97W LP750 DLC (CI-218TJ1)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["218KUT","IBL 24L WD SD125 CS93W LP740 DLC","IBL 24L WD SD125 CS93W LP740 DLC (CI-218KUT)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["233MP3","IBL 24L WD SD125 CS93W LP740 DLC USPOM","IBL 24L WD SD125 CS93W LP740 DLC USPOM (CI-233MP3)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["222K6J","IBL 24L WD SD125 CS93W LP740 DLC WGX","IBL 24L WD SD125 CS93W LP740 DLC WGX (CI-222K6J)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238PN3","IBL 24L WD SD125 CS93W LP740 DLC WGX OUTCTR","IBL 24L WD SD125 CS93W LP740 DLC WGX OUTCTR (CI-238PN3)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["227U9Y","IBL 24L WD SD125 CS93W LP740 DWH DLC","IBL 24L WD SD125 CS93W LP740 DWH DLC (CI-227U9Y)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["215JP0","IBL 24L WD SD125 CS93W LP750 DLC","IBL 24L WD SD125 CS93W LP750 DLC (CI-215JP0)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["224AK9","IBL 24L WD SD125 CS93W LP750 DWH DLC","IBL 24L WD SD125 CS93W LP750 DWH DLC (CI-224AK9)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234NTX","IBL 24L WD SD125 CS93W LP835","IBL 24L WD SD125 CS93W LP835 (CI-234NTX)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238V3R","IBL 24L WD SD125 CS93W LP840","IBL 24L WD SD125 CS93W LP840 (CI-238V3R)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["229AEW","IBL 24L WD SD125 CS93W LP850","IBL 24L WD SD125 CS93W LP850 (CI-229AEW)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236ERX","IBL 24L WD SD125 CS93WL10 LP740 DLC USPOM","IBL 24L WD SD125 CS93WL10 LP740 DLC USPOM (CI-236ERX)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234J71","IBL 24L WD SD125 CS93WL10 LP750 DLC","IBL 24L WD SD125 CS93WL10 LP750 DLC (CI-234J71)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239F1A","IBL 24L WD SD125 CS93WL10 LP840","IBL 24L WD SD125 CS93WL10 LP840 (CI-239F1A)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["227CJ0","IBL 24L WD SD125 IMP LP750 DLC","IBL 24L WD SD125 IMP LP750 DLC (CI-227CJ0)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["231A63","IBL 24L WD SD125 LP735","IBL 24L WD SD125 LP735 (CI-231A63)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239F0C","IBL 24L WD SD125 LP735 WGX","IBL 24L WD SD125 LP735 WGX (CI-239F0C)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["214ACV","IBL 24L WD SD125 LP740 DLC","IBL 24L WD SD125 LP740 DLC (CI-214ACV)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["216LUC","IBL 24L WD SD125 LP740 DLC USPOM","IBL 24L WD SD125 LP740 DLC USPOM (CI-216LUC)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["215GNA","IBL 24L WD SD125 LP740 DLC WGX","IBL 24L WD SD125 LP740 DLC WGX (CI-215GNA)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235AK4","IBL 24L WD SD125 LP740 DLC WGX USPOM","IBL 24L WD SD125 LP740 DLC WGX USPOM (CI-235AK4)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["214PP3","IBL 24L WD SD125 LP740 DWH DLC","IBL 24L WD SD125 LP740 DWH DLC (CI-214PP3)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
[{"$f":"(LEFT((RIGHT(C26140,7)),6))","v":"225VEH"},{"$f":"LEFT(C26140,SEARCH(\"(CI-\",C26140)-2)","v":"IBL 24L WD SD125 LP740 DWH DLC OUTCTR WGX"},"IBL 24L WD SD125 LP740 DWH DLC OUTCTR WGX (CI-225VEH)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["229L5U","IBL 24L WD SD125 LP740 DWH DLC USPOM","IBL 24L WD SD125 LP740 DWH DLC USPOM (CI-229L5U)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["215RRX","IBL 24L WD SD125 LP740 DWH DLC WGX","IBL 24L WD SD125 LP740 DWH DLC WGX (CI-215RRX)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["214AF9","IBL 24L WD SD125 LP750 DLC","IBL 24L WD SD125 LP750 DLC (CI-214AF9)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237W69","IBL 24L WD SD125 LP750 DLC NOM","IBL 24L WD SD125 LP750 DLC NOM (CI-237W69)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["215NAF","IBL 24L WD SD125 LP750 DLC WGX","IBL 24L WD SD125 LP750 DLC WGX (CI-215NAF)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["218G9R","IBL 24L WD SD125 LP750 DWH DLC","IBL 24L WD SD125 LP750 DWH DLC (CI-218G9R)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["227J1X","IBL 24L WD SD125 LP835","IBL 24L WD SD125 LP835 (CI-227J1X)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["231GT3","IBL 24L WD SD125 LP835 DWH","IBL 24L WD SD125 LP835 DWH (CI-231GT3)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["226TYE","IBL 24L WD SD125 LP835 WGX","IBL 24L WD SD125 LP835 WGX (CI-226TYE)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["225RAV","IBL 24L WD SD125 LP840","IBL 24L WD SD125 LP840 (CI-225RAV)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["227VEU","IBL 24L WD SD125 LP840 DWH","IBL 24L WD SD125 LP840 DWH (CI-227VEU)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["230CKK","IBL 24L WD SD125 LP840 DWH OUTCTR WGX","IBL 24L WD SD125 LP840 DWH OUTCTR WGX (CI-230CKK)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["233JU8","IBL 24L WD SD125 LP840 DWH WGX","IBL 24L WD SD125 LP840 DWH WGX (CI-233JU8)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["232PME","IBL 24L WD SD125 LP840 OUTCTR WGX","IBL 24L WD SD125 LP840 OUTCTR WGX (CI-232PME)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["230HFL","IBL 24L WD SD125 LP840 WGX","IBL 24L WD SD125 LP840 WGX (CI-230HFL)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["225J4R","IBL 24L WD SD125 LP850","IBL 24L WD SD125 LP850 (CI-225J4R)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["232YVC","IBL 24L WD SD125 LP850 DWH","IBL 24L WD SD125 LP850 DWH (CI-232YVC)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["225FF9","IBL 24L WD SD125 LP850 WGX","IBL 24L WD SD125 LP850 WGX (CI-225FF9)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238EE9","IBL 36L ND 120 LP850 NPP16D WGX USPOM","IBL 36L ND 120 LP850 NPP16D WGX USPOM (CI-238EE9)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["227MK7","IBL 36L ND 277 CS11W LP740 DLC","IBL 36L ND 277 CS11W LP740 DLC (CI-227MK7)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235EN7","IBL 36L ND 277 CS11W LP740 DWH DLC","IBL 36L ND 277 CS11W LP740 DWH DLC (CI-235EN7)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236JK6","IBL 36L ND 277 CS11W LP750 DLC MSI6XADL DSCXADL","IBL 36L ND 277 CS11W LP750 DLC MSI6XADL DSCXADL (CI-236JK6)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237TKV","IBL 36L ND 277 CS93W LP750 DLC LAOZU","IBL 36L ND 277 CS93W LP750 DLC LAOZU (CI-237TKV)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238GH9","IBL 36L ND 277 LP740 DLC LAM0SZU","IBL 36L ND 277 LP740 DLC LAM0SZU (CI-238GH9)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["232YWP","IBL 36L ND 277 LP850 DWH NPP16D","IBL 36L ND 277 LP850 DWH NPP16D (CI-232YWP)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["231HNE","IBL 36L ND CS93W LP750 DLC","IBL 36L ND CS93W LP750 DLC (CI-231HNE)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234Y3J","IBL 36L ND CS93WL15 LP750 DLC","IBL 36L ND CS93WL15 LP750 DLC (CI-234Y3J)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["221H73","IBL 36L ND LP740 DLC","IBL 36L ND LP740 DLC (CI-221H73)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234GN5","IBL 36L ND LP740 DLC WGX","IBL 36L ND LP740 DLC WGX (CI-234GN5)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["221H75","IBL 36L ND LP750 DLC","IBL 36L ND LP750 DLC (CI-221H75)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237X3N","IBL 36L ND LP750 DWH DLC","IBL 36L ND LP750 DWH DLC (CI-237X3N)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239FM3","IBL 36L ND LP840","IBL 36L ND LP840 (CI-239FM3)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["233GEH","IBL 36L ND LP850","IBL 36L ND LP850 (CI-233GEH)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238GTX","IBL 36L ND LP850 DWH NOM","IBL 36L ND LP850 DWH NOM (CI-238GTX)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235T8F","IBL 36L ND SD125 277 LP740 DLC NMSI360D","IBL 36L ND SD125 277 LP740 DLC NMSI360D (CI-235T8F)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237RJG","IBL 36L ND SD125 277 LP840 NPP16D WGX","IBL 36L ND SD125 277 LP840 NPP16D WGX (CI-237RJG)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236C85","IBL 36L ND SD125 277 OCS LP740 DLC","IBL 36L ND SD125 277 OCS LP740 DLC (CI-236C85)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236C82","IBL 36L ND SD125 277 OCS LP740 DLC MSE360","IBL 36L ND SD125 277 OCS LP740 DLC MSE360 (CI-236C82)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["226VVL","IBL 36L ND SD125 277 OCS LP750 DLC MSE360","IBL 36L ND SD125 277 OCS LP750 DLC MSE360 (CI-226VVL)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["229N3L","IBL 36L ND SD125 277 OCS LP750 DWH DLC MSI360","IBL 36L ND SD125 277 OCS LP750 DWH DLC MSI360 (CI-229N3L)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239M72","IBL 36L ND SD125 277 OCS10 LP740 DLC MSE360","IBL 36L ND SD125 277 OCS10 LP740 DLC MSE360 (CI-239M72)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239HM3","IBL 36L ND SD125 277 OCU22N LP750 DLC MSE360","IBL 36L ND SD125 277 OCU22N LP750 DLC MSE360 (CI-239HM3)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236C6W","IBL 36L ND SD125 CS93W LP835","IBL 36L ND SD125 CS93W LP835 (CI-236C6W)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["221H7A","IBL 36L ND SD125 LP740 DLC","IBL 36L ND SD125 LP740 DLC (CI-221H7A)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["221H7C","IBL 36L ND SD125 LP750 DLC","IBL 36L ND SD125 LP750 DLC (CI-221H7C)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236CVW","IBL 36L ND SD125 LP750 DLC USPOM","IBL 36L ND SD125 LP750 DLC USPOM (CI-236CVW)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235U4L","IBL 36L ND SD125 LP835 WGX","IBL 36L ND SD125 LP835 WGX (CI-235U4L)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239GR3","IBL 36L ND SD125 LP840 OUTCTR WGX","IBL 36L ND SD125 LP840 OUTCTR WGX (CI-239GR3)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["226T6P","IBL 36L ND SD125 LP850","IBL 36L ND SD125 LP850 (CI-226T6P)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236M3U","IBL 36L WD 120 CS1WL10 LP750 DLC LCPZU","IBL 36L WD 120 CS1WL10 LP750 DLC LCPZU (CI-236M3U)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236JYE","IBL 36L WD 277 CS11W LP740 DLC","IBL 36L WD 277 CS11W LP740 DLC (CI-236JYE)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["228V7H","IBL 36L WD 277 CS11W LP740 DLC LAOZU","IBL 36L WD 277 CS11W LP740 DLC LAOZU (CI-228V7H)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["227LC3","IBL 36L WD 277 CS11WL15 LP750 DLC","IBL 36L WD 277 CS11WL15 LP750 DLC (CI-227LC3)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235G3J","IBL 36L WD 277 CS93W LP750 DLC NMSID WGX","IBL 36L WD 277 CS93W LP750 DLC NMSID WGX (CI-235G3J)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234Y9U","IBL 36L WD 277 LP740 DLC MSI360","IBL 36L WD 277 LP740 DLC MSI360 (CI-234Y9U)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235KKJ","IBL 36L WD 277 LP740 DLC NMSI360D","IBL 36L WD 277 LP740 DLC NMSI360D (CI-235KKJ)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["233M6C","IBL 36L WD 277 LP740 DLC XPW","IBL 36L WD 277 LP740 DLC XPW (CI-233M6C)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["228JN5","IBL 36L WD 277 LP750 DLC MSE360","IBL 36L WD 277 LP750 DLC MSE360 (CI-228JN5)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237N1G","IBL 36L WD 277 OCS LP740 DLC","IBL 36L WD 277 OCS LP740 DLC (CI-237N1G)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239JXT","IBL 36L WD 277 OCS LP750 DLC","IBL 36L WD 277 OCS LP750 DLC (CI-239JXT)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236J34","IBL 36L WD 277 OCS LP850","IBL 36L WD 277 OCS LP850 (CI-236J34)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239KV5","IBL 36L WD ACL LP740 DWH DLC WGX","IBL 36L WD ACL LP740 DWH DLC WGX (CI-239KV5)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["229M1M","IBL 36L WD CS93W LP740 DLC","IBL 36L WD CS93W LP740 DLC (CI-229M1M)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
[{"$f":"(LEFT((RIGHT(C26204,7)),6))","v":"237LUP"},{"$f":"LEFT(C26204,SEARCH(\"(CI-\",C26204)-2)","v":"IBL 36L WD LP735"},"IBL 36L WD LP735 (CI-237LUP)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["221H7G","IBL 36L WD LP740 DLC","IBL 36L WD LP740 DLC (CI-221H7G)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234FC4","IBL 36L WD LP740 DLC USPOM","IBL 36L WD LP740 DLC USPOM (CI-234FC4)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["224HEM","IBL 36L WD LP740 DLC WGX","IBL 36L WD LP740 DLC WGX (CI-224HEM)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["221H7H","IBL 36L WD LP750 DLC","IBL 36L WD LP750 DLC (CI-221H7H)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["224NNF","IBL 36L WD LP750 DWH DLC","IBL 36L WD LP750 DWH DLC (CI-224NNF)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["233GMX","IBL 36L WD LP840","IBL 36L WD LP840 (CI-233GMX)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236NLA","IBL 36L WD LP840 OUTCTR","IBL 36L WD LP840 OUTCTR (CI-236NLA)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["225X2W","IBL 36L WD LP850","IBL 36L WD LP850 (CI-225X2W)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237UXK","IBL 36L WD SD125 120 LP740 DLC NPP16D WGX","IBL 36L WD SD125 120 LP740 DLC NPP16D WGX (CI-237UXK)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239R53","IBL 36L WD SD125 120 LP740 DWH DLC NPP16D WGX","IBL 36L WD SD125 120 LP740 DWH DLC NPP16D WGX (CI-239R53)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["233HT2","IBL 36L WD SD125 277 CS11W LP740 DLC LAH02ZU","IBL 36L WD SD125 277 CS11W LP740 DLC LAH02ZU (CI-233HT2)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234P4Y","IBL 36L WD SD125 277 CS11W LP835","IBL 36L WD SD125 277 CS11W LP835 (CI-234P4Y)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237VWF","IBL 36L WD SD125 277 CS11W LP840","IBL 36L WD SD125 277 CS11W LP840 (CI-237VWF)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237LX6","IBL 36L WD SD125 277 CS11WL10 LP740 DLC","IBL 36L WD SD125 277 CS11WL10 LP740 DLC (CI-237LX6)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["233F02","IBL 36L WD SD125 277 CS11WL10 LP850 LAH0SZU","IBL 36L WD SD125 277 CS11WL10 LP850 LAH0SZU (CI-233F02)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238VNP","IBL 36L WD SD125 277 GLR IMP LP850 DWH","IBL 36L WD SD125 277 GLR IMP LP850 DWH (CI-238VNP)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237TW0","IBL 36L WD SD125 277 GLR LP840 DWH WGX","IBL 36L WD SD125 277 GLR LP840 DWH WGX (CI-237TW0)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234KAM","IBL 36L WD SD125 277 LP740 DLC XPW WGX","IBL 36L WD SD125 277 LP740 DLC XPW WGX (CI-234KAM)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236FL6","IBL 36L WD SD125 277 LP750 DLC LAOZU","IBL 36L WD SD125 277 LP750 DLC LAOZU (CI-236FL6)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239HL6","IBL 36L WD SD125 277 OCS LP750 DLC MSE360","IBL 36L WD SD125 277 OCS LP750 DLC MSE360 (CI-239HL6)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239HM9","IBL 36L WD SD125 277 OCU22N LP750 DLC MSE360","IBL 36L WD SD125 277 OCU22N LP750 DLC MSE360 (CI-239HM9)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236HMU","IBL 36L WD SD125 CS93W LP740 DLC","IBL 36L WD SD125 CS93W LP740 DLC (CI-236HMU)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237LX9","IBL 36L WD SD125 CS93W LP740 DWH DLC WGX","IBL 36L WD SD125 CS93W LP740 DWH DLC WGX (CI-237LX9)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238N8F","IBL 36L WD SD125 CS93W LP840 WGX","IBL 36L WD SD125 CS93W LP840 WGX (CI-238N8F)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236C5J","IBL 36L WD SD125 LP735","IBL 36L WD SD125 LP735 (CI-236C5J)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["221H7L","IBL 36L WD SD125 LP740 DLC","IBL 36L WD SD125 LP740 DLC (CI-221H7L)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234K41","IBL 36L WD SD125 LP740 DLC DBMFXD","IBL 36L WD SD125 LP740 DLC DBMFXD (CI-234K41)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["222W0G","IBL 36L WD SD125 LP740 DLC WGX","IBL 36L WD SD125 LP740 DLC WGX (CI-222W0G)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["229U2N","IBL 36L WD SD125 LP740 DWH DLC WGX","IBL 36L WD SD125 LP740 DWH DLC WGX (CI-229U2N)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["221H7N","IBL 36L WD SD125 LP750 DLC","IBL 36L WD SD125 LP750 DLC (CI-221H7N)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236CVN","IBL 36L WD SD125 LP750 DLC USPOM","IBL 36L WD SD125 LP750 DLC USPOM (CI-236CVN)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236GXR","IBL 36L WD SD125 LP835 DWH","IBL 36L WD SD125 LP835 DWH (CI-236GXR)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234RLE","IBL 36L WD SD125 LP840 DWH WGX","IBL 36L WD SD125 LP840 DWH WGX (CI-234RLE)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["229R5P","IBL 36L WD SD125 LP840 WGX","IBL 36L WD SD125 LP840 WGX (CI-229R5P)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["232RN2","IBL 36L WD SD125 LP850","IBL 36L WD SD125 LP850 (CI-232RN2)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238WRE","IBL 48L ND 208 LP750 DLC XPW","IBL 48L ND 208 LP750 DLC XPW (CI-238WRE)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["226Y07","IBL 48L ND 277 CS11W LP740 DLC","IBL 48L ND 277 CS11W LP740 DLC (CI-226Y07)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238GPA","IBL 48L ND 277 CS11W LP740 DLC NPP16D WGX","IBL 48L ND 277 CS11W LP740 DLC NPP16D WGX (CI-238GPA)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["222LH8","IBL 48L ND 277 CS11W LP750 DLC","IBL 48L ND 277 CS11W LP750 DLC (CI-222LH8)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["223CP2","IBL 48L ND 277 CS11WL10 LP750 DLC","IBL 48L ND 277 CS11WL10 LP750 DLC (CI-223CP2)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["229P5M","IBL 48L ND 277 CS11WL10 LP750 DLC MSE360","IBL 48L ND 277 CS11WL10 LP750 DLC MSE360 (CI-229P5M)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235GE7","IBL 48L ND 277 CS11WL15 LP750 DLC MSI6XADL DSCXADL","IBL 48L ND 277 CS11WL15 LP750 DLC MSI6XADL DSCXADL (CI-235GE7)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238GHF","IBL 48L ND 277 LP740 DLC LAM0SZU","IBL 48L ND 277 LP740 DLC LAM0SZU (CI-238GHF)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235G02","IBL 48L ND 277 LP740 DLC XPW","IBL 48L ND 277 LP740 DLC XPW (CI-235G02)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238NX7","IBL 48L ND 277 OCS10 LP750 DLC","IBL 48L ND 277 OCS10 LP750 DLC (CI-238NX7)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237EK6","IBL 48L ND 277 OCS10 LP750 DLC LAPZU","IBL 48L ND 277 OCS10 LP750 DLC LAPZU (CI-237EK6)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["222V09","IBL 48L ND CS93W LP750 DLC","IBL 48L ND CS93W LP750 DLC (CI-222V09)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["220G75","IBL 48L ND LP740 DLC","IBL 48L ND LP740 DLC (CI-220G75)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["225LU6","IBL 48L ND LP740 DLC OUTCTR","IBL 48L ND LP740 DLC OUTCTR (CI-225LU6)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238E1Y","IBL 48L ND LP740 DWH DLC","IBL 48L ND LP740 DWH DLC (CI-238E1Y)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["220G76","IBL 48L ND LP750 DLC","IBL 48L ND LP750 DLC (CI-220G76)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["232E72","IBL 48L ND LP750 DLC OUTCTR","IBL 48L ND LP750 DLC OUTCTR (CI-232E72)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["225RAL","IBL 48L ND LP840","IBL 48L ND LP840 (CI-225RAL)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236WGA","IBL 48L ND SD125 277 CS11W LP740 DWH DLC XPW","IBL 48L ND SD125 277 CS11W LP740 DWH DLC XPW (CI-236WGA)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237Y70","IBL 48L ND SD125 277 CS11W LP750 DLC","IBL 48L ND SD125 277 CS11W LP750 DLC (CI-237Y70)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237Y66","IBL 48L ND SD125 277 CS93WL12 LP750 DLC MSI6XADL DSCXADL","IBL 48L ND SD125 277 CS93WL12 LP750 DLC MSI6XADL DSCXADL (CI-237Y66)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235A13","IBL 48L ND SD125 277 LP740 DLC LAOZU","IBL 48L ND SD125 277 LP740 DLC LAOZU (CI-235A13)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["233FPE","IBL 48L ND SD125 277 LP750 DLC MSI6XADL DSCXADL","IBL 48L ND SD125 277 LP750 DLC MSI6XADL DSCXADL (CI-233FPE)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237Y5V","IBL 48L ND SD125 277 OCS LP850","IBL 48L ND SD125 277 OCS LP850 (CI-237Y5V)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237N96","IBL 48L ND SD125 CS93W LP840 WGX","IBL 48L ND SD125 CS93W LP840 WGX (CI-237N96)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["220HP4","IBL 48L ND SD125 LP740 DLC","IBL 48L ND SD125 LP740 DLC (CI-220HP4)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239T07","IBL 48L ND SD125 LP740 DLC OUTCTR","IBL 48L ND SD125 LP740 DLC OUTCTR (CI-239T07)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237LJY","IBL 48L ND SD125 LP740 DLC OUTCTR USPOM","IBL 48L ND SD125 LP740 DLC OUTCTR USPOM (CI-237LJY)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
[{"$f":"(LEFT((RIGHT(C26268,7)),6))","v":"231MY0"},{"$f":"LEFT(C26268,SEARCH(\"(CI-\",C26268)-2)","v":"IBL 48L ND SD125 LP740 DWH DLC"},"IBL 48L ND SD125 LP740 DWH DLC (CI-231MY0)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["220HPK","IBL 48L ND SD125 LP750 DLC","IBL 48L ND SD125 LP750 DLC (CI-220HPK)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235V37","IBL 48L ND SD125 LP750 DWH DLC","IBL 48L ND SD125 LP750 DWH DLC (CI-235V37)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["234U5U","IBL 48L ND SD125 LP835 WGX","IBL 48L ND SD125 LP835 WGX (CI-234U5U)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["226EYM","IBL 48L ND SD125 LP840","IBL 48L ND SD125 LP840 (CI-226EYM)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235KJL","IBL 48L ND SD125 LP840 DWH","IBL 48L ND SD125 LP840 DWH (CI-235KJL)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["230XCX","IBL 48L ND SD125 LP850","IBL 48L ND SD125 LP850 (CI-230XCX)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237YGU","IBL 48L WD 120 LP740 DLC MSE360","IBL 48L WD 120 LP740 DLC MSE360 (CI-237YGU)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235ENK","IBL 48L WD 120 LP835 NPP16D","IBL 48L WD 120 LP835 NPP16D (CI-235ENK)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235WRL","IBL 48L WD 208 CS93WL20 LP750 DLC LAM04TU","IBL 48L WD 208 CS93WL20 LP750 DLC LAM04TU (CI-235WRL)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235VTX","IBL 48L WD 208 CS93WL20 LP750 DLC LAOZU","IBL 48L WD 208 CS93WL20 LP750 DLC LAOZU (CI-235VTX)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["223J61","IBL 48L WD 277 CS11W LP740 DLC","IBL 48L WD 277 CS11W LP740 DLC (CI-223J61)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236E8N","IBL 48L WD 277 CS11W LP840","IBL 48L WD 277 CS11W LP840 (CI-236E8N)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237WR0","IBL 48L WD 277 CS11W LP850","IBL 48L WD 277 CS11W LP850 (CI-237WR0)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["232F80","IBL 48L WD 277 GLR IMP LP750 DLC","IBL 48L WD 277 GLR IMP LP750 DLC (CI-232F80)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236G95","IBL 48L WD 277 LP740 DLC MSE360","IBL 48L WD 277 LP740 DLC MSE360 (CI-236G95)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238XG4","IBL 48L WD 277 LP750 DLC LAOZU","IBL 48L WD 277 LP750 DLC LAOZU (CI-238XG4)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235JFG","IBL 48L WD 277 LP750 DLC OUTCTR LAOZU","IBL 48L WD 277 LP750 DLC OUTCTR LAOZU (CI-235JFG)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["225RAF","IBL 48L WD 277 LP840 MSE360","IBL 48L WD 277 LP840 MSE360 (CI-225RAF)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236NMM","IBL 48L WD 277 OCS LP840","IBL 48L WD 277 OCS LP840 (CI-236NMM)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235CMP","IBL 48L WD 277 OCS20 LP740","IBL 48L WD 277 OCS20 LP740 (CI-235CMP)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237C5V","IBL 48L WD CS93W LP740 DLC","IBL 48L WD CS93W LP740 DLC (CI-237C5V)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["222V07","IBL 48L WD CS93W LP750 DLC","IBL 48L WD CS93W LP750 DLC (CI-222V07)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236U4J","IBL 48L WD CS93W LP850","IBL 48L WD CS93W LP850 (CI-236U4J)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["232P96","IBL 48L WD CS93WL15 LP750 DLC","IBL 48L WD CS93WL15 LP750 DLC (CI-232P96)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235VU2","IBL 48L WD CS93WL20 LP750 DLC","IBL 48L WD CS93WL20 LP750 DLC (CI-235VU2)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["220HN3","IBL 48L WD LP740 DLC","IBL 48L WD LP740 DLC (CI-220HN3)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["226EUM","IBL 48L WD LP740 DWH DLC","IBL 48L WD LP740 DWH DLC (CI-226EUM)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["220HP6","IBL 48L WD LP750 DLC","IBL 48L WD LP750 DLC (CI-220HP6)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235WRR","IBL 48L WD LP750 DLC OUTCTR","IBL 48L WD LP750 DLC OUTCTR (CI-235WRR)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["238M0K","IBL 48L WD LP750 DWH DLC NOM","IBL 48L WD LP750 DWH DLC NOM (CI-238M0K)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["230R47","IBL 48L WD LP835","IBL 48L WD LP835 (CI-230R47)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["233WHX","IBL 48L WD LP835 WGX","IBL 48L WD LP835 WGX (CI-233WHX)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["226E0Y","IBL 48L WD LP840","IBL 48L WD LP840 (CI-226E0Y)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237RJU","IBL 48L WD LP840 DWH","IBL 48L WD LP840 DWH (CI-237RJU)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["231WX2","IBL 48L WD LP840 WGX","IBL 48L WD LP840 WGX (CI-231WX2)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["231X7R","IBL 48L WD LP850","IBL 48L WD LP850 (CI-231X7R)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237RK4","IBL 48L WD LP850 DWH","IBL 48L WD LP850 DWH (CI-237RK4)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["229AYF","IBL 48L WD LP850 USPOM","IBL 48L WD LP850 USPOM (CI-229AYF)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235ENA","IBL 48L WD SD125 120 CS1W LP840","IBL 48L WD SD125 120 CS1W LP840 (CI-235ENA)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["228EKH","IBL 48L WD SD125 277 CS11W LP740 DLC","IBL 48L WD SD125 277 CS11W LP740 DLC (CI-228EKH)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236PP2","IBL 48L WD SD125 277 CS11W LP750 DLC","IBL 48L WD SD125 277 CS11W LP750 DLC (CI-236PP2)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237VWH","IBL 48L WD SD125 277 CS11W LP840","IBL 48L WD SD125 277 CS11W LP840 (CI-237VWH)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237JP5","IBL 48L WD SD125 277 CS11WL10 LP740 DLC","IBL 48L WD SD125 277 CS11WL10 LP740 DLC (CI-237JP5)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237Y6M","IBL 48L WD SD125 277 CS93WL12 LP750 DLC MSI6XADL DSCXADL","IBL 48L WD SD125 277 CS93WL12 LP750 DLC MSI6XADL DSCXADL (CI-237Y6M)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239JJ6","IBL 48L WD SD125 277 LP740 DLC XPW","IBL 48L WD SD125 277 LP740 DLC XPW (CI-239JJ6)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237K3M","IBL 48L WD SD125 277 LP840 DWH LAM0SZU","IBL 48L WD SD125 277 LP840 DWH LAM0SZU (CI-237K3M)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236H9W","IBL 48L WD SD125 277 LP840 DWH OUTCTR LAOZU WGX","IBL 48L WD SD125 277 LP840 DWH OUTCTR LAOZU WGX (CI-236H9W)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236P5F","IBL 48L WD SD125 277 LP840 NMSI360D","IBL 48L WD SD125 277 LP840 NMSI360D (CI-236P5F)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236NLV","IBL 48L WD SD125 277 LP850 LAM0SZU","IBL 48L WD SD125 277 LP850 LAM0SZU (CI-236NLV)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239FMX","IBL 48L WD SD125 277 OCS LP750 DLC","IBL 48L WD SD125 277 OCS LP750 DLC (CI-239FMX)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["235TA0","IBL 48L WD SD125 277 OCS10 LP840","IBL 48L WD SD125 277 OCS10 LP840 (CI-235TA0)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["224AGF","IBL 48L WD SD125 CS93W LP750 DLC","IBL 48L WD SD125 CS93W LP750 DLC (CI-224AGF)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237Y5Y","IBL 48L WD SD125 CS93WL12 LP750 DLC","IBL 48L WD SD125 CS93WL12 LP750 DLC (CI-237Y5Y)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237LV2","IBL 48L WD SD125 LP735","IBL 48L WD SD125 LP735 (CI-237LV2)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["220HNT","IBL 48L WD SD125 LP740 DLC","IBL 48L WD SD125 LP740 DLC (CI-220HNT)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["220MY3","IBL 48L WD SD125 LP740 DLC WGX","IBL 48L WD SD125 LP740 DLC WGX (CI-220MY3)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["220HP7","IBL 48L WD SD125 LP750 DLC","IBL 48L WD SD125 LP750 DLC (CI-220HP7)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["236CW0","IBL 48L WD SD125 LP750 DLC USPOM","IBL 48L WD SD125 LP750 DLC USPOM (CI-236CW0)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["225A4R","IBL 48L WD SD125 LP750 DLC WGX","IBL 48L WD SD125 LP750 DLC WGX (CI-225A4R)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["239AR4","IBL 48L WD SD125 LP840 DWH","IBL 48L WD SD125 LP840 DWH (CI-239AR4)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["237LV8","IBL 48L WD SD125 LP850","IBL 48L WD SD125 LP850 (CI-237LV8)","PS30250","Remote mount only","None","PS30250@250VDC_4 Boards in parallel Instructions","*251PT0"]
["229GNH","IBL 9L ND 120 CS3W LP740 DLC","IBL 9L ND 120 CS3W LP740 DLC (CI-229GNH)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["237EF2","IBL 9L ND 277 CS11WL15 LP740 DLC","IBL 9L ND 277 CS11WL15 LP740 DLC (CI-237EF2)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
[{"$f":"(LEFT((RIGHT(C26332,7)),6))","v":"234MLJ"},{"$f":"LEFT(C26332,SEARCH(\"(CI-\",C26332)-2)","v":"IBL 9L ND 277 LP840 LAM0SZU"},"IBL 9L ND 277 LP840 LAM0SZU (CI-234MLJ)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["237K2Y","IBL 9L ND 277 LP840 LCOZU","IBL 9L ND 277 LP840 LCOZU (CI-237K2Y)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["214P01","IBL 9L ND LP740 DLC","IBL 9L ND LP740 DLC (CI-214P01)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["226A45","IBL 9L ND LP740 DLC NOM","IBL 9L ND LP740 DLC NOM (CI-226A45)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["214NYU","IBL 9L ND LP750 DLC","IBL 9L ND LP750 DLC (CI-214NYU)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["237K3C","IBL 9L ND LP840","IBL 9L ND LP840 (CI-237K3C)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["238H1F","IBL 9L ND SD125 277 LP840 DWH NMSI360D","IBL 9L ND SD125 277 LP840 DWH NMSI360D (CI-238H1F)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["238H1E","IBL 9L ND SD125 277 LP840 DWH NMSID","IBL 9L ND SD125 277 LP840 DWH NMSID (CI-238H1E)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["234TFV","IBL 9L ND SD125 CS93W LP740 DLC","IBL 9L ND SD125 CS93W LP740 DLC (CI-234TFV)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["223GCF","IBL 9L ND SD125 LP740 DLC","IBL 9L ND SD125 LP740 DLC (CI-223GCF)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["236GX3","IBL 9L ND SD125 LP740 DWH DLC","IBL 9L ND SD125 LP740 DWH DLC (CI-236GX3)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["239U7G","IBL 9L ND SD125 LP740 DWH DLC WGX","IBL 9L ND SD125 LP740 DWH DLC WGX (CI-239U7G)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["226CHH","IBL 9L ND SD125 LP835","IBL 9L ND SD125 LP835 (CI-226CHH)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["238H15","IBL 9L ND SD125 LP840 DWH","IBL 9L ND SD125 LP840 DWH (CI-238H15)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["237HEY","IBL 9L ND SD125 LP850","IBL 9L ND SD125 LP850 (CI-237HEY)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["235Y1F","IBL 9L ND SD125 LP850 WGX","IBL 9L ND SD125 LP850 WGX (CI-235Y1F)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["230C41","IBL 9L WD 120 CS1W LP750 DLC","IBL 9L WD 120 CS1W LP750 DLC (CI-230C41)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["237N8F","IBL 9L WD 120 CS1W LP850","IBL 9L WD 120 CS1W LP850 (CI-237N8F)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["233P0P","IBL 9L WD 120 CS3W LP740 DLC","IBL 9L WD 120 CS3W LP740 DLC (CI-233P0P)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["236RAW","IBL 9L WD 120 CS3W LP840 LAOZU WGX","IBL 9L WD 120 CS3W LP840 LAOZU WGX (CI-236RAW)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["236UC3","IBL 9L WD 120 CS3W LP840 WGX","IBL 9L WD 120 CS3W LP840 WGX (CI-236UC3)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["237TUR","IBL 9L WD 120 GLR LP740 DWH DLC OUTCTR WGX","IBL 9L WD 120 GLR LP740 DWH DLC OUTCTR WGX (CI-237TUR)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["234HFH","IBL 9L WD 120 LP835 LAM0SZU","IBL 9L WD 120 LP835 LAM0SZU (CI-234HFH)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["237X4G","IBL 9L WD 120 LP840 DWH LAH0SZU WGX","IBL 9L WD 120 LP840 DWH LAH0SZU WGX (CI-237X4G)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["236RAL","IBL 9L WD 120 LP840 LAPZU","IBL 9L WD 120 LP840 LAPZU (CI-236RAL)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["228YE0","IBL 9L WD 277 CS11W LP840","IBL 9L WD 277 CS11W LP840 (CI-228YE0)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["239JWV","IBL 9L WD 277 CS11W LP840 LBM0SZU","IBL 9L WD 277 CS11W LP840 LBM0SZU (CI-239JWV)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["239JWU","IBL 9L WD 277 CS93WL10 LP750 DLC NPP16D","IBL 9L WD 277 CS93WL10 LP750 DLC NPP16D (CI-239JWU)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["230YPG","IBL 9L WD 277 LP740 DLC LAOZU","IBL 9L WD 277 LP740 DLC LAOZU (CI-230YPG)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["227H1C","IBL 9L WD 277 LP740 DLC NPP16D","IBL 9L WD 277 LP740 DLC NPP16D (CI-227H1C)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["233YJM","IBL 9L WD 277 LP750 DLC LAM0SZU","IBL 9L WD 277 LP750 DLC LAM0SZU (CI-233YJM)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["234PML","IBL 9L WD 277 LP840 LAOZU","IBL 9L WD 277 LP840 LAOZU (CI-234PML)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["237HET","IBL 9L WD 277 LP840 MSE360","IBL 9L WD 277 LP840 MSE360 (CI-237HET)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["238AW1","IBL 9L WD 347 IMP LP740 DLC","IBL 9L WD 347 IMP LP740 DLC (CI-238AW1)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["238CNA","IBL 9L WD 480 OCS LP740 DLC","IBL 9L WD 480 OCS LP740 DLC (CI-238CNA)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["235JH1","IBL 9L WD CS93WL10 LP740 DLC","IBL 9L WD CS93WL10 LP740 DLC (CI-235JH1)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["227MHY","IBL 9L WD LP735","IBL 9L WD LP735 (CI-227MHY)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["214NYT","IBL 9L WD LP740 DLC","IBL 9L WD LP740 DLC (CI-214NYT)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["224MNN","IBL 9L WD LP740 DLC WGX","IBL 9L WD LP740 DLC WGX (CI-224MNN)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["229NNW","IBL 9L WD LP740 DWH DLC","IBL 9L WD LP740 DWH DLC (CI-229NNW)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["214PLN","IBL 9L WD LP750","IBL 9L WD LP750 (CI-214PLN)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["214NYM","IBL 9L WD LP750 DLC","IBL 9L WD LP750 DLC (CI-214NYM)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["239A6F","IBL 9L WD LP750 DLC NOM","IBL 9L WD LP750 DLC NOM (CI-239A6F)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["237YFH","IBL 9L WD LP750 DLC WGX","IBL 9L WD LP750 DLC WGX (CI-237YFH)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["231CJN","IBL 9L WD LP835","IBL 9L WD LP835 (CI-231CJN)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["235L44","IBL 9L WD LP835 WGX","IBL 9L WD LP835 WGX (CI-235L44)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["230HUP","IBL 9L WD LP840","IBL 9L WD LP840 (CI-230HUP)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["236FLM","IBL 9L WD LP840 DWH","IBL 9L WD LP840 DWH (CI-236FLM)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["236CTU","IBL 9L WD LP840 DWH WGX","IBL 9L WD LP840 DWH WGX (CI-236CTU)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["233T18","IBL 9L WD LP840 WGX","IBL 9L WD LP840 WGX (CI-233T18)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["226VNC","IBL 9L WD LP850","IBL 9L WD LP850 (CI-226VNC)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["226YC4","IBL 9L WD SD125 120 CS1W LP740 DLC","IBL 9L WD SD125 120 CS1W LP740 DLC (CI-226YC4)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["237EF7","IBL 9L WD SD125 120 CS3W LP750 DLC","IBL 9L WD SD125 120 CS3W LP750 DLC (CI-237EF7)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["236LWC","IBL 9L WD SD125 120 CS3WL10 LP750 DLC","IBL 9L WD SD125 120 CS3WL10 LP750 DLC (CI-236LWC)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["235CLR","IBL 9L WD SD125 120 GLR LP740 DLC LAOZU","IBL 9L WD SD125 120 GLR LP740 DLC LAOZU (CI-235CLR)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["238A53","IBL 9L WD SD125 120 LP750 DLC MSE360 WGX","IBL 9L WD SD125 120 LP750 DLC MSE360 WGX (CI-238A53)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["237X47","IBL 9L WD SD125 120 LP750 DLC NMSI360D","IBL 9L WD SD125 120 LP750 DLC NMSI360D (CI-237X47)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["236ELX","IBL 9L WD SD125 120 LP840 LAH0SZU","IBL 9L WD SD125 120 LP840 LAH0SZU (CI-236ELX)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["236V0A","IBL 9L WD SD125 120 LP850 MSE360","IBL 9L WD SD125 120 LP850 MSE360 (CI-236V0A)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["232PA6","IBL 9L WD SD125 277 CS11W LP750 DLC","IBL 9L WD SD125 277 CS11W LP750 DLC (CI-232PA6)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["237EFC","IBL 9L WD SD125 277 CS11W LP750 DLC MSE360","IBL 9L WD SD125 277 CS11W LP750 DLC MSE360 (CI-237EFC)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["229NN3","IBL 9L WD SD125 277 CS11W LP840 DWH","IBL 9L WD SD125 277 CS11W LP840 DWH (CI-229NN3)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["239AXF","IBL 9L WD SD125 277 CS11W LP840 DWH NPP16D WGX","IBL 9L WD SD125 277 CS11W LP840 DWH NPP16D WGX (CI-239AXF)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["237K0W","IBL 9L WD SD125 277 CS7WL10 LP750 DLC","IBL 9L WD SD125 277 CS7WL10 LP750 DLC (CI-237K0W)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
[{"$f":"(LEFT((RIGHT(C26396,7)),6))","v":"239A6J"},{"$f":"LEFT(C26396,SEARCH(\"(CI-\",C26396)-2)","v":"IBL 9L WD SD125 277 CS93W LP840 LAH0SZU"},"IBL 9L WD SD125 277 CS93W LP840 LAH0SZU (CI-239A6J)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["237NY2","IBL 9L WD SD125 277 GLR LP835","IBL 9L WD SD125 277 GLR LP835 (CI-237NY2)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["235JH7","IBL 9L WD SD125 277 LP740 DLC LAOZU","IBL 9L WD SD125 277 LP740 DLC LAOZU (CI-235JH7)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["229P4V","IBL 9L WD SD125 277 LP740 DLC NMSI360D","IBL 9L WD SD125 277 LP740 DLC NMSI360D (CI-229P4V)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["237YFL","IBL 9L WD SD125 277 LP750 DLC NPP16D","IBL 9L WD SD125 277 LP750 DLC NPP16D (CI-237YFL)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["232VYJ","IBL 9L WD SD125 277 LP840 LAOZU","IBL 9L WD SD125 277 LP840 LAOZU (CI-232VYJ)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["235TM9","IBL 9L WD SD125 277 LP840 LAPZU","IBL 9L WD SD125 277 LP840 LAPZU (CI-235TM9)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["238R3K","IBL 9L WD SD125 277 LP840 LAPZU WGX","IBL 9L WD SD125 277 LP840 LAPZU WGX (CI-238R3K)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["235JHF","IBL 9L WD SD125 277 LP840 NPP16D","IBL 9L WD SD125 277 LP840 NPP16D (CI-235JHF)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["236G8W","IBL 9L WD SD125 277 LP840 NPP16D WGX","IBL 9L WD SD125 277 LP840 NPP16D WGX (CI-236G8W)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["239R6Y","IBL 9L WD SD125 277 OCS10 GMF LP750 DLC","IBL 9L WD SD125 277 OCS10 GMF LP750 DLC (CI-239R6Y)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["238A6X","IBL 9L WD SD125 347 LP740 DWH DLC NPP16D","IBL 9L WD SD125 347 LP740 DWH DLC NPP16D (CI-238A6X)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["229N3R","IBL 9L WD SD125 CS93W LP835","IBL 9L WD SD125 CS93W LP835 (CI-229N3R)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["232RY7","IBL 9L WD SD125 LP735","IBL 9L WD SD125 LP735 (CI-232RY7)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["236A82","IBL 9L WD SD125 LP735 DWH","IBL 9L WD SD125 LP735 DWH (CI-236A82)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["236KFV","IBL 9L WD SD125 LP735 WGX","IBL 9L WD SD125 LP735 WGX (CI-236KFV)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["224R55","IBL 9L WD SD125 LP740 DLC","IBL 9L WD SD125 LP740 DLC (CI-224R55)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["226Y2T","IBL 9L WD SD125 LP740 DLC DWH","IBL 9L WD SD125 LP740 DLC DWH (CI-226Y2T)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["223LH4","IBL 9L WD SD125 LP740 DLC USPOM","IBL 9L WD SD125 LP740 DLC USPOM (CI-223LH4)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["224R1U","IBL 9L WD SD125 LP740 DLC WGX","IBL 9L WD SD125 LP740 DLC WGX (CI-224R1U)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["228CPF","IBL 9L WD SD125 LP740 DWH DLC","IBL 9L WD SD125 LP740 DWH DLC (CI-228CPF)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["231CFK","IBL 9L WD SD125 LP740 DWH DLC OUTCTR","IBL 9L WD SD125 LP740 DWH DLC OUTCTR (CI-231CFK)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["238R87","IBL 9L WD SD125 LP740 DWH DLC USPOM","IBL 9L WD SD125 LP740 DWH DLC USPOM (CI-238R87)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["217TCV","IBL 9L WD SD125 LP750","IBL 9L WD SD125 LP750 (CI-217TCV)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["223H6L","IBL 9L WD SD125 LP750 DLC","IBL 9L WD SD125 LP750 DLC (CI-223H6L)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["238JVA","IBL 9L WD SD125 LP750 DLC NOM","IBL 9L WD SD125 LP750 DLC NOM (CI-238JVA)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["227GC6","IBL 9L WD SD125 LP835","IBL 9L WD SD125 LP835 (CI-227GC6)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["229FYF","IBL 9L WD SD125 LP840","IBL 9L WD SD125 LP840 (CI-229FYF)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["229J3M","IBL 9L WD SD125 LP840 DWH","IBL 9L WD SD125 LP840 DWH (CI-229J3M)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["231EMM","IBL 9L WD SD125 LP840 DWH WGX","IBL 9L WD SD125 LP840 DWH WGX (CI-231EMM)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["238CHW","IBL 9L WD SD125 LP840 WGX","IBL 9L WD SD125 LP840 WGX (CI-238CHW)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["229XG0","IBL 9L WD SD125 LP850","IBL 9L WD SD125 LP850 (CI-229XG0)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]
["232TE9","IBL 9L WD SD125 LP850 DWH","IBL 9L WD SD125 LP850 DWH (CI-232TE9)","PS30250","Remote mount only","None","PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","*251PT0"]

{"sheet":"Field Install Kits","index":2,"n_rows":54,"n_cols":4,"rows_kept":54,"cut":false,"hidden":false,"merged":[]}
["Field Install Instruction","Description","Catalog Number","Nomenclature"]
["*239MPR","PS730L For Field Installation","PS730L FIK",{"$f":"IF(ISBLANK(A2),\"\",CONCATENATE(C2,\" (CI-\",RIGHT(A2,6),\")\"))","v":"PS730L FIK (CI-239MPR)"}]
["*239MPW","PS730L with ELA PSRME IC for Field installation","PS730L FIKRE",{"$f":"IF(ISBLANK(A3),\"\",CONCATENATE(C3,\" (CI-\",RIGHT(A3,6),\")\"))","v":"PS730L FIKRE (CI-239MPW)"}]
["*239MR0","PS750L For Field Installation","PS750L FIK","PS750L FIK (CI-239MR0)"]
["*239MR4","PS750L with ELA PSRME IC for Field Installation","PS750L FIKRE","PS750L FIKRE (CI-239MR4)"]
["*239MR7","PS1030 For Field Installation","PS1030 FIK","PS1030 FIK (CI-239MR7)"]
["*239MR9","PS1030 with ELA PSRME IC for Field Installation","PS1030 FIKRE","PS1030 FIKRE (CI-239MR9)"]
["*239MRC","PS1050 For Field Installation","PS1050 FIK","PS1050 FIK (CI-239MRC)"]
["*239MRJ","PS1050 with ELA PSRME IC for Field Installation","PS1050 FIKRE","PS1050 FIKRE (CI-239MRJ)"]
["*251PRK","PS1050DL Field installation kit","PS1050DL FIK","PS1050DL FIK (CI-251PRK)"]
["*251PT0","PS30250 Field installation kit","PS30250 FIK","PS30250 FIK (CI-251PT0)"]
[]
[]
[null,null,null,{"$f":"IF(ISBLANK(A14),\"\",CONCATENATE(C14,\" (CI-\",RIGHT(A14,6),\")\"))","v":""}]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]
[null,null,null,""]

{"sheet":"Wiring","index":3,"n_rows":12,"n_cols":2,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
["Field Install Instruction","Address"]
["2 Boards in series & 2 Boards in parallel instructions","http://www.acuitybrands.com/products/detail/369448/Power-Sentry/PS1050/Reduced-Profile-LED-Emergency-Battery-Pack/-/media/products/Power_Sentry/369448/document/Power-Sentry-Field-Install-Instructions-2BS-2BP_pdf.pdf"]
["1 Board instructions","http://www.acuitybrands.com/products/detail/272879/Power-Sentry/PS1030/Emergency-LED-Battery-Backup/-/media/products/Power_Sentry/272879/document/Power-Sentry-Field-Install-Instructions-1B_pdf.pdf"]
["2 Boards in series instructions","http://www.acuitybrands.com/products/detail/369448/Power-Sentry/PS1050/Reduced-Profile-LED-Emergency-Battery-Pack/-/media/products/Power_Sentry/369448/document/Power-Sentry-Field-Install-Instructions-2BS_pdf.pdf"]
["3 Boards in parallel instructions","http://www.acuitybrands.com/products/detail/272879/Power-Sentry/PS1030/Emergency-LED-Battery-Backup/-/media/products/Power_Sentry/272879/document/Power-Sentry-Field-Install-Instructions-3BP_pdf.pdf"]
["2 Boards in parallel instructions","http://www.acuitybrands.com/products/detail/272879/Power-Sentry/PS1030/Emergency-LED-Battery-Backup/-/media/products/Power_Sentry/272879/document/Power-Sentry-Field-Install-Instructions-2BP_pdf.pdf"]
["4 Boards in parallel instructions","http://www.acuitybrands.com/products/detail/272879/Power-Sentry/PS1030/Emergency-LED-Battery-Backup/-/media/products/Power_Sentry/272879/document/Power-Sentry-Field-Install-Instructions-4BP_pdf.pdf"]
["PS30250@250VDC_3 Boards in series 2 Boards in parallel instructions","https://www.acuitybrands.com/products/detail/604739/Power-Sentry/PS30250/Emergency-LED-Battery-Backup/-/media/products/Power_Sentry/604739/document/Power-Sentry-Field-Install-Instructions-For-PS30250-3BS-2BP_pdf.pdf"]
["PS30250@100VDC_2 Boards in series 2 Boards in parallel instructions","https://www.acuitybrands.com/products/detail/604739/Power-Sentry/PS30250/Emergency-LED-Battery-Backup/-/media/products/Power_Sentry/604739/document/Power-Sentry-Field-Install-Instructions-For-PS30250-2BS-2BP_pdf.pdf"]
["1 Board instructions-DL","https://www.acuitybrands.com/products/detail/635710/Power-Sentry/PS1050DL/Emergency-LED-Battery-Backup/-/media/products/Power_Sentry/635710/document/Power-Sentry-Field-Install-Instructions-For-Downlighting_pdf.pdf"]
["PS30250@250VDC_2 Boards in parallel Instructions","https://www.acuitybrands.com/products/detail/604739/Power-Sentry/PS30250/Emergency-LED-Battery-Backup/-/media/products/Power_Sentry/604739/document/Power-Sentry-Field-Install-Instructions-For-PS30250-2BP_pdf.pdf"]
["PS30250@250VDC_4 Boards in parallel Instructions","https://www.acuitybrands.com/products/detail/604739/Power-Sentry/PS30250/Emergency-LED-Battery-Backup/-/media/products/Power_Sentry/604739/document/Power-Sentry-Field-Install-Instructions-For-PS30250-4BP_pdf.pdf"]

{"sheet":"PS Products","index":4,"n_rows":7,"n_cols":2,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
["PS Solution ","Address"]
["PS1050","http://www.acuitybrands.com/products/detail/369448/Power-Sentry/PS1050/Reduced-Profile-LED-Emergency-Battery-Pack/-/media/products/Power_Sentry/369448/document/PS1050_pdf.pdf"]
["PS1030","http://www.acuitybrands.com/products/detail/272879/Power-Sentry/PS1030/Emergency-LED-Battery-Backup/-/media/products/Power_Sentry/272879/document/PS1030_pdf.pdf"]
["PS750L","http://www.acuitybrands.com/products/detail/399070/Power-Sentry/PS730LPS750L/Emergency-Battery-Backup-for-Linear-LED-fixtures/-/media/products/Power_Sentry/399070/document/PS730L-Specification-Sheet_pdf.pdf"]
["PS730L","http://www.acuitybrands.com/products/detail/399070/Power-Sentry/PS730LPS750L/Emergency-Battery-Backup-for-Linear-LED-fixtures/-/media/products/Power_Sentry/399070/document/PS750L-Specification-Sheet_pdf.pdf"]
["PS30250","https://www.acuitybrands.com/products/detail/604739/Power-Sentry/PS30250/Emergency-LED-Battery-Backup/-/media/products/Power_Sentry/604739/document/PS30250_pdf.pdf"]
["PS1050DL","https://www.acuitybrands.com/products/detail/635710/Power-Sentry/PS1050DL/Emergency-LED-Battery-Backup/-/media/products/Power_Sentry/635710/document/PS1050DL_pdf.pdf"]